
hpeesofsim (*) 490.shp Nov 12 2018, MINT version 4
    (64-bit windows built: Tue Nov 13, 2018 02:20:54 +0000)


CT Sweep2[1] <DAC39RF10_dacout_lib:VoltageSource:schematic>   cornerid=(1->3)

AC Sweep2[1].AC1[1/3] <DAC39RF10_dacout_lib:VoltageSource:schematic>  cornerid=1  freq=(10 MHz->20 GHz)


AC Sweep2[1].AC1[2/3] <DAC39RF10_dacout_lib:VoltageSource:schematic>  cornerid=2  freq=(10 MHz->20 GHz)


AC Sweep2[1].AC1[3/3] <DAC39RF10_dacout_lib:VoltageSource:schematic>  cornerid=3  freq=(10 MHz->20 GHz)


Resource usage:
  Total stopwatch time     =     5.96 seconds.

