# TRF1208 ADS Model

2 Tone Harmonic Balance and S-parameter simulation testbenches designed to be used as a starting point for circuit analysis using 
the TRF1208 fully differential amplifier.

## Setup

1. Unzip this folder to an accessible location
2. Open Advanced System Design (ADS)
3. Click Unarchive (Under commands in startup page or File>Unarchive from main page)
4. Locate the zipped archive file (.7zads) and select open
5. Set the destination folder you would like to unarchive the workspace into
6. Open a testbench schematic and click the simulate button

