VNA settings
RF power -10dBm
IF freq: 1kHz
start freq: 10MHz
stop freq: 20GHz
401 points
char board input and output trace have been de-embedded at the instrument

port config:
	RX			TX
port 1					Port 2
   diff port 1 >>> DUT >>> diff port2
port 3					Port 4


file name description:
SN_channel_Vcc_temp_DC-config_EQ-config

EQ-config/17=EQ setting
DC-config: i.e. 80=1100mV linear range, 0dB DC gain