# Electrical Rule Check Report

Date: |  | 9/11/2025
Time: |  | 9:18:39 AM
Filename: |  | C:\Users\a0488740\AppData\Local\TempReleases\Snapshot\5\Validation\MCU178E1_ERC.html

Class | Document | Message
--- | --- | ---
Warning | MCU178E1_04_Power.SchDoc | +3V3_XDS110 contains Output Pin and Power Pin objects (Pin U3-1, Pin U5-14, Pin U5-16, Pin U9-8, Pin U15-7, Pin U15-8, Pin U15-9, Pin U15-16, Pin U15-26, Pin U15-28, Pin U15-39, Pin U15-47, Pin U15-51, Pin U15-52, Pin U15-69, Pin U15-79, Pin U15-90, Pin U15-101, Pin U15-113, Pin U15-122).
Warning | MCU178E1_10_Hardware.SchDoc | Component CE Logo1 CE Mark at 4200mil,9100mil: Component revision is Out of Date.
Warning | MCU178E1_08_MCAN.SchDoc | Component J6 61300311121: Component revision has inapplicable state
Warning | MCU178E1_03_USB-C.SchDoc | Component J8 61300211121: Component revision has inapplicable state
Warning | MCU178E1_03_USB-C.SchDoc | Component J9 61300211121: Component revision has inapplicable state
Warning | MCU178E1_05_AM13E230_MCU.SchDoc | Component J10 61300211121: Component revision has inapplicable state
Warning | MCU178E1_05_AM13E230_MCU.SchDoc | Component J11 61300211121: Component revision has inapplicable state
Warning | MCU178E1_05_AM13E230_MCU.SchDoc | Component J14 61300211121: Component revision has inapplicable state
Warning | MCU178E1_05_AM13E230_MCU.SchDoc | Component J15 61300211121: Component revision has inapplicable state
Warning | MCU178E1_04_Power.SchDoc | Component JP2 61300311121: Component revision has inapplicable state
Warning | MCU178E1_04_Power.SchDoc | Component JP3 61300311121: Component revision has inapplicable state
Warning | MCU178E1_08_MCAN.SchDoc | Component JP5 61300211121: Component revision has inapplicable state
Warning | MCU178E1_10_Hardware.SchDoc | Component Logo3 WEEE logo at 4200mil,8300mil: Component revision is Out of Date.
Warning | MCU178E1_04_Power.SchDoc | Component R15 ERJ-2GE0R00X: Component revision has inapplicable state
Warning | MCU178E1_05_AM13E230_MCU.SchDoc | Component R21 ERJ-2GE0R00X: Component revision has inapplicable state
Warning | MCU178E1_08_MCAN.SchDoc | Component R41 RC0603FR-07120RL: Component revision has inapplicable state
Warning | MCU178E1_08_MCAN.SchDoc | Component R42 ERJ-2GE0R00X: Component revision has inapplicable state
Warning | MCU178E1_08_MCAN.SchDoc | Component R48 ERJ-2GE0R00X: Component revision has inapplicable state
Warning | MCU178E1_08_MCAN.SchDoc | Component R49 ERJ-2GE0R00X: Component revision has inapplicable state
Warning | MCU178E1_04_Power.SchDoc | Component TP1 TESTPOINT at 14650mil,3250mil: Component revision is Out of Date.
Warning | MCU178E1_04_Power.SchDoc | Component TP2 TESTPOINT at 14650mil,2950mil: Component revision is Out of Date.
Warning | MCU178E1_04_Power.SchDoc | Component TP3 TESTPOINT at 14650mil,2650mil: Component revision is Out of Date.
Warning | MCU178E1_04_Power.SchDoc | Component TP4 TESTPOINT at 14700mil,2300mil: Component revision is Out of Date.
Warning | MCU178E1_05_AM13E230_MCU.SchDoc | Component TP5 TESTPOINT at 1500mil,6300mil: Component revision is Out of Date.
Warning | MCU178E1_05_AM13E230_MCU.SchDoc | Component TP6 TESTPOINT at 1500mil,6000mil: Component revision is Out of Date.
Warning | MCU178E1_08_MCAN.SchDoc | Component TP7 TESTPOINT at 6100mil,4200mil: Component revision is Out of Date.
Warning | MCU178E1_08_MCAN.SchDoc | Component TP8 TESTPOINT at 6100mil,3800mil: Component revision is Out of Date.
Warning | MCU178E1_09_XDS110.SchDoc | Component U9 TPD6E004RSER at 13000mil,5800mil: Component revision is Out of Date.
Warning | MCU178E1_09_XDS110.SchDoc | Component U11 TPD6E004RSER at 15300mil,5800mil: Component revision is Out of Date.
Warning | MCU178E1_05_AM13E230_MCU.SchDoc | Floating Power Object GND at (8600mil,3000mil)
Warning | MCU178E1_07_Headers.SchDoc | GND contains IO Pin and Power Pin objects (Pin U8-6, Pin U8-7, Pin U8-8, Pin U8-9, Pin U8-10, Pin U8-14, Pin U8-15, Pin U8-16, Pin U8-17, Pin U8-18, Pin J1/J3-22, Pin J2/J4-20, Pin U1-15, Pin U1-31, Pin U1-47, Pin U1-63, Pin U2-2, Pin U2-4, Pin U3-3, Pin U3-7, Pin U5-9, Pin U5-15, Pin U6-A2, Pin U7-2, Pin U8-11, Pin U8-12, Pin U8-13, Pin U9-4, Pin U10-2, Pin U11-4, Pin U14-2, Pin U15-10, Pin U15-17, Pin U15-48, Pin U15-55, Pin U15-58, Pin U15-80, Pin U15-114, Pin Y2-2, Pin Y2-4).
Warning | MCU178E1_10_Hardware.SchDoc | Incorrect link between project variant "001" and schematic component Component FID1 Fiducial
Warning | MCU178E1_10_Hardware.SchDoc | Incorrect link between project variant "001" and schematic component Component FID2 Fiducial
Warning | MCU178E1_10_Hardware.SchDoc | Incorrect link between project variant "001" and schematic component Component FID3 Fiducial
Warning | MCU178E1_09_XDS110.SchDoc | Net KEY has only one pin (Pin J7-7)

Back to top