
STEP {
    COL=1
    NAME=PCB
}


LAYER {
    ROW=1
    CONTEXT=BOARD
    TYPE=COMPONENT
    NAME=COMP_+_TOP
    POLARITY=POSITIVE
    START_NAME=
    END_NAME=
    OLD_NAME=
}

LAYER {
    ROW=2
    CONTEXT=BOARD
    TYPE=SOLDER_PASTE
    NAME=TOP_PASTE
    POLARITY=POSITIVE
    START_NAME=
    END_NAME=
    OLD_NAME=
}

LAYER {
    ROW=3
    CONTEXT=BOARD
    TYPE=SILK_SCREEN
    NAME=TOP_OVERLAY
    POLARITY=POSITIVE
    START_NAME=
    END_NAME=
    OLD_NAME=
}

LAYER {
    ROW=4
    CONTEXT=BOARD
    TYPE=SOLDER_MASK
    NAME=TOP_SOLDER
    POLARITY=POSITIVE
    START_NAME=
    END_NAME=
    OLD_NAME=
}

LAYER {
    ROW=5
    CONTEXT=BOARD
    TYPE=SIGNAL
    NAME=TOP_LAYER
    POLARITY=POSITIVE
    START_NAME=
    END_NAME=
    OLD_NAME=
}

LAYER {
    ROW=6
    CONTEXT=BOARD
    TYPE=DIELECTRIC
    NAME=DIELECTRIC_1
    POLARITY=POSITIVE
    START_NAME=
    END_NAME=
    OLD_NAME=
    DIELECTRIC_TYPE=PREPREG
    DIELECTRIC_NAME=FR-4
}

LAYER {
    ROW=7
    CONTEXT=BOARD
    TYPE=SIGNAL
    NAME=GROUND
    POLARITY=POSITIVE
    START_NAME=
    END_NAME=
    OLD_NAME=
}

LAYER {
    ROW=8
    CONTEXT=BOARD
    TYPE=DIELECTRIC
    NAME=DIELECTRIC_2
    POLARITY=POSITIVE
    START_NAME=
    END_NAME=
    OLD_NAME=
    DIELECTRIC_TYPE=CORE
    DIELECTRIC_NAME=FR-4
}

LAYER {
    ROW=9
    CONTEXT=BOARD
    TYPE=SIGNAL
    NAME=POWER
    POLARITY=POSITIVE
    START_NAME=
    END_NAME=
    OLD_NAME=
}

LAYER {
    ROW=10
    CONTEXT=BOARD
    TYPE=DIELECTRIC
    NAME=DIELECTRIC_3
    POLARITY=POSITIVE
    START_NAME=
    END_NAME=
    OLD_NAME=
    DIELECTRIC_TYPE=PREPREG
    DIELECTRIC_NAME=FR-4
}

LAYER {
    ROW=11
    CONTEXT=BOARD
    TYPE=SIGNAL
    NAME=BOTTOM_LAYER
    POLARITY=POSITIVE
    START_NAME=
    END_NAME=
    OLD_NAME=
}

LAYER {
    ROW=12
    CONTEXT=BOARD
    TYPE=SOLDER_MASK
    NAME=BOTTOM_SOLDER
    POLARITY=POSITIVE
    START_NAME=
    END_NAME=
    OLD_NAME=
}

LAYER {
    ROW=13
    CONTEXT=BOARD
    TYPE=SILK_SCREEN
    NAME=BOTTOM_OVERLAY
    POLARITY=POSITIVE
    START_NAME=
    END_NAME=
    OLD_NAME=
}

LAYER {
    ROW=14
    CONTEXT=BOARD
    TYPE=SOLDER_PASTE
    NAME=BOTTOM_PASTE
    POLARITY=POSITIVE
    START_NAME=
    END_NAME=
    OLD_NAME=
}

LAYER {
    ROW=15
    CONTEXT=BOARD
    TYPE=DRILL
    NAME=DRILL_PLATED_BOTTOM_LAYER-TOP_LAYER
    POLARITY=POSITIVE
    START_NAME=TOP_LAYER
    END_NAME=BOTTOM_LAYER
    OLD_NAME=
}

LAYER {
    ROW=16
    CONTEXT=BOARD
    TYPE=COMPONENT
    NAME=COMP_+_BOT
    POLARITY=POSITIVE
    START_NAME=
    END_NAME=
    OLD_NAME=
}

LAYER {
    ROW=17
    CONTEXT=MISC
    TYPE=DOCUMENT
    NAME=KEEP-OUT_LAYER
    POLARITY=POSITIVE
    START_NAME=
    END_NAME=
    OLD_NAME=
}

LAYER {
    ROW=18
    CONTEXT=MISC
    TYPE=DOCUMENT
    NAME=M1_BOARD_OUTLINE
    POLARITY=POSITIVE
    START_NAME=
    END_NAME=
    OLD_NAME=
}

LAYER {
    ROW=19
    CONTEXT=MISC
    TYPE=DOCUMENT
    NAME=M2_BOARD_DIMENSIONS
    POLARITY=POSITIVE
    START_NAME=
    END_NAME=
    OLD_NAME=
}

LAYER {
    ROW=20
    CONTEXT=MISC
    TYPE=DOCUMENT
    NAME=M9_TITLE_SHEET
    POLARITY=POSITIVE
    START_NAME=
    END_NAME=
    OLD_NAME=
}

LAYER {
    ROW=21
    CONTEXT=MISC
    TYPE=DOCUMENT
    NAME=M10_FAB_NOTES
    POLARITY=POSITIVE
    START_NAME=
    END_NAME=
    OLD_NAME=
}

LAYER {
    ROW=22
    CONTEXT=MISC
    TYPE=DOCUMENT
    NAME=M12_STACKUP
    POLARITY=POSITIVE
    START_NAME=
    END_NAME=
    OLD_NAME=
}

