#
#Component attribute names
#
@0 .comp_mount_type
@1 .comp_height

# CMP 0
CMP 2 3.3837795 1.780643 270 N R24 RC0603JR-071KL ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.yageo.com/pdf/Pu-RC0603_51_PbFree_L_2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Yageo'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'RC0603JR-071KL'
PRP Power_W '100mW'
PRP Res_ohm '1k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '311-1.0KGRCT-ND'
PRP Supplier_Part_Number_2 '603-RC0603JR-071KL'
PRP Supplier_Part_Number_3 '9233385'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '5%'
PRP Value '1.0k'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '1k00'
PRP ValueDisplayed '1.0k'
PRP VDC_V '75V'
TOP 0 3.3837795 1.7530839 180 N 74 7 1
TOP 1 3.3837795 1.808202 180 N 62 3 2
#
# CMP 1
CMP 16 1.2133137 0.5632321 270 N TP34 3V3_MCU ;0=2,1=0.1811
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName ''
PRP CNHeader 'FALSE'
PRP Color 'Red'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.keyelco.com/userAssets/file/M60-2p60.pdf'
PRP CompType 'Test Point'
PRP ContactFinish 'Silver'
PRP CT 'TRUE'
PRP Current_A ''
PRP Gender ''
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Keystone Electronics'
PRP MountType 'TH'
PRP Note ''
PRP Orientation ''
PRP PackageReference 'Red Miniature Testpoint'
PRP PartNumber '5000'
PRP PinCount ''
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '36-5000-ND'
PRP Supplier_Part_Number_2 '534-5000'
PRP Supplier_Part_Number_3 ''
PRP Voltage_V ''
TOP 0 1.2133137 0.5632321 270 N 59 22 1
#
# CMP 2
CMP 16 0.3744042 0.78437 270 N TP33 5V_USB ;0=2,1=0.1811
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName ''
PRP CNHeader 'FALSE'
PRP Color 'Red'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.keyelco.com/userAssets/file/M60-2p60.pdf'
PRP CompType 'Test Point'
PRP ContactFinish 'Silver'
PRP CT 'TRUE'
PRP Current_A ''
PRP Gender ''
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Keystone Electronics'
PRP MountType 'TH'
PRP Note ''
PRP Orientation ''
PRP PackageReference 'Red Miniature Testpoint'
PRP PartNumber '5000'
PRP PinCount ''
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '36-5000-ND'
PRP Supplier_Part_Number_2 '534-5000'
PRP Supplier_Part_Number_3 ''
PRP Voltage_V ''
TOP 0 0.3744042 0.78437 270 N 58 10 1
#
# CMP 3
CMP 16 1.0053917 0.5638312 270 N TP32 3V3COM ;0=2,1=0.1811
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName ''
PRP CNHeader 'FALSE'
PRP Color 'Red'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.keyelco.com/userAssets/file/M60-2p60.pdf'
PRP CompType 'Test Point'
PRP ContactFinish 'Silver'
PRP CT 'TRUE'
PRP Current_A ''
PRP Gender ''
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Keystone Electronics'
PRP MountType 'TH'
PRP Note ''
PRP Orientation ''
PRP PackageReference 'Red Miniature Testpoint'
PRP PartNumber '5000'
PRP PinCount ''
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '36-5000-ND'
PRP Supplier_Part_Number_2 '534-5000'
PRP Supplier_Part_Number_3 ''
PRP Voltage_V ''
TOP 0 1.0053917 0.5638312 270 N 60 15 1
#
# CMP 4
CMP 28 4.0325 2.6325 0 N H2 NY_PMS_440_0025_PH ;0=2,1=0.0750
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ClassName 'Mounting Holes'
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.fasnetdirect.com/refguide/Nylpanms.pdf'
PRP CompType 'Hardware'
PRP Key 'NY PMS 440 0025 PH'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'B&F Fastener Supply'
PRP MountType 'N/A'
PRP Note ''
PRP PackageReference 'Screw'
PRP PartNumber 'NY PMS 440 0025 PH'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'H542-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Value ''
TOP 0 4.0325 2.6325 0 N 0 53 1
#
# CMP 5
CMP 28 4.0325 0.2175 0 N H4 NY_PMS_440_0025_PH ;0=2,1=0.0750
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ClassName 'Mounting Holes'
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.fasnetdirect.com/refguide/Nylpanms.pdf'
PRP CompType 'Hardware'
PRP Key 'NY PMS 440 0025 PH'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'B&F Fastener Supply'
PRP MountType 'N/A'
PRP Note ''
PRP PackageReference 'Screw'
PRP PartNumber 'NY PMS 440 0025 PH'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'H542-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Value ''
TOP 0 4.0325 0.2175 0 N 0 52 1
#
# CMP 6
CMP 28 0.2175 0.2175 0 N H3 NY_PMS_440_0025_PH ;0=2,1=0.0750
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ClassName 'Mounting Holes'
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.fasnetdirect.com/refguide/Nylpanms.pdf'
PRP CompType 'Hardware'
PRP Key 'NY PMS 440 0025 PH'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'B&F Fastener Supply'
PRP MountType 'N/A'
PRP Note ''
PRP PackageReference 'Screw'
PRP PartNumber 'NY PMS 440 0025 PH'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'H542-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Value ''
TOP 0 0.2175 0.2175 0 N 0 51 1
#
# CMP 7
CMP 28 0.2175 2.6325 0 N H1 NY_PMS_440_0025_PH ;0=2,1=0.0750
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ClassName 'Mounting Holes'
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.fasnetdirect.com/refguide/Nylpanms.pdf'
PRP CompType 'Hardware'
PRP Key 'NY PMS 440 0025 PH'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'B&F Fastener Supply'
PRP MountType 'N/A'
PRP Note ''
PRP PackageReference 'Screw'
PRP PartNumber 'NY PMS 440 0025 PH'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'H542-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Value ''
TOP 0 0.2175 2.6325 0 N 0 50 1
#
# CMP 8
CMP 26 3.1093238 1.5604393 90 N NT1 Net-Tie ;0=1,1=0.0000
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ClassName ''
PRP ComponentLink1Description ''
PRP ComponentLink1URL ''
PRP CompType 'Net-Tie'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'N/A'
PRP MountType 'SMT'
PRP Note ''
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
PRP RoHS ''
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Value ''
TOP 0 3.1093238 1.5704393 90 N 61 1 1
TOP 1 3.1093238 1.5504393 90 N 83 9 2
#
# CMP 9
CMP 25 0.5211614 1.1072951 90 N Y1 CSTCR4M00G55B-R0 ;0=1,1=0.0472
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'https://www.murata.com/~/media/webrenewal/support/library/catalog/products/timingdevice/ceralock/p16e.ashx'
PRP CompType 'Resonator'
PRP Frequency_Fixed '4MHz'
PRP Frequency_Max ''
PRP Frequency_Min ''
PRP Frequency_Stability ''
PRP Frequency_Tolerance ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Load_Capacitance '39 pF'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '4.5x1.2x2 mm'
PRP PartNumber 'CSTCR4M00G55B-R0'
PRP REACh ''
PRP RoHS 'Y'
PRP SizeArea_mm2 '9'
PRP SizeAreaWB_mm2 '16.5'
PRP SizeX_mm '4.5'
PRP SizeY_mm '2'
PRP SizeZ_mm '1.2'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-40°C'
TOP 0 0.5211614 1.1663502 0 N 28 4 1
TOP 1 0.5211614 1.1072951 0 N 88 30 2
TOP 2 0.5211614 1.04824 0 N 27 3 3
#
# CMP 10
CMP 1 3.361004 2.2325 180 N R35 RC0603FR-0710KL ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.yageo.com/pdf/Pu-RC0603_51_PbFree_L_2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Yageo'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'RC0603FR-0710KL'
PRP Power_W '100mW'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '311-10.0KHRCT-ND'
PRP Supplier_Part_Number_2 '603-RC0603FR-0710KL'
PRP Supplier_Part_Number_3 '9238603'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '75V'
TOP 0 3.3925001 2.2325 90 N 87 24 1
TOP 1 3.329508 2.2325 90 N 21 2 2
#
# CMP 11
CMP 1 3.3283268 0.6414782 0 N R32 RC0603FR-0710KL ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.yageo.com/pdf/Pu-RC0603_51_PbFree_L_2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Yageo'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'RC0603FR-0710KL'
PRP Power_W '100mW'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '311-10.0KHRCT-ND'
PRP Supplier_Part_Number_2 '603-RC0603FR-0710KL'
PRP Supplier_Part_Number_3 '9238603'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '75V'
TOP 0 3.2968307 0.6414782 270 N 64 9 1
TOP 1 3.3598228 0.6414782 270 N 75 3 2
#
# CMP 12
CMP 2 2.7425 1.955197 270 N R21 ERJ-3GEY0R00V ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'ERJ-3GEY0R00V'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 'P0.0GCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-3GEY0R00V'
PRP Supplier_Part_Number_3 '2059527'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 2.7425 1.9276379 180 N 68 11 1
TOP 1 2.7425 1.982756 180 N 87 28 2
#
# CMP 13
CMP 8 0.115 1.7375 270 N R18 3352T-1-103LF ;0=2,1=0.1701
PRP AEC_Qualified 'No'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.bourns.com/docs/Product-Datasheets/3352.pdf'
PRP CompType ''
PRP datasheet 'https://www.bourns.com/docs/Product-Datasheets/3352.pdf'
PRP Datasheet_Path 'datasheets/Res-3352T-1-103LF.pdf'
PRP Digikey_Description 'THUMBWHEEL POT 10K OHM 0.5W TOP'
PRP Digikey_Part_Number '3352T-103LF-ND'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP helpURL 'https://upverter.com/upn/revision/808f9e37cf0afd24/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Bourns'
PRP MountType ''
PRP Mouser_Description 'Res Cermet Trimmer 10K Ohm 20% 1/2W 1(Elec)/1(Mech)Turn (8.89 X 9.53 X 3.81mm) Pin Thru-Hole Bag'
PRP Mouser_Part_Number '652-3352T-1-103LF'
PRP Operating_Temperature_Range '-55°C to +125°C'
PRP PackageReference 'PTM_PTH_8MM9_9MM53'
PRP Part_Number '3352T-1-103LF'
PRP PartNumber '3352T-1-103LF'
PRP Power '500mW'
PRP Power_W '0.5W'
PRP Res_ohm '10kO'
PRP RoHS 'TRUE'
PRP Series '3352'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm '4.32mm'
PRP Standoff_Height '0.64mm'
PRP TempCo '100ppm/°C'
PRP Tolerance__ '20%'
PRP Value '10k'
PRP Voltage '250V'
TOP 0 0.115 1.6375 270 N 1 3 1
TOP 1 0.115 1.7375 270 N 81 10 2
TOP 2 0.115 1.8375 270 N 2 3 3
#
# CMP 14
CMP 1 1.4283384 2.422641 0 N R8 RC0603FR-0710KL ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.yageo.com/pdf/Pu-RC0603_51_PbFree_L_2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Yageo'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'RC0603FR-0710KL'
PRP Power_W '100mW'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '311-10.0KHRCT-ND'
PRP Supplier_Part_Number_2 '603-RC0603FR-0710KL'
PRP Supplier_Part_Number_3 '9238603'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '75V'
TOP 0 1.3968423 2.422641 270 N 88 33 1
TOP 1 1.4598344 2.422641 270 N 3 2 2
#
# CMP 15
CMP 1 3.2669095 1.4335398 90 N C1 0603YD105KAT2A ;0=1,1=0.0394
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://datasheets.avx.com/cx5r.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'AVX'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber '0603YD105KAT2A'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '85°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X5R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '1uF'
PRP Value1 ''
PRP Value2 '16V'
PRP ValueDisplayed '1µF'
PRP VDC_V '16V'
TOP 0 3.2669095 1.4650359 0 N 64 7 1
TOP 1 3.2669095 1.4020438 0 N 63 8 2
#
# CMP 16
CMP 33 3.1783268 1.6548425 270 N U1 MCT8315Z0RRRYR ;0=1,1=0.0000
PRP Datasheet_Path 'datasheets/IC-MCT8315Z0RRRYR.pdf'
PRP helpURL 'https://upverter.com/upn/revision/b15b40dbbd5e221f/'
PRP Manufacturer 'Texas Instruments'
PRP Operating_Temperature_Range 'to'
PRP PackageReference 'WQFN32'
PRP Part_Number 'MCT8315Z0RRRYR'
PRP PartNumber 'MCT8315Z0RRRYR'
PRP RoHS 'UNKNOWN'
PRP SizeZ_mm '0.8mm'
PRP Standoff_Height '0mm'
TOP 0 3.0897441 1.5800394 270 N 52 6 1
TOP 1 3.1094292 1.5800394 270 N 61 0 2
TOP 2 3.1291142 1.5800394 270 N 88 38 3
TOP 3 3.1487992 1.5800394 270 N 66 5 4
TOP 4 3.1684843 1.5800394 270 N 85 2 5
TOP 5 3.1881693 1.5800394 270 N 86 2 6
TOP 6 3.2078544 1.5800394 270 N 64 8 7
TOP 7 3.2275394 1.5800394 270 N 63 12 8
TOP 8 3.2472244 1.5800394 270 N 63 11 9
TOP 9 3.2669095 1.5800394 270 N 69 15 10
TOP 10 3.2925 1.6056299 270 N 72 1 11
TOP 11 3.2925 1.6253149 270 N 71 1 12
TOP 12 3.2925 1.645 270 N 70 1 13
TOP 13 3.2925 1.664685 270 N 69 14 14
TOP 14 3.2925 1.6843701 270 N 84 5 15
TOP 15 3.2925 1.7040551 270 N 74 6 16
TOP 16 3.2669095 1.7296456 270 N 73 4 17
TOP 17 3.2472244 1.7296456 270 N 88 37 18
TOP 18 3.2275394 1.7296456 270 N 87 27 19
TOP 19 3.2078544 1.7296456 270 N 48 8 20
TOP 20 3.1881693 1.7296456 270 N 45 6 21
TOP 21 3.1684843 1.7296456 270 N 49 8 22
TOP 22 3.1487992 1.7296456 270 N 46 6 23
TOP 23 3.1291142 1.7296456 270 N 50 8 24
TOP 24 3.1094292 1.7296456 270 N 47 6 25
TOP 25 3.0897441 1.7296456 270 N 67 11 26
TOP 26 3.0641536 1.7040551 270 N 68 9 27
TOP 27 3.0641536 1.6843701 270 N 30 9 28
TOP 28 3.0641536 1.664685 270 N 37 3 29
TOP 29 3.0641536 1.645 270 N 81 7 30
TOP 30 3.0641536 1.6253149 270 N 56 5 31
TOP 31 3.0641536 1.6056299 270 N 34 1 32
TOP 32 3.1783268 1.6548425 270 N 88 36 33
#
# CMP 17
CMP 17 2.0961924 1.012126 270 N TP24 AGND ;0=2,1=0.1811
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName ''
PRP CNHeader 'FALSE'
PRP Color 'Black'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.keyelco.com/userAssets/file/M60-2p60.pdf'
PRP CompType 'Test Point'
PRP ContactFinish 'Silver'
PRP CT 'TRUE'
PRP Current_A ''
PRP Gender ''
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Keystone Electronics'
PRP MountType 'TH'
PRP Note ''
PRP Orientation ''
PRP PackageReference 'Black Miniature Testpoint'
PRP PartNumber '5001'
PRP PinCount ''
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '36-5001-ND'
PRP Supplier_Part_Number_2 '534-5001'
PRP Supplier_Part_Number_3 ''
PRP Voltage_V ''
TOP 0 2.0961924 1.012126 270 N 88 57 1
#
# CMP 18
CMP 15 4.005 2.13 270 N TP20 PGND ;0=2,1=0.2610
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName ''
PRP CNHeader 'False'
PRP Color ''
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://cdn.harwin.com/pdfs/D3080-D3083.pdf'
PRP CompType 'Jumper Wire'
PRP ContactFinish ''
PRP CT 'False'
PRP Current_A ''
PRP Gender ''
PRP Green_EU_RoHS 'Passed with Exemption'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '2017-07-12'
PRP Manufacturer 'Harwin'
PRP MountType 'TH'
PRP Note ''
PRP Orientation ''
PRP PackageReference 'Shorting Plug, 10.16mm spacing, TH'
PRP PartNumber 'D3082-05'
PRP PinCount ''
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '952-1873-ND'
PRP Supplier_Part_Number_2 '01E9240'
PRP Supplier_Part_Number_3 '855-D3082-05'
PRP Voltage_V ''
TOP 0 4.005 1.93 270 N 69 21 1
TOP 1 4.005 2.33 270 N 69 20 2
#
# CMP 19
CMP 31 1.5425 0.9025 180 N J1 Header_3x1 ;0=2,1=0.3300
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName 'Header'
PRP CNHeader 'TRUE'
PRP Color ''
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.sullinscorp.com/catalogs/77_Page78-79_HEADER_.100_2.54mm_MALE_BREAKAWAY.pdf'
PRP CompType 'Header'
PRP ContactFinish ''
PRP CT 'FALSE'
PRP Current_A ''
PRP Gender ''
PRP Green_EU_RoHS 'Incomplete'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Not Set'
PRP Green_REACh 'Incomplete'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Sullins Connector Solutions'
PRP MountType 'TH'
PRP Note ''
PRP Orientation ''
PRP PackageReference 'PBC03SAAN'
PRP PartNumber 'PBC03SAAN'
PRP PinCount ''
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'S1011E-03-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Voltage_V ''
TOP 0 1.6425 0.9025 180 N 36 3 1
TOP 1 1.5425 0.9025 180 N 10 2 2
TOP 2 1.4425 0.9025 180 N 35 5 3
#
# CMP 20
CMP 11 0.4471614 0.6091732 180 N U3 TPD4E004DRYR ;0=1,1=0.0236
PRP 1394_/_Firewire 'TRUE'
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Breakdown_Voltage(Min)(V) '6'
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/tpd4e004.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/tpd4e004'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/tpd4e004/datasheet'
PRP CompType 'IC'
PRP Ctotal(Typ)(pF) ''
PRP Differential_Capacitance(pF) ''
PRP Eco-Plan 'Green (RoHS & no Sb/Br)'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP HDMI ''
PRP IEC_61000-4-2_Air-Gap(+/-_kV) '12'
PRP IEC_61000-4-2_Air-Gap(Typ)(+/-_kV) ''
PRP IEC_61000-4-2_Contact(+/-_kV) '8'
PRP IEC_61000-4-2_Contact(Typ)(+/-_kV) ''
PRP IO_Capacitance(Typ)(pF) '1.6'
PRP IO_Leakage_Current(nA) '1'
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP Number_Of_Channels ''
PRP Operating_Temperature_Range '-40 to 85 C'
PRP PackageDescription 'USON-6'
PRP PackageReference 'DRY0006A'
PRP PartNumber 'TPD4E004DRYR'
PRP Rating 'Catalog'
PRP RoHS 'Y'
PRP Serial_ATA_/_eSATA 'TRUE'
PRP SizeArea_mm2 '1.45'
PRP SizeAreaWB_mm2 '4.9'
PRP SizeX_mm '1.0'
PRP SizeY_mm '1.45'
PRP SizeZ_mm '0.6'
PRP USB_Full_Speed ''
PRP USB_High_Speed 'TRUE'
PRP USB_Super_Speed ''
TOP 0 0.4579882 0.5894881 90 N 0 19 1
TOP 1 0.4589724 0.6091731 90 N 53 6 2
TOP 2 0.4589724 0.6288582 90 N 88 31 3
TOP 3 0.4353504 0.6288582 90 N 6 7 4
TOP 4 0.4353504 0.6091731 90 N 54 5 5
TOP 5 0.4353504 0.5894881 90 N 58 7 6
#
# CMP 21
CMP 2 0.2953 0.529825 180 N C8 C0603C104K8RACTU ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.kemet.com/kemet/web/homepage/kechome.nsf/vapubfiles/F3102_Y5V.pdf/$file/F3102_Y5V.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Kemet'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'C0603C104K8RACTU'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '399-1095-1-ND'
PRP Supplier_Part_Number_2 '80-C0603C104K8R'
PRP Supplier_Part_Number_3 '1640032'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '10V'
TOP 0 0.3228591 0.529825 90 N 58 8 1
TOP 1 0.267741 0.529825 90 N 88 44 2
#
# CMP 22
CMP 34 1.8625 1.8025 270 N J6 TSW-109-07-G-D ;0=2,1=0.3300
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA 'Y'
PRP Cert_CULUS 'N'
PRP Cert_UL 'Y'
PRP Cert_VDE 'N'
PRP ClassName 'Header'
PRP CNHeader 'True'
PRP Color 'Black'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.samtec.com/documents/webfiles/cpdf/TSW-XXX-XX-XXX-X-XX-XXX-MKT.pdf'
PRP CompType 'Header'
PRP ContactFinish 'Gold'
PRP CT 'False'
PRP Current_A '6.3A'
PRP Gender 'Male'
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '2017-07-12'
PRP Manufacturer 'Samtec'
PRP MountType 'TH'
PRP Note ''
PRP Orientation 'Vertical'
PRP PackageReference '9x2 Header'
PRP PartNumber 'TSW-109-07-G-D'
PRP PinCount '18'
PRP Pitch_mm '2.54'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count '2'
PRP RowSpacing_mm '2.54'
PRP Shrouded 'N'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 'SAM1028-09-ND'
PRP Supplier_Part_Number_2 '12P1721'
PRP Supplier_Part_Number_3 '2025256'
PRP Voltage_V '550V'
TOP 0 1.9125 1.4025 270 N 52 9 1
TOP 1 1.8125 1.4025 270 N 5 4 2
TOP 2 1.9125 1.5025 270 N 34 2 3
TOP 3 1.8125 1.5025 270 N 10 3 4
TOP 4 1.9125 1.6025 270 N 7 3 5
TOP 5 1.8125 1.6025 270 N 15 5 6
TOP 6 1.9125 1.7025 270 N 13 3 7
TOP 7 1.8125 1.7025 270 N 17 5 8
TOP 8 1.9125 1.8025 270 N 9 3 9
TOP 9 1.8125 1.8025 270 N 16 5 10
TOP 10 1.9125 1.9025 270 N 8 6 11
TOP 11 1.8125 1.9025 270 N 19 4 12
TOP 12 1.9125 2.0025 270 N 74 8 13
TOP 13 1.8125 2.0025 270 N 12 2 14
TOP 14 1.9125 2.1025 270 N 73 5 15
TOP 15 1.8125 2.1025 270 N 11 3 16
TOP 16 1.9125 2.2025 270 N 88 56 17
TOP 17 1.8125 2.2025 270 N 88 55 18
#
# CMP 23
CMP 42 0.0834475 1.09824 270 N J4 TSW-104-07-G-S ;0=2,1=0.3300
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA 'Y'
PRP Cert_CULUS 'N'
PRP Cert_UL 'Y'
PRP Cert_VDE 'N'
PRP ClassName 'Header'
PRP Color 'Black'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://samtec.com/ftppub/pdf/TSW_TH.PDF'
PRP CompType 'Header'
PRP ContactFinish 'Gold'
PRP Current_A '6.3A'
PRP Gender 'Male'
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP Manufacturer 'Samtec'
PRP MountType 'TH'
PRP Note ''
PRP Orientation 'Vertical'
PRP PackageReference '4x1 Header'
PRP PartNumber 'TSW-104-07-G-S'
PRP PinCount '4'
PRP Pitch_mm '2.54'
PRP RoHS 'Y'
PRP Row_Count '1'
PRP RowSpacing_mm ''
PRP Shrouded 'N'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'SAM1029-04-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Voltage_V '550V'
TOP 0 0.0834475 0.94824 270 N 88 54 1
TOP 1 0.0834475 1.04824 270 N 59 21 2
TOP 2 0.0834475 1.14824 270 N 31 12 3
TOP 3 0.0834475 1.24824 270 N 32 5 4
#
# CMP 24
CMP 16 1.195 0.1375 270 N TP14 3V3EXT ;0=2,1=0.1811
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName ''
PRP CNHeader 'FALSE'
PRP Color 'Red'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.keyelco.com/userAssets/file/M60-2p60.pdf'
PRP CompType 'Test Point'
PRP ContactFinish 'Silver'
PRP CT 'TRUE'
PRP Current_A ''
PRP Gender ''
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Keystone Electronics'
PRP MountType 'TH'
PRP Note ''
PRP Orientation ''
PRP PackageReference 'Red Miniature Testpoint'
PRP PartNumber '5000'
PRP PinCount ''
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '36-5000-ND'
PRP Supplier_Part_Number_2 '534-5000'
PRP Supplier_Part_Number_3 ''
PRP Voltage_V ''
TOP 0 1.195 0.1375 270 N 18 3 1
#
# CMP 25
CMP 19 3.6340527 0.7094592 180 N TP15 VBAT ;0=2,1=0.2200
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName ''
PRP CNHeader 'FALSE'
PRP Color 'Red'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.keyelco.com/userAssets/file/M60-2p60.pdf'
PRP CompType 'Test Point'
PRP ContactFinish 'Silver'
PRP CT 'TRUE'
PRP Current_A ''
PRP Gender ''
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Keystone Electronics'
PRP MountType 'TH'
PRP Note ''
PRP Orientation ''
PRP PackageReference 'Red Compact Testpoint'
PRP PartNumber '5005'
PRP PinCount ''
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '36-5005-ND'
PRP Supplier_Part_Number_2 '534-5005'
PRP Supplier_Part_Number_3 ''
PRP Voltage_V ''
TOP 0 3.6340527 0.7094592 180 N 65 5 1
#
# CMP 26
CMP 16 3.1820887 1.2302067 270 N TP7 SW_BUCK ;0=2,1=0.1811
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName ''
PRP CNHeader 'FALSE'
PRP Color 'Red'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.keyelco.com/userAssets/file/M60-2p60.pdf'
PRP CompType 'Test Point'
PRP ContactFinish 'Silver'
PRP CT 'TRUE'
PRP Current_A ''
PRP Gender ''
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Keystone Electronics'
PRP MountType 'TH'
PRP Note ''
PRP Orientation ''
PRP PackageReference 'Red Miniature Testpoint'
PRP PartNumber '5000'
PRP PinCount ''
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '36-5000-ND'
PRP Supplier_Part_Number_2 '534-5000'
PRP Supplier_Part_Number_3 ''
PRP Voltage_V ''
TOP 0 3.1820887 1.2302067 270 N 66 6 1
#
# CMP 27
CMP 2 2.2406083 1.9639191 270 N R12 CRCW06035K10JNEA ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'CRCW06035K10JNEA'
PRP Power_W '100mW'
PRP Res_ohm '5.1k'
PRP RoHS 'E'
PRP SizeArea_mm2 '1.28'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '541-5.1KGCT-ND'
PRP Supplier_Part_Number_2 '89M6773'
PRP Supplier_Part_Number_3 '1570751'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP Value '5.1k'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '5k10'
PRP ValueDisplayed '5.1k'
PRP VDC_V '75V'
TOP 0 2.2406083 1.93636 180 N 8 4 1
TOP 1 2.2406083 1.9914781 180 N 87 17 2
#
# CMP 28
CMP 2 0.2825 2.2 180 N R4 ERJ-3GEY0R00V ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'ERJ-3GEY0R00V'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 'P0.0GCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-3GEY0R00V'
PRP Supplier_Part_Number_3 '2059527'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 0.3100591 2.2 90 N 14 1 1
TOP 1 0.254941 2.2 90 N 20 2 2
#
# CMP 29
CMP 18 1.2649307 0.9025 270 N TP1 PWM_MSP ;0=2,1=0.1811
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName ''
PRP CNHeader 'FALSE'
PRP Color 'White'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.keyelco.com/userAssets/file/M60-2p60.pdf'
PRP CompType 'Test Point'
PRP ContactFinish 'Silver'
PRP CT 'TRUE'
PRP Current_A ''
PRP Gender ''
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Keystone Electronics'
PRP MountType 'TH'
PRP Note ''
PRP Orientation ''
PRP PackageReference 'White Miniature Testpoint'
PRP PartNumber '5002'
PRP PinCount ''
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '36-5002-ND'
PRP Supplier_Part_Number_2 '82H9632'
PRP Supplier_Part_Number_3 '534-5002'
PRP Voltage_V ''
TOP 0 1.2649307 0.9025 270 N 35 4 1
#
# CMP 30
CMP 17 3.0020151 0.77625 270 N TP26 PGND ;0=2,1=0.1811
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName ''
PRP CNHeader 'FALSE'
PRP Color 'Black'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.keyelco.com/userAssets/file/M60-2p60.pdf'
PRP CompType 'Test Point'
PRP ContactFinish 'Silver'
PRP CT 'TRUE'
PRP Current_A ''
PRP Gender ''
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Keystone Electronics'
PRP MountType 'TH'
PRP Note ''
PRP Orientation ''
PRP PackageReference 'Black Miniature Testpoint'
PRP PartNumber '5001'
PRP PinCount ''
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '36-5001-ND'
PRP Supplier_Part_Number_2 '534-5001'
PRP Supplier_Part_Number_3 ''
PRP Voltage_V ''
TOP 0 3.0020151 0.77625 270 N 69 19 1
#
# CMP 31
CMP 17 2.0967412 0.8525 270 N TP17 PGND ;0=2,1=0.1811
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName ''
PRP CNHeader 'FALSE'
PRP Color 'Black'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.keyelco.com/userAssets/file/M60-2p60.pdf'
PRP CompType 'Test Point'
PRP ContactFinish 'Silver'
PRP CT 'TRUE'
PRP Current_A ''
PRP Gender ''
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Keystone Electronics'
PRP MountType 'TH'
PRP Note ''
PRP Orientation ''
PRP PackageReference 'Black Miniature Testpoint'
PRP PartNumber '5001'
PRP PinCount ''
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '36-5001-ND'
PRP Supplier_Part_Number_2 '534-5001'
PRP Supplier_Part_Number_3 ''
PRP Voltage_V ''
TOP 0 2.0967412 0.8525 270 N 69 18 1
#
# CMP 32
CMP 10 2.975 2.325 0 N J11 PEC02SAAN ;0=2,1=0.3299
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL 'Y'
PRP Cert_VDE ''
PRP ClassName 'Header'
PRP CNHeader 'TRUE'
PRP Color 'Black'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.sullinscorp.com/catalogs/77_PAGE108-109_.100_MALE_HDR.pdf'
PRP CompType 'Header'
PRP ContactFinish 'Tin'
PRP CT 'FALSE'
PRP Current_A '3A'
PRP Gender 'Male'
PRP Green_EU_RoHS 'Incomplete'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Not Set'
PRP Green_REACh 'Incomplete'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Sullins Connector Solutions'
PRP MountType 'TH'
PRP Note ''
PRP Orientation 'Vertical'
PRP PackageReference 'Header, 2 PIN, 100mil, Tin'
PRP PartNumber 'PEC02SAAN'
PRP PinCount '2'
PRP Pitch_mm '2.54'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count '1'
PRP RowSpacing_mm ''
PRP Shrouded 'N'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'S1012E-02-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Voltage_V '1.8kV'
TOP 0 2.925 2.325 0 N 50 10 1
TOP 1 3.025 2.325 0 N 4 3 2
#
# CMP 33
CMP 10 3.2783268 2.325 0 N J10 PEC02SAAN ;0=2,1=0.3299
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL 'Y'
PRP Cert_VDE ''
PRP ClassName 'Header'
PRP CNHeader 'TRUE'
PRP Color 'Black'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.sullinscorp.com/catalogs/77_PAGE108-109_.100_MALE_HDR.pdf'
PRP CompType 'Header'
PRP ContactFinish 'Tin'
PRP CT 'FALSE'
PRP Current_A '3A'
PRP Gender 'Male'
PRP Green_EU_RoHS 'Incomplete'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Not Set'
PRP Green_REACh 'Incomplete'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Sullins Connector Solutions'
PRP MountType 'TH'
PRP Note ''
PRP Orientation 'Vertical'
PRP PackageReference 'Header, 2 PIN, 100mil, Tin'
PRP PartNumber 'PEC02SAAN'
PRP PinCount '2'
PRP Pitch_mm '2.54'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count '1'
PRP RowSpacing_mm ''
PRP Shrouded 'N'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'S1012E-02-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Voltage_V '1.8kV'
TOP 0 3.2283268 2.325 0 N 49 9 1
TOP 1 3.3283268 2.325 0 N 21 3 2
#
# CMP 34
CMP 10 3.5896496 2.325 0 N J9 PEC02SAAN ;0=2,1=0.3299
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL 'Y'
PRP Cert_VDE ''
PRP ClassName 'Header'
PRP CNHeader 'TRUE'
PRP Color 'Black'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.sullinscorp.com/catalogs/77_PAGE108-109_.100_MALE_HDR.pdf'
PRP CompType 'Header'
PRP ContactFinish 'Tin'
PRP CT 'FALSE'
PRP Current_A '3A'
PRP Gender 'Male'
PRP Green_EU_RoHS 'Incomplete'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Not Set'
PRP Green_REACh 'Incomplete'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Sullins Connector Solutions'
PRP MountType 'TH'
PRP Note ''
PRP Orientation 'Vertical'
PRP PackageReference 'Header, 2 PIN, 100mil, Tin'
PRP PartNumber 'PEC02SAAN'
PRP PinCount '2'
PRP Pitch_mm '2.54'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count '1'
PRP RowSpacing_mm ''
PRP Shrouded 'N'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'S1012E-02-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Voltage_V '1.8kV'
TOP 0 3.5396496 2.325 0 N 48 9 1
TOP 1 3.6396496 2.325 0 N 22 3 2
#
# CMP 35
CMP 24 0.03 0.685 90 N J2 1051640001 ;0=1,1=0.1063
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL 'Y'
PRP Cert_VDE ''
PRP ClassName ''
PRP CNHeader 'FALSE'
PRP Color 'Black'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.molex.com/pdm_docs/sd/1051640001_sd.pdf'
PRP CompType 'USB'
PRP ContactFinish 'Gold'
PRP CT 'TRUE'
PRP Current_A '1.8A'
PRP Gender 'Female'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Molex'
PRP MountType 'SMT'
PRP Note ''
PRP Orientation 'R/A'
PRP PackageReference 'Receptacle, USB 2.0, Micro B, 5 Pos, 0.65mm Pitch, R/A, SMT'
PRP PartNumber '1051640001'
PRP PinCount '5'
PRP Pitch_mm '0.65'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'WM11263CT-ND'
PRP Supplier_Part_Number_2 '99Y3224'
PRP Supplier_Part_Number_3 '538-105164-0001'
PRP Voltage_V '30V'
TOP 0 0.1918111 0.6338189 270 N 23 1 1
TOP 1 0.191811 0.6594095 270 N 54 3 2
TOP 2 0.1918111 0.685 270 N 53 4 3
TOP 3 0.191811 0.7105905 270 N 6 6 4
TOP 4 0.1918111 0.7361811 270 N 88 19 5
TOP 5 0.1776377 0.7819488 270 N 88 16 6
TOP 6 0.0870866 0.8405118 0 N 88 51 7
TOP 7 0.0870866 0.7219094 270 N 88 18 8
TOP 8 0.0870866 0.6480906 270 N 88 17 9
TOP 9 0.0870866 0.5294882 0 N 88 50 10
TOP 10 0.1776377 0.5880512 270 N 88 15 11
#
# CMP 36
CMP 16 2.51877 2.55 270 N TP27 HALL_PWR ;0=2,1=0.1811
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName ''
PRP CNHeader 'FALSE'
PRP Color 'Red'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.keyelco.com/userAssets/file/M60-2p60.pdf'
PRP CompType 'Test Point'
PRP ContactFinish 'Silver'
PRP CT 'TRUE'
PRP Current_A ''
PRP Gender ''
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Keystone Electronics'
PRP MountType 'TH'
PRP Note ''
PRP Orientation ''
PRP PackageReference 'Red Miniature Testpoint'
PRP PartNumber '5000'
PRP PinCount ''
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '36-5000-ND'
PRP Supplier_Part_Number_2 '534-5000'
PRP Supplier_Part_Number_3 ''
PRP Voltage_V ''
TOP 0 2.51877 2.55 270 N 82 4 1
#
# CMP 37
CMP 18 1.56 2.399506 270 N TP5 DRVOFF ;0=2,1=0.1811
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName ''
PRP CNHeader 'FALSE'
PRP Color 'White'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.keyelco.com/userAssets/file/M60-2p60.pdf'
PRP CompType 'Test Point'
PRP ContactFinish 'Silver'
PRP CT 'TRUE'
PRP Current_A ''
PRP Gender ''
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Keystone Electronics'
PRP MountType 'TH'
PRP Note ''
PRP Orientation ''
PRP PackageReference 'White Miniature Testpoint'
PRP PartNumber '5002'
PRP PinCount ''
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '36-5002-ND'
PRP Supplier_Part_Number_2 '82H9632'
PRP Supplier_Part_Number_3 '534-5002'
PRP Voltage_V ''
TOP 0 1.56 2.399506 270 N 84 6 1
#
# CMP 38
CMP 18 1.135 2.399506 270 N TP4 DIR ;0=2,1=0.1811
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName ''
PRP CNHeader 'FALSE'
PRP Color 'White'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.keyelco.com/userAssets/file/M60-2p60.pdf'
PRP CompType 'Test Point'
PRP ContactFinish 'Silver'
PRP CT 'TRUE'
PRP Current_A ''
PRP Gender ''
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Keystone Electronics'
PRP MountType 'TH'
PRP Note ''
PRP Orientation ''
PRP PackageReference 'White Miniature Testpoint'
PRP PartNumber '5002'
PRP PinCount ''
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '36-5002-ND'
PRP Supplier_Part_Number_2 '82H9632'
PRP Supplier_Part_Number_3 '534-5002'
PRP Voltage_V ''
TOP 0 1.135 2.399506 270 N 55 7 1
#
# CMP 39
CMP 18 0.71 2.399506 270 N TP3 BRAKE ;0=2,1=0.1811
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName ''
PRP CNHeader 'FALSE'
PRP Color 'White'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.keyelco.com/userAssets/file/M60-2p60.pdf'
PRP CompType 'Test Point'
PRP ContactFinish 'Silver'
PRP CT 'TRUE'
PRP Current_A ''
PRP Gender ''
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Keystone Electronics'
PRP MountType 'TH'
PRP Note ''
PRP Orientation ''
PRP PackageReference 'White Miniature Testpoint'
PRP PartNumber '5002'
PRP PinCount ''
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '36-5002-ND'
PRP Supplier_Part_Number_2 '82H9632'
PRP Supplier_Part_Number_3 '534-5002'
PRP Voltage_V ''
TOP 0 0.71 2.399506 270 N 56 6 1
#
# CMP 40
CMP 17 0.71 2.18375 270 N TP25 AGND ;0=2,1=0.1811
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName ''
PRP CNHeader 'FALSE'
PRP Color 'Black'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.keyelco.com/userAssets/file/M60-2p60.pdf'
PRP CompType 'Test Point'
PRP ContactFinish 'Silver'
PRP CT 'TRUE'
PRP Current_A ''
PRP Gender ''
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Keystone Electronics'
PRP MountType 'TH'
PRP Note ''
PRP Orientation ''
PRP PackageReference 'Black Miniature Testpoint'
PRP PartNumber '5001'
PRP PinCount ''
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '36-5001-ND'
PRP Supplier_Part_Number_2 '534-5001'
PRP Supplier_Part_Number_3 ''
PRP Voltage_V ''
TOP 0 0.71 2.18375 270 N 88 47 1
#
# CMP 41
CMP 1 3.0575 2.2325 180 N R36 RC0603FR-0710KL ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.yageo.com/pdf/Pu-RC0603_51_PbFree_L_2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Yageo'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'RC0603FR-0710KL'
PRP Power_W '100mW'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '311-10.0KHRCT-ND'
PRP Supplier_Part_Number_2 '603-RC0603FR-0710KL'
PRP Supplier_Part_Number_3 '9238603'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '75V'
TOP 0 3.0889961 2.2325 90 N 87 23 1
TOP 1 3.026004 2.2325 90 N 4 2 2
#
# CMP 42
CMP 1 0.115 1.97 270 N R11 RC0603FR-0751K1L ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.yageo.com/pdf/Pu-RC0603_51_PbFree_L_2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Yageo'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'RC0603FR-0751K1L'
PRP Power_W '100mW'
PRP Res_ohm '51.1k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '311-51.1KHRCT-ND'
PRP Supplier_Part_Number_2 '603-RC0603FR-0751K1L'
PRP Supplier_Part_Number_3 '1799349'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '51.1k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '51k1'
PRP ValueDisplayed '51.1k'
PRP VDC_V '75V'
TOP 0 0.115 1.9385039 180 N 2 2 1
TOP 1 0.115 2.001496 180 N 87 25 2
#
# CMP 43
CMP 16 2.41877 2.4375 270 N TP23 HALL_EXT ;0=2,1=0.1811
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName ''
PRP CNHeader 'FALSE'
PRP Color 'Red'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.keyelco.com/userAssets/file/M60-2p60.pdf'
PRP CompType 'Test Point'
PRP ContactFinish 'Silver'
PRP CT 'TRUE'
PRP Current_A ''
PRP Gender ''
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Keystone Electronics'
PRP MountType 'TH'
PRP Note ''
PRP Orientation ''
PRP PackageReference 'Red Miniature Testpoint'
PRP PartNumber '5000'
PRP PinCount ''
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '36-5000-ND'
PRP Supplier_Part_Number_2 '534-5000'
PRP Supplier_Part_Number_3 ''
PRP Voltage_V ''
TOP 0 2.41877 2.4375 270 N 51 2 1
#
# CMP 44
CMP 16 1.0050178 0.1375 270 N TP13 5V_EXT ;0=2,1=0.1811
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName ''
PRP CNHeader 'FALSE'
PRP Color 'Red'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.keyelco.com/userAssets/file/M60-2p60.pdf'
PRP CompType 'Test Point'
PRP ContactFinish 'Silver'
PRP CT 'TRUE'
PRP Current_A ''
PRP Gender ''
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Keystone Electronics'
PRP MountType 'TH'
PRP Note ''
PRP Orientation ''
PRP PackageReference 'Red Miniature Testpoint'
PRP PartNumber '5000'
PRP PinCount ''
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '36-5000-ND'
PRP Supplier_Part_Number_2 '534-5000'
PRP Supplier_Part_Number_3 ''
PRP Voltage_V ''
TOP 0 1.0050178 0.1375 270 N 26 2 1
#
# CMP 45
CMP 19 2.495 0.5301108 0 N TP16 VM ;0=2,1=0.2200
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName ''
PRP CNHeader 'FALSE'
PRP Color 'Red'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.keyelco.com/userAssets/file/M60-2p60.pdf'
PRP CompType 'Test Point'
PRP ContactFinish 'Silver'
PRP CT 'TRUE'
PRP Current_A ''
PRP Gender ''
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Keystone Electronics'
PRP MountType 'TH'
PRP Note ''
PRP Orientation ''
PRP PackageReference 'Red Compact Testpoint'
PRP PartNumber '5005'
PRP PinCount ''
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '36-5005-ND'
PRP Supplier_Part_Number_2 '534-5005'
PRP Supplier_Part_Number_3 ''
PRP Voltage_V ''
TOP 0 2.495 0.5301108 0 N 63 14 1
#
# CMP 46
CMP 32 0.844218 1.2363386 0 N U4 MSP430FR2355TPTR ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/msp430fr2355.pdf'
PRP Core_Architecture 'RISC'
PRP Data_Bus_Width '16bits'
PRP datasheet 'http://www.ti.com/lit/ds/symlink/msp430fr2355.pdf'
PRP Datasheet_Path 'datasheets/IC-MSP430FR2355TPTR.pdf'
PRP Device_Class_L1 'Integrated Circuits (ICs)'
PRP Device_Class_L2 'Embedded Processors and Controllers'
PRP Device_Class_L3 'Microcontrollers'
PRP Digikey_Description 'IC MCU 16BIT 32KB FRAM 48LQFP'
PRP Digikey_Part_Number '296-50261-1-ND'
PRP Frequency_Fixed '24MHz'
PRP helpURL 'https://upverter.com/upn/revision/f866b8320dbaa695/'
PRP Interface 'I2C,SPI,UART,USART,SCI,IrDA'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Texas Instruments'
PRP Max_Supply_Voltage '3.6V'
PRP Memory_Size '32KBytes'
PRP Memory_Type 'OTHER'
PRP Min_Supply_Voltage '1.8V'
PRP Mouser_Part_Number '595-MSP430FR2355TPTR'
PRP Number_Of_A/D_Converters '1'
PRP Number_Of_Adc_Channels '12'
PRP Number_Of_Cores '1'
PRP Number_Of_I2C_Channels '2'
PRP Number_Of_I/Os '44'
PRP Number_Of_Spi_Channels '4'
PRP Number_Of_Timers/Counters '4'
PRP Number_Of_Uart_Channels '2'
PRP Operating_Temperature_Range '-40°C to +105°C'
PRP PackageReference 'LQFP48'
PRP Part_Number 'MSP430FR2355TPTR'
PRP PartNumber 'MSP430FR2355TPTR'
PRP Ram_Size '4KBytes'
PRP RoHS 'TRUE'
PRP SizeZ_mm '1.6mm'
PRP Standoff_Height '0.05mm'
PRP TaMax_C '+105°C'
PRP TaMin_C '-40°C'
PRP TJmax_C '+115°C'
TOP 0 0.6768952 1.3446063 0 N 0 21 1
TOP 1 0.6768952 1.3249213 0 N 14 2 2
TOP 2 0.6768952 1.3052362 0 N 0 22 3
TOP 3 0.6768952 1.2855512 0 N 32 4 4
TOP 4 0.6768952 1.2658662 0 N 31 11 5
TOP 5 0.6768952 1.2461811 0 N 59 19 6
TOP 6 0.6768952 1.2264961 0 N 88 46 7
TOP 7 0.6768952 1.206811 0 N 28 5 8
TOP 8 0.6768952 1.187126 0 N 27 4 9
TOP 9 0.6768952 1.167441 0 N 0 23 10
TOP 10 0.6768952 1.1477559 0 N 0 24 11
TOP 11 0.6768952 1.1280709 0 N 19 3 12
TOP 12 0.7359503 1.0690158 0 N 16 4 13
TOP 13 0.7556353 1.0690158 0 N 17 4 14
TOP 14 0.7753204 1.0690158 0 N 15 4 15
TOP 15 0.7950054 1.0690158 0 N 0 25 16
TOP 16 0.8146904 1.0690158 0 N 0 26 17
TOP 17 0.8343755 1.0690158 0 N 0 27 18
TOP 18 0.8540605 1.0690158 0 N 0 28 19
TOP 19 0.8737456 1.0690158 0 N 0 29 20
TOP 20 0.8934306 1.0690158 0 N 0 30 21
TOP 21 0.9131156 1.0690158 0 N 0 31 22
TOP 22 0.9328007 1.0690158 0 N 33 2 23
TOP 23 0.9524857 1.0690158 0 N 29 3 24
TOP 24 1.0115408 1.1280709 0 N 0 32 25
TOP 25 1.0115408 1.1477559 0 N 0 33 26
TOP 26 1.0115408 1.167441 0 N 43 3 27
TOP 27 1.0115408 1.187126 0 N 44 3 28
TOP 28 1.0115408 1.206811 0 N 5 3 29
TOP 29 1.0115408 1.2264961 0 N 35 3 30
TOP 30 1.0115408 1.2461811 0 N 0 34 31
TOP 31 1.0115408 1.2658662 0 N 0 35 32
TOP 32 1.0115408 1.2855512 0 N 0 36 33
TOP 33 1.0115408 1.3052362 0 N 0 37 34
TOP 34 1.0115408 1.3249213 0 N 0 38 35
TOP 35 1.0115408 1.3446063 0 N 0 39 36
TOP 36 0.9524857 1.4036614 0 N 0 40 37
TOP 37 0.9328007 1.4036614 0 N 0 41 38
TOP 38 0.9131156 1.4036614 0 N 0 42 39
TOP 39 0.8934306 1.4036614 0 N 0 43 40
TOP 40 0.8737456 1.4036614 0 N 0 44 41
TOP 41 0.8540605 1.4036614 0 N 0 45 42
TOP 42 0.8343755 1.4036614 0 N 0 46 43
TOP 43 0.8146904 1.4036614 0 N 12 1 44
TOP 44 0.7950054 1.4036614 0 N 11 2 45
TOP 45 0.7753204 1.4036614 0 N 0 47 46
TOP 46 0.7556353 1.4036614 0 N 0 48 47
TOP 47 0.7359503 1.4036614 0 N 0 49 48
#
# CMP 47
CMP 39 0.6875 0.745 90 N U2 FT232RL ;0=1,1=0.0787
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT232R.pdf'
PRP LatestRevisionDate '09/03/2017'
PRP Manufacturer 'FTDI'
PRP MountType 'SMT'
PRP PackageReference 'SSOP28'
PRP PartNumber 'FT232RL'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '768-1007-1-ND'
PRP Supplier_Part_Number_2 '91K9918'
PRP Supplier_Part_Number_3 '895-FT232RL'
TOP 0 0.8538386 0.8808267 0 N 29 2 1
TOP 1 0.828248 0.8808267 0 N 0 1 2
TOP 2 0.8026575 0.8808267 0 N 0 2 3
TOP 3 0.7770669 0.8808267 0 N 60 11 4
TOP 4 0.7514764 0.8808267 0 N 33 1 5
TOP 5 0.7258858 0.8808267 0 N 0 3 6
TOP 6 0.7002953 0.8808267 0 N 88 20 7
TOP 7 0.6747047 0.8808267 0 N 0 4 8
TOP 8 0.6491142 0.8808267 0 N 0 5 9
TOP 9 0.6235236 0.8808267 0 N 0 6 10
TOP 10 0.5979331 0.8808267 0 N 0 7 11
TOP 11 0.5723425 0.8808267 0 N 0 8 12
TOP 12 0.546752 0.8808267 0 N 0 9 13
TOP 13 0.5211614 0.8808267 0 N 0 10 14
TOP 14 0.5211614 0.6091732 0 N 53 5 15
TOP 15 0.546752 0.6091732 0 N 54 4 16
TOP 16 0.5723425 0.6091732 0 N 60 12 17
TOP 17 0.5979331 0.6091732 0 N 88 24 18
TOP 18 0.6235236 0.6091732 0 N 0 16 19
TOP 19 0.6491142 0.6091732 0 N 57 4 20
TOP 20 0.6747047 0.6091732 0 N 88 23 21
TOP 21 0.7002953 0.6091732 0 N 0 15 22
TOP 22 0.7258858 0.6091732 0 N 0 14 23
TOP 23 0.7514764 0.6091732 0 N 0 13 24
TOP 24 0.7770669 0.6091732 0 N 88 22 25
TOP 25 0.8026575 0.6091732 0 N 88 21 26
TOP 26 0.828248 0.6091732 0 N 0 12 27
TOP 27 0.8538386 0.6091732 0 N 0 11 28
#
# CMP 48
CMP 40 0.2978 1.3754447 180 N S4 SW_SPST-single ;0=1,1=0.1043
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Circuit 'SPST'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://katalog.we-online.de/em/datasheet/434121025816.pdf'
PRP CompType 'Switch'
PRP CurrentRating_mA '50A'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Wurth Elektronik'
PRP MountType 'SMT'
PRP Orientation 'Top Actuated'
PRP PackageReference 'SMD, 6x3.9mm'
PRP PartNumber '434121025816'
PRP PositionCount '1'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm ''
PRP Supplier_1 'Newark'
PRP Supplier_2 'Farnell'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '31T8978'
PRP Supplier_Part_Number_2 '1867991'
PRP Supplier_Part_Number_3 ''
PRP SwitchFunction 'Off-On'
PRP VDC_V '12V'
TOP 0 0.4257528 1.3754447 180 N 31 10 1
TOP 1 0.1698472 1.3754447 180 N 88 25 2
#
# CMP 49
CMP 41 1.56 2.655 270 N S3 SW_SPDT_COM2_1_3 ;0=2,1=0.9094
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Circuit 'SPDT'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.nkkswitches.com/pdf/Btoggles.pdf'
PRP CompType 'Switch'
PRP CurrentRating_mA '100A'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'NKK Switches'
PRP MountType 'TH'
PRP Orientation 'Top Actuated'
PRP PackageReference '6.8x23.1x8.8mm'
PRP PartNumber 'B12AP'
PRP PositionCount '2'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '360-1012-ND'
PRP Supplier_Part_Number_2 '09X8543'
PRP Supplier_Part_Number_3 '633-B12AP'
PRP SwitchFunction 'On-On'
PRP VDC_V '28V'
TOP 0 1.46 2.6156299 270 N 3 3 1
TOP 1 1.56 2.6156299 270 N 84 7 2
TOP 2 1.66 2.6156299 270 N 38 3 3
#
# CMP 50
CMP 41 1.135 2.655 270 N S2 SW_SPDT_COM2_1_3 ;0=2,1=0.9094
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Circuit 'SPDT'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.nkkswitches.com/pdf/Btoggles.pdf'
PRP CompType 'Switch'
PRP CurrentRating_mA '100A'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'NKK Switches'
PRP MountType 'TH'
PRP Orientation 'Top Actuated'
PRP PackageReference '6.8x23.1x8.8mm'
PRP PartNumber 'B12AP'
PRP PositionCount '2'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '360-1012-ND'
PRP Supplier_Part_Number_2 '09X8543'
PRP Supplier_Part_Number_3 '633-B12AP'
PRP SwitchFunction 'On-On'
PRP VDC_V '28V'
TOP 0 1.035 2.6156299 270 N 24 3 1
TOP 1 1.135 2.6156299 270 N 55 8 2
TOP 2 1.235 2.6156299 270 N 39 3 3
#
# CMP 51
CMP 41 0.71 2.655 270 N S1 SW_SPDT_COM2_1_3 ;0=2,1=0.9094
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Circuit 'SPDT'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.nkkswitches.com/pdf/Btoggles.pdf'
PRP CompType 'Switch'
PRP CurrentRating_mA '100A'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'NKK Switches'
PRP MountType 'TH'
PRP Orientation 'Top Actuated'
PRP PackageReference '6.8x23.1x8.8mm'
PRP PartNumber 'B12AP'
PRP PositionCount '2'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '360-1012-ND'
PRP Supplier_Part_Number_2 '09X8543'
PRP Supplier_Part_Number_3 '633-B12AP'
PRP SwitchFunction 'On-On'
PRP VDC_V '28V'
TOP 0 0.61 2.6156299 270 N 25 3 1
TOP 1 0.71 2.6156299 270 N 56 7 2
TOP 2 0.81 2.6156299 270 N 40 3 3
#
# CMP 52
CMP 1 3.67 2.2325 180 N R34 RC0603FR-0710KL ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.yageo.com/pdf/Pu-RC0603_51_PbFree_L_2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Yageo'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'RC0603FR-0710KL'
PRP Power_W '100mW'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '311-10.0KHRCT-ND'
PRP Supplier_Part_Number_2 '603-RC0603FR-0710KL'
PRP Supplier_Part_Number_3 '9238603'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '75V'
TOP 0 3.7014961 2.2325 90 N 87 22 1
TOP 1 3.638504 2.2325 90 N 22 2 2
#
# CMP 53
CMP 1 3.3285039 0.5458372 0 N R33 RC0603FR-0710KL ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.yageo.com/pdf/Pu-RC0603_51_PbFree_L_2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Yageo'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'RC0603FR-0710KL'
PRP Power_W '100mW'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '311-10.0KHRCT-ND'
PRP Supplier_Part_Number_2 '603-RC0603FR-0710KL'
PRP Supplier_Part_Number_3 '9238603'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '75V'
TOP 0 3.2970078 0.5458372 270 N 69 11 1
TOP 1 3.3599999 0.5458372 270 N 76 2 2
#
# CMP 54
CMP 2 1.1915127 1.2142625 180 N R31 RC0603JR-07470RL ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.yageo.com/pdf/Pu-RC0603_51_PbFree_L_2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Yageo'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'RC0603JR-07470RL'
PRP Power_W '100mW'
PRP Res_ohm '470'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '311-470GRCT-ND'
PRP Supplier_Part_Number_2 '603-RC0603JR-07470RL'
PRP Supplier_Part_Number_3 '9233334'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '5%'
PRP Value '470'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '470R'
PRP ValueDisplayed '470'
PRP VDC_V '75V'
TOP 0 1.2190718 1.2142625 90 N 41 2 1
TOP 1 1.1639537 1.2142625 90 N 59 14 2
#
# CMP 55
CMP 2 1.1915127 1.3525 180 N R30 RC0603JR-07470RL ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.yageo.com/pdf/Pu-RC0603_51_PbFree_L_2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Yageo'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'RC0603JR-07470RL'
PRP Power_W '100mW'
PRP Res_ohm '470'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '311-470GRCT-ND'
PRP Supplier_Part_Number_2 '603-RC0603JR-07470RL'
PRP Supplier_Part_Number_3 '9233334'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '5%'
PRP Value '470'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '470R'
PRP ValueDisplayed '470'
PRP VDC_V '75V'
TOP 0 1.2190718 1.3525 90 N 42 2 1
TOP 1 1.1639537 1.3525 90 N 59 15 2
#
# CMP 56
CMP 2 0.3772042 1.4850789 0 N R29 RC0603JR-0747KL ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.yageo.com/pdf/Pu-RC0603_51_PbFree_L_2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Yageo'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'RC0603JR-0747KL'
PRP Power_W '100mW'
PRP Res_ohm '47k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '311-47KGRCT-ND'
PRP Supplier_Part_Number_2 '603-RC0603JR-0747KL'
PRP Supplier_Part_Number_3 '9233580'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '5%'
PRP Value '47k'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '47k0'
PRP ValueDisplayed '47k'
PRP VDC_V '75V'
TOP 0 0.3496451 1.4850789 270 N 31 8 1
TOP 1 0.4047632 1.4850789 270 N 59 16 2
#
# CMP 57
CMP 2 2.8225 1.827741 270 N R28 ERA-3AEB104V ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/lecs/www-data/pdf/AOA0000/AOA0000CE26.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E192'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'ERA-3AEB104V'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '100k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P100KDBCT-ND'
PRP Supplier_Part_Number_2 '08N2096'
PRP Supplier_Part_Number_3 '667-ERA-3AEB104V'
PRP Technology 'Thin Film'
PRP TempCo '25 ppm/C'
PRP Tolerance__ '0.1%'
PRP U/M 'EA'
PRP Value '100k'
PRP Value1 '0.1%'
PRP Value2 '0.1W'
PRP Value_Code '100k'
PRP ValueDisplayed '100k'
PRP VDC_V '75V'
TOP 0 2.8225 1.8001819 180 N 88 42 1
TOP 1 2.8225 1.8553 180 N 67 12 2
#
# CMP 58
CMP 2 2.6575 1.824941 270 N R26 ERJ-3GEY0R00V ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'ERJ-3GEY0R00V'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 'P0.0GCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-3GEY0R00V'
PRP Supplier_Part_Number_3 '2059527'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 2.6575 1.7973819 180 N 88 39 1
TOP 1 2.6575 1.8525 180 N 30 10 2
#
# CMP 59
CMP 2 2.7425 1.827741 270 N R27 ERJ-3GEY0R00V ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'ERJ-3GEY0R00V'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 'P0.0GCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-3GEY0R00V'
PRP Supplier_Part_Number_3 '2059527'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 2.7425 1.8001819 180 N 88 41 1
TOP 1 2.7425 1.8553 180 N 68 10 2
#
# CMP 60
CMP 2 2.6902808 0.724108 180 N R25 RT0603BRD074K7L ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.yageo.com/pdf/PYu-RT_1-to-0.05_RoHS_L_3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E192'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Yageo America'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'RT0603BRD074K7L'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '4.7k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thin Film'
PRP TempCo '25 ppm/C'
PRP Tolerance__ '0.1%'
PRP U/M 'EA'
PRP Value '4.70k'
PRP Value1 '0.1%'
PRP Value2 '0.1W'
PRP Value_Code '4k70'
PRP ValueDisplayed '4.70k'
PRP VDC_V '75V'
TOP 0 2.7178399 0.724108 90 N 69 4 1
TOP 1 2.6627218 0.724108 90 N 78 2 2
#
# CMP 61
CMP 2 3.0009521 1.1012558 180 N R23 RC0603FR-07330RL ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.yageo.com/pdf/Pu-RC0603_51_PbFree_L_2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Yageo'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'RC0603FR-07330RL'
PRP Power_W '100mW'
PRP Res_ohm '330'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '311-330HRCT-ND'
PRP Supplier_Part_Number_2 '603-RC0603FR-07330RL'
PRP Supplier_Part_Number_3 '9238425'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '330'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '330R'
PRP ValueDisplayed '330'
PRP VDC_V '75V'
TOP 0 3.0285112 1.1012558 90 N 88 35 1
TOP 1 2.9733931 1.1012558 90 N 79 3 2
#
# CMP 62
CMP 2 2.8225 1.955197 270 N R22 ERJ-3EKF2202V ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/lecs/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'ERJ-3EKF2202V'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '22k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P22.0KHCT-ND'
PRP Supplier_Part_Number_2 '64R5330'
PRP Supplier_Part_Number_3 '667-ERJ-3EKF2202V'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '22.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '22k0'
PRP ValueDisplayed '22.0k'
PRP VDC_V '50V'
TOP 0 2.8225 1.9276379 180 N 67 13 1
TOP 1 2.8225 1.982756 180 N 87 31 2
#
# CMP 63
CMP 2 2.6575 1.955197 270 N R20 ERA-3AEB104V ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/lecs/www-data/pdf/AOA0000/AOA0000CE26.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E192'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'ERA-3AEB104V'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '100k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P100KDBCT-ND'
PRP Supplier_Part_Number_2 '08N2096'
PRP Supplier_Part_Number_3 '667-ERA-3AEB104V'
PRP Technology 'Thin Film'
PRP TempCo '25 ppm/C'
PRP Tolerance__ '0.1%'
PRP U/M 'EA'
PRP Value '100k'
PRP Value1 '0.1%'
PRP Value2 '0.1W'
PRP Value_Code '100k'
PRP ValueDisplayed '100k'
PRP VDC_V '75V'
TOP 0 2.6575 1.9276379 180 N 30 11 1
TOP 1 2.6575 1.982756 180 N 87 29 2
#
# CMP 64
CMP 1 0.1470133 1.5433508 180 N R19 RC0603FR-0741K2L ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.yageo.com/pdf/Pu-RC0603_51_PbFree_L_2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Yageo'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'RC0603FR-0741K2L'
PRP Power_W '100mW'
PRP Res_ohm '41.2k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '311-41.2KHRCT-ND'
PRP Supplier_Part_Number_2 '603-RC0603FR-0741K2L'
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '41.2k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '41k2'
PRP ValueDisplayed '41.2k'
PRP VDC_V '75V'
TOP 0 0.1785094 1.5433508 90 N 88 34 1
TOP 1 0.1155173 1.5433508 90 N 1 2 2
#
# CMP 65
CMP 2 2.9325 1.5746024 180 N R9 CRCW06035K10JNEA ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'CRCW06035K10JNEA'
PRP Power_W '100mW'
PRP Res_ohm '5.1k'
PRP RoHS 'E'
PRP SizeArea_mm2 '1.28'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '541-5.1KGCT-ND'
PRP Supplier_Part_Number_2 '89M6773'
PRP Supplier_Part_Number_3 '1570751'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP Value '5.1k'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '5k10'
PRP ValueDisplayed '5.1k'
PRP VDC_V '75V'
TOP 0 2.9600591 1.5746024 90 N 52 7 1
TOP 1 2.904941 1.5746024 90 N 87 30 2
#
# CMP 66
CMP 2 2.2996323 1.6028076 0 N R17 ERJ-3GEY0R00V ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'ERJ-3GEY0R00V'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 'P0.0GCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-3GEY0R00V'
PRP Supplier_Part_Number_3 '2059527'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 2.2720732 1.6028076 270 N 55 6 1
TOP 1 2.3271913 1.6028076 270 N 37 5 2
#
# CMP 67
CMP 2 2.3719456 1.700643 0 N R16 ERJ-3GEY0R00V ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'ERJ-3GEY0R00V'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 'P0.0GCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-3GEY0R00V'
PRP Supplier_Part_Number_3 '2059527'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 2.3443865 1.700643 270 N 7 2 1
TOP 1 2.3995046 1.700643 270 N 37 4 2
#
# CMP 68
CMP 2 2.3719456 1.936332 0 N R15 ERJ-3GEY0R00V ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'ERJ-3GEY0R00V'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 'P0.0GCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-3GEY0R00V'
PRP Supplier_Part_Number_3 '2059527'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 2.3443865 1.936332 270 N 8 5 1
TOP 1 2.3995046 1.936332 270 N 67 10 2
#
# CMP 69
CMP 2 2.3719456 1.858143 0 N R14 ERJ-3GEY0R00V ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'ERJ-3GEY0R00V'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 'P0.0GCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-3GEY0R00V'
PRP Supplier_Part_Number_3 '2059527'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 2.3443865 1.858143 270 N 9 2 1
TOP 1 2.3995046 1.858143 270 N 68 12 2
#
# CMP 70
CMP 2 2.3719456 1.780643 0 N R13 ERJ-3GEY0R00V ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'ERJ-3GEY0R00V'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 'P0.0GCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-3GEY0R00V'
PRP Supplier_Part_Number_3 '2059527'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 2.3443865 1.780643 270 N 13 2 1
TOP 1 2.3995046 1.780643 270 N 30 12 2
#
# CMP 71
CMP 1 1.0034606 2.4225242 0 N R7 RC0603FR-0710KL ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.yageo.com/pdf/Pu-RC0603_51_PbFree_L_2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Yageo'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'RC0603FR-0710KL'
PRP Power_W '100mW'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '311-10.0KHRCT-ND'
PRP Supplier_Part_Number_2 '603-RC0603FR-0710KL'
PRP Supplier_Part_Number_3 '9238603'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '75V'
TOP 0 0.9719645 2.4225242 270 N 88 28 1
TOP 1 1.0349566 2.4225242 270 N 24 2 2
#
# CMP 72
CMP 1 0.5784068 2.4224786 0 N R6 RC0603FR-0710KL ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.yageo.com/pdf/Pu-RC0603_51_PbFree_L_2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Yageo'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'RC0603FR-0710KL'
PRP Power_W '100mW'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '311-10.0KHRCT-ND'
PRP Supplier_Part_Number_2 '603-RC0603FR-0710KL'
PRP Supplier_Part_Number_3 '9238603'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '75V'
TOP 0 0.5469107 2.4224786 270 N 88 27 1
TOP 1 0.6099028 2.4224786 270 N 25 2 2
#
# CMP 73
CMP 8 0.115 2.2 270 N R5 3352T-1-253LF ;0=2,1=0.1701
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.bourns.com/data/global/PDFs/3352.pdf'
PRP CompType 'Trimmer'
PRP LatestRevisionDate '09/03/2017'
PRP Manufacturer 'Bourns'
PRP MountType 'TH'
PRP PackageReference '9.53x8.89mm'
PRP PartNumber '3352T-1-253LF'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '3352T-253LF-ND'
PRP Supplier_Part_Number_2 '32K8170'
PRP Supplier_Part_Number_3 '652-3352T-1-253LF'
PRP Value '25k'
TOP 0 0.115 2.1 270 N 87 32 1
TOP 1 0.115 2.2 270 N 20 3 2
TOP 2 0.115 2.3 270 N 88 53 3
#
# CMP 74
CMP 1 1.6916608 2.4226406 0 N R3 RC0603FR-0710KL ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.yageo.com/pdf/Pu-RC0603_51_PbFree_L_2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Yageo'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'RC0603FR-0710KL'
PRP Power_W '100mW'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '311-10.0KHRCT-ND'
PRP Supplier_Part_Number_2 '603-RC0603FR-0710KL'
PRP Supplier_Part_Number_3 '9238603'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '75V'
TOP 0 1.6601647 2.4226406 270 N 38 2 1
TOP 1 1.7231568 2.4226406 270 N 87 21 2
#
# CMP 75
CMP 1 1.2665232 2.4225242 0 N R2 RC0603FR-0710KL ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.yageo.com/pdf/Pu-RC0603_51_PbFree_L_2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Yageo'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'RC0603FR-0710KL'
PRP Power_W '100mW'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '311-10.0KHRCT-ND'
PRP Supplier_Part_Number_2 '603-RC0603FR-0710KL'
PRP Supplier_Part_Number_3 '9238603'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '75V'
TOP 0 1.2350271 2.4225242 270 N 39 2 1
TOP 1 1.2980192 2.4225242 270 N 87 20 2
#
# CMP 76
CMP 1 0.84 2.4225 0 N R1 RC0603FR-0710KL ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.yageo.com/pdf/Pu-RC0603_51_PbFree_L_2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Yageo'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'RC0603FR-0710KL'
PRP Power_W '100mW'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '311-10.0KHRCT-ND'
PRP Supplier_Part_Number_2 '603-RC0603FR-0710KL'
PRP Supplier_Part_Number_3 '9238603'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '75V'
TOP 0 0.8085039 2.4225 270 N 40 2 1
TOP 1 0.871496 2.4225 270 N 87 19 2
#
# CMP 77
CMP 13 3.473189 0.7669094 0 N Q2 BUK9D23-40EX ;0=1,1=0.0276
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ChMode 'False'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://assets.nexperia.com/documents/data-sheet/BUK9D23-40E.pdf'
PRP datasheet 'https://assets.nexperia.com/documents/data-sheet/BUK9D23-40E.pdf'
PRP Datasheet_Path 'datasheets/Trans-BUK9D23-40EX.pdf'
PRP Device_Class_L1 'Discrete Semiconductors'
PRP Device_Class_L2 'Transistors'
PRP Device_Class_L3 'MOSFETs'
PRP Digikey_Description 'MOSFET N-CH 40V 8A 6DFN2020MD'
PRP Digikey_Part_Number '1727-7413-1-ND'
PRP Drain_To_Source_Breakdown_Voltage '40V'
PRP helpURL 'https://upverter.com/upn/revision/bf3b926f6919405d/'
PRP IdsMax_A '8A'
PRP Input_Capacitace_At_Vds '637pF @ 20V'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Nexperia'
PRP Mouser_Part_Number '771-BUK9D23-40EX'
PRP Number_Of_Channels '1'
PRP Number_Of_N_Channels '1'
PRP Operating_Temperature_Range '-55°C to +175°C'
PRP PackageReference 'SOT1220'
PRP Part_Number 'BUK9D23-40EX'
PRP PartNumber 'BUK9D23-40EX'
PRP Power_W '2.3W'
PRP Pulse_Drain_Current '76A'
PRP QgTyp_nC '11.5nC @ 10V'
PRP Rdson45_ohm '0.018'
PRP Reverse_Recovery_Charge '5.3nC'
PRP Reverse_Recovery_Time '12.9ns'
PRP RoHS 'TRUE'
PRP Rthja_Max '57K/W'
PRP SizeZ_mm '0.65mm'
PRP TaMax_C '+175°C'
PRP TaMin_C '-55°C'
PRP Threshold_Vgs_Max '2.1V'
PRP Threshold_Vgs_Min '1.4V'
PRP TJmax_C '+175°C'
PRP Transconductance '39S'
PRP Turn_Off_Delay_Time '12ns'
PRP Turn_On_Delay_Time '2ns'
PRP Typ_Forward_Diode_Voltage '0.8V'
PRP VdsMax_V '1.2V'
PRP Vgs_V '15V'
TOP 0 3.436378 0.7925 0 N 80 11 1
TOP 1 3.436378 0.7669094 0 N 80 10 2
TOP 2 3.436378 0.7413188 0 N 75 2 3
TOP 3 3.51 0.7413188 0 N 65 2 4
TOP 4 3.51 0.7669094 0 N 80 9 5
TOP 5 3.51 0.7925 0 N 80 8 6
TOP 6 3.473189 0.7781299 0 N 80 7 7
TOP 7 3.473189 0.7363976 0 N 65 1 8
#
# CMP 78
CMP 37 3.48375 0.5875517 270 N Q1 FMMT620TA ;0=1,1=0.0433
PRP AEC_Category 'Q101'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.diodes.com/datasheets/FMMT620.pdf'
PRP CompType 'BJT'
PRP HfeMax '900'
PRP IcRated_A '1.5A'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Diodes Inc.'
PRP MountType 'SMT'
PRP NPN '1'
PRP PackageReference 'SOT-23'
PRP PartNumber 'FMMT620TA'
PRP PNP '0'
PRP Published '2008-07-31'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '7.5'
PRP SizeAreaWB_mm2 '14'
PRP SizeX_mm '2.5'
PRP SizeY_mm '3'
PRP SizeZ_mm '1.1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'FMMT620CT-ND'
PRP Supplier_Part_Number_2 '65T9129'
PRP Supplier_Part_Number_3 '522-FMMT620TA'
PRP TaMax_C '150°C'
PRP TaMin_C '-55°C'
PRP U/M 'EA'
PRP Value '80 V'
PRP Value1 '1.5 A'
PRP Value2 '900'
PRP Vceo_V '80V'
PRP Vcesat1_V '160mV'
TOP 0 3.4463484 0.5442446 180 N 76 1 1
TOP 1 3.5211515 0.5442446 180 N 77 1 2
TOP 2 3.48375 0.6308588 180 N 75 1 3
#
# CMP 79
CMP 18 1.6425 0.6721974 270 N TP2 PWM_EXT ;0=2,1=0.1811
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName ''
PRP CNHeader 'FALSE'
PRP Color 'White'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.keyelco.com/userAssets/file/M60-2p60.pdf'
PRP CompType 'Test Point'
PRP ContactFinish 'Silver'
PRP CT 'TRUE'
PRP Current_A ''
PRP Gender ''
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Keystone Electronics'
PRP MountType 'TH'
PRP Note ''
PRP Orientation ''
PRP PackageReference 'White Miniature Testpoint'
PRP PartNumber '5002'
PRP PinCount ''
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '36-5002-ND'
PRP Supplier_Part_Number_2 '82H9632'
PRP Supplier_Part_Number_3 '534-5002'
PRP Voltage_V ''
TOP 0 1.6425 0.6721974 270 N 36 2 1
#
# CMP 80
CMP 15 3.9856096 0.5813892 180 N TP19 PGND ;0=2,1=0.2610
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName ''
PRP CNHeader 'False'
PRP Color ''
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://cdn.harwin.com/pdfs/D3080-D3083.pdf'
PRP CompType 'Jumper Wire'
PRP ContactFinish ''
PRP CT 'False'
PRP Current_A ''
PRP Gender ''
PRP Green_EU_RoHS 'Passed with Exemption'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '2017-07-12'
PRP Manufacturer 'Harwin'
PRP MountType 'TH'
PRP Note ''
PRP Orientation ''
PRP PackageReference 'Shorting Plug, 10.16mm spacing, TH'
PRP PartNumber 'D3082-05'
PRP PinCount ''
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '952-1873-ND'
PRP Supplier_Part_Number_2 '01E9240'
PRP Supplier_Part_Number_3 '855-D3082-05'
PRP Voltage_V ''
TOP 0 4.1856096 0.5813892 180 N 69 24 1
TOP 1 3.7856096 0.5813892 180 N 69 25 2
#
# CMP 81
CMP 38 2.82 0.33 180 N L4 SRP1038A-1R0M ;0=1,1=0.1575
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.bourns.com/docs/Product-Datasheets/SRP1038A.pdf'
PRP CompType 'Inductor'
PRP DCR_ohm '3m'
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP Imax_A '18A'
PRP Ind_H '1µH'
PRP Irms '18A @ 40C rise'
PRP Isat '36A @ 20% inductance drop'
PRP LatestRevisionDate '2017-06-02'
PRP Manufacturer 'Bourns'
PRP Material 'Powdered Iron'
PRP MountType 'SMT'
PRP PackageReference '11x10mm'
PRP PartNumber 'SRP1038A-1R0M'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '110'
PRP SizeAreaWB_mm2 '156'
PRP SizeX_mm '11'
PRP SizeY_mm '10'
PRP SizeZ_mm '4'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'SRP1038A-1R0MCT-ND'
PRP Supplier_Part_Number_2 '64X8595'
PRP Supplier_Part_Number_3 '652-SRP1038A-1R0M'
PRP Technology 'Shielded'
PRP Value '1uH'
PRP Value1 '0.003 ohm'
PRP Value2 '18A'
PRP ValueDisplayed '1uH'
TOP 0 3.0070079 0.33 180 N 80 6 1
TOP 1 2.6329921 0.33 0 N 63 6 2
#
# CMP 82
CMP 2 0.295 0.5975 180 N L3 BLM18SG121TZ1D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://www.murata.com/en-us/products/productdata/8796750610462/QNFA9122.pdf'
PRP CompType 'Inductor'
PRP DCR_ohm '120 ohm'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Imax_A '3A'
PRP Ind_H ''
PRP Irms ''
PRP Isat ''
PRP Manufacturer 'MuRata'
PRP Material 'Ferrite'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'BLM18SG121TZ1D'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Ferrite Bead'
PRP Value ''
PRP Value1 '120 ohm'
PRP Value2 '3A'
PRP ValueDisplayed ''
TOP 0 0.3225591 0.5975 90 N 58 6 1
TOP 1 0.267441 0.5975 90 N 23 2 2
#
# CMP 83
CMP 43 3.0470709 1.3602102 180 N L1 78438335470 ;0=1,1=0.0591
PRP AccessRights ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP AncestorItemRevisionGUID ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://katalog.we-online.de/pbs/datasheet/78438335470.pdf'
PRP ComponentType ''
PRP CompType 'Inductor'
PRP ContentType ''
PRP ContentTypeGUID ''
PRP DCR_ohm '2.3'
PRP Folder ''
PRP FolderGUID ''
PRP FootprintDescription1 ''
PRP FootprintName1 ''
PRP FootprintRevisionID1 ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Imax_A '390mA'
PRP Ind_H '47µH'
PRP Irms '0.39A @ 40C rise'
PRP Isat '1.18A @ 20% inductance drop'
PRP ItemDescription ''
PRP ItemGUID ''
PRP ItemHRID ''
PRP LatestRevisionDate '2017-06-02'
PRP LifeCycle ''
PRP LifeCycleStateGUID ''
PRP Manufacturer 'Wurth Elektronik'
PRP Material 'Powdered Iron'
PRP MountType 'SMT'
PRP PackageReference 'SMD, 2-Leads, Body 3x3mm'
PRP PartNumber '78438335470'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP ReleaseDate ''
PRP ReleaseNote ''
PRP RevisionId ''
PRP RevisionNamingSchemeGUID ''
PRP RoHS 'Y'
PRP SizeArea_mm2 '9'
PRP SizeAreaWB_mm2 '16'
PRP SizeX_mm '3'
PRP SizeY_mm '3'
PRP SizeZ_mm '1.5'
PRP SourceGUID ''
PRP SourceVaultGUID ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '732-6947-1-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Shielded'
PRP Value '47uH'
PRP Value1 '2.3 ohm'
PRP Value2 '0.39A'
PRP ValueDisplayed '47uH'
TOP 0 3.0884095 1.3602102 180 N 66 4 1
TOP 1 3.0057323 1.3602102 0 N 83 6 2
#
# CMP 84
CMP 29 4.005 1.565831 270 N J8 MOTOR_OUT ;0=2,1=0.5118
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS 'Y'
PRP Cert_UL ''
PRP Cert_VDE 'Y'
PRP ClassName ''
PRP CNHeader 'False'
PRP Color 'Blue'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.on-shore.com/sites/default/files/manuals/ed120ds.pdf'
PRP CompType 'Terminal Block'
PRP ContactFinish 'Brass'
PRP CT 'True'
PRP Current_A '15A'
PRP Gender 'Female'
PRP Green_EU_RoHS 'Incomplete'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Not Set'
PRP Green_REACh 'Incomplete'
PRP LatestRevisionDate '2017-07-12'
PRP Manufacturer 'On-Shore Technology'
PRP MountType 'TH'
PRP Note ''
PRP Orientation 'Vertical'
PRP PackageReference '3x1 5.08 mm Terminal Block'
PRP PartNumber 'ED120/3DS'
PRP PinCount '3'
PRP Pitch_mm '5.08'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count '1'
PRP RowSpacing_mm ''
PRP Shrouded 'N'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'ED1610-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Voltage_V '300V'
TOP 0 4.005 1.365831 0 N 72 2 1
TOP 1 4.005 1.565831 0 N 71 3 2
TOP 2 4.005 1.765831 0 N 70 3 3
#
# CMP 85
CMP 31 2.51877 2.2241473 0 N J13 HALL_PWR_SEL ;0=2,1=0.3300
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName 'Header'
PRP CNHeader 'TRUE'
PRP Color ''
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.sullinscorp.com/catalogs/77_Page78-79_HEADER_.100_2.54mm_MALE_BREAKAWAY.pdf'
PRP CompType 'Header'
PRP ContactFinish ''
PRP CT 'FALSE'
PRP Current_A ''
PRP Gender ''
PRP Green_EU_RoHS 'Incomplete'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Not Set'
PRP Green_REACh 'Incomplete'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Sullins Connector Solutions'
PRP MountType 'TH'
PRP Note ''
PRP Orientation ''
PRP PackageReference 'PBC03SAAN'
PRP PartNumber 'PBC03SAAN'
PRP PinCount ''
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'S1011E-03-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Voltage_V ''
TOP 0 2.41877 2.2241473 0 N 51 3 1
TOP 1 2.51877 2.2241473 0 N 82 5 2
TOP 2 2.61877 2.2241473 0 N 83 10 3
#
# CMP 86
CMP 30 3.1952165 2.625 180 N J12 OSTTE080161 ;0=2,1=0.3307
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName ''
PRP CNHeader 'False'
PRP Color ''
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.on-shore.com/sites/default/files/manuals/osttexx0161.pdf'
PRP CompType 'Terminal Block'
PRP ContactFinish ''
PRP CT 'True'
PRP Current_A ''
PRP Gender ''
PRP Green_EU_RoHS 'Incomplete'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Not Set'
PRP Green_REACh 'Incomplete'
PRP LatestRevisionDate '2017-07-12'
PRP Manufacturer 'On-Shore Technology'
PRP MountType 'TH'
PRP Note ''
PRP Orientation ''
PRP PackageReference '8x1 Terminal Block'
PRP PartNumber 'OSTTE080161'
PRP PinCount ''
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'ED2641-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Voltage_V ''
TOP 0 3.6775 2.625 180 N 88 52 1
TOP 1 3.5397047 2.625 180 N 48 11 2
TOP 2 3.4019094 2.625 180 N 45 8 3
TOP 3 3.2641142 2.625 180 N 49 11 4
TOP 4 3.1263189 2.625 180 N 46 8 5
TOP 5 2.9885236 2.625 180 N 50 11 6
TOP 6 2.8507283 2.625 180 N 47 8 7
TOP 7 2.7129331 2.625 180 N 82 6 8
#
# CMP 87
CMP 29 3.45 0.2618411 0 N J7 MOTOR_OUT ;0=2,1=0.5118
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS 'Y'
PRP Cert_UL ''
PRP Cert_VDE 'Y'
PRP ClassName ''
PRP CNHeader 'False'
PRP Color 'Blue'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.on-shore.com/sites/default/files/manuals/ed120ds.pdf'
PRP CompType 'Terminal Block'
PRP ContactFinish 'Brass'
PRP CT 'True'
PRP Current_A '15A'
PRP Gender 'Female'
PRP Green_EU_RoHS 'Incomplete'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Not Set'
PRP Green_REACh 'Incomplete'
PRP LatestRevisionDate '2017-07-12'
PRP Manufacturer 'On-Shore Technology'
PRP MountType 'TH'
PRP Note ''
PRP Orientation 'Vertical'
PRP PackageReference '3x1 5.08 mm Terminal Block'
PRP PartNumber 'ED120/3DS'
PRP PinCount '3'
PRP Pitch_mm '5.08'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count '1'
PRP RowSpacing_mm ''
PRP Shrouded 'N'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'ED1610-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Voltage_V '300V'
TOP 0 3.25 0.2618411 90 N 63 16 1
TOP 1 3.45 0.2618411 90 N 69 23 2
TOP 2 3.65 0.2618411 90 N 65 4 3
#
# CMP 88
CMP 31 1.5425 0.1375 180 N J5 Header_3x1 ;0=2,1=0.3300
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName 'Header'
PRP CNHeader 'TRUE'
PRP Color ''
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.sullinscorp.com/catalogs/77_Page78-79_HEADER_.100_2.54mm_MALE_BREAKAWAY.pdf'
PRP CompType 'Header'
PRP ContactFinish ''
PRP CT 'FALSE'
PRP Current_A ''
PRP Gender ''
PRP Green_EU_RoHS 'Incomplete'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Not Set'
PRP Green_REACh 'Incomplete'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Sullins Connector Solutions'
PRP MountType 'TH'
PRP Note ''
PRP Orientation ''
PRP PackageReference 'PBC03SAAN'
PRP PartNumber 'PBC03SAAN'
PRP PinCount ''
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'S1011E-03-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Voltage_V ''
TOP 0 1.6425 0.1375 180 N 18 2 1
TOP 1 1.5425 0.1375 180 N 59 20 2
TOP 2 1.4425 0.1375 180 N 60 14 3
#
# CMP 89
CMP 31 0.6808858 0.1375 180 N J3 Header_3x1 ;0=2,1=0.3300
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName 'Header'
PRP CNHeader 'TRUE'
PRP Color ''
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.sullinscorp.com/catalogs/77_Page78-79_HEADER_.100_2.54mm_MALE_BREAKAWAY.pdf'
PRP CompType 'Header'
PRP ContactFinish ''
PRP CT 'FALSE'
PRP Current_A ''
PRP Gender ''
PRP Green_EU_RoHS 'Incomplete'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Not Set'
PRP Green_REACh 'Incomplete'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Sullins Connector Solutions'
PRP MountType 'TH'
PRP Note ''
PRP Orientation ''
PRP PackageReference 'PBC03SAAN'
PRP PartNumber 'PBC03SAAN'
PRP PinCount ''
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'S1011E-03-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Voltage_V ''
TOP 0 0.7808858 0.1375 180 N 26 3 1
TOP 1 0.6808858 0.1375 180 N 57 7 2
TOP 2 0.5808858 0.1375 180 N 58 9 3
#
# CMP 90
CMP 18 2.4523172 1.1375 270 N TP12 ILIM ;0=2,1=0.1811
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName ''
PRP CNHeader 'FALSE'
PRP Color 'White'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.keyelco.com/userAssets/file/M60-2p60.pdf'
PRP CompType 'Test Point'
PRP ContactFinish 'Silver'
PRP CT 'TRUE'
PRP Current_A ''
PRP Gender ''
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Keystone Electronics'
PRP MountType 'TH'
PRP Note ''
PRP Orientation ''
PRP PackageReference 'White Miniature Testpoint'
PRP PartNumber '5002'
PRP PinCount ''
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '36-5002-ND'
PRP Supplier_Part_Number_2 '82H9632'
PRP Supplier_Part_Number_3 '534-5002'
PRP Voltage_V ''
TOP 0 2.4523172 1.1375 270 N 81 9 1
#
# CMP 91
CMP 18 3.4019094 2.13 270 N TP30 HNA ;0=2,1=0.1811
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName ''
PRP CNHeader 'FALSE'
PRP Color 'White'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.keyelco.com/userAssets/file/M60-2p60.pdf'
PRP CompType 'Test Point'
PRP ContactFinish 'Silver'
PRP CT 'TRUE'
PRP Current_A ''
PRP Gender ''
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Keystone Electronics'
PRP MountType 'TH'
PRP Note ''
PRP Orientation ''
PRP PackageReference 'White Miniature Testpoint'
PRP PartNumber '5002'
PRP PinCount ''
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '36-5002-ND'
PRP Supplier_Part_Number_2 '82H9632'
PRP Supplier_Part_Number_3 '534-5002'
PRP Voltage_V ''
TOP 0 3.4019094 2.13 270 N 45 7 1
#
# CMP 92
CMP 18 3.1263189 2.13 270 N TP28 HNB ;0=2,1=0.1811
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName ''
PRP CNHeader 'FALSE'
PRP Color 'White'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.keyelco.com/userAssets/file/M60-2p60.pdf'
PRP CompType 'Test Point'
PRP ContactFinish 'Silver'
PRP CT 'TRUE'
PRP Current_A ''
PRP Gender ''
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Keystone Electronics'
PRP MountType 'TH'
PRP Note ''
PRP Orientation ''
PRP PackageReference 'White Miniature Testpoint'
PRP PartNumber '5002'
PRP PinCount ''
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '36-5002-ND'
PRP Supplier_Part_Number_2 '82H9632'
PRP Supplier_Part_Number_3 '534-5002'
PRP Voltage_V ''
TOP 0 3.1263189 2.13 270 N 46 7 1
#
# CMP 93
CMP 18 2.8507283 2.13 270 N TP21 HNC ;0=2,1=0.1811
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName ''
PRP CNHeader 'FALSE'
PRP Color 'White'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.keyelco.com/userAssets/file/M60-2p60.pdf'
PRP CompType 'Test Point'
PRP ContactFinish 'Silver'
PRP CT 'TRUE'
PRP Current_A ''
PRP Gender ''
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Keystone Electronics'
PRP MountType 'TH'
PRP Note ''
PRP Orientation ''
PRP PackageReference 'White Miniature Testpoint'
PRP PartNumber '5002'
PRP PinCount ''
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '36-5002-ND'
PRP Supplier_Part_Number_2 '82H9632'
PRP Supplier_Part_Number_3 '534-5002'
PRP Voltage_V ''
TOP 0 2.8507283 2.13 270 N 47 7 1
#
# CMP 94
CMP 18 3.5396496 2.13 90 N TP31 HPA ;0=2,1=0.1811
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName ''
PRP CNHeader 'FALSE'
PRP Color 'White'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.keyelco.com/userAssets/file/M60-2p60.pdf'
PRP CompType 'Test Point'
PRP ContactFinish 'Silver'
PRP CT 'TRUE'
PRP Current_A ''
PRP Gender ''
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Keystone Electronics'
PRP MountType 'TH'
PRP Note ''
PRP Orientation ''
PRP PackageReference 'White Miniature Testpoint'
PRP PartNumber '5002'
PRP PinCount ''
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '36-5002-ND'
PRP Supplier_Part_Number_2 '82H9632'
PRP Supplier_Part_Number_3 '534-5002'
PRP Voltage_V ''
TOP 0 3.5396496 2.13 90 N 48 10 1
#
# CMP 95
CMP 18 3.2641142 2.13 270 N TP29 HPB ;0=2,1=0.1811
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName ''
PRP CNHeader 'FALSE'
PRP Color 'White'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.keyelco.com/userAssets/file/M60-2p60.pdf'
PRP CompType 'Test Point'
PRP ContactFinish 'Silver'
PRP CT 'TRUE'
PRP Current_A ''
PRP Gender ''
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Keystone Electronics'
PRP MountType 'TH'
PRP Note ''
PRP Orientation ''
PRP PackageReference 'White Miniature Testpoint'
PRP PartNumber '5002'
PRP PinCount ''
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '36-5002-ND'
PRP Supplier_Part_Number_2 '82H9632'
PRP Supplier_Part_Number_3 '534-5002'
PRP Voltage_V ''
TOP 0 3.2641142 2.13 270 N 49 10 1
#
# CMP 96
CMP 18 2.9885236 2.13 270 N TP22 HPC ;0=2,1=0.1811
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName ''
PRP CNHeader 'FALSE'
PRP Color 'White'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.keyelco.com/userAssets/file/M60-2p60.pdf'
PRP CompType 'Test Point'
PRP ContactFinish 'Silver'
PRP CT 'TRUE'
PRP Current_A ''
PRP Gender ''
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Keystone Electronics'
PRP MountType 'TH'
PRP Note ''
PRP Orientation ''
PRP PackageReference 'White Miniature Testpoint'
PRP PartNumber '5002'
PRP PinCount ''
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '36-5002-ND'
PRP Supplier_Part_Number_2 '82H9632'
PRP Supplier_Part_Number_3 '534-5002'
PRP Voltage_V ''
TOP 0 2.9885236 2.13 270 N 50 9 1
#
# CMP 97
CMP 12 4.125 0.465 0 N FID3 Fiducial ;0=1,1=0.0276
PRP ClassName 'FiducialMark'
PRP CompType 'Fiducial'
PRP Manufacturer 'N/A'
PRP MountType 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 4.125 0.465 0 N 0 17 1
#
# CMP 98
CMP 12 3.88 2.445 0 N FID2 Fiducial ;0=1,1=0.0276
PRP ClassName 'FiducialMark'
PRP CompType 'Fiducial'
PRP Manufacturer 'N/A'
PRP MountType 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 3.88 2.445 0 N 0 18 1
#
# CMP 99
CMP 12 0.395 2.47 0 N FID1 Fiducial ;0=1,1=0.0276
PRP ClassName 'FiducialMark'
PRP CompType 'Fiducial'
PRP Manufacturer 'N/A'
PRP MountType 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 0.395 2.47 0 N 0 20 1
#
# CMP 100
CMP 18 2.240636 1.4025 270 N TP11 FGOUT ;0=2,1=0.1811
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName ''
PRP CNHeader 'FALSE'
PRP Color 'White'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.keyelco.com/userAssets/file/M60-2p60.pdf'
PRP CompType 'Test Point'
PRP ContactFinish 'Silver'
PRP CT 'TRUE'
PRP Current_A ''
PRP Gender ''
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Keystone Electronics'
PRP MountType 'TH'
PRP Note ''
PRP Orientation ''
PRP PackageReference 'White Miniature Testpoint'
PRP PartNumber '5002'
PRP PinCount ''
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '36-5002-ND'
PRP Supplier_Part_Number_2 '82H9632'
PRP Supplier_Part_Number_3 '534-5002'
PRP Voltage_V ''
TOP 0 2.240636 1.4025 270 N 52 8 1
#
# CMP 101
CMP 36 3.5975 0.5225 180 N D7 BAS516,115 ;0=1,1=0.0276
PRP AEC_Category 'Q101'
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.nexperia.com/documents/data_sheet/BAS16_SER.pdf'
PRP CompType 'Diode'
PRP Green_EU_RoHS 'Incomplete'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Not Set'
PRP Green_REACh 'Incomplete'
PRP Io_A '250mA'
PRP Manufacturer 'Nexperia'
PRP MountType 'SMT'
PRP PackageReference 'SOD-523'
PRP PartNumber 'BAS516,115'
PRP RJC_CperW ''
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.53'
PRP SizeAreaWB_mm2 '5.13'
PRP SizeX_mm '1.7'
PRP SizeY_mm '0.9'
PRP SizeZ_mm '0.65'
PRP TJmax_C '150°C'
PRP Type 'Switching'
PRP Value '100V'
PRP Value1 '0.25A'
PRP Value2 '1.25V'
PRP Vf_V '1.25V'
PRP Vr_V '100V'
TOP 0 3.6191535 0.5225 90 N 65 3 1
TOP 1 3.5758465 0.5225 90 N 77 2 2
#
# CMP 102
CMP 21 1.1895234 1.1480431 180 N D6 LTST-C190GKT ;0=1,1=0.0354
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Angle ''
PRP Color 'green'
PRP ColorTemperature ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://sps06.itg.ti.com/sites/KMS/crossdivteams/altium/docs/ComponentDatasheets/LTST-C190GKT.pdf'
PRP CompType 'LED'
PRP DynamicResistance ''
PRP Family_Io ''
PRP FamilyName ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Io_A '20mA'
PRP Ir_A ''
PRP LambdaD ''
PRP LambdaP ''
PRP Luminance_Lv ''
PRP LuminousFlux_PhiV ''
PRP LuminousIntensity_IV ''
PRP Manufacturer 'Lite-On'
PRP MountType 'SMT'
PRP NumParallelLEDs ''
PRP NumSeriesLEDs ''
PRP PackageReference '1.6x0.8x0.8mm'
PRP PartNumber 'LTST-C190GKT'
PRP Power_TotalModule '100mW'
PRP RJC_CperW ''
PRP RoHS 'Y'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm ''
PRP TJmax_C ''
PRP Type '?'
PRP Value 'Green'
PRP Value1 '0.1W'
PRP Value2 '2.1V'
PRP Vf_V '2.1V'
PRP Vr_V ''
TOP 0 1.2190509 1.1480431 180 N 41 3 1
TOP 1 1.1599958 1.1480431 180 N 43 2 2
#
# CMP 103
CMP 22 1.1895234 1.2951494 180 N D5 LTST-C190KRKT ;0=1,1=0.0354
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Angle '130'
PRP Color 'Red'
PRP ColorTemperature ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://optoelectronics.liteon.com/upload/download/DS-22-99-0151/LTST-C190KRKT.pdf'
PRP CompType 'LED'
PRP DynamicResistance ''
PRP Family_Io ''
PRP FamilyName ''
PRP Green_EU_RoHS 'Incomplete'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Not Set'
PRP Green_REACh 'Incomplete'
PRP Io_A '20mA'
PRP Ir_A '10µA'
PRP LambdaD ''
PRP LambdaP ''
PRP Luminance_Lv ''
PRP LuminousFlux_PhiV ''
PRP LuminousIntensity_IV ''
PRP Manufacturer 'Lite-On'
PRP MountType 'SMT'
PRP NumParallelLEDs ''
PRP NumSeriesLEDs ''
PRP PackageReference 'Red LED, 1.6x0.8x0.8mm'
PRP PartNumber 'LTST-C190KRKT'
PRP Power_TotalModule '62.5mW'
PRP RJC_CperW ''
PRP RoHS 'Y'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm ''
PRP TJmax_C ''
PRP Type 'AlInGaP'
PRP Value 'Red'
PRP Value1 '.0625W'
PRP Value2 '2V'
PRP Vf_V '2V'
PRP Vr_V '5V'
TOP 0 1.2190509 1.2951494 180 N 42 3 1
TOP 1 1.1599958 1.2951494 180 N 44 2 2
#
# CMP 104
CMP 35 1.17 0.4473553 180 N D4 BAT165E6327HTSA1 ;0=1,1=0.0453
PRP AEC_Category 'Q101'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.infineon.com/dgdl/bat165series.pdf?folderId=db3a304313d846880113def5812204a1&fileId=db3a304313d846880113df01f69804d6'
PRP CompType 'Diode'
PRP Green_EU_RoHS 'Incomplete'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Not Set'
PRP Green_REACh 'Incomplete'
PRP Io_A '750mA'
PRP Manufacturer 'Infineon Technologies'
PRP MountType 'SMT'
PRP PackageReference 'SOD-323'
PRP PartNumber 'BAT165E6327HTSA1'
PRP RJC_CperW ''
PRP RoHS 'Y'
PRP SizeArea_mm2 '3.645'
PRP SizeAreaWB_mm2 '8.695'
PRP SizeX_mm '2.7'
PRP SizeY_mm '1.35'
PRP SizeZ_mm '1'
PRP TJmax_C '150°C'
PRP Type 'Schottky'
PRP Value '40V'
PRP Value1 '0.75A'
PRP Value2 '0.74V'
PRP Vf_V '740mV'
PRP Vr_V '40V'
TOP 0 1.213307 0.4473553 0 N 59 17 1
TOP 1 1.1266928 0.4473553 0 N 60 10 2
#
# CMP 105
CMP 23 2.6625196 0.6151108 270 N D3 LTST-C170KGKT ;0=1,1=0.0472
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Angle ''
PRP Color 'Green'
PRP ColorTemperature ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://optoelectronics.liteon.com/upload/download/DS22-2000-073/S_110_LTST-C170KGKT.pdf'
PRP CompType 'LED'
PRP DynamicResistance ''
PRP Family_Io ''
PRP FamilyName ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Io_A '20mA'
PRP Ir_A ''
PRP LambdaD ''
PRP LambdaP ''
PRP Luminance_Lv ''
PRP LuminousFlux_PhiV ''
PRP LuminousIntensity_IV ''
PRP Manufacturer 'Lite-On'
PRP MountType 'SMT'
PRP NumParallelLEDs ''
PRP NumSeriesLEDs ''
PRP PackageReference 'LED_0805'
PRP PartNumber 'LTST-C170KGKT'
PRP Power_TotalModule ''
PRP RJC_CperW ''
PRP RoHS 'Y'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm ''
PRP TJmax_C ''
PRP Type 'AlInGaP'
PRP Value 'Green'
PRP Value1 'W'
PRP Value2 '2V'
PRP Vf_V '2V'
PRP Vr_V ''
TOP 0 2.6625196 0.5737722 270 N 63 7 1
TOP 1 2.6625196 0.6564494 270 N 78 3 2
#
# CMP 106
CMP 20 3.3424409 1.88 0 N D2 LTST-C170KRKT ;0=1,1=0.0433
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Angle ''
PRP Color 'red'
PRP ColorTemperature ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://optoelectronics.liteon.com/upload/download/DS-22-99-0150/P_100_LTST-C170KRKT.pdf'
PRP CompType 'LED'
PRP DynamicResistance ''
PRP Family_Io ''
PRP FamilyName ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Io_A '20mA'
PRP Ir_A ''
PRP LambdaD ''
PRP LambdaP ''
PRP Luminance_Lv ''
PRP LuminousFlux_PhiV ''
PRP LuminousIntensity_IV ''
PRP Manufacturer 'Lite-On'
PRP MountType 'SMT'
PRP NumParallelLEDs ''
PRP NumSeriesLEDs ''
PRP PackageReference 'Red 0805 LED'
PRP PartNumber 'LTST-C170KRKT'
PRP Power_TotalModule ''
PRP RJC_CperW ''
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.2'
PRP TJmax_C ''
PRP Type 'AlInGaP'
PRP Value 'Red'
PRP Value1 'W'
PRP Value2 '2V'
PRP Vf_V '2V'
PRP Vr_V ''
TOP 0 3.3011023 1.88 0 N 87 26 1
TOP 1 3.3837795 1.88 0 N 62 2 2
#
# CMP 107
CMP 23 2.9733931 1.216377 90 N D1 LTST-C170KGKT ;0=1,1=0.0472
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Angle ''
PRP Color 'Green'
PRP ColorTemperature ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://optoelectronics.liteon.com/upload/download/DS22-2000-073/S_110_LTST-C170KGKT.pdf'
PRP CompType 'LED'
PRP DynamicResistance ''
PRP Family_Io ''
PRP FamilyName ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Io_A '20mA'
PRP Ir_A ''
PRP LambdaD ''
PRP LambdaP ''
PRP Luminance_Lv ''
PRP LuminousFlux_PhiV ''
PRP LuminousIntensity_IV ''
PRP Manufacturer 'Lite-On'
PRP MountType 'SMT'
PRP NumParallelLEDs ''
PRP NumSeriesLEDs ''
PRP PackageReference 'LED_0805'
PRP PartNumber 'LTST-C170KGKT'
PRP Power_TotalModule ''
PRP RJC_CperW ''
PRP RoHS 'Y'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm ''
PRP TJmax_C ''
PRP Type 'AlInGaP'
PRP Value 'Green'
PRP Value1 'W'
PRP Value2 '2V'
PRP Vf_V '2V'
PRP Vr_V ''
TOP 0 2.9733931 1.2577156 90 N 83 7 1
TOP 1 2.9733931 1.1750384 90 N 79 2 2
#
# CMP 108
CMP 2 3.4294684 2.0040158 0 N C25 0603YC104K4T4A ;0=1,1=0.0394
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://datasheets.avx.com/AutoMLCC.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'AVX'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber '0603YC104K4T4A'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '478-9382-1-ND'
PRP Supplier_Part_Number_2 '581-0603YC104K4T4A'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.1uF'
PRP Value1 ''
PRP Value2 '16V'
PRP ValueDisplayed '0.1µF'
PRP VDC_V '16V'
TOP 0 3.4019093 2.0040158 270 N 45 5 1
TOP 1 3.4570274 2.0040158 270 N 48 7 2
#
# CMP 109
CMP 2 3.1897441 2.005 0 N C24 0603YC104K4T4A ;0=1,1=0.0394
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://datasheets.avx.com/AutoMLCC.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'AVX'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber '0603YC104K4T4A'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '478-9382-1-ND'
PRP Supplier_Part_Number_2 '581-0603YC104K4T4A'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.1uF'
PRP Value1 ''
PRP Value2 '16V'
PRP ValueDisplayed '0.1µF'
PRP VDC_V '16V'
TOP 0 3.162185 2.005 270 N 46 5 1
TOP 1 3.2173031 2.005 270 N 49 7 2
#
# CMP 110
CMP 2 2.9885236 2.005 0 N C23 0603YC104K4T4A ;0=1,1=0.0394
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://datasheets.avx.com/AutoMLCC.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'AVX'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber '0603YC104K4T4A'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '478-9382-1-ND'
PRP Supplier_Part_Number_2 '581-0603YC104K4T4A'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.1uF'
PRP Value1 ''
PRP Value2 '16V'
PRP ValueDisplayed '0.1µF'
PRP VDC_V '16V'
TOP 0 2.9609645 2.005 270 N 47 5 1
TOP 1 3.0160826 2.005 270 N 50 7 2
#
# CMP 111
CMP 4 3.0275 0.5875517 0 N C22 GRM31CR72A105KA01L ;0=1,1=0.0709
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '2220'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM31CR72A105KA01L&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '1206'
PRP PartNumber 'GRM31CR72A105KA01L'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '5.12'
PRP SizeAreaWB_mm2 '10.92'
PRP SizeX_mm '3.2'
PRP SizeY_mm '1.6'
PRP SizeZ_mm '1.8'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '490-3909-1-ND'
PRP Supplier_Part_Number_2 '81-GRM31CR72A105KA01'
PRP Supplier_Part_Number_3 '1735543'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '100V'
PRP ValueDisplayed '1uF'
PRP VDC_V '100V'
TOP 0 2.9605709 0.5875517 270 N 63 5 1
TOP 1 3.0944291 0.5875517 270 N 69 10 2
#
# CMP 112
CMP 2 2.8975 0.6324514 270 N C21 CGA3E3X7S2A104K080AB ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=CGA3E3X7S2A104K080AB'
PRP CompType 'Capacitor'
PRP ESR_ohm '0.04959'
PRP IRMS_A '751.618mA'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'CGA3E3X7S2A104K080AB'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '445-6938-1-ND'
PRP Supplier_Part_Number_2 '04X3163'
PRP Supplier_Part_Number_3 '810-CGA3E3X7S2A104K'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7S'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 '0.04959 ohm'
PRP Value2 '100V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '100V'
TOP 0 2.8975 0.6048923 180 N 63 3 1
TOP 1 2.8975 0.6600104 180 N 69 5 2
#
# CMP 113
CMP 2 2.8429527 0.6324514 270 N C20 CGA3E2X7R2A103K080AA ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '10nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=CGA3E2X7R2A103K080AA'
PRP CompType 'Capacitor'
PRP ESR_ohm '0.235428'
PRP IRMS_A '396.995mA'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'CGA3E2X7R2A103K080AA'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '445-5812-1-ND'
PRP Supplier_Part_Number_2 '810-CGA3E2X7R2A103K080AA'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.01uF'
PRP Value1 '0.235428 ohm'
PRP Value2 '100V'
PRP ValueDisplayed '0.01uF'
PRP VDC_V '100V'
TOP 0 2.8429527 0.6048923 180 N 63 4 1
TOP 1 2.8429527 0.6600104 180 N 69 6 2
#
# CMP 114
CMP 2 2.785 0.6324514 270 N C19 06031C102JAT2A ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '1nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://datasheets.avx.com/X7RDielectric.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm '2.76d'
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'AVX'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber '06031C102JAT2A'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '478-3698-1-ND'
PRP Supplier_Part_Number_2 '96M1234'
PRP Supplier_Part_Number_3 '581-06031C102J'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '1000pF'
PRP Value1 '0.276 ohm'
PRP Value2 '100V'
PRP ValueDisplayed '1000pF'
PRP VDC_V '100V'
TOP 0 2.785 0.6048923 180 N 63 13 1
TOP 1 2.785 0.6600104 180 N 69 17 2
#
# CMP 115
CMP 2 3.2661799 0.8038806 270 N C18 06031C102JAT2A ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '1nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://datasheets.avx.com/X7RDielectric.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm '2.76d'
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'AVX'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber '06031C102JAT2A'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '478-3698-1-ND'
PRP Supplier_Part_Number_2 '96M1234'
PRP Supplier_Part_Number_3 '581-06031C102J'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '1000pF'
PRP Value1 '0.276 ohm'
PRP Value2 '100V'
PRP ValueDisplayed '1000pF'
PRP VDC_V '100V'
TOP 0 3.2661799 0.7763215 180 N 80 12 1
TOP 1 3.2661799 0.8314396 180 N 69 16 2
#
# CMP 116
CMP 2 3.2104332 0.8037746 270 N C17 CGA3E2X7R2A103K080AA ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '10nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=CGA3E2X7R2A103K080AA'
PRP CompType 'Capacitor'
PRP ESR_ohm '0.235428'
PRP IRMS_A '396.995mA'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'CGA3E2X7R2A103K080AA'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '445-5812-1-ND'
PRP Supplier_Part_Number_2 '810-CGA3E2X7R2A103K080AA'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.01uF'
PRP Value1 '0.235428 ohm'
PRP Value2 '100V'
PRP ValueDisplayed '0.01uF'
PRP VDC_V '100V'
TOP 0 3.2104332 0.7762155 180 N 80 3 1
TOP 1 3.2104332 0.8313336 180 N 69 7 2
#
# CMP 117
CMP 2 3.1578867 0.8035172 270 N C16 CGA3E3X7S2A104K080AB ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=CGA3E3X7S2A104K080AB'
PRP CompType 'Capacitor'
PRP ESR_ohm '0.04959'
PRP IRMS_A '751.618mA'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'CGA3E3X7S2A104K080AB'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '445-6938-1-ND'
PRP Supplier_Part_Number_2 '04X3163'
PRP Supplier_Part_Number_3 '810-CGA3E3X7S2A104K'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7S'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 '0.04959 ohm'
PRP Value2 '100V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '100V'
TOP 0 3.1578867 0.7759581 180 N 80 4 1
TOP 1 3.1578867 0.8310762 180 N 69 8 2
#
# CMP 118
CMP 4 3.3472244 0.845059 270 N C15 GRM31CR72A105KA01L ;0=1,1=0.0709
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '2220'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM31CR72A105KA01L&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '1206'
PRP PartNumber 'GRM31CR72A105KA01L'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '5.12'
PRP SizeAreaWB_mm2 '10.92'
PRP SizeX_mm '3.2'
PRP SizeY_mm '1.6'
PRP SizeZ_mm '1.8'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '490-3909-1-ND'
PRP Supplier_Part_Number_2 '81-GRM31CR72A105KA01'
PRP Supplier_Part_Number_3 '1735543'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '100V'
PRP ValueDisplayed '1uF'
PRP VDC_V '100V'
TOP 0 3.3472244 0.7781299 180 N 80 5 1
TOP 1 3.3472244 0.9119881 180 N 69 9 2
#
# CMP 119
CMP 9 2.1590748 0.33 180 N C14 ELXZ630ELL331MK20S ;0=2,1=0.8465
PRP AC_Derating ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '2'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '12.5x20mm'
PRP Cap_F '330µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.chemi-con.co.jp/cgi-bin/CAT_DB/SEARCH/cat_db_al.cgi?e=e&j=p&pdfname=lxz'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A '1.29A'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Chemi-Con'
PRP MountType 'TH'
PRP PackageReference 'D12.5xL20mm'
PRP PartNumber 'ELXZ630ELL331MK20S'
PRP Polarized 'Y'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Series 'LXZ'
PRP SizeArea_mm2 '156.25'
PRP SizeAreaWB_mm2 '210.25'
PRP SizeX_mm '12.5'
PRP SizeY_mm '12.5'
PRP SizeZ_mm '21.5'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '565-2043-ND'
PRP Supplier_Part_Number_2 '661-ELXZ630ELL331MK2'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '105°C'
PRP TaMin_C '-55°C'
PRP Technology 'AL'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '330uF'
PRP Value1 'Unknown'
PRP Value2 '63V'
PRP ValueDisplayed '330uF'
PRP VDC_V '63V'
TOP 0 2.2575 0.33 180 N 63 15 1
TOP 1 2.0606496 0.33 180 N 69 22 2
#
# CMP 120
CMP 3 0.5211614 1.2461811 180 N C13 C0805C105K5RACTU ;0=1,1=0.0571
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0805'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.kemet.com/docfinder?Partnumber=C0805C105K5RACTU'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Kemet'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'C0805C105K5RACTU'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '399-7409-1-ND'
PRP Supplier_Part_Number_2 '07W3955'
PRP Supplier_Part_Number_3 '80-C0805C105K5R'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '50V'
PRP ValueDisplayed '1uF'
PRP VDC_V '50V'
TOP 0 0.5611613 1.2461811 180 N 59 18 1
TOP 1 0.4811613 1.2461811 180 N 88 29 2
#
# CMP 121
CMP 2 0.2623555 1.4850789 180 N C12 885012206034 ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '1nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://katalog.we-online.de/pbs/datasheet/885012206034.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Wurth Elektronik'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber '885012206034'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '710-885012206034'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '1000pF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '1000pF'
PRP VDC_V '16V'
TOP 0 0.2899146 1.4850789 90 N 31 9 1
TOP 1 0.2347965 1.4850789 90 N 88 13 2
#
# CMP 122
CMP 2 0.7083797 0.464825 0 N C11 C0603C104K8RACTU ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.kemet.com/kemet/web/homepage/kechome.nsf/vapubfiles/F3102_Y5V.pdf/$file/F3102_Y5V.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Kemet'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'C0603C104K8RACTU'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '399-1095-1-ND'
PRP Supplier_Part_Number_2 '80-C0603C104K8R'
PRP Supplier_Part_Number_3 '1640032'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '10V'
TOP 0 0.6808206 0.464825 270 N 57 6 1
TOP 1 0.7359387 0.464825 270 N 88 45 2
#
# CMP 123
CMP 2 0.5979331 0.464825 0 N C10 GRM188Z71A475ME15D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '4.7µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM188Z71A475ME15-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GRM188Z71A475ME15D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 '81-GRM188Z71A475ME5D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '4.7uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '4.7uF'
PRP VDC_V '10V'
TOP 0 0.570374 0.464825 270 N 88 32 1
TOP 1 0.6254921 0.464825 270 N 57 5 2
#
# CMP 124
CMP 1 0.8425 0.9675 0 N C9 C0603C104K8RACTU ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.kemet.com/kemet/web/homepage/kechome.nsf/vapubfiles/F3102_Y5V.pdf/$file/F3102_Y5V.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Kemet'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'C0603C104K8RACTU'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '399-1095-1-ND'
PRP Supplier_Part_Number_2 '80-C0603C104K8R'
PRP Supplier_Part_Number_3 '1640032'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '10V'
TOP 0 0.8110039 0.9675 270 N 60 13 1
TOP 1 0.873996 0.9675 270 N 88 26 2
#
# CMP 125
CMP 16 3.6671496 1.765831 270 N TP10 OUTC ;0=2,1=0.1811
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName ''
PRP CNHeader 'FALSE'
PRP Color 'Red'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.keyelco.com/userAssets/file/M60-2p60.pdf'
PRP CompType 'Test Point'
PRP ContactFinish 'Silver'
PRP CT 'TRUE'
PRP Current_A ''
PRP Gender ''
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Keystone Electronics'
PRP MountType 'TH'
PRP Note ''
PRP Orientation ''
PRP PackageReference 'Red Miniature Testpoint'
PRP PartNumber '5000'
PRP PinCount ''
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '36-5000-ND'
PRP Supplier_Part_Number_2 '534-5000'
PRP Supplier_Part_Number_3 ''
PRP Voltage_V ''
TOP 0 3.6671496 1.765831 270 N 70 2 1
#
# CMP 126
CMP 0 2.9340175 1.67175 180 N C7 C1005X5R1A104K050BA ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://product.tdk.com/en/catalog/datasheets/mlcc_commercial_general_en.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'C1005X5R1A104K050BA'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '445-1265-1-ND'
PRP Supplier_Part_Number_2 '90R7585'
PRP Supplier_Part_Number_3 '810-C1005X5R1A104K'
PRP TaMax_C '85°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X5R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '10V'
TOP 0 2.9576395 1.67175 90 N 81 8 1
TOP 1 2.9103954 1.67175 90 N 88 43 2
#
# CMP 127
CMP 3 3.1881693 1.4449965 270 N C5 C2012X7R2A473K125AA ;0=1,1=0.0571
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0805'
PRP Cap_F '47nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=C2012X7R2A473K125AA'
PRP CompType 'Capacitor'
PRP ESR_ohm '0.049089'
PRP IRMS_A '9.63171dA'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'C2012X7R2A473K125AA'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '445-2276-1-ND'
PRP Supplier_Part_Number_2 '810-C2012X7R2A473K125AA'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.047uF'
PRP Value1 '0.049089 ohm'
PRP Value2 '100V'
PRP ValueDisplayed '0.047uF'
PRP VDC_V '100V'
TOP 0 3.1881693 1.4049966 270 N 86 1 1
TOP 1 3.1881693 1.4849966 270 N 85 1 2
#
# CMP 128
CMP 1 3.3544094 1.5314504 0 N C4 GCJ188R72A104KA01D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GCJ188R72A104KA01-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-06-05'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCJ188R72A104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-13420-1-ND'
PRP Supplier_Part_Number_2 '81-GCJ188R72A104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '100V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '100V'
TOP 0 3.3229133 1.5314504 270 N 63 9 1
TOP 1 3.3859054 1.5314504 270 N 69 12 2
#
# CMP 129
CMP 14 3.3424409 1.4049965 270 N C3 C3216X6S2A106K160AC ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP Cap_F '10µF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=C3216X6S2A106K160AC'
PRP datasheet 'https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=C3216X6S2A106K160AC'
PRP Datasheet_Path 'datasheets/Cap-C3216X6S2A106K160AC.pdf'
PRP Digikey_Description 'CAP CER 10UF 100V X6S 1206'
PRP Digikey_Part_Number '445-C3216X6S2A106K160ACCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/f5a893ee60c9a292/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'TDK'
PRP Mouser_Description 'Multilayer Ceramic Capacitors MLCC - SMD/SMT 1206 100VDC 10uF 10% X6S'
PRP Mouser_Part_Number '810-C3216X6S2A106K16'
PRP Operating_Temperature_Range '-55°C to +105°C'
PRP PackageReference '1206'
PRP Part_Number 'C3216X6S2A106K160AC'
PRP PartNumber 'C3216X6S2A106K160AC'
PRP RoHS 'TRUE'
PRP SizeZ_mm '1.9mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 '445-C3216X6S2A106K160ACCT-ND'
PRP Supplier_Part_Number_2 '810-C3216X6S2A106K16'
PRP TempCo '22%'
PRP Temperature_Characteristic 'X6S'
PRP Tolerance__ '10%'
PRP Value '10µF'
PRP ValueDisplayed '10uF'
PRP VDC_V '100V'
TOP 0 3.3424409 1.3400359 270 N 69 13 1
TOP 1 3.3424409 1.4699571 270 N 63 10 2
#
# CMP 130
CMP 5 2.9605709 1.493522 180 N C6 GRM31CR71A226KE15L ;0=1,1=0.0709
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '1206'
PRP Cap_F '22µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM31CR71A226KE15L&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '1206'
PRP PartNumber 'GRM31CR71A226KE15L'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '5.12'
PRP SizeAreaWB_mm2 '10.92'
PRP SizeX_mm '3.2'
PRP SizeY_mm '1.6'
PRP SizeZ_mm '1.8'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '490-5309-1-ND'
PRP Supplier_Part_Number_2 '81-GRM31CR71A226K15L'
PRP Supplier_Part_Number_3 '1797016'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '22uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '22uF'
PRP VDC_V '10V'
TOP 0 3.0137205 1.493522 90 N 83 8 1
TOP 1 2.9074213 1.493522 90 N 88 40 2
#
# CMP 131
CMP 2 3.2641142 1.79 180 N C2 C0603C105K9RACAUTO ;0=1,1=0.0394
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://content.kemet.com/datasheets/KEM_C1023_X7R_AUTO_SMD.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'Kemet'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'C0603C105K9RACAUTO'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '1uF'
PRP Value1 ''
PRP Value2 '6.3V'
PRP ValueDisplayed '1µF'
PRP VDC_V '6.3V'
TOP 0 3.2916733 1.79 90 N 88 14 1
TOP 1 3.2365552 1.79 90 N 87 18 2
#
# CMP 132
CMP 16 3.6635 1.565831 270 N TP9 OUTB ;0=2,1=0.1811
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName ''
PRP CNHeader 'FALSE'
PRP Color 'Red'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.keyelco.com/userAssets/file/M60-2p60.pdf'
PRP CompType 'Test Point'
PRP ContactFinish 'Silver'
PRP CT 'TRUE'
PRP Current_A ''
PRP Gender ''
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Keystone Electronics'
PRP MountType 'TH'
PRP Note ''
PRP Orientation ''
PRP PackageReference 'Red Miniature Testpoint'
PRP PartNumber '5000'
PRP PinCount ''
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '36-5000-ND'
PRP Supplier_Part_Number_2 '534-5000'
PRP Supplier_Part_Number_3 ''
PRP Voltage_V ''
TOP 0 3.6635 1.565831 270 N 71 2 1
#
# CMP 133
CMP 15 1.5451947 0.529825 180 N TP18 AGND ;0=2,1=0.2610
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName ''
PRP CNHeader 'False'
PRP Color ''
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://cdn.harwin.com/pdfs/D3080-D3083.pdf'
PRP CompType 'Jumper Wire'
PRP ContactFinish ''
PRP CT 'False'
PRP Current_A ''
PRP Gender ''
PRP Green_EU_RoHS 'Passed with Exemption'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '2017-07-12'
PRP Manufacturer 'Harwin'
PRP MountType 'TH'
PRP Note ''
PRP Orientation ''
PRP PackageReference 'Shorting Plug, 10.16mm spacing, TH'
PRP PartNumber 'D3082-05'
PRP PinCount ''
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '952-1873-ND'
PRP Supplier_Part_Number_2 '01E9240'
PRP Supplier_Part_Number_3 '855-D3082-05'
PRP Voltage_V ''
TOP 0 1.7451947 0.529825 180 N 88 48 1
TOP 1 1.3451947 0.529825 180 N 88 49 2
#
# CMP 134
CMP 16 3.6635 1.365831 270 N TP6 OUTA ;0=2,1=0.1811
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName ''
PRP CNHeader 'FALSE'
PRP Color 'Red'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.keyelco.com/userAssets/file/M60-2p60.pdf'
PRP CompType 'Test Point'
PRP ContactFinish 'Silver'
PRP CT 'TRUE'
PRP Current_A ''
PRP Gender ''
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Keystone Electronics'
PRP MountType 'TH'
PRP Note ''
PRP Orientation ''
PRP PackageReference 'Red Miniature Testpoint'
PRP PartNumber '5000'
PRP PinCount ''
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '36-5000-ND'
PRP Supplier_Part_Number_2 '534-5000'
PRP Supplier_Part_Number_3 ''
PRP Voltage_V ''
TOP 0 3.6635 1.365831 270 N 72 3 1
#
# CMP 135
CMP 16 2.8570709 1.2302102 270 N TP8 VBK ;0=2,1=0.1811
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName ''
PRP CNHeader 'FALSE'
PRP Color 'Red'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.keyelco.com/userAssets/file/M60-2p60.pdf'
PRP CompType 'Test Point'
PRP ContactFinish 'Silver'
PRP CT 'TRUE'
PRP Current_A ''
PRP Gender ''
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Keystone Electronics'
PRP MountType 'TH'
PRP Note ''
PRP Orientation ''
PRP PackageReference 'Red Miniature Testpoint'
PRP PartNumber '5000'
PRP PinCount ''
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '36-5000-ND'
PRP Supplier_Part_Number_2 '534-5000'
PRP Supplier_Part_Number_3 ''
PRP Voltage_V ''
TOP 0 2.8570709 1.2302102 270 N 83 11 1
#
