Error Report for  - Users\a0271760\AppData\Local\Temp\Pro3142.tmp
5/9/2022 12:23:58 PM

Warning arcs were not exported.

Net AM263_ADC_VREFHI_G2 with allias 1 too long.
Net AM263_ADC0_AIN4 with allias 10 too long.
Net AM263_ICSSM_MII0_RXD3_R with allias 100 too long.
Net AM263_ICSSM_MII0_RXDV with allias 101 too long.
Net AM263_ICSSM_MII0_RXDV_R with allias 102 too long.
Net AM263_ICSSM_MII0_RXER with allias 103 too long.
Net AM263_ICSSM_MII0_RXLINK with allias 104 too long.
Net AM263_ICSSM_MII0_TXCLK with allias 105 too long.
Net AM263_ICSSM_MII0_TXD0 with allias 106 too long.
Net AM263_ICSSM_MII0_TXD1 with allias 107 too long.
Net AM263_ICSSM_MII0_TXD2 with allias 108 too long.
Net AM263_ICSSM_MII0_TXD3 with allias 109 too long.
Net AM263_ADC0_AIN5 with allias 11 too long.
Net AM263_ICSSM_MII0_TXEN with allias 110 too long.
Net AM263_ICSSM_MII1_COL with allias 111 too long.
Net AM263_ICSSM_MII1_RXCLK with allias 112 too long.
Net AM263_ICSSM_MII1_RXD0 with allias 113 too long.
Net AM263_ICSSM_MII1_RXD1 with allias 114 too long.
Net AM263_ICSSM_MII1_RXD2 with allias 115 too long.
Net AM263_ICSSM_MII1_RXD3 with allias 116 too long.
Net AM263_ICSSM_MII1_RXDV with allias 117 too long.
Net AM263_ICSSM_MII1_RXER with allias 118 too long.
Net AM263_ICSSM_MII1_RXLINK with allias 119 too long.
Net AM263_ADC1_AIN0 with allias 12 too long.
Net AM263_ICSSM_MII1_TXCLK with allias 120 too long.
Net AM263_ICSSM_MII1_TXCLK_R with allias 121 too long.
Net AM263_ICSSM_MII1_TXD0 with allias 122 too long.
Net AM263_ICSSM_MII1_TXD0_R with allias 123 too long.
Net AM263_ICSSM_MII1_TXD1 with allias 124 too long.
Net AM263_ICSSM_MII1_TXD1_R with allias 125 too long.
Net AM263_ICSSM_MII1_TXD2 with allias 126 too long.
Net AM263_ICSSM_MII1_TXD2_R with allias 127 too long.
Net AM263_ICSSM_MII1_TXD3 with allias 128 too long.
Net AM263_ICSSM_MII1_TXD3_R with allias 129 too long.
Net AM263_ADC1_AIN1 with allias 13 too long.
Net AM263_ICSSM_MII1_TXEN with allias 130 too long.
Net AM263_ICSSM_MII1_TXEN_R with allias 131 too long.
Net AM263_IEP0_EDC_SYNC_OUT0 with allias 132 too long.
Net AM263_IEP0_EDC_SYNC_OUT0_R with allias 133 too long.
Net AM263_IEP0_EDIO_DATA_IN_OUT31 with allias 134 too long.
Net AM263_IEP0_EDIO_DATA_IN_OUT31_R with allias 135 too long.
Net AM263_INT1_PB_GPIO123 with allias 136 too long.
Net AM263_LED_ENABLE_GPIO25 with allias 137 too long.
Net AM263_LED_GPIO26 with allias 138 too long.
Net AM263_LIN1_TXD_R with allias 139 too long.
Net AM263_ADC1_AIN2 with allias 14 too long.
Net AM263_LIN2_RXD_PR0_PRU0_GPIO11 with allias 140 too long.
Net AM263_LIN2_TXD_PR0_PRU0_GPIO9 with allias 141 too long.
Net AM263_LIN2_TXD_R with allias 142 too long.
Net AM263_MCAN0_TX_R with allias 143 too long.
Net AM263_MCAN1_TX_R with allias 144 too long.
Net AM263_MDIO0_MDC with allias 145 too long.
Net AM263_MDIO0_MDC_R with allias 146 too long.
Net AM263_MDIO0_MDIO with allias 147 too long.
Net AM263_MDIO0_MDIO_R with allias 148 too long.
Net AM263_MMC0_CLK_R with allias 149 too long.
Net AM263_ADC1_AIN2_SDFM0_D2 with allias 15 too long.
Net AM263_MMC0_CMD_R with allias 150 too long.
Net AM263_MMC0_D0_R with allias 151 too long.
Net AM263_MMC0_D1_R with allias 152 too long.
Net AM263_MMC0_D2_R with allias 153 too long.
Net AM263_MMC0_D3_R with allias 154 too long.
Net AM263_MUX_EN_GPIO58 with allias 155 too long.
Net AM263_PR0_MDIO0_MDC with allias 156 too long.
Net AM263_PR0_MDIO0_MDC_R with allias 157 too long.
Net AM263_PR0_MDIO0_MDIO with allias 158 too long.
Net AM263_PR0_MDIO0_MDIO_R with allias 159 too long.
Net AM263_ADC1_AIN3 with allias 16 too long.
Net AM263_PRU_MUX_SEL_GPIO64 with allias 160 too long.
Net AM263_QSPI0_CLK with allias 161 too long.
Net AM263_QSPI0_CLK_R with allias 162 too long.
Net AM263_QSPI0_CSN0 with allias 163 too long.
Net AM263_RESETN_PB with allias 164 too long.
Net AM263_RGMII1_RD0 with allias 165 too long.
Net AM263_RGMII1_RD1 with allias 166 too long.
Net AM263_RGMII1_RD2 with allias 167 too long.
Net AM263_RGMII1_RD3 with allias 168 too long.
Net AM263_RGMII1_RX_CTL with allias 169 too long.
Net AM263_ADC1_AIN4 with allias 17 too long.
Net AM263_RGMII1_RXC with allias 170 too long.
Net AM263_RGMII1_TD0 with allias 171 too long.
Net AM263_RGMII1_TD0_R with allias 172 too long.
Net AM263_RGMII1_TD1 with allias 173 too long.
Net AM263_RGMII1_TD1_R with allias 174 too long.
Net AM263_RGMII1_TD2 with allias 175 too long.
Net AM263_RGMII1_TD2_R with allias 176 too long.
Net AM263_RGMII1_TD3 with allias 177 too long.
Net AM263_RGMII1_TD3_R with allias 178 too long.
Net AM263_RGMII1_TX_CTL with allias 179 too long.
Net AM263_ADC1_AIN5 with allias 18 too long.
Net AM263_RGMII1_TX_CTL_R with allias 180 too long.
Net AM263_RGMII1_TXC with allias 181 too long.
Net AM263_RGMII1_TXC_R with allias 182 too long.
Net AM263_SAFETY_ERRORN with allias 183 too long.
Net AM263_SD_ENABLE_GPIO122 with allias 184 too long.
Net AM263_SDFM0_CLK1 with allias 185 too long.
Net AM263_SDFM0_CLK2 with allias 186 too long.
Net AM263_SDFM0_CLK3 with allias 187 too long.
Net AM263_SPI0_CLK_PR0_PRU0_GPIO16 with allias 188 too long.
Net AM263_SPI0_CLK_R with allias 189 too long.
Net AM263_ADC2_AIN0 with allias 19 too long.
Net AM263_SPI0_CS0_PR0_PRU0_GPIO8 with allias 190 too long.
Net AM263_SPI0_D0_R with allias 191 too long.
Net AM263_SPI1_CLK_R with allias 192 too long.
Net AM263_SPI1_D0_PR0_PRU0_GPIO13 with allias 193 too long.
Net AM263_SPI1_D0_R with allias 194 too long.
Net AM263_SPI1_D1_PR0_PRU0_GPIO14 with allias 195 too long.
Net AM263_UART0_RXD with allias 196 too long.
Net AM263_UART0_RXD_R with allias 197 too long.
Net AM263_UART0_RXD_XDS with allias 198 too long.
Net AM263_UART0_TXD with allias 199 too long.
Net AM263_ADC_VREFHI_G01 with allias 2 too long.
Net AM263_ADC2_AIN1 with allias 20 too long.
Net AM263_UART0_TXD_R with allias 200 too long.
Net AM263_UART0_TXD_XDS with allias 201 too long.
Net AM263_UART1_RXD with allias 202 too long.
Net AM263_UART1_TXD with allias 203 too long.
Net AM263_UART1_TXD_R with allias 204 too long.
Net MUX_EN_GPIO58_INV with allias 205 too long.
Net PR0_PRU0_GPIO0_MUX with allias 206 too long.
Net PR0_PRU0_GPIO1_MUX with allias 207 too long.
Net PR0_PRU0_GPIO2_MUX with allias 208 too long.
Net PR0_PRU0_GPIO3_MUX with allias 209 too long.
Net AM263_ADC2_AIN1_MCAN1_RX with allias 21 too long.
Net PR0_PRU0_GPIO4_MUX with allias 210 too long.
Net PR0_PRU0_GPIO5_MUX with allias 211 too long.
Net PR0_PRU0_GPIO6_MUX with allias 212 too long.
Net PR0_PRU0_GPIO8_MUX with allias 213 too long.
Net PR0_PRU0_GPIO9_MUX with allias 214 too long.
Net PR0_PRU0_GPIO10 with allias 215 too long.
Net PR0_PRU0_GPIO10_MUX with allias 216 too long.
Net PR0_PRU0_GPIO10_R with allias 217 too long.
Net PR0_PRU0_GPIO11 with allias 218 too long.
Net PR0_PRU0_GPIO11_MUX with allias 219 too long.
Net AM263_ADC2_AIN2 with allias 22 too long.
Net PR0_PRU0_GPIO11_R with allias 220 too long.
Net PR0_PRU0_GPIO12 with allias 221 too long.
Net PR0_PRU0_GPIO12_MUX with allias 222 too long.
Net PR0_PRU0_GPIO12_R with allias 223 too long.
Net PR0_PRU0_GPIO13 with allias 224 too long.
Net PR0_PRU0_GPIO13_MUX with allias 225 too long.
Net PR0_PRU0_GPIO13_R with allias 226 too long.
Net PR0_PRU0_GPIO14 with allias 227 too long.
Net PR0_PRU0_GPIO14_MUX with allias 228 too long.
Net PR0_PRU0_GPIO14_R with allias 229 too long.
Net AM263_ADC2_AIN2_SDFM0_CLK2 with allias 23 too long.
Net PR0_PRU0_GPIO15 with allias 230 too long.
Net PR0_PRU0_GPIO15_MUX with allias 231 too long.
Net PR0_PRU0_GPIO15_R with allias 232 too long.
Net PR0_PRU0_GPIO16 with allias 233 too long.
Net PR0_PRU0_GPIO16_MUX with allias 234 too long.
Net PR0_PRU0_GPIO16_R with allias 235 too long.
Net RGMII1_ICSSM_MUX_EN_GPIO1 with allias 236 too long.
Net RGMII1_ICSSM_MUX_SEL_GPIO105 with allias 237 too long.
Net RJ45_1_LED1_GREEN with allias 238 too long.
Net RJ45_1_LED1_YELLOW with allias 239 too long.
Net AM263_ADC2_AIN3 with allias 24 too long.
Net RJ45_1_LED2_GREEN with allias 240 too long.
Net RJ45_1_LED2_YELLOW with allias 241 too long.
Net RJ45_2_LED1_GREEN with allias 242 too long.
Net RJ45_2_LED1_YELLOW with allias 243 too long.
Net RJ45_2_LED2_GREEN with allias 244 too long.
Net RJ45_2_LED2_YELLOW with allias 245 too long.
Net SOC_TA_I2C3_SCL with allias 246 too long.
Net SOC_TA_I2C3_SDA with allias 247 too long.
Net SOP_DRIVE_OEN_R with allias 248 too long.
Net TPS_VSYS_5V0_ON with allias 249 too long.
Net AM263_ADC2_AIN4 with allias 25 too long.
Net TPS62913_1_EN_SYNC with allias 250 too long.
Net TPS62913_1_NR_SS with allias 251 too long.
Net TPS62913_1_SCONF with allias 252 too long.
Net TPS62913_2_EN_SYNC with allias 253 too long.
Net TPS62913_2_NR_SS with allias 254 too long.
Net TPS62913_2_SCONF with allias 255 too long.
Net TPS74801_1_BIAS with allias 256 too long.
Net TPS74801_2_BIAS with allias 257 too long.
Net VDD_ETH1_1V1_FILT with allias 258 too long.
Net VDD_ETH1_2V5_FILT with allias 259 too long.
Net AM263_ADC2_AIN5 with allias 26 too long.
Net VDD_ETH2_1V1_FILT with allias 260 too long.
Net VDD_ETH2_2V5_FILT with allias 261 too long.
Net VDDA_AM263_1V8_LDO with allias 262 too long.
Net VDDA18_AM263_OSC_PLL with allias 263 too long.
Net VDDS_AM263_LDO_1V8 with allias 264 too long.
Net VSYS_MON_AM263_ with allias 265 too long.
Net VSYS_TA_3V3_SLEEP with allias 266 too long.
Net XDS_VBUS_DETECT with allias 267 too long.
Net AM263_ADC3_AIN0 with allias 27 too long.
Net AM263_ADC3_AIN1 with allias 28 too long.
Net AM263_ADC3_AIN1_MCAN1_TX with allias 29 too long.
Net AM263_ADC_VREFLO_G2 with allias 3 too long.
Net AM263_ADC3_AIN2 with allias 30 too long.
Net AM263_ADC3_AIN2_SDFM0_D3 with allias 31 too long.
Net AM263_ADC3_AIN3 with allias 32 too long.
Net AM263_ADC3_AIN4 with allias 33 too long.
Net AM263_ADC3_AIN5 with allias 34 too long.
Net AM263_ADC4_AIN0 with allias 35 too long.
Net AM263_ADC4_AIN1 with allias 36 too long.
Net AM263_ADC4_AIN1_LIN1_RXD with allias 37 too long.
Net AM263_ADC4_AIN2 with allias 38 too long.
Net AM263_ADC4_AIN3 with allias 39 too long.
Net AM263_ADC_VREFLO_G01 with allias 4 too long.
Net AM263_ADC4_AIN4 with allias 40 too long.
Net AM263_ADC4_AIN5 with allias 41 too long.
Net AM263_BP_MUX_SEL_GPIO63 with allias 42 too long.
Net AM263_CAN_STB_GPIO51 with allias 43 too long.
Net AM263_CLKOUT0_R with allias 44 too long.
Net AM263_DAC_OUT_R with allias 45 too long.
Net AM263_DAC_OUT2_SDFM0_CLK3 with allias 46 too long.
Net AM263_EPWM0_A_R with allias 47 too long.
Net AM263_EPWM0_B_R with allias 48 too long.
Net AM263_EPWM1_A_R with allias 49 too long.
Net AM263_ADC0_AIN0 with allias 5 too long.
Net AM263_EPWM1_B_R with allias 50 too long.
Net AM263_EPWM2_A_R with allias 51 too long.
Net AM263_EPWM2_B_R with allias 52 too long.
Net AM263_EPWM3_A_R with allias 53 too long.
Net AM263_EPWM3_B_R with allias 54 too long.
Net AM263_EPWM9_A_R with allias 55 too long.
Net AM263_EPWM9_B_R with allias 56 too long.
Net AM263_EPWM11_A_R with allias 57 too long.
Net AM263_EPWM11_B_R with allias 58 too long.
Net AM263_EPWM12_A_R with allias 59 too long.
Net AM263_ADC0_AIN1 with allias 6 too long.
Net AM263_EPWM12_B_R with allias 60 too long.
Net AM263_EPWM13_A_R with allias 61 too long.
Net AM263_EPWM13_B_R with allias 62 too long.
Net AM263_EPWM14_A_R with allias 63 too long.
Net AM263_EPWM14_B_R with allias 64 too long.
Net AM263_EPWM15_A_R with allias 65 too long.
Net AM263_EPWM15_B_R with allias 66 too long.
Net AM263_EQEP0_A_R with allias 67 too long.
Net AM263_EQEP0_B_R with allias 68 too long.
Net AM263_EQEP0_INDEX with allias 69 too long.
Net AM263_ADC0_AIN2 with allias 7 too long.
Net AM263_EQEP0_INDEX_R with allias 70 too long.
Net AM263_EQEP0_STROBE with allias 71 too long.
Net AM263_EQEP0_STROBE_R with allias 72 too long.
Net AM263_EQEP2_A_R with allias 73 too long.
Net AM263_EQEP2_B_R with allias 74 too long.
Net AM263_EQEP2_INDEX with allias 75 too long.
Net AM263_EQEP2_INDEX_R with allias 76 too long.
Net AM263_EQEP2_STROBE with allias 77 too long.
Net AM263_EQEP2_STROBE_R with allias 78 too long.
Net AM263_EXT_REFCLK0 with allias 79 too long.
Net AM263_ADC0_AIN2_LIN1_TXD with allias 8 too long.
Net AM263_FSIRX1_CLK with allias 80 too long.
Net AM263_FSIRX1_DATA0 with allias 81 too long.
Net AM263_FSIRX1_DATA1 with allias 82 too long.
Net AM263_FSITX1_CLK with allias 83 too long.
Net AM263_FSITX1_CLK_R with allias 84 too long.
Net AM263_FSITX1_DATA0 with allias 85 too long.
Net AM263_FSITX1_DATA0_R with allias 86 too long.
Net AM263_FSITX1_DATA1 with allias 87 too long.
Net AM263_FSITX1_DATA1_R with allias 88 too long.
Net AM263_ICSSM_MII0_COL with allias 89 too long.
Net AM263_ADC0_AIN3 with allias 9 too long.
Net AM263_ICSSM_MII0_CRS with allias 90 too long.
Net AM263_ICSSM_MII0_RXCLK with allias 91 too long.
Net AM263_ICSSM_MII0_RXCLK_R with allias 92 too long.
Net AM263_ICSSM_MII0_RXD0 with allias 93 too long.
Net AM263_ICSSM_MII0_RXD0_R with allias 94 too long.
Net AM263_ICSSM_MII0_RXD1 with allias 95 too long.
Net AM263_ICSSM_MII0_RXD1_R with allias 96 too long.
Net AM263_ICSSM_MII0_RXD2 with allias 97 too long.
Net AM263_ICSSM_MII0_RXD2_R with allias 98 too long.
Net AM263_ICSSM_MII0_RXD3 with allias 99 too long.
Warning pad shape change for J5-B11 from  to rectangular 0.3mm,0.4mm
Warning pad shape change for J5-B10 from  to rectangular 0.3mm,0.4mm
Warning pad shape change for J5-B8 from  to rectangular 0.3mm,0.4mm
Warning pad shape change for J5-B7 from  to rectangular 0.3mm,0.4mm
Warning pad shape change for J5-B6 from  to rectangular 0.3mm,0.4mm
Warning pad shape change for J5-B3 from  to rectangular 0.3mm,0.4mm
Warning pad shape change for J5-B2 from  to rectangular 0.3mm,0.4mm
Warning pad shape change for J5-A11 from  to rectangular 0.3mm,0.4mm
Warning pad shape change for J5-A10 from  to rectangular 0.3mm,0.4mm
Warning pad shape change for J5-A8 from  to rectangular 0.3mm,0.4mm
Warning pad shape change for J5-A7 from  to rectangular 0.3mm,0.4mm
Warning pad shape change for J5-A6 from  to rectangular 0.3mm,0.4mm
Warning pad shape change for J5-A3 from  to rectangular 0.3mm,0.4mm
Warning pad shape change for J5-A2 from  to rectangular 0.3mm,0.4mm
Warning pad shape change for U3-10 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U3-9 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U3-8 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U3-7 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U8-4 from  to rounded 0.6mm,0.6mm
Warning pad shape change for U36-4 from  to rounded 0.25mm,0.25mm
Warning pad shape change for U44-5 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U44-6 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U45-7 from  to rounded 0.3mm,0.3mm
Warning pad shape change for U52-16 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U52-15 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U46-1 from  to rectangular 0.4mm,0.45mm
Warning pad shape change for U6-1 from  to rectangular 0.4mm,0.45mm
Warning pad shape change for U10-5 from  to rectangular 0.3mm,0.37mm
Warning pad shape change for U10-2 from  to rectangular 0.3mm,0.37mm
Warning pad shape change for U20-10 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U20-9 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U20-2 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U20-1 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U33-1 from  to rectangular 0.4mm,0.45mm
Warning pad shape change for J6-35 from  to rectangular 0.3mm,1mm
Warning pad shape change for J6-29 from  to rectangular 0.3mm,1mm
Warning pad shape change for J6-24 from  to rectangular 0.3mm,1mm
Warning pad shape change for J6-23 from  to rectangular 0.3mm,1mm
Warning pad shape change for J6-22 from  to rectangular 0.3mm,1mm
Warning pad shape change for J6-21 from  to rectangular 0.3mm,1mm
Warning pad shape change for J6-20 from  to rectangular 0.3mm,1mm
Warning pad shape change for J6-19 from  to rectangular 0.3mm,1mm
Warning pad shape change for J6-18 from  to rectangular 0.3mm,1mm
Warning pad shape change for J6-17 from  to rectangular 0.3mm,1mm
Warning pad shape change for J6-15 from  to rectangular 0.3mm,1mm
Warning pad shape change for J6-14 from  to rectangular 0.3mm,1mm
Warning pad shape change for J6-13 from  to rectangular 0.3mm,1mm
Warning pad shape change for J6-12 from  to rectangular 0.3mm,1mm
Warning pad shape change for J6-11 from  to rectangular 0.3mm,1mm
Warning pad shape change for J6-10 from  to rectangular 0.3mm,1mm
Warning pad shape change for J6-9 from  to rectangular 0.3mm,1mm
Warning pad shape change for J6-8 from  to rectangular 0.3mm,1mm
Warning pad shape change for J6-6 from  to rectangular 0.3mm,1mm
Warning pad shape change for J6-5 from  to rectangular 0.3mm,1mm
Warning pad shape change for J6-4 from  to rectangular 0.3mm,1mm
Warning pad shape change for U37-24 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U37-23 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U37-21 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U37-17 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U37-16 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U37-15 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U37-14 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U24-128 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-127 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-126 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-125 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-124 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-123 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-121 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-120 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-119 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-118 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-117 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-116 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-112 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-111 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-110 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-109 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-108 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-107 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-106 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-105 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-104 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-103 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-102 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-92 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-91 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-86 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-85 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-84 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-83 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-82 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-81 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-78 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-77 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-76 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-75 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-74 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-73 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-72 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-71 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-67 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-65 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-57 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-56 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-54 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-53 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-50 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-49 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-46 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-45 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-44 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-41 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-40 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-32 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-31 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-30 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-29 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-27 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-25 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-24 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-23 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-22 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-21 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-20 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-19 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-18 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-15 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-14 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-13 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-12 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-11 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-6 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-5 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-2 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U22-14 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U22-15 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U22-16 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U22-17 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U22-21 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U22-23 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U22-24 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U12-10 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U12-1 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U13-9 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U13-2 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U52-32 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U52-7 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U14-6 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U14-5 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U13-6 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U13-5 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U12-9 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U12-2 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U13-7 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U13-4 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U52-29 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U52-11 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U15-10 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U15-1 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for D16-1 from  to rounded 0.25mm,0.25mm
Warning pad shape change for U12-7 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U12-4 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U52-38 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U52-4 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U14-10 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U14-1 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U52-27 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U52-12 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U15-9 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U15-2 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U15-6 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U15-5 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U12-6 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U12-5 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U52-36 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U52-5 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U14-9 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U14-2 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U52-25 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U52-13 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U15-7 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U15-4 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for D15-2 from  to rounded 0.25mm,0.25mm
Warning pad shape change for U13-10 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U13-1 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U52-34 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U52-6 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U14-7 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U14-4 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U51-1 from rounded 0.4mm,1.2mm to rectangular 0.4mm,0.8mm
Warning pad shape change for U52-10 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U52-9 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U52-23 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U52-14 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U43-1 from rounded 0.24mm,0.6mm to rectangular 0.24mm,0.36mm
Warning pad shape change for U43-3 from rounded 0.24mm,0.6mm to rectangular 0.24mm,0.36mm
Warning pad shape change for U43-4 from rounded 0.24mm,0.6mm to rectangular 0.24mm,0.36mm
Warning pad shape change for U43-5 from rounded 0.24mm,0.6mm to rectangular 0.24mm,0.36mm
Warning pad shape change for U43-6 from rounded 0.24mm,0.6mm to rectangular 0.24mm,0.36mm
Warning pad shape change for U43-7 from rounded 0.24mm,0.6mm to rectangular 0.24mm,0.36mm
Warning pad shape change for U43-8 from rounded 0.24mm,0.6mm to rectangular 0.24mm,0.36mm
Warning pad shape change for U43-9 from rounded 0.24mm,0.6mm to rectangular 0.24mm,0.36mm
Warning pad shape change for U48-15 from rounded 0.6mm,1.45mm to rectangular 0.6mm,0.85mm
Warning pad shape change for U16-6 from  to rectangular 0.6mm,0.85mm
Warning pad shape change for U48-2 from rounded 0.6mm,1.45mm to rectangular 0.6mm,0.85mm
Warning pad shape change for U16-5 from  to rectangular 0.6mm,0.85mm
Warning pad shape change for U35-2 from rounded 0.45mm,1.35mm to rectangular 0.45mm,0.9mm
Warning pad shape change for U35-3 from rounded 0.45mm,1.35mm to rectangular 0.45mm,0.9mm
Warning pad shape change for U49-11 from rounded 0.4mm,1.2mm to rectangular 0.4mm,0.8mm
Warning pad shape change for U37-45 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U49-14 from rounded 0.4mm,1.2mm to rectangular 0.4mm,0.8mm
Warning pad shape change for U23-32 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U37-32 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U23-41 from  to rectangular 0.25mm,0.35mm
Warning pad shape change for U37-33 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U23-39 from  to rectangular 0.25mm,0.35mm
Warning pad shape change for U37-34 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U23-38 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U37-35 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U23-36 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U37-36 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U23-34 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U37-38 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U49-2 from rounded 0.4mm,1.2mm to rectangular 0.4mm,0.8mm
Warning pad shape change for U37-46 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U49-5 from rounded 0.4mm,1.2mm to rectangular 0.4mm,0.8mm
Warning pad shape change for U37-47 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U23-19 from  to rectangular 0.25mm,0.35mm
Warning pad shape change for U37-29 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U23-29 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U37-28 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U23-27 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U37-27 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U23-25 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U37-26 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U23-23 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U37-25 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U23-21 from  to rectangular 0.25mm,0.35mm
Warning pad shape change for U37-37 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U22-45 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U50-31 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U50-42 from  to rectangular 0.25mm,0.35mm
Warning pad shape change for U50-40 from  to rectangular 0.25mm,0.35mm
Warning pad shape change for U50-37 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U50-35 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U50-33 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U22-46 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U22-47 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U50-18 from  to rectangular 0.25mm,0.35mm
Warning pad shape change for U50-28 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U50-26 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U50-24 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U50-22 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U50-20 from  to rectangular 0.25mm,0.35mm
Warning pad shape change for U34-4 from  to rectangular 0.43mm,0.17mm
Warning pad shape change for U48-8 from rounded 0.6mm,1.45mm to rectangular 0.6mm,0.85mm
Warning pad shape change for U52-33 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U52-31 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U52-41 from  to rectangular 0.25mm,0.35mm
Warning pad shape change for U52-2 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U52-39 from  to rectangular 0.25mm,0.35mm
Warning pad shape change for U52-3 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U52-37 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U52-35 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U17-9 from rounded 0.3mm,1.35mm to rectangular 0.3mm,1.05mm
Warning pad shape change for U17-7 from rounded 0.3mm,1.35mm to rectangular 0.3mm,1.05mm
Warning pad shape change for U10-3 from  to rectangular 0.3mm,0.37mm
Warning pad shape change for J2-9 from  to rounded 0.8mm,0.8mm
Warning pad shape change for J2-5 from  to rounded 0.7mm,0.7mm
Warning pad shape change for J2-3 from  to rounded 0.7mm,0.7mm
Warning pad shape change for J2-7 from  to rounded 0.7mm,0.7mm
Warning pad shape change for J2-8 from  to rounded 0.7mm,0.7mm
Warning pad shape change for J2-1 from  to rounded 0.7mm,0.7mm
Warning pad shape change for J2-2 from  to rounded 0.7mm,0.7mm
Warning pad shape change for U52-8 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U46-2 from  to rectangular 0.4mm,0.45mm
Warning pad shape change for U23-8 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U2-4 from  to rounded 0.6mm,0.6mm
Warning pad shape change for U34-6 from  to rectangular 0.43mm,0.17mm
Warning pad shape change for U2-1 from  to rounded 0.6mm,0.6mm
Warning pad shape change for U6-2 from  to rectangular 0.4mm,0.45mm
Warning pad shape change for U17-2 from rounded 0.3mm,1.35mm to rectangular 0.3mm,1.05mm
Warning pad shape change for U17-4 from rounded 0.3mm,1.35mm to rectangular 0.3mm,1.05mm
Warning pad shape change for U23-9 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U23-10 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U49-1 from rounded 0.4mm,1.2mm to rectangular 0.4mm,0.8mm
Warning pad shape change for U7-6 from  to rectangular 0.5686mm,0.3925mm
Warning pad shape change for U7-1 from  to rectangular 0.5686mm,0.3925mm
Warning pad shape change for U33-4 from  to rectangular 0.4mm,0.45mm
Warning pad shape change for U50-41 from  to rectangular 0.25mm,0.35mm
Warning pad shape change for U50-39 from  to rectangular 0.25mm,0.35mm
Warning pad shape change for U50-38 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U50-36 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U50-34 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U50-32 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U50-29 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U50-27 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U50-25 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U50-23 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U50-21 from  to rectangular 0.25mm,0.35mm
Warning pad shape change for U50-19 from  to rectangular 0.25mm,0.35mm
Warning pad shape change for U9-2 from  to rounded 0.6mm,0.6mm
Warning pad shape change for U52-26 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U52-22 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U52-28 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U52-24 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U51-2 from rounded 0.4mm,1.2mm to rectangular 0.4mm,0.8mm
Warning pad shape change for U51-4 from rounded 0.4mm,1.2mm to rectangular 0.4mm,0.8mm
Warning pad shape change for U51-14 from rounded 0.4mm,1.2mm to rectangular 0.4mm,0.8mm
Warning pad shape change for U51-12 from rounded 0.4mm,1.2mm to rectangular 0.4mm,0.8mm
Warning pad shape change for U51-11 from rounded 0.4mm,1.2mm to rectangular 0.4mm,0.8mm
Warning pad shape change for U51-9 from rounded 0.4mm,1.2mm to rectangular 0.4mm,0.8mm
Warning pad shape change for U51-5 from rounded 0.4mm,1.2mm to rectangular 0.4mm,0.8mm
Warning pad shape change for U51-7 from rounded 0.4mm,1.2mm to rectangular 0.4mm,0.8mm
Warning pad shape change for U25-7 from rounded 0.6mm,1.397mm to rectangular 0.6mm,0.797mm
Warning pad shape change for U25-2 from rounded 0.6mm,1.397mm to rectangular 0.6mm,0.797mm
Warning pad shape change for U26-2 from  to rectangular 0.6mm,0.8mm
Warning pad shape change for U26-7 from  to rectangular 0.6mm,0.8mm
Warning pad shape change for U26-3 from  to rectangular 0.6mm,0.8mm
Warning pad shape change for U26-6 from  to rectangular 0.6mm,0.8mm
Warning pad shape change for U24-37 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U25-6 from rounded 0.6mm,1.397mm to rectangular 0.6mm,0.797mm
Warning pad shape change for U25-3 from rounded 0.6mm,1.397mm to rectangular 0.6mm,0.797mm
Warning pad shape change for U27-2 from  to rectangular 0.6mm,0.8mm
Warning pad shape change for U27-7 from  to rectangular 0.6mm,0.8mm
Warning pad shape change for U27-3 from  to rectangular 0.6mm,0.8mm
Warning pad shape change for U27-6 from  to rectangular 0.6mm,0.8mm
Warning pad shape change for U9-1 from  to rounded 0.6mm,0.6mm
Warning pad shape change for U37-43 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U22-43 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for Y1-1 from  to rounded 0.85mm,0.85mm
Warning pad shape change for Y1-3 from  to rounded 0.85mm,0.85mm
Warning pad shape change for U42-8 from  to rounded 0.31mm,0.31mm
Warning pad shape change for U42-6 from  to rounded 0.31mm,0.31mm
Warning pad shape change for U42-7 from  to rounded 0.31mm,0.31mm
Warning pad shape change for U16-1 from  to rectangular 0.6mm,0.85mm
Warning pad shape change for U16-2 from  to rectangular 0.6mm,0.85mm
Warning pad shape change for U16-3 from  to rectangular 0.6mm,0.85mm
Warning pad shape change for U16-7 from  to rectangular 0.6mm,0.85mm
Warning pad shape change for U43-20 from rounded 0.24mm,0.6mm to rectangular 0.24mm,0.36mm
Warning pad shape change for U43-18 from rounded 0.24mm,0.6mm to rectangular 0.24mm,0.36mm
Warning pad shape change for U43-17 from rounded 0.24mm,0.6mm to rectangular 0.24mm,0.36mm
Warning pad shape change for U43-16 from rounded 0.24mm,0.6mm to rectangular 0.24mm,0.36mm
Warning pad shape change for U43-15 from rounded 0.24mm,0.6mm to rectangular 0.24mm,0.36mm
Warning pad shape change for U43-14 from rounded 0.24mm,0.6mm to rectangular 0.24mm,0.36mm
Warning pad shape change for U43-13 from rounded 0.24mm,0.6mm to rectangular 0.24mm,0.36mm
Warning pad shape change for U43-12 from rounded 0.24mm,0.6mm to rectangular 0.24mm,0.36mm
Warning pad shape change for U22-40 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U22-22 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for Q5-1 from  to rounded 0.6mm,0.6mm
Warning pad shape change for Q6-1 from  to rounded 0.6mm,0.6mm
Warning pad shape change for Q4-1 from  to rounded 0.6mm,0.6mm
Warning pad shape change for U22-44 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U22-12 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U50-2 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U22-33 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U50-3 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U22-34 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U50-4 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U22-35 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U50-5 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U22-36 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U50-6 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U22-38 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U50-7 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U22-32 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U38-9 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U38-2 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U22-2 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U38-10 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U38-1 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U22-1 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U38-5 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U38-6 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U22-5 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U38-4 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U38-7 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U22-4 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U39-2 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U39-9 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U22-8 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U39-1 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U39-10 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U22-7 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U39-5 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U39-6 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U22-11 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U39-4 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U39-7 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U22-10 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U50-11 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U22-28 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U50-12 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U22-27 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U50-13 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U22-26 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U50-14 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U22-25 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U50-15 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U22-37 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U50-16 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U22-29 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U22-20 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U22-19 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for Y2-1 from  to rounded 0.85mm,0.85mm
Warning pad shape change for Y2-3 from  to rounded 0.85mm,0.85mm
Warning pad shape change for U37-40 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U37-22 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for Q8-1 from  to rounded 0.6mm,0.6mm
Warning pad shape change for Q9-1 from  to rounded 0.6mm,0.6mm
Warning pad shape change for Q7-1 from  to rounded 0.6mm,0.6mm
Warning pad shape change for U37-44 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U37-12 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U37-2 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U40-9 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U40-2 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U37-1 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U40-10 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U40-1 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U37-5 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U40-5 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U40-6 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U37-4 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U40-4 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U40-7 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U37-8 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U41-2 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U41-9 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U37-7 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U41-1 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U41-10 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U37-11 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U41-5 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U41-6 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U37-10 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U41-4 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U41-7 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U37-20 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U37-19 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for Y4-1 from  to rounded 0.85mm,0.85mm
Warning pad shape change for Y4-3 from  to rounded 0.85mm,0.85mm
Warning pad shape change for U45-5 from  to rounded 0.3mm,0.3mm
Warning pad shape change for U47-3 from  to rounded 0.6mm,0.6mm
Warning pad shape change for J5-B12 from  to rounded 0.7mm,0.7mm
Warning pad shape change for J5-B1 from  to rounded 0.7mm,0.7mm
Warning pad shape change for J5-A12 from  to rectangular 0.3mm,0.4mm
Warning pad shape change for J5-A1 from  to rectangular 0.3mm,0.4mm
Warning pad shape change for SW4-1 from  to rounded 1mm,1mm
Warning pad shape change for SW4-3 from  to rounded 1mm,1mm
Warning pad shape change for U3-6 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U7-9 from  to rounded 4.75mm,4.75mm
Warning pad shape change for U7-4 from  to rectangular 0.5686mm,0.3925mm
Warning pad shape change for U8-2 from  to rounded 0.6mm,0.6mm
Warning pad shape change for U18-10 from  to rectangular 0.3mm,0.2mm
Warning pad shape change for U19-5 from  to rounded 0.25mm,0.25mm
Warning pad shape change for U19-9 from  to rounded 0.9mm,0.9mm
Warning pad shape change for U21-3 from  to rectangular 0.3mm,0.37mm
Warning pad shape change for U31-6 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U32-4 from  to rectangular 0.8mm,0.2mm
Warning pad shape change for U32-7 from  to rectangular 0.25mm,0.3mm
Warning pad shape change for U34-2 from  to rectangular 0.43mm,0.17mm
Warning pad shape change for U35-4 from rounded 0.45mm,1.35mm to rectangular 0.45mm,0.9mm
Warning pad shape change for U36-1 from  to rounded 0.25mm,0.25mm
Warning pad shape change for U36-5 from  to rounded 0.25mm,0.25mm
Warning pad shape change for U36-6 from  to rounded 0.25mm,0.25mm
Warning pad shape change for U36-11 from  to rectangular 0.84mm,1.56mm
Warning pad shape change for U48-16 from rounded 0.6mm,1.45mm to rectangular 0.6mm,0.85mm
Warning pad shape change for U26-4 from  to rectangular 0.6mm,0.8mm
Warning pad shape change for U25-5 from rounded 0.6mm,1.397mm to rectangular 0.6mm,0.797mm
Warning pad shape change for Q13-2 from  to rounded 0.47mm,0.47mm
Warning pad shape change for U51-8 from rounded 0.4mm,1.2mm to rectangular 0.4mm,0.8mm
Warning pad shape change for U52-43 from  to rectangular 2.05mm,5.5mm
Warning pad shape change for D16-2 from  to rounded 0.25mm,0.25mm
Warning pad shape change for U16-4 from  to rectangular 0.6mm,0.85mm
Warning pad shape change for U46-3 from  to rectangular 0.4mm,0.45mm
Warning pad shape change for U50-43 from  to rectangular 2.05mm,5.5mm
Warning pad shape change for U23-43 from  to rectangular 2.05mm,5.5mm
Warning pad shape change for U49-8 from rounded 0.4mm,1.2mm to rectangular 0.4mm,0.8mm
Warning pad shape change for Q11-2 from  to rounded 0.47mm,0.47mm
Warning pad shape change for D15-1 from  to rounded 0.25mm,0.25mm
Warning pad shape change for SW3-3 from  to rounded 1mm,1mm
Warning pad shape change for SW3-1 from  to rounded 1mm,1mm
Warning pad shape change for SW2-3 from  to rounded 1mm,1mm
Warning pad shape change for SW2-1 from  to rounded 1mm,1mm
Warning pad shape change for Q5-2 from  to rounded 0.6mm,0.6mm
Warning pad shape change for Q10-3 from  to rounded 0.47mm,0.47mm
Warning pad shape change for Y1-4 from  to rounded 0.85mm,0.85mm
Warning pad shape change for Y1-2 from  to rounded 0.85mm,0.85mm
Warning pad shape change for U27-4 from  to rectangular 0.6mm,0.8mm
Warning pad shape change for U30-6 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U29-7 from  to rectangular 0.25mm,0.3mm
Warning pad shape change for U29-4 from  to rectangular 0.8mm,0.2mm
Warning pad shape change for U5-3 from  to rounded 0.6mm,0.6mm
Warning pad shape change for U6-3 from  to rectangular 0.4mm,0.45mm
Warning pad shape change for U2-2 from  to rounded 0.6mm,0.6mm
Warning pad shape change for U13-8 from  to rounded 0.4mm,0.4mm
Warning pad shape change for U13-3 from  to rounded 0.4mm,0.4mm
Warning pad shape change for U12-8 from  to rounded 0.4mm,0.4mm
Warning pad shape change for U12-3 from  to rounded 0.4mm,0.4mm
Warning pad shape change for U14-8 from  to rounded 0.4mm,0.4mm
Warning pad shape change for U14-3 from  to rounded 0.4mm,0.4mm
Warning pad shape change for U15-8 from  to rounded 0.4mm,0.4mm
Warning pad shape change for U15-3 from  to rounded 0.4mm,0.4mm
Warning pad shape change for U20-8 from  to rounded 0.4mm,0.4mm
Warning pad shape change for U20-3 from  to rounded 0.4mm,0.4mm
Warning pad shape change for U33-3 from  to rectangular 0.4mm,0.45mm
Warning pad shape change for Q3-3 from  to rounded 0.6mm,0.6mm
Warning pad shape change for Q2-3 from  to rounded 0.6mm,0.6mm
Warning pad shape change for J2-6 from  to rounded 0.7mm,0.7mm
Warning pad shape change for J2-10 from  to rounded 0.7mm,0.7mm
Warning pad shape change for J2-S1 from  to rounded 1mm,1mm
Warning pad shape change for J2-S3 from  to rectangular 1.2mm,2mm
Warning pad shape change for J6-42 from  to rounded 1.8mm,1.8mm
Warning pad shape change for J6-41 from  to rounded 1.8mm,1.8mm
Warning pad shape change for J6-40 from  to rectangular 0.3mm,1mm
Warning pad shape change for J6-34 from  to rectangular 0.3mm,1mm
Warning pad shape change for J6-25 from  to rectangular 0.3mm,1mm
Warning pad shape change for J6-16 from  to rectangular 0.3mm,1mm
Warning pad shape change for J6-7 from  to rectangular 0.3mm,1mm
Warning pad shape change for Q9-2 from  to rounded 0.6mm,0.6mm
Warning pad shape change for U9-3 from  to rounded 0.6mm,0.6mm
Warning pad shape change for U17-3 from rounded 0.3mm,1.35mm to rectangular 0.3mm,1.05mm
Warning pad shape change for U42-9 from  to rounded 1.65mm,1.65mm
Warning pad shape change for U42-2 from  to rounded 0.31mm,0.31mm
Warning pad shape change for U43-11 from rounded 0.24mm,0.6mm to rectangular 0.24mm,0.36mm
Warning pad shape change for Y4-2 from  to rounded 0.85mm,0.85mm
Warning pad shape change for Y4-4 from  to rounded 0.85mm,0.85mm
Warning pad shape change for C30-1 from  to rounded 0.3mm,0.3mm
Warning pad shape change for C47-1 from  to rounded 0.3mm,0.3mm
Warning pad shape change for C46-1 from  to rounded 0.3mm,0.3mm
Warning pad shape change for C45-1 from  to rounded 0.3mm,0.3mm
Warning pad shape change for C44-1 from  to rounded 0.3mm,0.3mm
Warning pad shape change for C42-1 from  to rounded 0.3mm,0.3mm
Warning pad shape change for C41-1 from  to rounded 0.3mm,0.3mm
Warning pad shape change for C40-1 from  to rounded 0.3mm,0.3mm
Warning pad shape change for C39-1 from  to rounded 0.3mm,0.3mm
Warning pad shape change for C32-1 from  to rounded 0.3mm,0.3mm
Warning pad shape change for C31-1 from  to rounded 0.3mm,0.3mm
Warning pad shape change for C29-1 from  to rounded 0.3mm,0.3mm
Warning pad shape change for C22-1 from  to rounded 0.3mm,0.3mm
Warning pad shape change for C21-1 from  to rounded 0.3mm,0.3mm
Warning pad shape change for C20-1 from  to rounded 0.3mm,0.3mm
Warning pad shape change for C19-1 from  to rounded 0.3mm,0.3mm
Warning pad shape change for Q8-2 from  to rounded 0.6mm,0.6mm
Warning pad shape change for Y2-4 from  to rounded 0.85mm,0.85mm
Warning pad shape change for Y2-2 from  to rounded 0.85mm,0.85mm
Warning pad shape change for Q7-2 from  to rounded 0.6mm,0.6mm
Warning pad shape change for Q1-3 from  to rounded 0.6mm,0.6mm
Warning pad shape change for Q6-2 from  to rounded 0.6mm,0.6mm
Warning pad shape change for Q4-2 from  to rounded 0.6mm,0.6mm
Warning pad shape change for U41-3 from  to rounded 0.4mm,0.4mm
Warning pad shape change for U41-8 from  to rounded 0.4mm,0.4mm
Warning pad shape change for U40-3 from  to rounded 0.4mm,0.4mm
Warning pad shape change for U40-8 from  to rounded 0.4mm,0.4mm
Warning pad shape change for U39-3 from  to rounded 0.4mm,0.4mm
Warning pad shape change for U39-8 from  to rounded 0.4mm,0.4mm
Warning pad shape change for U38-3 from  to rounded 0.4mm,0.4mm
Warning pad shape change for U38-8 from  to rounded 0.4mm,0.4mm
Warning pad shape change for U44-3 from  to rounded 0.4mm,0.4mm
Warning pad shape change for U44-8 from  to rounded 0.4mm,0.4mm
Warning pad shape change for U45-9 from  to rounded 1.65mm,1.65mm
Warning pad shape change for U45-6 from  to rounded 0.3mm,0.3mm
Warning pad shape change for U28-2 from  to rounded 0.6mm,0.6mm
Warning pad shape change for U26-5 from  to rectangular 0.6mm,0.8mm
Warning pad shape change for U25-4 from rounded 0.6mm,1.397mm to rectangular 0.6mm,0.797mm
Warning pad shape change for J34-5 from  to rectangular 0.45mm,0.93mm
Warning pad shape change for U27-5 from  to rectangular 0.6mm,0.8mm
Warning pad shape change for U24-114 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-80 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-66 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-64 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-58 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-55 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-48 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-17 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-10 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for SW4-2 from  to rounded 1mm,1mm
Warning pad shape change for SW4-4 from  to rounded 1mm,1mm
Warning pad shape change for U34-3 from  to rectangular 0.43mm,0.17mm
Warning pad shape change for Q3-2 from  to rounded 0.6mm,0.6mm
Warning pad shape change for U48-9 from rounded 0.6mm,1.45mm to rectangular 0.6mm,0.85mm
Warning pad shape change for U48-10 from rounded 0.6mm,1.45mm to rectangular 0.6mm,0.85mm
Warning pad shape change for U48-7 from rounded 0.6mm,1.45mm to rectangular 0.6mm,0.85mm
Warning pad shape change for U48-3 from rounded 0.6mm,1.45mm to rectangular 0.6mm,0.85mm
Warning pad shape change for U48-4 from rounded 0.6mm,1.45mm to rectangular 0.6mm,0.85mm
Warning pad shape change for U48-5 from rounded 0.6mm,1.45mm to rectangular 0.6mm,0.85mm
Warning pad shape change for U48-6 from rounded 0.6mm,1.45mm to rectangular 0.6mm,0.85mm
Warning pad shape change for U48-11 from rounded 0.6mm,1.45mm to rectangular 0.6mm,0.85mm
Warning pad shape change for U48-12 from rounded 0.6mm,1.45mm to rectangular 0.6mm,0.85mm
Warning pad shape change for U48-13 from rounded 0.6mm,1.45mm to rectangular 0.6mm,0.85mm
Warning pad shape change for U48-14 from rounded 0.6mm,1.45mm to rectangular 0.6mm,0.85mm
Warning pad shape change for U17-10 from rounded 0.3mm,1.35mm to rectangular 0.3mm,1.05mm
Warning pad shape change for U37-42 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U22-42 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U17-6 from rounded 0.3mm,1.35mm to rectangular 0.3mm,1.05mm
Warning pad shape change for U37-41 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U22-41 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U51-15 from rounded 0.4mm,1.2mm to rectangular 0.4mm,0.8mm
Warning pad shape change for U46-4 from  to rectangular 0.4mm,0.45mm
Warning pad shape change for U49-15 from rounded 0.4mm,1.2mm to rectangular 0.4mm,0.8mm
Warning pad shape change for Q13-3 from  to rounded 0.47mm,0.47mm
Warning pad shape change for Q10-2 from  to rounded 0.47mm,0.47mm
Warning pad shape change for Q11-3 from  to rounded 0.47mm,0.47mm
Warning pad shape change for U36-9 from  to rounded 0.25mm,0.25mm
Warning pad shape change for Q10-1 from  to rounded 0.47mm,0.47mm
Warning pad shape change for Q11-1 from  to rounded 0.47mm,0.47mm
Warning pad shape change for Q13-1 from  to rounded 0.47mm,0.47mm
Warning pad shape change for SW1-1 from  to rounded 0.76mm,0.76mm
Warning pad shape change for SW1-2 from  to rounded 0.76mm,0.76mm
Warning pad shape change for SW1-3 from  to rounded 0.76mm,0.76mm
Warning pad shape change for SW1-4 from  to rounded 0.76mm,0.76mm
Warning pad shape change for U42-1 from  to rounded 0.31mm,0.31mm
Warning pad shape change for U42-4 from  to rounded 0.31mm,0.31mm
Warning pad shape change for U52-21 from  to rectangular 0.25mm,0.35mm
Warning pad shape change for U52-20 from  to rectangular 0.25mm,0.35mm
Warning pad shape change for U52-19 from  to rectangular 0.25mm,0.35mm
Warning pad shape change for U52-18 from  to rectangular 0.25mm,0.35mm
Warning pad shape change for U10-4 from  to rectangular 0.3mm,0.37mm
Warning pad shape change for U29-5 from  to rectangular 0.45mm,0.2mm
Warning pad shape change for U2-3 from  to rounded 0.6mm,0.6mm
Warning pad shape change for U32-5 from  to rectangular 0.45mm,0.2mm
Warning pad shape change for U2-6 from  to rounded 0.6mm,0.6mm
Warning pad shape change for U5-2 from  to rounded 0.6mm,0.6mm
Warning pad shape change for U6-4 from  to rectangular 0.4mm,0.45mm
Warning pad shape change for U34-1 from  to rectangular 0.43mm,0.17mm
Warning pad shape change for SW2-4 from  to rounded 1mm,1mm
Warning pad shape change for SW2-2 from  to rounded 1mm,1mm
Warning pad shape change for Q1-2 from  to rounded 0.6mm,0.6mm
Warning pad shape change for U23-2 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U23-42 from  to rectangular 0.25mm,0.35mm
Warning pad shape change for U23-3 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U23-40 from  to rectangular 0.25mm,0.35mm
Warning pad shape change for U23-4 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U23-37 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U23-5 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U23-35 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U23-6 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U23-33 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U49-4 from rounded 0.4mm,1.2mm to rectangular 0.4mm,0.8mm
Warning pad shape change for U49-3 from rounded 0.4mm,1.2mm to rectangular 0.4mm,0.8mm
Warning pad shape change for U23-7 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U23-31 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U49-7 from rounded 0.4mm,1.2mm to rectangular 0.4mm,0.8mm
Warning pad shape change for U51-13 from rounded 0.4mm,1.2mm to rectangular 0.4mm,0.8mm
Warning pad shape change for U49-6 from rounded 0.4mm,1.2mm to rectangular 0.4mm,0.8mm
Warning pad shape change for U49-9 from rounded 0.4mm,1.2mm to rectangular 0.4mm,0.8mm
Warning pad shape change for U52-40 from  to rectangular 0.25mm,0.35mm
Warning pad shape change for U49-10 from rounded 0.4mm,1.2mm to rectangular 0.4mm,0.8mm
Warning pad shape change for U49-12 from rounded 0.4mm,1.2mm to rectangular 0.4mm,0.8mm
Warning pad shape change for U49-13 from rounded 0.4mm,1.2mm to rectangular 0.4mm,0.8mm
Warning pad shape change for U23-11 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U52-42 from  to rectangular 0.25mm,0.35mm
Warning pad shape change for U23-28 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U23-12 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U23-26 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U23-13 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U51-10 from rounded 0.4mm,1.2mm to rectangular 0.4mm,0.8mm
Warning pad shape change for U23-24 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U23-14 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U51-6 from rounded 0.4mm,1.2mm to rectangular 0.4mm,0.8mm
Warning pad shape change for U23-22 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U23-15 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U23-20 from  to rectangular 0.25mm,0.35mm
Warning pad shape change for U23-16 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U51-3 from rounded 0.4mm,1.2mm to rectangular 0.4mm,0.8mm
Warning pad shape change for U23-18 from  to rectangular 0.25mm,0.35mm
Warning pad shape change for U7-5 from  to rectangular 0.5686mm,0.3925mm
Warning pad shape change for U7-2 from  to rectangular 0.5686mm,0.3925mm
Warning pad shape change for U7-3 from  to rectangular 0.5686mm,0.3925mm
Warning pad shape change for U7-7 from  to rectangular 0.5686mm,0.3925mm
Warning pad shape change for SW3-4 from  to rounded 1mm,1mm
Warning pad shape change for SW3-2 from  to rounded 1mm,1mm
Warning pad shape change for U33-2 from  to rectangular 0.4mm,0.45mm
Warning pad shape change for Q2-2 from  to rounded 0.6mm,0.6mm
Warning pad shape change for U50-8 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U50-9 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U50-10 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U17-1 from rounded 0.3mm,1.35mm to rectangular 0.3mm,1.05mm
Warning pad shape change for U17-5 from rounded 0.3mm,1.35mm to rectangular 0.3mm,1.05mm
Warning pad shape change for Q4-3 from  to rounded 0.6mm,0.6mm
Warning pad shape change for Q5-3 from  to rounded 0.6mm,0.6mm
Warning pad shape change for Q6-3 from  to rounded 0.6mm,0.6mm
Warning pad shape change for Q7-3 from  to rounded 0.6mm,0.6mm
Warning pad shape change for Q8-3 from  to rounded 0.6mm,0.6mm
Warning pad shape change for Q9-3 from  to rounded 0.6mm,0.6mm
Warning pad shape change for U8-3 from  to rounded 0.6mm,0.6mm
Warning pad shape change for U9-4 from  to rounded 0.6mm,0.6mm
Warning pad shape change for J5-4 from  to rectangular 1.1mm,2.5mm
Warning pad shape change for J5-3 from  to rectangular 1.1mm,2.5mm
Warning pad shape change for J5-4 from  to rectangular 1.1mm,2.5mm
Warning pad shape change for J5-3 from  to rectangular 1.1mm,2.5mm
Warning pad shape change for J34-8 from  to rounded 1.375mm,1.375mm
Warning pad shape change for J34-9 from  to rounded 1.375mm,1.375mm
Warning pad shape change for J34-6 from  to rounded 1.475mm,1.475mm
Warning pad shape change for J34-11 from  to rounded 1.475mm,1.475mm
Warning pad shape change for U35-7 from rounded 0.45mm,1.35mm to rectangular 0.45mm,0.9mm
Warning pad shape change for J6-36 from  to rectangular 0.3mm,1mm
Warning pad shape change for U35-6 from rounded 0.45mm,1.35mm to rectangular 0.45mm,0.9mm
Warning pad shape change for J6-38 from  to rectangular 0.3mm,1mm
Warning pad shape change for U5-4 from  to rounded 0.6mm,0.6mm
Warning pad shape change for SW1-8 from  to rounded 0.76mm,0.76mm
Warning pad shape change for U3-2 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for SW1-7 from  to rounded 0.76mm,0.76mm
Warning pad shape change for U3-3 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for SW1-6 from  to rounded 0.76mm,0.76mm
Warning pad shape change for U3-4 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for SW1-5 from  to rounded 0.76mm,0.76mm
Warning pad shape change for U3-5 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for Q3-1 from  to rounded 0.6mm,0.6mm
Warning pad shape change for J6-30 from  to rectangular 0.3mm,1mm
Warning pad shape change for J6-31 from  to rectangular 0.3mm,1mm
Warning pad shape change for U5-1 from  to rounded 0.6mm,0.6mm
Warning pad shape change for J6-32 from  to rectangular 0.3mm,1mm
Warning pad shape change for U3-1 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for J6-33 from  to rectangular 0.3mm,1mm
Warning pad shape change for U3-12 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for J6-37 from  to rectangular 0.3mm,1mm
Warning pad shape change for U3-13 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for J6-39 from  to rectangular 0.3mm,1mm
Warning pad shape change for J6-27 from  to rectangular 0.3mm,1mm
Warning pad shape change for Q1-1 from  to rounded 0.6mm,0.6mm
Warning pad shape change for U47-2 from  to rounded 0.6mm,0.6mm
Warning pad shape change for J6-26 from  to rectangular 0.3mm,1mm
Warning pad shape change for Q2-1 from  to rounded 0.6mm,0.6mm
Warning pad shape change for J6-28 from  to rectangular 0.3mm,1mm
Warning pad shape change for U3-16 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U3-11 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U24-100 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-98 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-97 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-99 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U19-6 from  to rounded 0.25mm,0.25mm
Warning pad shape change for U47-4 from  to rounded 0.6mm,0.6mm
Warning pad shape change for U19-3 from  to rounded 0.25mm,0.25mm
Warning pad shape change for U29-1 from  to rectangular 0.45mm,0.2mm
Warning pad shape change for U29-9 from  to rectangular 0.25mm,0.3mm
Warning pad shape change for U29-8 from  to rectangular 0.25mm,0.3mm
Warning pad shape change for U29-10 from  to rectangular 0.25mm,0.3mm
Warning pad shape change for U29-2 from  to rectangular 0.8mm,0.2mm
Warning pad shape change for U32-1 from  to rectangular 0.45mm,0.2mm
Warning pad shape change for U32-9 from  to rectangular 0.25mm,0.3mm
Warning pad shape change for U32-8 from  to rectangular 0.25mm,0.3mm
Warning pad shape change for U32-10 from  to rectangular 0.25mm,0.3mm
Warning pad shape change for U32-2 from  to rectangular 0.8mm,0.2mm
Warning pad shape change for U30-4 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U30-5 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U30-8 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U30-3 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U30-7 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U31-4 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U31-5 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U31-8 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U31-3 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U31-7 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U18-5 from  to rectangular 0.3mm,0.2mm
Warning pad shape change for U18-11 from  to rectangular 0.3mm,0.2mm
Warning pad shape change for U18-9 from  to rectangular 0.3mm,0.2mm
Warning pad shape change for U47-1 from  to rounded 0.6mm,0.6mm
Warning pad shape change for U21-4 from  to rectangular 0.3mm,0.37mm
Warning pad shape change for U21-1 from  to rectangular 0.3mm,0.37mm
Warning pad shape change for U18-7 from  to rectangular 0.5mm,0.2mm
Warning pad shape change for U21-2 from  to rectangular 0.3mm,0.37mm
Warning pad shape change for U18-8 from  to rectangular 0.5mm,0.2mm
Warning pad shape change for U18-6 from  to rectangular 0.3mm,0.2mm
Warning pad shape change for U18-3 from  to rectangular 0.3mm,0.2mm
Warning pad shape change for U18-4 from  to rectangular 0.3mm,0.2mm
Warning pad shape change for J5-A5 from  to rectangular 0.3mm,0.4mm
Warning pad shape change for U18-1 from  to rectangular 0.5mm,0.2mm
Warning pad shape change for U20-7 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U20-4 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for J5-B5 from  to rectangular 0.3mm,0.4mm
Warning pad shape change for U18-2 from  to rectangular 0.5mm,0.2mm
Warning pad shape change for U20-6 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U20-5 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for J5-B9 from  to rectangular 0.3mm,0.4mm
Warning pad shape change for J5-B4 from  to rectangular 0.3mm,0.4mm
Warning pad shape change for J5-A9 from  to rectangular 0.3mm,0.4mm
Warning pad shape change for J5-A4 from  to rectangular 0.3mm,0.4mm
Warning pad shape change for U45-8 from  to rounded 0.3mm,0.3mm
Warning pad shape change for U45-2 from  to rounded 0.3mm,0.3mm
Warning pad shape change for U45-1 from  to rounded 0.3mm,0.3mm
Warning pad shape change for J34-1 from  to rectangular 0.45mm,0.93mm
Warning pad shape change for U29-3 from  to rectangular 0.45mm,0.2mm
Warning pad shape change for C30-2 from  to rounded 0.3mm,0.3mm
Warning pad shape change for C47-2 from  to rounded 0.3mm,0.3mm
Warning pad shape change for C46-2 from  to rounded 0.3mm,0.3mm
Warning pad shape change for C45-2 from  to rounded 0.3mm,0.3mm
Warning pad shape change for C44-2 from  to rounded 0.3mm,0.3mm
Warning pad shape change for C42-2 from  to rounded 0.3mm,0.3mm
Warning pad shape change for C41-2 from  to rounded 0.3mm,0.3mm
Warning pad shape change for C40-2 from  to rounded 0.3mm,0.3mm
Warning pad shape change for C39-2 from  to rounded 0.3mm,0.3mm
Warning pad shape change for C32-2 from  to rounded 0.3mm,0.3mm
Warning pad shape change for C31-2 from  to rounded 0.3mm,0.3mm
Warning pad shape change for C29-2 from  to rounded 0.3mm,0.3mm
Warning pad shape change for C22-2 from  to rounded 0.3mm,0.3mm
Warning pad shape change for C21-2 from  to rounded 0.3mm,0.3mm
Warning pad shape change for C20-2 from  to rounded 0.3mm,0.3mm
Warning pad shape change for C19-2 from  to rounded 0.3mm,0.3mm
Warning pad shape change for U31-9 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U31-10 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for FB3-1 from  to rounded 0.65mm,0.65mm
Warning pad shape change for FB5-1 from  to rounded 0.65mm,0.65mm
Warning pad shape change for FB6-1 from  to rounded 0.65mm,0.65mm
Warning pad shape change for U30-9 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U30-10 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for FB4-1 from  to rounded 0.65mm,0.65mm
Warning pad shape change for FB3-2 from  to rounded 0.65mm,0.65mm
Warning pad shape change for U22-6 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U22-31 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U22-39 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for FB4-2 from  to rounded 0.65mm,0.65mm
Warning pad shape change for U22-3 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U22-9 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for FB5-2 from  to rounded 0.65mm,0.65mm
Warning pad shape change for U37-39 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U37-31 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U37-6 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for FB6-2 from  to rounded 0.65mm,0.65mm
Warning pad shape change for U37-9 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U37-3 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U45-4 from  to rounded 0.3mm,0.3mm
Warning pad shape change for U45-3 from  to rounded 0.3mm,0.3mm
Warning pad shape change for U26-8 from  to rectangular 0.6mm,0.8mm
Warning pad shape change for U25-1 from rounded 0.6mm,1.397mm to rectangular 0.6mm,0.797mm
Warning pad shape change for U27-8 from  to rectangular 0.6mm,0.8mm
Warning pad shape change for U24-122 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-113 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-101 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-90 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-79 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-69 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-52 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-51 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-47 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-39 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-28 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-26 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-16 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-8 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-7 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for FB2-1 from  to rounded 0.65mm,0.65mm
Warning pad shape change for FB1-2 from  to rounded 0.65mm,0.65mm
Warning pad shape change for U22-13 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U22-48 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U37-48 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U37-13 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for FB2-2 from  to rounded 0.65mm,0.65mm
Warning pad shape change for U24-115 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-87 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U8-5 from  to rounded 0.6mm,0.6mm
Warning pad shape change for U8-6 from  to rounded 0.6mm,0.6mm
Warning pad shape change for U10-1 from  to rectangular 0.3mm,0.37mm
Warning pad shape change for J2-4 from  to rounded 0.7mm,0.7mm
Warning pad shape change for U7-8 from  to rectangular 0.5686mm,0.3925mm
Warning pad shape change for U8-1 from  to rounded 0.6mm,0.6mm
Warning pad shape change for U32-3 from  to rectangular 0.45mm,0.2mm
Warning pad shape change for U34-5 from  to rectangular 0.43mm,0.17mm
Warning pad shape change for U35-5 from rounded 0.45mm,1.35mm to rectangular 0.45mm,0.9mm
Warning pad shape change for U35-1 from rounded 0.45mm,1.35mm to rectangular 0.45mm,0.9mm
Warning pad shape change for U48-1 from rounded 0.6mm,1.45mm to rectangular 0.6mm,0.85mm
Warning pad shape change for U26-1 from  to rectangular 0.6mm,0.8mm
Warning pad shape change for U25-8 from rounded 0.6mm,1.397mm to rectangular 0.6mm,0.797mm
Warning pad shape change for U51-16 from rounded 0.4mm,1.2mm to rectangular 0.4mm,0.8mm
Warning pad shape change for U52-30 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U52-17 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U52-1 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U16-8 from  to rectangular 0.6mm,0.85mm
Warning pad shape change for U46-5 from  to rectangular 0.4mm,0.45mm
Warning pad shape change for U50-1 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U50-17 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U50-30 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U23-1 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U23-17 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U23-30 from  to rectangular 0.35mm,0.25mm
Warning pad shape change for U49-16 from rounded 0.4mm,1.2mm to rectangular 0.4mm,0.8mm
Warning pad shape change for U27-1 from  to rectangular 0.6mm,0.8mm
Warning pad shape change for U2-5 from  to rounded 0.6mm,0.6mm
Warning pad shape change for U33-5 from  to rectangular 0.4mm,0.45mm
Warning pad shape change for U9-5 from  to rounded 0.6mm,0.6mm
Warning pad shape change for U17-8 from rounded 0.3mm,1.35mm to rectangular 0.3mm,1.05mm
Warning pad shape change for U37-30 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U37-18 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U42-5 from  to rounded 0.31mm,0.31mm
Warning pad shape change for U43-10 from rounded 0.24mm,0.6mm to rectangular 0.24mm,0.36mm
Warning pad shape change for U43-2 from rounded 0.24mm,0.6mm to rectangular 0.24mm,0.36mm
Warning pad shape change for FB1-1 from  to rounded 0.65mm,0.65mm
Warning pad shape change for U22-18 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U22-30 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U19-7 from  to rounded 0.25mm,0.25mm
Warning pad shape change for U19-8 from  to rounded 0.25mm,0.25mm
Warning pad shape change for U31-1 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U31-2 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U32-6 from  to rectangular 0.8mm,0.2mm
Warning pad shape change for U30-1 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U30-2 from  to rectangular 0.36mm,0.24mm
Warning pad shape change for U29-6 from  to rectangular 0.8mm,0.2mm
Warning pad shape change for U42-3 from  to rounded 0.31mm,0.31mm
Warning pad shape change for U43-19 from rounded 0.24mm,0.6mm to rectangular 0.24mm,0.36mm
Warning pad shape change for U3-15 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U3-14 from  to rectangular 0.24mm,0.36mm
Warning pad shape change for U35-8 from rounded 0.45mm,1.35mm to rectangular 0.45mm,0.9mm
Warning pad shape change for U36-10 from  to rounded 0.25mm,0.25mm
Warning pad shape change for U5-5 from  to rounded 0.6mm,0.6mm
Warning pad shape change for U6-5 from  to rectangular 0.4mm,0.45mm
Warning pad shape change for J6-3 from  to rectangular 0.3mm,1mm
Warning pad shape change for J6-2 from  to rectangular 0.3mm,1mm
Warning pad shape change for J6-1 from  to rectangular 0.3mm,1mm
Warning pad shape change for U36-3 from  to rounded 0.25mm,0.25mm
Warning pad shape change for U36-7 from  to rounded 0.25mm,0.25mm
Warning pad shape change for U36-8 from  to rounded 0.25mm,0.25mm
Warning pad shape change for U47-5 from  to rounded 0.6mm,0.6mm
Warning pad shape change for U18-12 from  to rectangular 0.3mm,0.2mm
Warning pad shape change for U19-1 from  to rounded 0.25mm,0.25mm
Warning pad shape change for U19-2 from  to rounded 0.25mm,0.25mm
Warning pad shape change for U19-4 from  to rounded 0.25mm,0.25mm
Warning pad shape change for U21-5 from  to rectangular 0.3mm,0.37mm
Warning pad shape change for U36-2 from  to rounded 0.25mm,0.25mm
Warning pad shape change for U24-63 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-62 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-61 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-60 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-42 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-43 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-4 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-3 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-1 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U44-1 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U44-10 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for J34-2 from  to rectangular 0.45mm,0.93mm
Warning pad shape change for U24-93 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U44-2 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U44-9 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for J34-3 from  to rectangular 0.45mm,0.93mm
Warning pad shape change for U24-94 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U44-4 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for U44-7 from  to rectangular 0.2mm,0.365mm
Warning pad shape change for J34-4 from  to rectangular 0.45mm,0.93mm
Warning pad shape change for U24-95 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-70 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-88 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-89 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-59 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-35 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-38 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-36 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-33 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-34 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-68 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U28-3 from  to rounded 0.6mm,0.6mm
Warning pad shape change for U28-1 from  to rounded 0.6mm,0.6mm
Warning pad shape change for U24-9 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
Warning pad shape change for U24-96 from rounded 0.2mm,1.4mm to rectangular 0.2mm,1.2mm
