#
#Component attribute names
#
@0 .comp_mount_type
@1 .comp_height

# CMP 0
CMP 1 5.4780099 0.3735123 90 N R335 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 5.4780099 0.3971343 180 N 520 0 R335-1
TOP 1 5.4780099 0.3498902 180 N 9 0 R335-2
#
# CMP 1
CMP 1 5.4280601 0.3735123 90 N R334 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 5.4280601 0.3971343 180 N 521 0 R334-1
TOP 1 5.4280601 0.3498902 180 N 10 0 R334-2
#
# CMP 2
CMP 1 5.377446 0.3735123 90 N R333 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 5.377446 0.3971343 180 N 522 0 R333-1
TOP 1 5.377446 0.3498902 180 N 11 0 R333-2
#
# CMP 3
CMP 1 5.327446 0.3735123 90 N R332 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 5.327446 0.3971343 180 N 523 0 R332-1
TOP 1 5.327446 0.3498902 180 N 12 0 R332-2
#
# CMP 4
CMP 1 5.277446 0.3735123 90 N R331 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 5.277446 0.3971343 180 N 524 0 R331-1
TOP 1 5.277446 0.3498902 180 N 13 0 R331-2
#
# CMP 5
CMP 1 5.229436 0.3735123 90 N R330 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 5.229436 0.3971343 180 N 525 0 R330-1
TOP 1 5.229436 0.3498902 180 N 14 0 R330-2
#
# CMP 6
CMP 1 5.325 0.1350915 180 N R329 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 5.301378 0.1350915 90 N 526 0 R329-1
TOP 1 5.3486221 0.1350915 90 N 15 0 R329-2
#
# CMP 7
CMP 1 5.325 0.075 180 N R328 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 5.301378 0.075 90 N 527 0 R328-1
TOP 1 5.3486221 0.075 90 N 16 0 R328-2
#
# CMP 8
CMP 66 1.7247061 1.19 0 N S2 CAS-D20TA ;0=1,1=0.0984
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Circuit 'SPDT'
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.nidec-copal-electronics.com/e/catalog/switch/cas.pdf'
PRP CompType 'Switch'
PRP CurrentRating_mA '100A'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Copal Electronics'
PRP MountType 'SMT'
PRP Orientation 'Top Actuated'
PRP PackageReference '5.4x3.9mm'
PRP PartNumber 'CAS-D20TA'
PRP PositionCount '2'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'CASD20JCT-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP SwitchFunction 'On-On'
PRP VDC_V '6V'
TOP 0 1.7975407 1.2588976 180 N 0 7 S2-1
TOP 1 1.7975407 1.19 180 N 564 2 S2-2
TOP 2 1.7975407 1.1211024 180 N 596 0 S2-3
TOP 3 1.6518715 1.2588976 180 N 0 8 S2-4
TOP 4 1.6518715 1.19 180 N 24 1 S2-5
TOP 5 1.6518715 1.1211024 180 N 596 1 S2-6
#
# CMP 9
CMP 1 5.8353063 0.6110215 0 N R322 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 5.8589283 0.6110215 270 N 284 168 R322-1
TOP 1 5.8116842 0.6110215 270 N 21 1 R322-2
#
# CMP 10
CMP 1 5.8353063 0.675 0 N R319 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 5.8589283 0.675 270 N 159 46 R319-1
TOP 1 5.8116842 0.675 270 N 21 0 R319-2
#
# CMP 11
CMP 1 5.57 0.5450446 180 N R316 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 5.546378 0.5450446 90 N 19 0 R316-1
TOP 1 5.5936221 0.5450446 90 N 284 166 R316-2
#
# CMP 12
CMP 1 5.57 0.4870346 0 N C99 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 5.593622 0.4870346 270 N 284 167 C99-1
TOP 1 5.5463779 0.4870346 270 N 159 45 C99-2
#
# CMP 13
CMP 3 6.9527969 0.091771 270 N R246 CRCW040261R9FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040261R9FKED'
PRP Power_W '63mW'
PRP Res_ohm '61.9'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-61.9LCT-ND'
PRP Supplier_Part_Number_2 '52K7198'
PRP Supplier_Part_Number_3 '71-CRCW0402-61.9-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '61.9'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '61R9'
PRP ValueDisplayed '61.9'
PRP VDC_V '50V'
TOP 0 6.9527969 0.072086 0 N 261 1 R246-1
TOP 1 6.9527969 0.1114561 0 N 354 0 R246-2
#
# CMP 14
CMP 4 3.4949822 1.1779479 0 N C98 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 3.5149822 1.1779479 270 N 162 12 C98-1
TOP 1 3.4749822 1.1779479 270 N 284 173 C98-2
#
# CMP 15
CMP 5 4.107941 0.6249207 180 N C23 C1608X7S1A335K080AC ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '3.3µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=C1608X7S1A335K080AC'
PRP CompType 'Capacitor'
PRP ESR_ohm '4.796m'
PRP IRMS_A '2.3752A'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'C1608X7S1A335K080AC'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '445-14256-1-ND'
PRP Supplier_Part_Number_2 '52X3755'
PRP Supplier_Part_Number_3 '810-C1608X7S1A335K0C'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7S'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '3.3uF'
PRP Value1 '0.004796 ohm'
PRP Value2 '10V'
PRP ValueDisplayed '3.3uF'
PRP VDC_V '10V'
TOP 0 4.0764449 0.6249207 90 N 159 38 C23-1
TOP 1 4.139437 0.6249207 90 N 284 126 C23-2
#
# CMP 16
CMP 39 3.815 1.2737502 0 N C30 GRM033C80J105ME05D ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.murata.com/en-us/products/productdetail?partno=GRM033C80J105ME05%23'
PRP DataSheet 'https://www.murata.com/en-us/products/productdetail?partno=GRM033C80J105ME05%23'
PRP Datasheet_Path 'datasheets/Cap-GRM033C80J105ME05D.pdf'
PRP helpURL 'https://upverter.com/upn/revision/64a3db239e8cbfc8/'
PRP Lead_free 'Yes'
PRP Manufacturer 'Murata'
PRP Operating_Temperature_Range '-55°C to +105°C'
PRP PackageReference '0201'
PRP Part_Number 'GRM033C80J105ME05D'
PRP PartNumber 'GRM033C80J105ME05D'
PRP RoHS 'TRUE'
PRP SizeZ_mm '0.39mm'
PRP TempCo '22%'
PRP Temperature_Characteristic 'X6S'
PRP Tolerance__ '20%'
PRP Value '1µF'
PRP ValueDisplayed '1.0uF'
PRP VDC_V '6.3V'
TOP 0 3.826122 1.2737502 180 N 284 174 C30-1
TOP 1 3.803878 1.2737502 180 N 175 31 C30-2
#
# CMP 17
CMP 1 4.3365115 1.65252 0 N R300 ERJ-2GEJ102X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/DMA0000COL9.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS 'Passed with Exemption'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GEJ102X'
PRP Power_W '100mW'
PRP Published ''
PRP Publisher ''
PRP Res_ohm '1k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P1.0KJCT-ND'
PRP Supplier_Part_Number_2 '65T8247'
PRP Supplier_Part_Number_3 '667-ERJ-2GEJ102X'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '1.0k'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '1k00'
PRP ValueDisplayed '1.0k'
PRP VDC_V '50V'
TOP 0 4.3601335 1.65252 270 N 284 169 R300-1
TOP 1 4.3128894 1.65252 270 N 123 1 R300-2
#
# CMP 18
CMP 1 4.3365115 1.7154906 0 N R298 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 4.3601335 1.7154906 270 N 159 47 R298-1
TOP 1 4.3128894 1.7154906 270 N 123 0 R298-2
#
# CMP 19
CMP 1 4.6152579 1.2153327 0 N R293 ERJ-2GEJ102X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/DMA0000COL9.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS 'Passed with Exemption'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GEJ102X'
PRP Power_W '100mW'
PRP Published ''
PRP Publisher ''
PRP Res_ohm '1k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P1.0KJCT-ND'
PRP Supplier_Part_Number_2 '65T8247'
PRP Supplier_Part_Number_3 '667-ERJ-2GEJ102X'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '1.0k'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '1k00'
PRP ValueDisplayed '1.0k'
PRP VDC_V '50V'
TOP 0 4.6388799 1.2153327 270 N 284 170 R293-1
TOP 1 4.5916358 1.2153327 270 N 46 1 R293-2
#
# CMP 20
CMP 1 4.565 1.1523621 180 N R291 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 4.541378 1.1523621 90 N 159 48 R291-1
TOP 1 4.5886221 1.1523621 90 N 46 0 R291-2
#
# CMP 21
CMP 3 4.2829332 0.6746845 270 N R284 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 4.2829332 0.6549995 0 N 529 0 R284-1
TOP 1 4.2829332 0.6943696 0 N 110 0 R284-2
#
# CMP 22
CMP 3 4.19 0.674685 270 N R283 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 4.19 0.655 0 N 530 0 R283-1
TOP 1 4.19 0.6943701 0 N 111 0 R283-2
#
# CMP 23
CMP 3 3.075 1.2395981 180 N R281 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 3.055315 1.2395981 90 N 536 0 R281-1
TOP 1 3.0946851 1.2395981 90 N 113 0 R281-2
#
# CMP 24
CMP 13 4.5541718 1.9999997 90 N J6/J8 SSQ-110-03-T-D ;0=2,1=0.3402
PRP Alternate_Manufacturer 'Major League Electronics'
PRP Alternate_PartNumber 'CRD-081413-A-G'
PRP ClassName ''
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'https://www.samtec.com/ftppub/cpdf/SSQ-1XX-XX-XXX-X-XX-XXX-XX-X-MKT.pdf'
PRP CompType 'Receptacle'
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Incomplete'
PRP Manufacturer 'Samtec'
PRP MountType 'TH'
PRP Note 'Booster Pack 40 pin J6 and J8'
PRP PackageReference '10x2 Receptacle'
PRP PartNumber 'SSQ-110-03-T-D'
PRP RoHS 'Y'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'SAM1204-10-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Value ''
TOP 0 5.0041718 2.0499997 0 N 539 0 J6/J8-51
TOP 1 4.9041718 2.0499997 0 N 538 0 J6/J8-52
TOP 2 4.8041718 2.0499997 0 N 537 0 J6/J8-53
TOP 3 4.7041718 2.0499997 0 N 377 0 J6/J8-54
TOP 4 4.6041718 2.0499997 0 N 378 0 J6/J8-55
TOP 5 4.5041718 2.0499997 0 N 355 1 J6/J8-56
TOP 6 4.4041718 2.0499997 0 N 536 1 J6/J8-57
TOP 7 4.3041718 2.0499997 0 N 374 0 J6/J8-58
TOP 8 4.2041718 2.0499997 0 N 554 0 J6/J8-59
TOP 9 4.1041718 2.0499997 0 N 284 209 J6/J8-60
TOP 10 5.0041718 1.9499997 0 N 455 1 J6/J8-71
TOP 11 4.9041718 1.9499997 0 N 457 1 J6/J8-72
TOP 12 4.8041718 1.9499997 0 N 386 0 J6/J8-73
TOP 13 4.7041718 1.9499997 0 N 391 0 J6/J8-74
TOP 14 4.6041718 1.9499997 0 N 541 0 J6/J8-75
TOP 15 4.5041718 1.9499997 0 N 540 0 J6/J8-76
TOP 16 4.4041718 1.9499997 0 N 544 0 J6/J8-77
TOP 17 4.3041718 1.9499997 0 N 542 1 J6/J8-78
TOP 18 4.2041718 1.9499997 0 N 534 1 J6/J8-79
TOP 19 4.1041718 1.9499997 0 N 532 1 J6/J8-80
#
# CMP 25
CMP 12 4.5541718 0.2999995 90 N J5/J7 SSQ-110-03-T-D ;0=2,1=0.3402
PRP Alternate_Manufacturer 'Major League Electronics'
PRP Alternate_PartNumber 'CRD-081413-A-G'
PRP ClassName ''
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'https://www.samtec.com/ftppub/cpdf/SSQ-1XX-XX-XXX-X-XX-XXX-XX-X-MKT.pdf'
PRP CompType 'Receptacle'
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Incomplete'
PRP Manufacturer 'Samtec'
PRP MountType 'TH'
PRP Note 'Booster Pack 40 pin J5 and J7'
PRP PackageReference '10x2 Receptacle'
PRP PartNumber 'SSQ-110-03-T-D'
PRP RoHS 'Y'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'SAM1204-10-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Value ''
TOP 0 4.1041718 0.2499995 0 N 160 2 J5/J7-41
TOP 1 4.2041718 0.2499995 0 N 574 0 J5/J7-42
TOP 2 4.3041718 0.2499995 0 N 102 0 J5/J7-43
TOP 3 4.4041718 0.2499995 0 N 101 0 J5/J7-44
TOP 4 4.5041718 0.2499995 0 N 528 0 J5/J7-45
TOP 5 4.6041718 0.2499995 0 N 25 0 J5/J7-46
TOP 6 4.7041718 0.2499995 0 N 375 0 J5/J7-47
TOP 7 4.8041718 0.2499995 0 N 68 0 J5/J7-48
TOP 8 4.9041718 0.2499995 0 N 509 0 J5/J7-49
TOP 9 5.0041718 0.2499995 0 N 508 0 J5/J7-50
TOP 10 4.1041718 0.3499995 0 N 158 2 J5/J7-61
TOP 11 4.2041718 0.3499995 0 N 284 210 J5/J7-62
TOP 12 4.3041718 0.3499995 0 N 583 0 J5/J7-63
TOP 13 4.4041718 0.3499995 0 N 582 0 J5/J7-64
TOP 14 4.5041718 0.3499995 0 N 581 0 J5/J7-65
TOP 15 4.6041718 0.3499995 0 N 580 0 J5/J7-66
TOP 16 4.7041718 0.3499995 0 N 577 0 J5/J7-67
TOP 17 4.8041718 0.3499995 0 N 576 0 J5/J7-68
TOP 18 4.9041718 0.3499995 0 N 575 0 J5/J7-69
TOP 19 5.0041718 0.3499995 0 N 120 0 J5/J7-70
#
# CMP 26
CMP 11 2.0541736 1.9999997 90 N J2/J4 SSQ-110-03-T-D ;0=2,1=0.3402
PRP Alternate_Manufacturer 'Major League Electronics'
PRP Alternate_PartNumber 'CRD-081413-A-G'
PRP ClassName ''
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'https://www.samtec.com/ftppub/cpdf/SSQ-1XX-XX-XXX-X-XX-XXX-XX-X-MKT.pdf'
PRP CompType 'Receptacle'
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Incomplete'
PRP Manufacturer 'Samtec'
PRP MountType 'TH'
PRP Note 'Booster Pack 40 pin J2 and J4'
PRP PackageReference '10x2 Receptacle'
PRP PartNumber 'SSQ-110-03-T-D'
PRP RoHS 'Y'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'SAM1204-10-ND'
PRP Supplier_Part_Number_2 '11P8392'
PRP Supplier_Part_Number_3 ''
PRP Value ''
TOP 0 2.5041736 2.0499997 0 N 556 0 J2/J4-11
TOP 1 2.4041736 2.0499997 0 N 51 0 J2/J4-12
TOP 2 2.3041736 2.0499997 0 N 70 0 J2/J4-13
TOP 3 2.2041736 2.0499997 0 N 93 0 J2/J4-14
TOP 4 2.1041736 2.0499997 0 N 94 0 J2/J4-15
TOP 5 2.0041736 2.0499997 0 N 355 2 J2/J4-16
TOP 6 1.9041736 2.0499997 0 N 72 0 J2/J4-17
TOP 7 1.8041736 2.0499997 0 N 95 0 J2/J4-18
TOP 8 1.7041736 2.0499997 0 N 74 0 J2/J4-19
TOP 9 1.6041736 2.0499997 0 N 284 211 J2/J4-20
TOP 10 2.5041736 1.9499997 0 N 76 0 J2/J4-31
TOP 11 2.4041736 1.9499997 0 N 78 0 J2/J4-32
TOP 12 2.3041736 1.9499997 0 N 80 0 J2/J4-33
TOP 13 2.2041736 1.9499997 0 N 529 1 J2/J4-34
TOP 14 2.1041736 1.9499997 0 N 531 0 J2/J4-35
TOP 15 2.0041736 1.9499997 0 N 530 1 J2/J4-36
TOP 16 1.9041736 1.9499997 0 N 552 1 J2/J4-37
TOP 17 1.8041736 1.9499997 0 N 550 0 J2/J4-38
TOP 18 1.7041736 1.9499997 0 N 548 0 J2/J4-39
TOP 19 1.6041736 1.9499997 0 N 546 0 J2/J4-40
#
# CMP 27
CMP 10 2.0541736 0.2999995 90 N J1/J3 SSQ-110-03-T-D ;0=2,1=0.3402
PRP Alternate_Manufacturer 'Major League Electronics'
PRP Alternate_PartNumber 'CRD-081413-A-G'
PRP ClassName ''
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'https://www.samtec.com/ftppub/cpdf/SSQ-1XX-XX-XXX-X-XX-XXX-XX-X-MKT.pdf'
PRP CompType 'Receptacle'
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Incomplete'
PRP Manufacturer 'Samtec'
PRP MountType 'TH'
PRP Note 'Booster Pack 40 pin J1 and J3'
PRP PackageReference '10x2 Receptacle'
PRP PartNumber 'SSQ-110-03-T-D'
PRP RoHS 'Y'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'SAM1204-10-ND'
PRP Supplier_Part_Number_2 '11P8392'
PRP Supplier_Part_Number_3 ''
PRP Value ''
TOP 0 1.6041736 0.2499995 0 N 160 3 J1/J3-1
TOP 1 1.7041736 0.2499995 0 N 586 0 J1/J3-2
TOP 2 1.8041736 0.2499995 0 N 361 0 J1/J3-3
TOP 3 1.9041736 0.2499995 0 N 359 1 J1/J3-4
TOP 4 2.0041736 0.2499995 0 N 57 0 J1/J3-5
TOP 5 2.1041736 0.2499995 0 N 30 0 J1/J3-6
TOP 6 2.2041736 0.2499995 0 N 96 0 J1/J3-7
TOP 7 2.3041736 0.2499995 0 N 62 0 J1/J3-8
TOP 8 2.4041736 0.2499995 0 N 507 0 J1/J3-9
TOP 9 2.5041736 0.2499995 0 N 506 0 J1/J3-10
TOP 10 1.6041736 0.3499995 0 N 158 3 J1/J3-21
TOP 11 1.7041736 0.3499995 0 N 284 212 J1/J3-22
TOP 12 1.8041736 0.3499995 0 N 595 0 J1/J3-23
TOP 13 1.9041736 0.3499995 0 N 594 0 J1/J3-24
TOP 14 2.0041736 0.3499995 0 N 593 0 J1/J3-25
TOP 15 2.1041736 0.3499995 0 N 592 0 J1/J3-26
TOP 16 2.2041736 0.3499995 0 N 589 0 J1/J3-27
TOP 17 2.3041736 0.3499995 0 N 588 0 J1/J3-28
TOP 18 2.4041736 0.3499995 0 N 587 0 J1/J3-29
TOP 19 2.5041736 0.3499995 0 N 121 0 J1/J3-30
#
# CMP 28
CMP 1 4.635 0.5404529 90 N C244 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 4.635 0.5640749 180 N 284 172 C244-1
TOP 1 4.635 0.5168308 180 N 159 50 C244-2
#
# CMP 29
CMP 1 4.4952316 0.6253149 270 N C243 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 4.4952316 0.6016929 0 N 284 171 C243-1
TOP 1 4.4952316 0.648937 0 N 159 49 C243-2
#
# CMP 30
CMP 1 1.2055004 0.97422 0 N C134 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 1.2291224 0.97422 270 N 285 10 C134-1
TOP 1 1.1818783 0.97422 270 N 148 1 C134-2
#
# CMP 31
CMP 1 0.325 1.1053779 90 N C135 GRM155R71E103KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '10nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R71E103KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E103KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '490-1312-1-ND'
PRP Supplier_Part_Number_2 '81-GRM36X103K25'
PRP Supplier_Part_Number_3 '8819734'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.01uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.01uF'
PRP VDC_V '25V'
TOP 0 0.325 1.1289999 180 N 285 11 C135-1
TOP 1 0.325 1.0817558 180 N 135 2 C135-2
#
# CMP 32
CMP 1 1.1913608 1.5549295 180 N C142 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 1.1677388 1.5549295 90 N 146 1 C142-1
TOP 1 1.2149829 1.5549295 90 N 285 12 C142-2
#
# CMP 33
CMP 1 1.1927236 1.1413274 270 N C143 GCM1555C1H8R0DA16D ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category ''
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case ''
PRP Cap_F '8pF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GCM1555C1H8R0DA16-01.pdf'
PRP CompType ''
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'Murata Electronics North America'
PRP MountType ''
PRP PackageReference '0402'
PRP PartNumber 'GCM1555C1H8R0DA16D'
PRP Polarized ''
PRP RoHS 'TRUE'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm '0.55mm'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C ''
PRP TaMin_C ''
PRP Technology ''
PRP TempCo '30ppm/°C'
PRP Tolerance__ ''
PRP U/M ''
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value ''
PRP Value1 ''
PRP Value2 ''
PRP ValueDisplayed ''
PRP VDC_V ''
TOP 0 1.1927236 1.1177054 0 N 285 7 C143-1
TOP 1 1.1927236 1.1649495 0 N 139 0 C143-2
#
# CMP 34
CMP 1 1.1927236 1.2561296 90 N C144 GCM1555C1H8R0DA16D ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category ''
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case ''
PRP Cap_F '8pF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GCM1555C1H8R0DA16-01.pdf'
PRP CompType ''
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'Murata Electronics North America'
PRP MountType ''
PRP PackageReference '0402'
PRP PartNumber 'GCM1555C1H8R0DA16D'
PRP Polarized ''
PRP RoHS 'TRUE'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm '0.55mm'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C ''
PRP TaMin_C ''
PRP Technology ''
PRP TempCo '30ppm/°C'
PRP Tolerance__ ''
PRP U/M ''
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value ''
PRP Value1 ''
PRP Value2 ''
PRP ValueDisplayed ''
PRP VDC_V ''
TOP 0 1.1927236 1.2797516 180 N 285 6 C144-1
TOP 1 1.1927236 1.2325075 180 N 138 0 C144-2
#
# CMP 35
CMP 1 1.1905004 1.3479921 180 N C149 GRM155R71E103KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '10nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R71E103KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E103KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '490-1312-1-ND'
PRP Supplier_Part_Number_2 '81-GRM36X103K25'
PRP Supplier_Part_Number_3 '8819734'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.01uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.01uF'
PRP VDC_V '25V'
TOP 0 1.1668784 1.3479921 90 N 168 8 C149-1
TOP 1 1.2141225 1.3479921 90 N 285 16 C149-2
#
# CMP 36
CMP 1 0.3608154 1.2256658 90 N C151 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 0.3608154 1.2492878 180 N 285 13 C151-1
TOP 1 0.3608154 1.2020437 180 N 147 0 C151-2
#
# CMP 37
CMP 1 0.4158154 1.2256658 90 N C152 GRM155R71E103KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '10nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R71E103KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E103KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '490-1312-1-ND'
PRP Supplier_Part_Number_2 '81-GRM36X103K25'
PRP Supplier_Part_Number_3 '8819734'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.01uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.01uF'
PRP VDC_V '25V'
TOP 0 0.4158154 1.2492878 180 N 285 14 C152-1
TOP 1 0.4158154 1.2020437 180 N 147 1 C152-2
#
# CMP 38
CMP 1 0.7749811 0.9418502 0 N C154 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 0.7986031 0.9418502 270 N 285 15 C154-1
TOP 1 0.751359 0.9418502 270 N 130 0 C154-2
#
# CMP 39
CMP 8 1.3988583 1.025 180 N C234 GR442QR73D102KW01L ;0=1,1=0.0799
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '1808'
PRP Cap_F '1nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.murata.com/capacitor/product/GR442QR73D102KW01%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '1808'
PRP PartNumber 'GR442QR73D102KW01L'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '9'
PRP SizeAreaWB_mm2 '16.5'
PRP SizeX_mm '4.5'
PRP SizeY_mm '2'
PRP SizeZ_mm '2.03'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-8145-1-ND'
PRP Supplier_Part_Number_2 '31Y1776'
PRP Supplier_Part_Number_3 '81-GR442QR73D102KW01'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '1000pF'
PRP Value1 'Unknown'
PRP Value2 '2000V'
PRP ValueDisplayed '1000pF'
PRP VDC_V '2kV'
TOP 0 1.3161812 1.025 90 N 285 18 C234-1
TOP 1 1.4815355 1.025 90 N 284 148 C234-2
#
# CMP 40
CMP 1 0.4805004 1.7440085 90 N R129 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP INSTALLATION 'DNP'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 0.4805004 1.7676305 180 N 129 0 R129-1
TOP 1 0.4805004 1.7203864 180 N 145 0 R129-2
#
# CMP 41
CMP 3 1.2055004 1.0542123 0 N R130 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 1.2251854 1.0542123 270 N 149 0 R130-1
TOP 1 1.1858153 1.0542123 270 N 136 0 R130-2
#
# CMP 42
CMP 1 0.5305004 1.7440081 90 N R131 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP INSTALLATION 'DNP'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 0.5305004 1.7676301 180 N 128 0 R131-1
TOP 1 0.5305004 1.720386 180 N 144 0 R131-2
#
# CMP 43
CMP 3 1.2055004 1.0142204 180 N R132 ERJ-2GEJ101X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C84.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GEJ101X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '100'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 'P100JCT-ND'
PRP Supplier_Part_Number_2 '65T8246'
PRP Supplier_Part_Number_3 '2059210'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '100'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '100R'
PRP ValueDisplayed '100'
PRP VDC_V ''
TOP 0 1.1858154 1.0142204 90 N 148 0 R132-1
TOP 1 1.2251855 1.0142204 90 N 176 3 R132-2
#
# CMP 44
CMP 1 0.5805004 1.7440077 90 N R133 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 0.5805004 1.7676297 180 N 124 0 R133-1
TOP 1 0.5805004 1.7203856 180 N 141 0 R133-2
#
# CMP 45
CMP 1 0.6305004 1.7440073 90 N R134 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 0.6305004 1.7676293 180 N 127 0 R134-1
TOP 1 0.6305004 1.7203852 180 N 143 0 R134-2
#
# CMP 46
CMP 1 0.6805008 1.7440081 90 N R135 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 0.6805008 1.7676301 180 N 125 0 R135-1
TOP 1 0.6805008 1.720386 180 N 142 0 R135-2
#
# CMP 47
CMP 3 0.275175 1.1013778 270 N R136 CRCW0402330KFKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW0402330KFKED'
PRP Power_W '63mW'
PRP Res_ohm '330k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-330KLCT-ND'
PRP Supplier_Part_Number_2 '72M6783'
PRP Supplier_Part_Number_3 '71-CRCW0402-330K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '330k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '330k'
PRP ValueDisplayed '330k'
PRP VDC_V '50V'
TOP 0 0.275175 1.0816928 0 N 135 1 R136-1
TOP 1 0.275175 1.1210629 0 N 176 2 R136-2
#
# CMP 48
CMP 3 0.3714666 1.1013779 90 N R137 CRCW0402330KFKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW0402330KFKED'
PRP Power_W '63mW'
PRP Res_ohm '330k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-330KLCT-ND'
PRP Supplier_Part_Number_2 '72M6783'
PRP Supplier_Part_Number_3 '71-CRCW0402-330K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '330k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '330k'
PRP ValueDisplayed '330k'
PRP VDC_V '50V'
TOP 0 0.3714666 1.1210629 180 N 285 5 R137-1
TOP 1 0.3714666 1.0816928 180 N 135 0 R137-2
#
# CMP 49
CMP 3 1.1876237 1.6563871 180 N R138 CRCW04021K00FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04021K00FKED'
PRP Power_W '63mW'
PRP Res_ohm '1k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-1.00KLCT-ND'
PRP Supplier_Part_Number_2 '52K6545'
PRP Supplier_Part_Number_3 '71-CRCW0402-1.0K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '1.00k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '1k00'
PRP ValueDisplayed '1.00k'
PRP VDC_V '50V'
TOP 0 1.1679387 1.6563871 90 N 131 0 R138-1
TOP 1 1.2073088 1.6563871 90 N 168 7 R138-2
#
# CMP 50
CMP 3 1.0933451 1.724685 270 N R139 CRCW04021K00FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04021K00FKED'
PRP Power_W '63mW'
PRP Res_ohm '1k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-1.00KLCT-ND'
PRP Supplier_Part_Number_2 '52K6545'
PRP Supplier_Part_Number_3 '71-CRCW0402-1.0K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '1.00k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '1k00'
PRP ValueDisplayed '1.00k'
PRP VDC_V '50V'
TOP 0 1.0933451 1.705 0 N 132 0 R139-1
TOP 1 1.0933451 1.7443701 0 N 168 6 R139-2
#
# CMP 51
CMP 3 1.0391325 1.724685 270 N R140 CRCW04021K00FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04021K00FKED'
PRP Power_W '63mW'
PRP Res_ohm '1k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-1.00KLCT-ND'
PRP Supplier_Part_Number_2 '52K6545'
PRP Supplier_Part_Number_3 '71-CRCW0402-1.0K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '1.00k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '1k00'
PRP ValueDisplayed '1.00k'
PRP VDC_V '50V'
TOP 0 1.0391325 1.705 0 N 133 0 R140-1
TOP 1 1.0391325 1.7443701 0 N 168 5 R140-2
#
# CMP 52
CMP 3 0.9922427 1.724685 270 N R141 CRCW04021K00FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04021K00FKED'
PRP Power_W '63mW'
PRP Res_ohm '1k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-1.00KLCT-ND'
PRP Supplier_Part_Number_2 '52K6545'
PRP Supplier_Part_Number_3 '71-CRCW0402-1.0K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '1.00k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '1k00'
PRP ValueDisplayed '1.00k'
PRP VDC_V '50V'
TOP 0 0.9922427 1.705 0 N 134 0 R141-1
TOP 1 0.9922427 1.7443701 0 N 168 4 R141-2
#
# CMP 53
CMP 3 1.1913612 1.5149295 180 N R142 CRCW040249R9FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040249R9FKED'
PRP Power_W '63mW'
PRP Res_ohm '49.9'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-49.9LCT-ND'
PRP Supplier_Part_Number_2 '52K7114'
PRP Supplier_Part_Number_3 '71-CRCW0402-49.9-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '49.9'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '49R9'
PRP ValueDisplayed '49.9'
PRP VDC_V '50V'
TOP 0 1.1716762 1.5149295 90 N 146 0 R142-1
TOP 1 1.2110463 1.5149295 90 N 168 3 R142-2
#
# CMP 54
CMP 3 1.1913612 1.476929 180 N R143 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 1.1716762 1.476929 90 N 137 0 R143-1
TOP 1 1.2110463 1.476929 90 N 168 2 R143-2
#
# CMP 55
CMP 3 0.9117872 1.7136212 180 N R145 CRCW04024K87FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04024K87FKED'
PRP Power_W '63mW'
PRP Res_ohm '4.87k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-4.87KLCT-ND'
PRP Supplier_Part_Number_2 '52K7047'
PRP Supplier_Part_Number_3 '71-CRCW0402-4.87K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '4.87k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '4k87'
PRP ValueDisplayed '4.87k'
PRP VDC_V '50V'
TOP 0 0.8921022 1.7136212 90 N 285 4 R145-1
TOP 1 0.9314723 1.7136212 90 N 140 0 R145-2
#
# CMP 56
CMP 48 0.7955004 1.32437 180 N U24 TM4C1294NCPDTT3 ;0=1,1=0.0472
PRP ADC_Channels '20'
PRP ADC_Resolution '12 Bits'
PRP ComponentLink1Description 'Manufacturer URL'
PRP ComponentLink1URL 'http://www.ti.com/'
PRP ComponentLink2Description 'Datasheet'
PRP ComponentLink2URL 'http://www.ti.com/lit/ds/symlink/tm4c1294ncpdt.pdf'
PRP ComponentLink3Description 'Package Specification'
PRP ComponentLink3URL 'http://www.ti.com/lit/ml/mpqf013/mpqf013.pdf'
PRP CompType 'IC'
PRP CPU 'ARM Cortex-M4'
PRP DatasheetVersion '15863.2743'
PRP Eco-Plan 'Green (RoHS & no Sb/Br)'
PRP Flash '1024 KB'
PRP Manufacturer 'Texas Instruments'
PRP Max_Speed '120 MHz'
PRP Mounting_Technology 'Surface Mount'
PRP MountType 'SMT'
PRP PackageDescription '128-Pin Thin Quad Flat Package, Body 14 x 14 mm, Pitch 0.4 mm'
PRP PackageReference 'PDT0128A'
PRP PackageVersion '4087726/A'
PRP Packing 'Tray'
PRP PartId '1'
PRP PartNumber 'TM4C1294NCPDTT3'
PRP SizeArea_mm2 '256.0'
PRP SizeAreaWB_mm2 '324.0'
PRP SizeX_mm '16.0'
PRP SizeY_mm '16.0'
PRP SizeZ_mm '1.2'
PRP SRAM '256 KB'
PRP Temperature_Range '-40 to 105 degC'
TOP 0 0.4923508 1.0802755 90 N 135 3 U24-1
TOP 1 0.4923508 1.0960235 90 N 0 9 U24-2
TOP 2 0.4923508 1.1117716 90 N 33 0 U24-3
TOP 3 0.4923508 1.1275196 90 N 34 0 U24-4
TOP 4 0.4923508 1.1432676 90 N 0 10 U24-5
TOP 5 0.4923508 1.1590157 90 N 0 11 U24-6
TOP 6 0.4923508 1.1747637 90 N 168 9 U24-7
TOP 7 0.4923509 1.1905117 90 N 168 10 U24-8
TOP 8 0.4923508 1.2062598 90 N 147 2 U24-9
TOP 9 0.4923509 1.2220078 90 N 285 19 U24-10
TOP 10 0.4923509 1.2377558 90 N 0 12 U24-11
TOP 11 0.4923509 1.2535039 90 N 0 13 U24-12
TOP 12 0.4923508 1.2692519 90 N 0 14 U24-13
TOP 13 0.4923508 1.2849999 90 N 0 15 U24-14
TOP 14 0.4923508 1.300748 90 N 0 16 U24-15
TOP 15 0.4923508 1.316496 90 N 168 11 U24-16
TOP 16 0.4923508 1.332244 90 N 285 20 U24-17
TOP 17 0.4923508 1.3479921 90 N 0 17 U24-18
TOP 18 0.4923508 1.3637401 90 N 0 18 U24-19
TOP 19 0.4923508 1.3794881 90 N 0 19 U24-20
TOP 20 0.4923509 1.3952361 90 N 0 20 U24-21
TOP 21 0.4923509 1.4109842 90 N 0 21 U24-22
TOP 22 0.4923509 1.4267322 90 N 0 22 U24-23
TOP 23 0.4923508 1.4424802 90 N 0 23 U24-24
TOP 24 0.4923509 1.4582283 90 N 0 24 U24-25
TOP 25 0.4923508 1.4739763 90 N 168 12 U24-26
TOP 26 0.4923508 1.4897243 90 N 0 25 U24-27
TOP 27 0.4923508 1.5054724 90 N 168 13 U24-28
TOP 28 0.4923508 1.5212204 90 N 0 26 U24-29
TOP 29 0.4923508 1.5369684 90 N 0 27 U24-30
TOP 30 0.4923508 1.5527165 90 N 0 28 U24-31
TOP 31 0.4923508 1.5684645 90 N 0 29 U24-32
TOP 32 0.5514059 1.6275196 0 N 145 1 U24-33
TOP 33 0.5671539 1.6275196 0 N 144 1 U24-34
TOP 34 0.582902 1.6275196 0 N 141 1 U24-35
TOP 35 0.59865 1.6275196 0 N 143 1 U24-36
TOP 36 0.614398 1.6275196 0 N 126 0 U24-37
TOP 37 0.6301461 1.6275196 0 N 142 1 U24-38
TOP 38 0.6458941 1.6275196 0 N 168 14 U24-39
TOP 39 0.6616421 1.6275195 0 N 0 30 U24-40
TOP 40 0.6773902 1.6275196 0 N 0 31 U24-41
TOP 41 0.6931382 1.6275195 0 N 36 0 U24-42
TOP 42 0.7088862 1.6275195 0 N 35 0 U24-43
TOP 43 0.7246343 1.6275195 0 N 0 32 U24-44
TOP 44 0.7403823 1.6275196 0 N 0 33 U24-45
TOP 45 0.7561303 1.6275196 0 N 0 34 U24-46
TOP 46 0.7718784 1.6275196 0 N 168 15 U24-47
TOP 47 0.7876264 1.6275196 0 N 285 21 U24-48
TOP 48 0.8033744 1.6275196 0 N 0 35 U24-49
TOP 49 0.8191225 1.6275196 0 N 0 36 U24-50
TOP 50 0.8348705 1.6275196 0 N 168 16 U24-51
TOP 51 0.8506185 1.6275196 0 N 168 17 U24-52
TOP 52 0.8663665 1.6275195 0 N 0 37 U24-53
TOP 53 0.8821146 1.6275195 0 N 0 38 U24-54
TOP 54 0.8978626 1.6275195 0 N 285 22 U24-55
TOP 55 0.9136106 1.6275196 0 N 0 39 U24-56
TOP 56 0.9293587 1.6275195 0 N 0 40 U24-57
TOP 57 0.9451067 1.6275196 0 N 285 23 U24-58
TOP 58 0.9608547 1.6275196 0 N 140 1 U24-59
TOP 59 0.9766028 1.6275196 0 N 134 1 U24-60
TOP 60 0.9923508 1.6275196 0 N 133 1 U24-61
TOP 61 1.0080988 1.6275196 0 N 132 1 U24-62
TOP 62 1.0238469 1.6275196 0 N 131 1 U24-63
TOP 63 1.0395949 1.6275196 0 N 285 24 U24-64
TOP 64 1.09865 1.5684645 90 N 0 41 U24-65
TOP 65 1.09865 1.5527165 90 N 285 25 U24-66
TOP 66 1.09865 1.5369684 90 N 0 42 U24-67
TOP 67 1.09865 1.5212204 90 N 146 2 U24-68
TOP 68 1.09865 1.5054724 90 N 168 18 U24-69
TOP 69 1.09865 1.4897243 90 N 137 1 U24-70
TOP 70 1.09865 1.4739763 90 N 0 43 U24-71
TOP 71 1.0986499 1.4582283 90 N 0 44 U24-72
TOP 72 1.09865 1.4424802 90 N 0 45 U24-73
TOP 73 1.0986499 1.4267322 90 N 0 46 U24-74
TOP 74 1.0986499 1.4109842 90 N 0 47 U24-75
TOP 75 1.0986499 1.3952361 90 N 0 48 U24-76
TOP 76 1.09865 1.3794881 90 N 0 49 U24-77
TOP 77 1.09865 1.3637401 90 N 0 50 U24-78
TOP 78 1.09865 1.3479921 90 N 168 19 U24-79
TOP 79 1.09865 1.332244 90 N 285 26 U24-80
TOP 80 1.09865 1.316496 90 N 0 51 U24-81
TOP 81 1.09865 1.300748 90 N 0 52 U24-82
TOP 82 1.09865 1.2849999 90 N 0 53 U24-83
TOP 83 1.09865 1.2692519 90 N 0 54 U24-84
TOP 84 1.0986499 1.2535039 90 N 0 55 U24-85
TOP 85 1.0986499 1.2377558 90 N 0 56 U24-86
TOP 86 1.0986499 1.2220078 90 N 130 1 U24-87
TOP 87 1.09865 1.2062598 90 N 138 1 U24-88
TOP 88 1.0986499 1.1905117 90 N 139 1 U24-89
TOP 89 1.09865 1.1747637 90 N 168 20 U24-90
TOP 90 1.09865 1.1590157 90 N 0 57 U24-91
TOP 91 1.09865 1.1432676 90 N 0 58 U24-92
TOP 92 1.09865 1.1275196 90 N 151 0 U24-93
TOP 93 1.09865 1.1117716 90 N 150 0 U24-94
TOP 94 1.09865 1.0960235 90 N 136 1 U24-95
TOP 95 1.09865 1.0802755 90 N 148 2 U24-96
TOP 96 1.0395949 1.0212204 0 N 39 0 U24-97
TOP 97 1.0238469 1.0212204 0 N 40 0 U24-98
TOP 98 1.0080988 1.0212204 0 N 38 0 U24-99
TOP 99 0.9923508 1.0212204 0 N 41 0 U24-100
TOP 100 0.9766028 1.0212204 0 N 168 21 U24-101
TOP 101 0.9608547 1.0212204 0 N 0 59 U24-102
TOP 102 0.9451067 1.0212204 0 N 0 60 U24-103
TOP 103 0.9293587 1.0212205 0 N 0 61 U24-104
TOP 104 0.9136106 1.0212204 0 N 0 62 U24-105
TOP 105 0.8978626 1.0212205 0 N 0 63 U24-106
TOP 106 0.8821146 1.0212205 0 N 0 64 U24-107
TOP 107 0.8663665 1.0212205 0 N 0 65 U24-108
TOP 108 0.8506185 1.0212204 0 N 0 66 U24-109
TOP 109 0.8348705 1.0212204 0 N 0 67 U24-110
TOP 110 0.8191225 1.0212204 0 N 0 68 U24-111
TOP 111 0.8033744 1.0212204 0 N 0 69 U24-112
TOP 112 0.7876264 1.0212204 0 N 168 22 U24-113
TOP 113 0.7718784 1.0212204 0 N 285 27 U24-114
TOP 114 0.7561303 1.0212204 0 N 130 2 U24-115
TOP 115 0.7403823 1.0212204 0 N 0 70 U24-116
TOP 116 0.7246343 1.0212205 0 N 0 71 U24-117
TOP 117 0.7088862 1.0212205 0 N 0 72 U24-118
TOP 118 0.6931382 1.0212205 0 N 0 73 U24-119
TOP 119 0.6773902 1.0212204 0 N 0 74 U24-120
TOP 120 0.6616421 1.0212205 0 N 0 75 U24-121
TOP 121 0.6458941 1.0212204 0 N 168 23 U24-122
TOP 122 0.6301461 1.0212204 0 N 0 76 U24-123
TOP 123 0.614398 1.0212204 0 N 0 77 U24-124
TOP 124 0.59865 1.0212204 0 N 0 78 U24-125
TOP 125 0.582902 1.0212204 0 N 0 79 U24-126
TOP 126 0.5671539 1.0212204 0 N 0 80 U24-127
TOP 127 0.5514059 1.0212204 0 N 0 81 U24-128
#
# CMP 57
CMP 45 1.287133 1.2043195 0 N Y3 NX3225GA-16.000M-STD-CRG-1 ;0=1,1=0.0354
PRP AEC_Category ''
PRP AEC_Grade ''
PRP AEC_Qualified ''
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ndk.com/images/products/catalog/c_NX3225GA-STD-CRG-1_e.pdf'
PRP CompType 'Crystal'
PRP Frequency_Fixed '16MHz'
PRP Frequency_Max ''
PRP Frequency_Min ''
PRP Frequency_Stability '+/-30ppm'
PRP Frequency_Tolerance ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Load_Capacitance ''
PRP Manufacturer 'NDK'
PRP MountType 'SMT'
PRP PackageReference '3.2x0.75x2.5mm'
PRP PartNumber 'NX3225GA-16.000M-STD-CRG-1'
PRP REACh ''
PRP RoHS 'Y'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '644-1157-1-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '70°C'
PRP TaMin_C '-10°C'
TOP 0 1.318629 1.2476266 180 N 138 2 Y3-1
TOP 1 1.318629 1.1610124 180 N 285 29 Y3-2
TOP 2 1.2556369 1.1610124 180 N 139 2 Y3-3
TOP 3 1.2556369 1.2476266 180 N 285 28 Y3-4
#
# CMP 58
CMP 1 3.553629 0.743748 90 N C15 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 3.553629 0.76737 180 N 162 8 C15-1
TOP 1 3.553629 0.7201259 180 N 284 110 C15-2
#
# CMP 59
CMP 1 3.6036293 0.743748 90 N C7 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 3.6036293 0.76737 180 N 159 29 C7-1
TOP 1 3.6036293 0.7201259 180 N 284 109 C7-2
#
# CMP 60
CMP 9 6.6 1.2684112 180 N Y4 ABM10W-25.0000MHZ-4-D1X-T3 ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'https://abracon.com/Resonators/ABM10W.pdf'
PRP CompType 'Crystal'
PRP Frequency_Fixed '25MHz'
PRP Frequency_Max ''
PRP Frequency_Min ''
PRP Frequency_Stability '20 ppm'
PRP Frequency_Tolerance '10 ppm'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Load_Capacitance '4 pF'
PRP Manufacturer 'Abracon Corporation'
PRP MountType 'SMT'
PRP PackageReference '2x2.5mm'
PRP PartNumber 'ABM10W-25.0000MHZ-4-D1X-T3'
PRP REACh ''
PRP RoHS 'Y'
PRP SizeArea_mm2 '5'
PRP SizeAreaWB_mm2 '10.5'
PRP SizeX_mm '2'
PRP SizeY_mm '2.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '85°C'
PRP TaMin_C '-40°C'
TOP 0 6.576378 1.236423 270 N 288 2 Y4-1
TOP 1 6.576378 1.3003994 270 N 284 176 Y4-2
TOP 2 6.6236221 1.3003994 270 N 287 2 Y4-3
TOP 3 6.6236221 1.236423 270 N 284 175 Y4-4
#
# CMP 61
CMP 9 6.8345987 0.4404981 270 N Y2 ABM10W-25.0000MHZ-4-D1X-T3 ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'https://abracon.com/Resonators/ABM10W.pdf'
PRP CompType 'Crystal'
PRP Frequency_Fixed '25MHz'
PRP Frequency_Max ''
PRP Frequency_Min ''
PRP Frequency_Stability '20 ppm'
PRP Frequency_Tolerance '10 ppm'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Load_Capacitance '4 pF'
PRP Manufacturer 'Abracon Corporation'
PRP MountType 'SMT'
PRP PackageReference '2x2.5mm'
PRP PartNumber 'ABM10W-25.0000MHZ-4-D1X-T3'
PRP REACh ''
PRP RoHS 'Y'
PRP SizeArea_mm2 '5'
PRP SizeAreaWB_mm2 '10.5'
PRP SizeX_mm '2'
PRP SizeY_mm '2.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '85°C'
PRP TaMin_C '-40°C'
TOP 0 6.8665869 0.4168761 180 N 306 2 Y2-1
TOP 1 6.8026105 0.4168761 180 N 284 115 Y2-2
TOP 2 6.8026105 0.4641202 180 N 305 2 Y2-3
TOP 3 6.8665869 0.4641202 180 N 284 116 Y2-4
#
# CMP 62
CMP 51 5.6036603 0.2406245 180 N U43 TXB0108RGYR ;0=1,1=0.0394
PRP Alternate_Manufacturer 'Texas Instruments'
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/txb0108.pdf'
PRP CompType 'IC'
PRP LatestRevisionDate '2017-06-09'
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP PackageDescription 'VQFN-20'
PRP PackageReference 'RGY0020A'
PRP PartNumber 'TXB0108RGYR'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '15.75'
PRP SizeAreaWB_mm2 '24.75'
PRP SizeX_mm '3.5'
PRP SizeY_mm '4.5'
PRP SizeZ_mm '1.0'
PRP U/M 'EA'
TOP 0 5.5741327 0.1559787 180 N 16 1 U43-1
TOP 1 5.5386997 0.1717268 270 N 159 51 U43-2
TOP 2 5.5386997 0.1914118 270 N 15 1 U43-3
TOP 3 5.5386997 0.2110969 270 N 14 1 U43-4
TOP 4 5.5386997 0.2307819 270 N 13 1 U43-5
TOP 5 5.5386997 0.2504669 270 N 12 1 U43-6
TOP 6 5.5386997 0.270152 270 N 11 1 U43-7
TOP 7 5.5386997 0.289837 270 N 10 1 U43-8
TOP 8 5.5386997 0.3095221 270 N 9 1 U43-9
TOP 9 5.5741327 0.3252701 180 N 159 52 U43-10
TOP 10 5.6331879 0.3252701 180 N 284 178 U43-11
TOP 11 5.6686209 0.3095221 270 N 343 0 U43-12
TOP 12 5.6686209 0.289837 270 N 344 2 U43-13
TOP 13 5.6686209 0.270152 270 N 345 2 U43-14
TOP 14 5.6686209 0.2504669 270 N 346 2 U43-15
TOP 15 5.6686209 0.2307819 270 N 347 2 U43-16
TOP 16 5.6686209 0.2110969 270 N 348 2 U43-17
TOP 17 5.6686209 0.1914118 270 N 349 2 U43-18
TOP 18 5.6686209 0.1717268 270 N 157 29 U43-19
TOP 19 5.6331879 0.1559787 180 N 350 2 U43-20
TOP 20 5.6036603 0.2406244 270 N 284 177 U43-21
#
# CMP 63
CMP 27 7.0727969 0.136456 0 N U42 TCAN1044VDRBTQ1 ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer 'Texas Instruments'
PRP Alternate_PartNumber 'TCAN1044VDRBRQ1'
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/tcan1044v-q1.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/tcan1044v-q1'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/tcan1044v-q1/datasheet'
PRP CompType 'IC'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP Operating_Temperature_Range ''
PRP PackageDescription 'VSON-8'
PRP PackageReference 'DRB0008J'
PRP PartNumber 'TCAN1044VDRBTQ1'
PRP Rating ''
PRP RoHS ''
PRP SizeArea_mm2 '9'
PRP SizeAreaWB_mm2 '16'
PRP SizeX_mm '3'
PRP SizeY_mm '3'
PRP SizeZ_mm '1'
TOP 0 7.127915 0.1748419 270 N 250 1 U42-1
TOP 1 7.127915 0.1492513 270 N 284 179 U42-2
TOP 2 7.127915 0.1236608 270 N 157 30 U42-3
TOP 3 7.127915 0.0980702 270 N 249 1 U42-4
TOP 4 7.0176788 0.0980702 270 N 159 53 U42-5
TOP 5 7.0176788 0.1236608 270 N 354 1 U42-6
TOP 6 7.0176788 0.1492513 270 N 353 1 U42-7
TOP 7 7.0176788 0.1748419 270 N 449 3 U42-8
TOP 8 7.0727968 0.136456 180 N 284 180 U42-9
#
# CMP 64
CMP 24 6.9893088 1.6095982 0 N U41 TPD4E05U06DQAR ;0=1,1=0.0217
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer 'Texas Instruments'
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/tpd4e05u06.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/tpd4e05u06'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/tpd4e05u06/datasheet'
PRP CompType 'IC'
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP PackageDescription 'USON-10'
PRP PackageReference 'DQA0010A'
PRP PartNumber 'TPD4E05U06DQAR'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '7.0'
PRP SizeX_mm '1.0'
PRP SizeY_mm '2.5'
PRP SizeZ_mm '0.55'
TOP 0 7.0057458 1.6489683 270 N 293 1 U41-1
TOP 1 7.0057458 1.6292833 270 N 294 1 U41-2
TOP 2 7.0057458 1.6095983 270 N 284 40 U41-3
TOP 3 7.0057458 1.5899132 270 N 291 1 U41-4
TOP 4 7.0057458 1.5702282 270 N 292 1 U41-5
TOP 5 6.9728718 1.5702282 270 N 292 0 U41-6
TOP 6 6.9728718 1.5899132 270 N 291 0 U41-7
TOP 7 6.9728718 1.6095983 270 N 284 39 U41-8
TOP 8 6.9728718 1.6292833 270 N 294 0 U41-9
TOP 9 6.9728718 1.6489683 270 N 293 0 U41-10
#
# CMP 65
CMP 24 6.9895788 1.7389369 0 N U40 TPD4E05U06DQAR ;0=1,1=0.0217
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer 'Texas Instruments'
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/tpd4e05u06.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/tpd4e05u06'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/tpd4e05u06/datasheet'
PRP CompType 'IC'
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP PackageDescription 'USON-10'
PRP PackageReference 'DQA0010A'
PRP PartNumber 'TPD4E05U06DQAR'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '7.0'
PRP SizeX_mm '1.0'
PRP SizeY_mm '2.5'
PRP SizeZ_mm '0.55'
TOP 0 7.0060158 1.778307 270 N 297 0 U40-1
TOP 1 7.0060158 1.758622 270 N 298 0 U40-2
TOP 2 7.0060158 1.738937 270 N 284 38 U40-3
TOP 3 7.0060158 1.7192519 270 N 295 1 U40-4
TOP 4 7.0060158 1.6995669 270 N 296 1 U40-5
TOP 5 6.9731418 1.6995669 270 N 296 0 U40-6
TOP 6 6.9731418 1.7192519 270 N 295 0 U40-7
TOP 7 6.9731418 1.738937 270 N 284 37 U40-8
TOP 8 6.9731418 1.758622 270 N 298 1 U40-9
TOP 9 6.9731418 1.778307 270 N 297 1 U40-10
#
# CMP 66
CMP 24 6.9893088 0.6195982 0 N U39 TPD4E05U06DQAR ;0=1,1=0.0217
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer 'Texas Instruments'
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/tpd4e05u06.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/tpd4e05u06'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/tpd4e05u06/datasheet'
PRP CompType 'IC'
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP PackageDescription 'USON-10'
PRP PackageReference 'DQA0010A'
PRP PartNumber 'TPD4E05U06DQAR'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '7.0'
PRP SizeX_mm '1.0'
PRP SizeY_mm '2.5'
PRP SizeZ_mm '0.55'
TOP 0 7.0057458 0.6589683 270 N 313 2 U39-1
TOP 1 7.0057458 0.6392833 270 N 314 2 U39-2
TOP 2 7.0057458 0.6195983 270 N 284 36 U39-3
TOP 3 7.0057458 0.5999132 270 N 311 2 U39-4
TOP 4 7.0057458 0.5802282 270 N 312 2 U39-5
TOP 5 6.9728718 0.5802282 270 N 312 1 U39-6
TOP 6 6.9728718 0.5999132 270 N 311 1 U39-7
TOP 7 6.9728718 0.6195983 270 N 284 35 U39-8
TOP 8 6.9728718 0.6392833 270 N 314 1 U39-9
TOP 9 6.9728718 0.6589683 270 N 313 1 U39-10
#
# CMP 67
CMP 24 6.9895788 0.7889369 0 N U38 TPD4E05U06DQAR ;0=1,1=0.0217
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer 'Texas Instruments'
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/tpd4e05u06.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/tpd4e05u06'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/tpd4e05u06/datasheet'
PRP CompType 'IC'
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP PackageDescription 'USON-10'
PRP PackageReference 'DQA0010A'
PRP PartNumber 'TPD4E05U06DQAR'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '7.0'
PRP SizeX_mm '1.0'
PRP SizeY_mm '2.5'
PRP SizeZ_mm '0.55'
TOP 0 7.0060158 0.828307 270 N 317 1 U38-1
TOP 1 7.0060158 0.808622 270 N 318 1 U38-2
TOP 2 7.0060158 0.788937 270 N 284 34 U38-3
TOP 3 7.0060158 0.7692519 270 N 315 2 U38-4
TOP 4 7.0060158 0.7495669 270 N 316 2 U38-5
TOP 5 6.9731418 0.7495669 270 N 316 1 U38-6
TOP 6 6.9731418 0.7692519 270 N 315 1 U38-7
TOP 7 6.9731418 0.788937 270 N 284 33 U38-8
TOP 8 6.9731418 0.808622 270 N 318 2 U38-9
TOP 9 6.9731418 0.828307 270 N 317 2 U38-10
#
# CMP 68
CMP 52 6.625175 1.670039 0 N U37 DP83869HMRGZT ;0=1,1=0.0461
PRP AEC_Qualified 'No'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/dp83869hm.pdf'
PRP Data_Rate '1000Mbits/s'
PRP DataSheet 'http://www.ti.com/lit/ds/symlink/dp83869hm.pdf'
PRP Datasheet_Path 'datasheets/IC-DP83869HMRGZT.pdf'
PRP Digikey_Description 'IC TRANSCEIVER 1/1 48FN'
PRP Digikey_Part_Number '296-53377-1-ND'
PRP helpURL 'https://upverter.com/upn/revision/bc27fdb8fd73be3f/'
PRP Interface 'Ethernet'
PRP Lead_free 'Yes'
PRP Manufacturer 'Texas Instruments'
PRP Max_Supply_Voltage '3.45V'
PRP Min_Supply_Voltage '990mV'
PRP Mouser_Description 'Phy 1-CH 10MBPS/100MBPS/1GBPS 1.8V/2.5V/3.3V 48-PIN VQFN Ep T/r'
PRP Mouser_Part_Number '595-DP83869HMRGZT'
PRP Number_of_Channels '1'
PRP Operating_Temperature_Range '-40°C to +125°C'
PRP PackageReference 'VQFN48'
PRP Part_Number 'DP83869HMRGZT'
PRP PartNumber 'DP83869HMRGZT'
PRP RoHS 'TRUE'
PRP Simplex_Duplex 'Full-Duplex'
PRP SizeZ_mm '1mm'
PRP Standoff_Height '0mm'
PRP TaMax_C '+125°C'
PRP TaMin_C '-40°C'
TOP 0 6.7590333 1.7783067 180 N 297 2 U37-1
TOP 1 6.7590333 1.7586217 180 N 298 2 U37-2
TOP 2 6.7590333 1.7389366 180 N 171 3 U37-3
TOP 3 6.7590333 1.7192516 180 N 295 2 U37-4
TOP 4 6.7590333 1.6995666 180 N 296 2 U37-5
TOP 5 6.7590333 1.6798815 180 N 172 4 U37-6
TOP 6 6.7590333 1.6601965 180 N 293 2 U37-7
TOP 7 6.7590333 1.6405114 180 N 294 2 U37-8
TOP 8 6.7590333 1.6208264 180 N 171 4 U37-9
TOP 9 6.7590333 1.6011414 180 N 291 2 U37-10
TOP 10 6.7590333 1.5814563 180 N 292 2 U37-11
TOP 11 6.7590333 1.5617713 180 N 299 1 U37-12
TOP 12 6.7334427 1.5361807 180 N 163 0 U37-13
TOP 13 6.7137577 1.5361807 180 N 0 82 U37-14
TOP 14 6.6940726 1.5361807 180 N 0 83 U37-15
TOP 15 6.6743876 1.5361807 180 N 0 84 U37-16
TOP 16 6.6547026 1.5361807 180 N 0 85 U37-17
TOP 17 6.6350175 1.5361807 180 N 159 54 U37-18
TOP 18 6.6153325 1.5361807 180 N 289 1 U37-19
TOP 19 6.5956474 1.5361807 180 N 290 2 U37-20
TOP 20 6.5759624 1.5361807 180 N 0 86 U37-21
TOP 21 6.5562774 1.5361807 180 N 303 0 U37-22
TOP 22 6.5365923 1.5361807 180 N 0 87 U37-23
TOP 23 6.5169073 1.5361807 180 N 0 88 U37-24
TOP 24 6.4913167 1.5617713 180 N 482 0 U37-25
TOP 25 6.4913167 1.5814563 180 N 484 0 U37-26
TOP 26 6.4913167 1.6011414 180 N 486 0 U37-27
TOP 27 6.4913167 1.6208264 180 N 488 0 U37-28
TOP 28 6.4913167 1.6405114 180 N 490 0 U37-29
TOP 29 6.4913167 1.6601965 180 N 159 55 U37-30
TOP 30 6.4913167 1.6798815 180 N 172 5 U37-31
TOP 31 6.4913167 1.6995666 180 N 504 1 U37-32
TOP 32 6.4913167 1.7192516 180 N 502 1 U37-33
TOP 33 6.4913167 1.7389366 180 N 500 1 U37-34
TOP 34 6.4913167 1.7586217 180 N 498 1 U37-35
TOP 35 6.4913167 1.7783067 180 N 496 1 U37-36
TOP 36 6.5169073 1.8038973 180 N 480 0 U37-37
TOP 37 6.5365923 1.8038973 180 N 494 1 U37-38
TOP 38 6.5562774 1.8038973 180 N 172 6 U37-39
TOP 39 6.5759624 1.8038973 180 N 304 0 U37-40
TOP 40 6.5956474 1.8038973 180 N 262 1 U37-41
TOP 41 6.6153325 1.8038973 180 N 263 1 U37-42
TOP 42 6.6350175 1.8038973 180 N 358 2 U37-43
TOP 43 6.6547026 1.8038973 180 N 300 0 U37-44
TOP 44 6.6743876 1.8038973 180 N 505 2 U37-45
TOP 45 6.6940726 1.8038973 180 N 492 1 U37-46
TOP 46 6.7137577 1.8038973 180 N 107 2 U37-47
TOP 47 6.7334427 1.8038973 180 N 163 1 U37-48
TOP 48 6.625175 1.670039 180 N 284 181 U37-49
#
# CMP 69
CMP 52 6.625175 0.720039 0 N U22 DP83869HMRGZT ;0=1,1=0.0461
PRP AEC_Qualified 'No'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/dp83869hm.pdf'
PRP Data_Rate '1000Mbits/s'
PRP DataSheet 'http://www.ti.com/lit/ds/symlink/dp83869hm.pdf'
PRP Datasheet_Path 'datasheets/IC-DP83869HMRGZT.pdf'
PRP Digikey_Description 'IC TRANSCEIVER 1/1 48FN'
PRP Digikey_Part_Number '296-53377-1-ND'
PRP helpURL 'https://upverter.com/upn/revision/bc27fdb8fd73be3f/'
PRP Interface 'Ethernet'
PRP Lead_free 'Yes'
PRP Manufacturer 'Texas Instruments'
PRP Max_Supply_Voltage '3.45V'
PRP Min_Supply_Voltage '990mV'
PRP Mouser_Description 'Phy 1-CH 10MBPS/100MBPS/1GBPS 1.8V/2.5V/3.3V 48-PIN VQFN Ep T/r'
PRP Mouser_Part_Number '595-DP83869HMRGZT'
PRP Number_of_Channels '1'
PRP Operating_Temperature_Range '-40°C to +125°C'
PRP PackageReference 'VQFN48'
PRP Part_Number 'DP83869HMRGZT'
PRP PartNumber 'DP83869HMRGZT'
PRP RoHS 'TRUE'
PRP Simplex_Duplex 'Full-Duplex'
PRP SizeZ_mm '1mm'
PRP Standoff_Height '0mm'
PRP TaMax_C '+125°C'
PRP TaMin_C '-40°C'
TOP 0 6.7590333 0.8283067 180 N 317 0 U22-1
TOP 1 6.7590333 0.8086217 180 N 318 0 U22-2
TOP 2 6.7590333 0.7889366 180 N 173 2 U22-3
TOP 3 6.7590333 0.7692516 180 N 315 0 U22-4
TOP 4 6.7590333 0.7495666 180 N 316 0 U22-5
TOP 5 6.7590333 0.7298815 180 N 174 4 U22-6
TOP 6 6.7590333 0.7101965 180 N 313 0 U22-7
TOP 7 6.7590333 0.6905114 180 N 314 0 U22-8
TOP 8 6.7590333 0.6708264 180 N 173 1 U22-9
TOP 9 6.7590333 0.6511414 180 N 311 0 U22-10
TOP 10 6.7590333 0.6314563 180 N 312 0 U22-11
TOP 11 6.7590333 0.6117713 180 N 335 0 U22-12
TOP 12 6.7334427 0.5861807 180 N 164 1 U22-13
TOP 13 6.7137577 0.5861807 180 N 0 6 U22-14
TOP 14 6.6940726 0.5861807 180 N 0 5 U22-15
TOP 15 6.6743876 0.5861807 180 N 0 4 U22-16
TOP 16 6.6547026 0.5861807 180 N 0 3 U22-17
TOP 17 6.6350175 0.5861807 180 N 159 7 U22-18
TOP 18 6.6153325 0.5861807 180 N 307 0 U22-19
TOP 19 6.5956474 0.5861807 180 N 308 0 U22-20
TOP 20 6.5759624 0.5861807 180 N 0 2 U22-21
TOP 21 6.5562774 0.5861807 180 N 340 0 U22-22
TOP 22 6.5365923 0.5861807 180 N 0 1 U22-23
TOP 23 6.5169073 0.5861807 180 N 0 0 U22-24
TOP 24 6.4913167 0.6117713 180 N 319 0 U22-25
TOP 25 6.4913167 0.6314563 180 N 320 0 U22-26
TOP 26 6.4913167 0.6511414 180 N 321 0 U22-27
TOP 27 6.4913167 0.6708264 180 N 322 0 U22-28
TOP 28 6.4913167 0.6905114 180 N 309 0 U22-29
TOP 29 6.4913167 0.7101965 180 N 159 6 U22-30
TOP 30 6.4913167 0.7298815 180 N 174 3 U22-31
TOP 31 6.4913167 0.7495666 180 N 324 0 U22-32
TOP 32 6.4913167 0.7692516 180 N 334 0 U22-33
TOP 33 6.4913167 0.7889366 180 N 332 0 U22-34
TOP 34 6.4913167 0.8086217 180 N 330 0 U22-35
TOP 35 6.4913167 0.8283067 180 N 328 0 U22-36
TOP 36 6.5169073 0.8538973 180 N 310 0 U22-37
TOP 37 6.5365923 0.8538973 180 N 326 0 U22-38
TOP 38 6.5562774 0.8538973 180 N 174 2 U22-39
TOP 39 6.5759624 0.8538973 180 N 342 0 U22-40
TOP 40 6.5956474 0.8538973 180 N 262 0 U22-41
TOP 41 6.6153325 0.8538973 180 N 263 0 U22-42
TOP 42 6.6350175 0.8538973 180 N 358 0 U22-43
TOP 43 6.6547026 0.8538973 180 N 336 0 U22-44
TOP 44 6.6743876 0.8538973 180 N 479 0 U22-45
TOP 45 6.6940726 0.8538973 180 N 472 0 U22-46
TOP 46 6.7137577 0.8538973 180 N 471 0 U22-47
TOP 47 6.7334427 0.8538973 180 N 164 0 U22-48
TOP 48 6.625175 0.720039 180 N 284 32 U22-49
#
# CMP 70
CMP 22 4.7676772 1.0437455 180 N U17 TS5A23159DGSR ;0=1,1=0.0433
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer 'Texas Instruments'
PRP Alternate_PartNumber 'TS5A23159DGST'
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/ts5a23159.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/ts5a23159'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/ts5a23159/datasheet'
PRP CompType 'IC'
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP Operating_Temperature_Range '-40 to 85 C'
PRP PackageDescription 'VSSOP-10'
PRP PackageReference 'DGS0010A'
PRP PartNumber 'TS5A23159DGSR'
PRP Rating 'Catalog'
PRP RoHS 'Y'
PRP SizeArea_mm2 '14.7'
PRP SizeAreaWB_mm2 '23.6'
PRP SizeX_mm '4.9'
PRP SizeY_mm '3.0'
PRP SizeZ_mm '1.1'
TOP 0 4.6800788 1.0043754 90 N 46 3 U17-1
TOP 1 4.6800788 1.0240604 90 N 421 1 U17-2
TOP 2 4.6800788 1.0437455 90 N 284 182 U17-3
TOP 3 4.6800788 1.0634305 90 N 419 1 U17-4
TOP 4 4.6800788 1.0831156 90 N 46 2 U17-5
TOP 5 4.8552757 1.0831156 90 N 262 2 U17-6
TOP 6 4.8552757 1.0634305 90 N 440 2 U17-7
TOP 7 4.8552757 1.0437455 90 N 159 56 U17-8
TOP 8 4.8552757 1.0240604 90 N 442 2 U17-9
TOP 9 4.8552757 1.0043754 90 N 263 2 U17-10
#
# CMP 71
CMP 17 2.1639665 1.6242984 90 N U9 SN74LVC1G08DBVR ;0=1,1=0.0571
PRP 3-State_Output 'No'
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer 'Texas Instruments'
PRP Alternate_PartNumber ''
PRP Bits(#) '1'
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/SN74LVC1G08.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/SN74LVC1G08'
PRP CompType 'IC'
PRP DatasheetVersion 'SCES217Y'
PRP F_@_Nom_Voltage(Max)(Mhz) '150'
PRP Gate_Type 'AND'
PRP Generic_Part_Number 'SN74LVC1G08'
PRP ICC_@_Nom_Voltage(Max)(mA) '0.01'
PRP Input_Type 'CMOS/TTL'
PRP Logic 'True'
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP Operating_Temperature_Range(C) '-40 to 125,-40 to 85'
PRP Output_Drive_(IOL/IOH)(Max)(mA) '32/-32'
PRP Output_Type 'CMOS'
PRP PackageDescription 'SOT-23-5'
PRP PackageReference 'DBV0005A'
PRP PartId '1'
PRP PartNumber 'SN74LVC1G08DBVR'
PRP Rating 'Catalog'
PRP RoHS 'Y'
PRP Schmitt_Trigger 'No'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm ''
PRP Sub-Family 'AND Gate'
PRP Technology_Family 'LVC'
PRP tpd_@_Nom_Voltage(Max)(ns) '4.5,6,4,5'
PRP U/M ''
PRP VCC(Max)(V) '5.5'
PRP VCC(Min)(V) '1.65'
PRP Voltage(Nom)(V) '1.8,2.5,3.3,5'
TOP 0 2.1265649 1.6784323 180 N 358 3 U9-1
TOP 1 2.1639665 1.6784323 180 N 97 0 U9-2
TOP 2 2.201368 1.6784323 180 N 284 183 U9-3
TOP 3 2.201368 1.5701646 180 N 231 0 U9-4
TOP 4 2.1265649 1.5701646 180 N 159 57 U9-5
#
# CMP 72
CMP 55 3.6660717 0.1877801 270 N U4 SN74AVC4T245RSVR ;0=1,1=0.0217
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer 'Texas Instruments'
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/sn74avc4t245.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/sn74avc4t245'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/sn74avc4t245/datasheet'
PRP CompType 'IC'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP PackageDescription 'UQFN-16'
PRP PackageReference 'RSV0016A'
PRP PartNumber 'SN74AVC4T245RSVR'
PRP RoHS 'Y'
PRP SizeArea_mm2 '4.68'
PRP SizeAreaWB_mm2 '10.08'
PRP SizeX_mm '1.8'
PRP SizeY_mm '2.6'
PRP SizeZ_mm '0.55'
TOP 0 3.6896938 0.1582525 0 N 223 0 U4-1
TOP 1 3.6739458 0.156284 0 N 159 58 U4-2
TOP 2 3.6581977 0.156284 0 N 153 13 U4-3
TOP 3 3.6424497 0.156284 0 N 255 1 U4-4
TOP 4 3.6188276 0.1641581 270 N 255 2 U4-5
TOP 5 3.6188276 0.1799061 270 N 228 0 U4-6
TOP 6 3.6188276 0.1956541 270 N 227 0 U4-7
TOP 7 3.6188276 0.2114022 270 N 226 0 U4-8
TOP 8 3.6424497 0.2192762 0 N 225 0 U4-9
TOP 9 3.6581977 0.2192762 0 N 284 184 U4-10
TOP 10 3.6739458 0.2192762 0 N 284 185 U4-11
TOP 11 3.6896938 0.2192762 0 N 382 0 U4-12
TOP 12 3.7133158 0.2114022 270 N 383 0 U4-13
TOP 13 3.7133158 0.1956541 270 N 384 1 U4-14
TOP 14 3.7133158 0.1799061 270 N 385 0 U4-15
TOP 15 3.7133158 0.1641581 270 N 223 1 U4-16
#
# CMP 73
CMP 6 0.1228901 1.3480598 270 N R253 ERJ-6ENF1004V ;0=1,1=0.0571
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'ERJ-6ENF1004V'
PRP Power_W '125mW'
PRP Res_ohm '1M'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 'P1.00MCCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-6ENF1004V'
PRP Supplier_Part_Number_3 '1748405'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '1.00Meg'
PRP Value1 '1%'
PRP Value2 '0.125W'
PRP Value_Code '1M00'
PRP ValueDisplayed '1.00M'
PRP VDC_V ''
TOP 0 0.1228901 1.3080599 270 N 42 4 R253-1
TOP 1 0.1228901 1.3880599 270 N 285 8 R253-2
#
# CMP 74
CMP 3 6.895 0.2875541 90 N R250 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 6.895 0.3072391 180 N 284 50 R250-1
TOP 1 6.895 0.267869 180 N 449 2 R250-2
#
# CMP 75
CMP 3 7.2 0.061456 0 N R249 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 7.219685 0.061456 270 N 100 0 R249-1
TOP 1 7.1803149 0.061456 270 N 249 0 R249-2
#
# CMP 76
CMP 3 6.8550004 0.287554 270 N R248 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 6.8550004 0.267869 0 N 449 1 R248-1
TOP 1 6.8550004 0.3072391 0 N 122 0 R248-2
#
# CMP 77
CMP 3 6.9527969 0.1811412 90 N R247 CRCW040261R9FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040261R9FKED'
PRP Power_W '63mW'
PRP Res_ohm '61.9'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-61.9LCT-ND'
PRP Supplier_Part_Number_2 '52K7198'
PRP Supplier_Part_Number_3 '71-CRCW0402-61.9-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '61.9'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '61R9'
PRP ValueDisplayed '61.9'
PRP VDC_V '50V'
TOP 0 6.9527969 0.2008262 180 N 261 0 R247-1
TOP 1 6.9527969 0.1614561 180 N 353 0 R247-2
#
# CMP 78
CMP 3 7.2 0.2114557 0 N R245 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 7.219685 0.2114557 270 N 447 0 R245-1
TOP 1 7.1803149 0.2114557 270 N 250 0 R245-2
#
# CMP 79
CMP 3 6.935 0.2875536 270 N R244 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 6.935 0.2678686 0 N 449 0 R244-1
TOP 1 6.935 0.3072387 0 N 159 10 R244-2
#
# CMP 80
CMP 1 6.4851339 0.3555313 180 N R242 ERJ-2RKF4992X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF4992X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '49.9k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P49.9KLCT-ND'
PRP Supplier_Part_Number_2 '73T6530'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF4992X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '49.9k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '49k9'
PRP ValueDisplayed '49.9k'
PRP VDC_V '50V'
TOP 0 6.4615119 0.3555313 90 N 347 1 R242-1
TOP 1 6.508756 0.3555313 90 N 157 28 R242-2
#
# CMP 81
CMP 1 5.9399997 0.4721261 270 N R241 ERJ-2RKF4992X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF4992X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '49.9k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P49.9KLCT-ND'
PRP Supplier_Part_Number_2 '73T6530'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF4992X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '49.9k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '49k9'
PRP ValueDisplayed '49.9k'
PRP VDC_V '50V'
TOP 0 5.9399997 0.4485041 0 N 344 1 R241-1
TOP 1 5.9399997 0.4957482 0 N 157 24 R241-2
#
# CMP 82
CMP 1 6.0641757 0.4721259 270 N R240 ERJ-2RKF4992X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF4992X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '49.9k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P49.9KLCT-ND'
PRP Supplier_Part_Number_2 '73T6530'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF4992X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '49.9k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '49k9'
PRP ValueDisplayed '49.9k'
PRP VDC_V '50V'
TOP 0 6.0641757 0.4485039 0 N 345 1 R240-1
TOP 1 6.0641757 0.495748 0 N 157 23 R240-2
#
# CMP 83
CMP 1 6.2591753 0.4721249 270 N R239 ERJ-2RKF4992X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF4992X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '49.9k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P49.9KLCT-ND'
PRP Supplier_Part_Number_2 '73T6530'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF4992X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '49.9k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '49k9'
PRP ValueDisplayed '49.9k'
PRP VDC_V '50V'
TOP 0 6.2591753 0.4485029 0 N 346 1 R239-1
TOP 1 6.2591753 0.495747 0 N 157 22 R239-2
#
# CMP 84
CMP 1 5.9399997 0.2221261 270 N R238 ERJ-2RKF4992X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF4992X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '49.9k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P49.9KLCT-ND'
PRP Supplier_Part_Number_2 '73T6530'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF4992X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '49.9k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '49k9'
PRP ValueDisplayed '49.9k'
PRP VDC_V '50V'
TOP 0 5.9399997 0.1985041 0 N 348 0 R238-1
TOP 1 5.9399997 0.2457482 0 N 157 19 R238-2
#
# CMP 85
CMP 1 6.0641757 0.2221259 270 N R237 ERJ-2RKF4992X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF4992X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '49.9k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P49.9KLCT-ND'
PRP Supplier_Part_Number_2 '73T6530'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF4992X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '49.9k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '49k9'
PRP ValueDisplayed '49.9k'
PRP VDC_V '50V'
TOP 0 6.0641757 0.1985039 0 N 349 1 R237-1
TOP 1 6.0641757 0.245748 0 N 157 18 R237-2
#
# CMP 86
CMP 1 6.2591753 0.2221249 270 N R236 ERJ-2RKF4992X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF4992X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '49.9k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P49.9KLCT-ND'
PRP Supplier_Part_Number_2 '73T6530'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF4992X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '49.9k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '49k9'
PRP ValueDisplayed '49.9k'
PRP VDC_V '50V'
TOP 0 6.2591753 0.1985029 0 N 350 1 R236-1
TOP 1 6.2591753 0.245747 0 N 157 20 R236-2
#
# CMP 87
CMP 3 6.848 1.8963779 90 N R235 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 6.848 1.9160629 180 N 301 0 R235-1
TOP 1 6.848 1.8766928 180 N 492 0 R235-2
#
# CMP 88
CMP 1 7.6039476 1.25 180 N R234 CRCW0402220RJNED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW0402220RJNED'
PRP Power_W '63mW'
PRP Res_ohm '220'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-220JCT-ND'
PRP Supplier_Part_Number_2 '59M6718'
PRP Supplier_Part_Number_3 '71-CRCW0402J-220-E3'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP Value '220'
PRP Value1 '5%'
PRP Value2 '0.063W'
PRP Value_Code '220R'
PRP ValueDisplayed '220'
PRP VDC_V '50V'
TOP 0 7.5803256 1.25 90 N 232 0 R234-1
TOP 1 7.6275697 1.25 90 N 159 15 R234-2
#
# CMP 89
CMP 3 6.795 1.8963779 90 N R233 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 6.795 1.9160629 180 N 302 0 R233-1
TOP 1 6.795 1.8766928 180 N 107 1 R233-2
#
# CMP 90
CMP 1 7.4574909 1.2512752 180 N R232 CRCW0402220RJNED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW0402220RJNED'
PRP Power_W '63mW'
PRP Res_ohm '220'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-220JCT-ND'
PRP Supplier_Part_Number_2 '59M6718'
PRP Supplier_Part_Number_3 '71-CRCW0402J-220-E3'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP Value '220'
PRP Value1 '5%'
PRP Value2 '0.063W'
PRP Value_Code '220R'
PRP ValueDisplayed '220'
PRP VDC_V '50V'
TOP 0 7.4338689 1.2512752 90 N 233 1 R232-1
TOP 1 7.481113 1.2512752 90 N 159 31 R232-2
#
# CMP 91
CMP 3 6.7 2.0046851 90 N R231 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 6.7 2.0243701 180 N 92 0 R231-1
TOP 1 6.7 1.985 180 N 505 1 R231-2
#
# CMP 92
CMP 1 7.22 2.165 90 N R230 CRCW0402220RJNED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW0402220RJNED'
PRP Power_W '63mW'
PRP Res_ohm '220'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-220JCT-ND'
PRP Supplier_Part_Number_2 '59M6718'
PRP Supplier_Part_Number_3 '71-CRCW0402J-220-E3'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP Value '220'
PRP Value1 '5%'
PRP Value2 '0.063W'
PRP Value_Code '220R'
PRP ValueDisplayed '220'
PRP VDC_V '50V'
TOP 0 7.22 2.188622 180 N 159 16 R230-1
TOP 1 7.22 2.1413779 180 N 235 0 R230-2
#
# CMP 93
CMP 3 6.846592 0.947666 90 N R229 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 6.846592 0.967351 180 N 338 0 R229-1
TOP 1 6.846592 0.9279809 180 N 472 1 R229-2
#
# CMP 94
CMP 1 7.300378 0.221456 0 N R228 CRCW0402220RJNED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW0402220RJNED'
PRP Power_W '63mW'
PRP Res_ohm '220'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-220JCT-ND'
PRP Supplier_Part_Number_2 '59M6718'
PRP Supplier_Part_Number_3 '71-CRCW0402J-220-E3'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP Value '220'
PRP Value1 '5%'
PRP Value2 '0.063W'
PRP Value_Code '220R'
PRP ValueDisplayed '220'
PRP VDC_V '50V'
TOP 0 7.324 0.221456 270 N 237 0 R228-1
TOP 1 7.2767559 0.221456 270 N 159 12 R228-2
#
# CMP 95
CMP 3 6.7627345 1.085 90 N R227 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 6.7627345 1.104685 180 N 339 0 R227-1
TOP 1 6.7627345 1.0653149 180 N 471 2 R227-2
#
# CMP 96
CMP 3 6.715 1.084624 90 N R225 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 6.715 1.104309 180 N 337 1 R225-1
TOP 1 6.715 1.0649389 180 N 479 2 R225-2
#
# CMP 97
CMP 1 7.1602033 1.135 90 N R224 CRCW0402220RJNED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW0402220RJNED'
PRP Power_W '63mW'
PRP Res_ohm '220'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-220JCT-ND'
PRP Supplier_Part_Number_2 '59M6718'
PRP Supplier_Part_Number_3 '71-CRCW0402J-220-E3'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP Value '220'
PRP Value1 '5%'
PRP Value2 '0.063W'
PRP Value_Code '220R'
PRP ValueDisplayed '220'
PRP VDC_V '50V'
TOP 0 7.1602033 1.158622 180 N 159 8 R224-1
TOP 1 7.1602033 1.1113779 180 N 240 0 R224-2
#
# CMP 98
CMP 1 6.443006 2.0129705 90 N R223 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 6.443006 2.0365925 180 N 284 70 R223-1
TOP 1 6.443006 1.9893484 180 N 495 0 R223-2
#
# CMP 99
CMP 1 6.383005 2.0129705 90 N R222 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 6.383005 2.0365925 180 N 284 72 R222-1
TOP 1 6.383005 1.9893484 180 N 497 1 R222-2
#
# CMP 100
CMP 1 6.729387 1.9000779 90 N R220 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 6.729387 1.9236999 180 N 284 73 R220-1
TOP 1 6.729387 1.8764558 180 N 107 0 R220-2
#
# CMP 101
CMP 1 6.674387 1.9000779 90 N R219 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 6.674387 1.9236999 180 N 284 69 R219-1
TOP 1 6.674387 1.8764558 180 N 505 0 R219-2
#
# CMP 102
CMP 1 6.506277 2.0130485 90 N R217 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 6.506277 2.0366705 180 N 284 68 R217-1
TOP 1 6.506277 1.9894264 180 N 493 0 R217-2
#
# CMP 103
CMP 1 6.2513781 1.8309624 180 N R216 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 6.2277561 1.8309624 90 N 284 79 R216-1
TOP 1 6.2750002 1.8309624 90 N 499 1 R216-2
#
# CMP 104
CMP 1 6.2513 1.7526528 180 N R215 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 6.227678 1.7526528 90 N 284 82 R215-1
TOP 1 6.2749221 1.7526528 90 N 501 1 R215-2
#
# CMP 105
CMP 1 6.62 1.4449989 270 N R214 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 6.62 1.4213769 0 N 287 1 R214-1
TOP 1 6.62 1.468621 0 N 289 0 R214-2
#
# CMP 106
CMP 1 6.52 1.4449999 270 N R213 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 6.52 1.4213779 0 N 341 0 R213-1
TOP 1 6.52 1.468622 0 N 290 0 R213-2
#
# CMP 107
CMP 1 6.57 1.4449989 270 N R212 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 6.57 1.4213769 0 N 288 1 R212-1
TOP 1 6.57 1.468621 0 N 290 1 R212-2
#
# CMP 108
CMP 1 6.815 1.5033709 270 N R202 ERJ-2RKF1152X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1152X'
PRP Power_W '100mW'
PRP Res_ohm '11.5k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '11.5k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '11k5'
PRP ValueDisplayed '11.5k'
PRP VDC_V ''
TOP 0 6.815 1.4797489 0 N 284 80 R202-1
TOP 1 6.815 1.526993 0 N 299 0 R202-2
#
# CMP 109
CMP 1 6.456277 1.8949999 90 N R201 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 6.456277 1.9186219 180 N 495 1 R201-1
TOP 1 6.456277 1.8713778 180 N 496 0 R201-2
#
# CMP 110
CMP 1 6.406277 1.8949999 90 N R200 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 6.406277 1.9186219 180 N 497 0 R200-1
TOP 1 6.406277 1.8713778 180 N 498 0 R200-2
#
# CMP 111
CMP 1 6.375514 1.7950389 180 N R199 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 6.351892 1.7950389 90 N 499 0 R199-1
TOP 1 6.3991361 1.7950389 90 N 500 0 R199-2
#
# CMP 112
CMP 1 6.375514 1.7450379 180 N R198 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 6.351892 1.7450379 90 N 501 0 R198-1
TOP 1 6.3991361 1.7450379 90 N 502 0 R198-2
#
# CMP 113
CMP 1 6.506277 1.8949999 90 N R197 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 6.506277 1.9186219 180 N 493 1 R197-1
TOP 1 6.506277 1.8713778 180 N 494 0 R197-2
#
# CMP 114
CMP 1 6.375514 1.6950379 180 N R196 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 6.351892 1.6950379 90 N 503 0 R196-1
TOP 1 6.3991361 1.6950379 90 N 504 0 R196-2
#
# CMP 115
CMP 1 1.3125221 1.92 90 N R191 CRCW04024K70JNED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04024K70JNED'
PRP Power_W '63mW'
PRP Res_ohm '4.7k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-4.7KJCT-ND'
PRP Supplier_Part_Number_2 '59M6733'
PRP Supplier_Part_Number_3 '71-CRCW0402J-4.7K-E3'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP Value '4.7k'
PRP Value1 '5%'
PRP Value2 '0.063W'
PRP Value_Code '4k70'
PRP ValueDisplayed '4.7k'
PRP VDC_V '50V'
TOP 0 1.3125221 1.943622 180 N 218 0 R191-1
TOP 1 1.3125221 1.8963779 180 N 153 10 R191-2
#
# CMP 116
CMP 1 1.468 2.007 270 N R189 CRCW04024K70JNED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04024K70JNED'
PRP Power_W '63mW'
PRP Res_ohm '4.7k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-4.7KJCT-ND'
PRP Supplier_Part_Number_2 '59M6733'
PRP Supplier_Part_Number_3 '71-CRCW0402J-4.7K-E3'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP Value '4.7k'
PRP Value1 '5%'
PRP Value2 '0.063W'
PRP Value_Code '4k70'
PRP ValueDisplayed '4.7k'
PRP VDC_V '50V'
TOP 0 1.468 1.983378 0 N 217 0 R189-1
TOP 1 1.468 2.0306221 0 N 153 9 R189-2
#
# CMP 117
CMP 1 1.0298422 1.9213784 270 N R188 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 1.0298422 1.8977564 0 N 153 4 R188-1
TOP 1 1.0298422 1.9450005 0 N 215 0 R188-2
#
# CMP 118
CMP 1 1.0798422 1.9213784 270 N R187 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 1.0798422 1.8977564 0 N 153 5 R187-1
TOP 1 1.0798422 1.9450005 0 N 216 2 R187-2
#
# CMP 119
CMP 1 1.1298425 1.9213779 270 N R186 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 1.1298425 1.8977559 0 N 153 6 R186-1
TOP 1 1.1298425 1.945 0 N 214 0 R186-2
#
# CMP 120
CMP 1 1.1909044 1.9209079 270 N R185 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 1.1909044 1.8972859 0 N 153 8 R185-1
TOP 1 1.1909044 1.94453 0 N 222 0 R185-2
#
# CMP 121
CMP 1 1.6273898 1.765 0 N R183 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 1.6510118 1.765 270 N 153 11 R183-1
TOP 1 1.6037677 1.765 270 N 220 0 R183-2
#
# CMP 122
CMP 1 1.255 1.92 270 N R182 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 1.255 1.896378 0 N 153 7 R182-1
TOP 1 1.255 1.9436221 0 N 219 0 R182-2
#
# CMP 123
CMP 3 0.7256863 1.9473219 0 N R180 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 0.7453713 1.9473219 270 N 216 1 R180-1
TOP 1 0.7060012 1.9473219 270 N 355 0 R180-2
#
# CMP 124
CMP 1 0.9668716 1.9236221 90 N R177 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 0.9668716 1.9472441 180 N 244 0 R177-1
TOP 1 0.9668716 1.9 180 N 159 14 R177-2
#
# CMP 125
CMP 3 3.4921893 1.009406 270 N R165 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 3.4921893 0.989721 0 N 359 0 R165-1
TOP 1 3.4921893 1.0290911 0 N 360 0 R165-2
#
# CMP 126
CMP 1 2.9651181 1.5378832 180 N R156 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 2.9414961 1.5378832 90 N 206 0 R156-1
TOP 1 2.9887402 1.5378832 90 N 157 14 R156-2
#
# CMP 127
CMP 1 2.6023308 0.9066816 180 N R146 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 2.5787088 0.9066816 90 N 211 0 R146-1
TOP 1 2.6259528 0.9066816 90 N 157 12 R146-2
#
# CMP 128
CMP 1 6.443006 1.0629705 90 N R128 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 6.443006 1.0865925 180 N 284 58 R128-1
TOP 1 6.443006 1.0393484 180 N 327 1 R128-2
#
# CMP 129
CMP 1 6.379136 1.0629706 90 N R127 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 6.379136 1.0865926 180 N 284 59 R127-1
TOP 1 6.379136 1.0393485 180 N 329 1 R127-2
#
# CMP 130
CMP 1 6.506277 1.059685 90 N R125 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 6.506277 1.083307 180 N 284 64 R125-1
TOP 1 6.506277 1.0360629 180 N 325 1 R125-2
#
# CMP 131
CMP 1 6.6743876 0.950078 90 N R124 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 6.6743876 0.9737 180 N 284 63 R124-1
TOP 1 6.6743876 0.9264559 180 N 479 1 R124-2
#
# CMP 132
CMP 1 6.7293876 0.9500781 90 N R122 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 6.7293876 0.9737001 180 N 284 60 R122-1
TOP 1 6.7293876 0.926456 180 N 471 1 R122-2
#
# CMP 133
CMP 1 6.2514859 0.8808543 180 N R121 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 6.2278639 0.8808543 90 N 284 61 R121-1
TOP 1 6.275108 0.8808543 90 N 331 1 R121-2
#
# CMP 134
CMP 1 6.2512998 0.8026527 180 N R120 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 6.2276778 0.8026527 90 N 284 62 R120-1
TOP 1 6.2749219 0.8026527 90 N 333 1 R120-2
#
# CMP 135
CMP 1 6.62 0.4949995 270 N R119 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 6.62 0.4713775 0 N 305 0 R119-1
TOP 1 6.62 0.5186216 0 N 307 1 R119-2
#
# CMP 136
CMP 1 6.52 0.495 270 N R118 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 6.52 0.471378 0 N 559 0 R118-1
TOP 1 6.52 0.5186221 0 N 308 1 R118-2
#
# CMP 137
CMP 1 6.5699999 0.4949995 270 N R117 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 6.5699999 0.4713775 0 N 306 0 R117-1
TOP 1 6.5699999 0.5186216 0 N 308 2 R117-2
#
# CMP 138
CMP 1 6.815 0.5533706 270 N R107 ERJ-2RKF1152X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1152X'
PRP Power_W '100mW'
PRP Res_ohm '11.5k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '11.5k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '11k5'
PRP ValueDisplayed '11.5k'
PRP VDC_V ''
TOP 0 6.815 0.5297486 0 N 284 67 R107-1
TOP 1 6.815 0.5769927 0 N 335 1 R107-2
#
# CMP 139
CMP 1 6.456277 0.945 90 N R105 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 6.456277 0.968622 180 N 327 0 R105-1
TOP 1 6.456277 0.9213779 180 N 328 1 R105-2
#
# CMP 140
CMP 1 6.406277 0.945 90 N R104 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 6.406277 0.968622 180 N 329 0 R104-1
TOP 1 6.406277 0.9213779 180 N 330 1 R104-2
#
# CMP 141
CMP 1 6.3755138 0.8450388 180 N R103 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 6.3518918 0.8450388 90 N 331 0 R103-1
TOP 1 6.3991359 0.8450388 90 N 332 1 R103-2
#
# CMP 142
CMP 1 6.3755138 0.7950384 180 N R102 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 6.3518918 0.7950384 90 N 333 0 R102-1
TOP 1 6.3991359 0.7950384 90 N 334 1 R102-2
#
# CMP 143
CMP 1 6.506277 0.945 90 N R101 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 6.506277 0.968622 180 N 325 0 R101-1
TOP 1 6.506277 0.9213779 180 N 326 1 R101-2
#
# CMP 144
CMP 1 6.3755139 0.7450385 180 N R100 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 6.3518919 0.7450385 90 N 323 0 R100-1
TOP 1 6.399136 0.7450385 90 N 324 1 R100-2
#
# CMP 145
CMP 3 4.0789746 1.8122433 0 N R88 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 4.0986596 1.8122433 270 N 457 0 R88-1
TOP 1 4.0592895 1.8122433 270 N 458 0 R88-2
#
# CMP 146
CMP 3 4.0789746 1.7692435 0 N R87 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 4.0986596 1.7692435 270 N 455 0 R87-1
TOP 1 4.0592895 1.7692435 270 N 456 0 R87-2
#
# CMP 147
CMP 3 4.4496652 1.0868779 0 N R79 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 4.4693502 1.0868779 270 N 50 0 R79-1
TOP 1 4.4299801 1.0868779 270 N 481 0 R79-2
#
# CMP 148
CMP 3 4.4516136 1.0298714 0 N R75 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 4.4712986 1.0298714 270 N 58 0 R75-1
TOP 1 4.4319285 1.0298714 270 N 489 0 R75-2
#
# CMP 149
CMP 1 4.5647925 1.0749014 0 N R74 CRCW04024K70JNED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04024K70JNED'
PRP Power_W '63mW'
PRP Res_ohm '4.7k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-4.7KJCT-ND'
PRP Supplier_Part_Number_2 '59M6733'
PRP Supplier_Part_Number_3 '71-CRCW0402J-4.7K-E3'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP Value '4.7k'
PRP Value1 '5%'
PRP Value2 '0.063W'
PRP Value_Code '4k70'
PRP ValueDisplayed '4.7k'
PRP VDC_V '50V'
TOP 0 4.5884145 1.0749014 270 N 419 0 R74-1
TOP 1 4.5411704 1.0749014 270 N 159 32 R74-2
#
# CMP 150
CMP 1 4.5647925 1.0105484 0 N R73 CRCW04024K70JNED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04024K70JNED'
PRP Power_W '63mW'
PRP Res_ohm '4.7k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-4.7KJCT-ND'
PRP Supplier_Part_Number_2 '59M6733'
PRP Supplier_Part_Number_3 '71-CRCW0402J-4.7K-E3'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP Value '4.7k'
PRP Value1 '5%'
PRP Value2 '0.063W'
PRP Value_Code '4k70'
PRP ValueDisplayed '4.7k'
PRP VDC_V '50V'
TOP 0 4.5884145 1.0105484 270 N 421 0 R73-1
TOP 1 4.5411704 1.0105484 270 N 159 33 R73-2
#
# CMP 151
CMP 1 4.9592125 1.0684304 180 N R64 CRCW04024K70JNED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04024K70JNED'
PRP Power_W '63mW'
PRP Res_ohm '4.7k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-4.7KJCT-ND'
PRP Supplier_Part_Number_2 '59M6733'
PRP Supplier_Part_Number_3 '71-CRCW0402J-4.7K-E3'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP Value '4.7k'
PRP Value1 '5%'
PRP Value2 '0.063W'
PRP Value_Code '4k70'
PRP ValueDisplayed '4.7k'
PRP VDC_V '50V'
TOP 0 4.9355905 1.0684304 90 N 440 0 R64-1
TOP 1 4.9828346 1.0684304 90 N 159 34 R64-2
#
# CMP 152
CMP 1 4.9592125 1.0190605 180 N R63 CRCW04024K70JNED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04024K70JNED'
PRP Power_W '63mW'
PRP Res_ohm '4.7k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-4.7KJCT-ND'
PRP Supplier_Part_Number_2 '59M6733'
PRP Supplier_Part_Number_3 '71-CRCW0402J-4.7K-E3'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP Value '4.7k'
PRP Value1 '5%'
PRP Value2 '0.063W'
PRP Value_Code '4k70'
PRP ValueDisplayed '4.7k'
PRP VDC_V '50V'
TOP 0 4.9355905 1.0190605 90 N 442 1 R63-1
TOP 1 4.9828346 1.0190605 90 N 159 35 R63-2
#
# CMP 153
CMP 3 4.9552755 1.1117044 180 N R62 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 4.9355905 1.1117044 90 N 440 1 R62-1
TOP 1 4.9749606 1.1117044 90 N 441 0 R62-2
#
# CMP 154
CMP 3 4.9552755 0.9757865 180 N R61 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 4.9355905 0.9757865 90 N 442 0 R61-1
TOP 1 4.9749606 0.9757865 90 N 443 0 R61-2
#
# CMP 155
CMP 3 3.0777737 1.1350452 180 N R60 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 3.0580887 1.1350452 90 N 532 0 R60-1
TOP 1 3.0974588 1.1350452 90 N 533 0 R60-2
#
# CMP 156
CMP 3 3.075 1.1815118 180 N R59 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 3.055315 1.1815118 90 N 534 0 R59-1
TOP 1 3.0946851 1.1815118 90 N 535 0 R59-2
#
# CMP 157
CMP 3 3.075 1.3363414 180 N R53 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 3.055315 1.3363414 90 N 542 0 R53-1
TOP 1 3.0946851 1.3363414 90 N 543 0 R53-2
#
# CMP 158
CMP 3 3.2346853 1.4949996 180 N R48 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 3.2150003 1.4949996 90 N 552 0 R48-1
TOP 1 3.2543704 1.4949996 90 N 553 0 R48-2
#
# CMP 159
CMP 1 2.7769849 1.285 180 N R43 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 2.7533629 1.285 90 N 414 0 R43-1
TOP 1 2.800607 1.285 90 N 384 0 R43-2
#
# CMP 160
CMP 3 3.6780079 1.73 270 N R41 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 3.6780079 1.710315 0 N 426 0 R41-1
TOP 1 3.6780079 1.7496851 0 N 159 39 R41-2
#
# CMP 161
CMP 1 3.56314 0.1097713 180 N R8 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 3.539518 0.1097713 90 N 153 3 R8-1
TOP 1 3.5867621 0.1097713 90 N 255 0 R8-2
#
# CMP 162
CMP 1 2.0481061 1.654665 90 N R5 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 2.0481061 1.678287 180 N 411 0 R5-1
TOP 1 2.0481061 1.6310429 180 N 358 1 R5-2
#
# CMP 163
CMP 60 7.5803255 1.1393922 270 N Q9 BSS123 ;0=1,1=0.0433
PRP AEC_Category 'Q101'
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer 'None'
PRP Alternate_PartNumber ''
PRP ChType 'N'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.fairchildsemi.com/ds/BS/BSS123.pdf'
PRP CompType 'MOSFET'
PRP IdsMax_A '1.7dA'
PRP LatestRevisionDate '2017-03-09'
PRP LatestRevisionNote 'Added parts.'
PRP Manufacturer 'Fairchild Semiconductor'
PRP MountType 'SMT'
PRP PackageReference 'SOT-23'
PRP PartNumber 'BSS123'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP QgTyp_nC '1.8'
PRP Rdson45_ohm '10'
PRP RoHS 'Y'
PRP SizeArea_mm2 '7.5'
PRP SizeAreaWB_mm2 '14'
PRP SizeX_mm '2.5'
PRP SizeY_mm '3'
PRP SizeZ_mm '1.1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'BSS123NCT-ND'
PRP Supplier_Part_Number_2 '58K8768'
PRP Supplier_Part_Number_3 '512-BSS123'
PRP U/M 'EA'
PRP Value '100V'
PRP Value1 '1'
PRP Value2 '1.8 nC'
PRP Vault_Folder ''
PRP VdsMax_V '100V'
PRP Vgs_V '20V'
TOP 0 7.6177271 1.0921481 0 N 301 1 Q9-1
TOP 1 7.542924 1.0921481 0 N 284 186 Q9-2
TOP 2 7.5803255 1.1866363 0 N 232 1 Q9-3
#
# CMP 164
CMP 60 7.4338688 1.1406674 270 N Q8 BSS123 ;0=1,1=0.0433
PRP AEC_Category 'Q101'
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer 'None'
PRP Alternate_PartNumber ''
PRP ChType 'N'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.fairchildsemi.com/ds/BS/BSS123.pdf'
PRP CompType 'MOSFET'
PRP IdsMax_A '1.7dA'
PRP LatestRevisionDate '2017-03-09'
PRP LatestRevisionNote 'Added parts.'
PRP Manufacturer 'Fairchild Semiconductor'
PRP MountType 'SMT'
PRP PackageReference 'SOT-23'
PRP PartNumber 'BSS123'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP QgTyp_nC '1.8'
PRP Rdson45_ohm '10'
PRP RoHS 'Y'
PRP SizeArea_mm2 '7.5'
PRP SizeAreaWB_mm2 '14'
PRP SizeX_mm '2.5'
PRP SizeY_mm '3'
PRP SizeZ_mm '1.1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'BSS123NCT-ND'
PRP Supplier_Part_Number_2 '58K8768'
PRP Supplier_Part_Number_3 '512-BSS123'
PRP U/M 'EA'
PRP Value '100V'
PRP Value1 '1'
PRP Value2 '1.8 nC'
PRP Vault_Folder ''
PRP VdsMax_V '100V'
PRP Vgs_V '20V'
TOP 0 7.4712704 1.0934233 0 N 302 1 Q8-1
TOP 1 7.3964673 1.0934233 0 N 284 117 Q8-2
TOP 2 7.4338688 1.1879115 0 N 233 0 Q8-3
#
# CMP 165
CMP 60 7.34 2.165 90 N Q7 BSS123 ;0=1,1=0.0433
PRP AEC_Category 'Q101'
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer 'None'
PRP Alternate_PartNumber ''
PRP ChType 'N'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.fairchildsemi.com/ds/BS/BSS123.pdf'
PRP CompType 'MOSFET'
PRP IdsMax_A '1.7dA'
PRP LatestRevisionDate '2017-03-09'
PRP LatestRevisionNote 'Added parts.'
PRP Manufacturer 'Fairchild Semiconductor'
PRP MountType 'SMT'
PRP PackageReference 'SOT-23'
PRP PartNumber 'BSS123'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP QgTyp_nC '1.8'
PRP Rdson45_ohm '10'
PRP RoHS 'Y'
PRP SizeArea_mm2 '7.5'
PRP SizeAreaWB_mm2 '14'
PRP SizeX_mm '2.5'
PRP SizeY_mm '3'
PRP SizeZ_mm '1.1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'BSS123NCT-ND'
PRP Supplier_Part_Number_2 '58K8768'
PRP Supplier_Part_Number_3 '512-BSS123'
PRP U/M 'EA'
PRP Value '100V'
PRP Value1 '1'
PRP Value2 '1.8 nC'
PRP Vault_Folder ''
PRP VdsMax_V '100V'
PRP Vgs_V '20V'
TOP 0 7.3025984 2.2122441 180 N 92 1 Q7-1
TOP 1 7.3774015 2.2122441 180 N 284 92 Q7-2
TOP 2 7.34 2.1177559 180 N 234 0 Q7-3
#
# CMP 166
CMP 60 7.324 0.1136601 270 N Q6 BSS123 ;0=1,1=0.0433
PRP AEC_Category 'Q101'
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer 'None'
PRP Alternate_PartNumber ''
PRP ChType 'N'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.fairchildsemi.com/ds/BS/BSS123.pdf'
PRP CompType 'MOSFET'
PRP IdsMax_A '1.7dA'
PRP LatestRevisionDate '2017-03-09'
PRP LatestRevisionNote 'Added parts.'
PRP Manufacturer 'Fairchild Semiconductor'
PRP MountType 'SMT'
PRP PackageReference 'SOT-23'
PRP PartNumber 'BSS123'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP QgTyp_nC '1.8'
PRP Rdson45_ohm '10'
PRP RoHS 'Y'
PRP SizeArea_mm2 '7.5'
PRP SizeAreaWB_mm2 '14'
PRP SizeX_mm '2.5'
PRP SizeY_mm '3'
PRP SizeZ_mm '1.1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'BSS123NCT-ND'
PRP Supplier_Part_Number_2 '58K8768'
PRP Supplier_Part_Number_3 '512-BSS123'
PRP U/M 'EA'
PRP Value '100V'
PRP Value1 '1'
PRP Value2 '1.8 nC'
PRP Vault_Folder ''
PRP VdsMax_V '100V'
PRP Vgs_V '20V'
TOP 0 7.3614016 0.066416 0 N 338 1 Q6-1
TOP 1 7.2865985 0.066416 0 N 284 66 Q6-2
TOP 2 7.324 0.1609042 0 N 237 1 Q6-3
#
# CMP 167
CMP 60 7.2740952 1.14 90 N Q4 BSS123 ;0=1,1=0.0433
PRP AEC_Category 'Q101'
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer 'None'
PRP Alternate_PartNumber ''
PRP ChType 'N'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.fairchildsemi.com/ds/BS/BSS123.pdf'
PRP CompType 'MOSFET'
PRP IdsMax_A '1.7dA'
PRP LatestRevisionDate '2017-03-09'
PRP LatestRevisionNote 'Added parts.'
PRP Manufacturer 'Fairchild Semiconductor'
PRP MountType 'SMT'
PRP PackageReference 'SOT-23'
PRP PartNumber 'BSS123'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP QgTyp_nC '1.8'
PRP Rdson45_ohm '10'
PRP RoHS 'Y'
PRP SizeArea_mm2 '7.5'
PRP SizeAreaWB_mm2 '14'
PRP SizeX_mm '2.5'
PRP SizeY_mm '3'
PRP SizeZ_mm '1.1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'BSS123NCT-ND'
PRP Supplier_Part_Number_2 '58K8768'
PRP Supplier_Part_Number_3 '512-BSS123'
PRP U/M 'EA'
PRP Value '100V'
PRP Value1 '1'
PRP Value2 '1.8 nC'
PRP Vault_Folder ''
PRP VdsMax_V '100V'
PRP Vgs_V '20V'
TOP 0 7.2366936 1.1872441 180 N 337 0 Q4-1
TOP 1 7.3114967 1.1872441 180 N 284 65 Q4-2
TOP 2 7.2740952 1.0927559 180 N 239 0 Q4-3
#
# CMP 168
CMP 60 0.8529798 1.9077559 90 N Q1 IRLML6401TRPBF ;0=1,1=0.0433
PRP AEC_Category 'Q101'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer 'None'
PRP Alternate_PartNumber ''
PRP ChMode 'Enhancement'
PRP ChType 'P'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://www.infineon.com/dgdl/irlml6401pbf.pdf?fileId=5546d462533600a401535668b96d2634'
PRP CompType 'MOSFET'
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP IdsMax_A '-4.3A'
PRP Manufacturer 'Infineon Technologies'
PRP MountType 'SMT'
PRP PackageReference 'SOT-23'
PRP PartNumber 'IRLML6401TRPBF'
PRP QgTyp_nC '10'
PRP Rdson45_ohm '50m'
PRP RoHS 'Y'
PRP SizeArea_mm2 '7.5'
PRP SizeAreaWB_mm2 '14'
PRP SizeX_mm '2.5'
PRP SizeY_mm '3'
PRP SizeZ_mm '1.1'
PRP Value '-12V'
PRP Value1 '0.05 ohm'
PRP Value2 '10 nC'
PRP VdsMax_V '-12V'
PRP Vgs_V '-8V'
TOP 0 0.8155782 1.955 180 N 216 0 Q1-1
TOP 1 0.8903813 1.955 180 N 244 1 Q1-2
TOP 2 0.8529798 1.8605118 180 N 284 91 Q1-3
#
# CMP 169
CMP 38 0.9456286 2.2 0 N J6 FH12A-40S-0.5SH(55) ;0=1,1=0.0461
PRP AEC_Qualified 'No'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.hirose.com/en/product/document?clcode=CL0586-0557-8-55&productname=FH12A-40S-0.5SH(55)&series=FH12&documenttype=Catalog&lang=en&documentid=D31648_en'
PRP Conn_Gender 'Female'
PRP Conn_Orientation 'Horizontal'
PRP ContactFinish 'Gold,Nickel'
PRP Current_A '500mA'
PRP DataSheet 'https://www.hirose.com/en/product/document?clcode=CL0586-0557-8-55&productname=FH12A-40S-0.5SH(55)&series=FH12&documenttype=Catalog&lang=en&documentid=D31648_en'
PRP Datasheet_Path 'datasheets/Conn-FH12A-40S-0.5SH(55).pdf'
PRP Digikey_Description 'CONN FFC TOP 40POS 0.50MM R/A'
PRP Digikey_Part_Number 'HFK140CT-ND'
PRP DUT-Pitch_mm '0.5mm'
PRP helpURL 'https://upverter.com/upn/revision/71a45bc64d0f18d2/'
PRP Is_Female 'yes'
PRP Lead_free 'Yes'
PRP Manufacturer 'Hirose'
PRP Mouser_Description 'FFC & FPC Connectors 0.5MM 40 POS R/A TOP SMT GLD'
PRP Mouser_Part_Number '798-FH12A-40S0.5SH55'
PRP Operating_Temperature_Range '-40°C to +85°C'
PRP PackageReference 'FFC40'
PRP Part_Number 'FH12A-40S-0.5SH(55)'
PRP PartNumber 'FH12A-40S-0.5SH(55)'
PRP PinCount '40'
PRP RoHS 'TRUE'
PRP SizeZ_mm '3.6mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'HFK140CT-ND'
PRP Supplier_Part_Number_2 '798-FH12A-40S0.5SH55'
PRP Voltage_V '50V'
TOP 0 0.5617703 2.0533465 180 N 153 14 J6-1
TOP 1 0.5814554 2.0533465 180 N 153 15 J6-2
TOP 2 0.6011404 2.0533465 180 N 153 16 J6-3
TOP 3 0.6208255 2.0533465 180 N 0 89 J6-4
TOP 4 0.6405105 2.0533465 180 N 0 90 J6-5
TOP 5 0.6601955 2.0533465 180 N 0 91 J6-6
TOP 6 0.6798806 2.0533465 180 N 284 187 J6-7
TOP 7 0.6995656 2.0533465 180 N 0 92 J6-8
TOP 8 0.7192506 2.0533465 180 N 0 93 J6-9
TOP 9 0.7389357 2.0533465 180 N 0 94 J6-10
TOP 10 0.7586207 2.0533465 180 N 0 95 J6-11
TOP 11 0.7783058 2.0533465 180 N 0 96 J6-12
TOP 12 0.7979908 2.0533465 180 N 0 97 J6-13
TOP 13 0.8176758 2.0533465 180 N 0 98 J6-14
TOP 14 0.8373609 2.0533465 180 N 0 99 J6-15
TOP 15 0.8570459 2.0533465 180 N 284 188 J6-16
TOP 16 0.876731 2.0533465 180 N 0 100 J6-17
TOP 17 0.896416 2.0533465 180 N 0 101 J6-18
TOP 18 0.916101 2.0533465 180 N 0 102 J6-19
TOP 19 0.9357861 2.0533465 180 N 0 103 J6-20
TOP 20 0.9554711 2.0533465 180 N 0 104 J6-21
TOP 21 0.9751562 2.0533465 180 N 0 105 J6-22
TOP 22 0.9948412 2.0533465 180 N 0 106 J6-23
TOP 23 1.0145262 2.0533465 180 N 0 107 J6-24
TOP 24 1.0342113 2.0533465 180 N 284 189 J6-25
TOP 25 1.0538963 2.0533465 180 N 215 1 J6-26
TOP 26 1.0735814 2.0533465 180 N 216 3 J6-27
TOP 27 1.0932664 2.0533465 180 N 214 1 J6-28
TOP 28 1.1129514 2.0533465 180 N 0 108 J6-29
TOP 29 1.1326365 2.0533465 180 N 222 1 J6-30
TOP 30 1.1523215 2.0533465 180 N 221 0 J6-31
TOP 31 1.1720066 2.0533465 180 N 220 1 J6-32
TOP 32 1.1916916 2.0533465 180 N 219 1 J6-33
TOP 33 1.2113766 2.0533465 180 N 284 190 J6-34
TOP 34 1.2310617 2.0533465 180 N 0 109 J6-35
TOP 35 1.2507467 2.0533465 180 N 230 0 J6-36
TOP 36 1.2704317 2.0533465 180 N 218 1 J6-37
TOP 37 1.2901168 2.0533465 180 N 229 0 J6-38
TOP 38 1.3098018 2.0533465 180 N 217 1 J6-39
TOP 39 1.3294869 2.0533465 180 N 284 191 J6-40
TOP 40 1.40429 2.1812992 180 N 284 192 J6-41
TOP 41 0.4869672 2.1812992 180 N 284 193 J6-42
#
# CMP 170
CMP 43 0.57 0.3625196 0 N J2 DM3BT-DSF-PEJS ;0=1,1=0.0937
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName ''
PRP Color ''
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'https://www.hirose.com/product/en/download_file/key_name/DM3/category/Catalog/doc_file_id/49662/?file_category_id=4&item_id=195&is_series=1'
PRP CompType 'Connector'
PRP ContactFinish 'Gold'
PRP Current_A ''
PRP Gender 'Female'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Hirose Electric Co. Ltd.'
PRP MountType 'SMT'
PRP Note ''
PRP Orientation 'R/A'
PRP PackageReference 'Conncetor, micro SD, 8+2 Pos, R/A, SMT'
PRP PartNumber 'DM3BT-DSF-PEJS'
PRP PinCount '10'
PRP Pitch_mm '1.1'
PRP RoHS 'Y'
PRP Row_Count '1'
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'HR1942CT-ND'
PRP Supplier_Part_Number_2 '35R0580'
PRP Supplier_Part_Number_3 '798-DM3BT-DSF-PEJS'
PRP Voltage_V ''
TOP 0 0.6959843 0.6696063 180 N 429 0 J2-1
TOP 1 0.6526772 0.6696063 180 N 427 0 J2-2
TOP 2 0.6093701 0.6696063 180 N 435 0 J2-3
TOP 3 0.566063 0.6696063 180 N 161 3 J2-4
TOP 4 0.5227559 0.6696063 180 N 437 0 J2-5
TOP 5 0.4794489 0.6696063 180 N 284 199 J2-6
TOP 6 0.4361418 0.6696063 180 N 433 0 J2-7
TOP 7 0.3928347 0.6696063 180 N 431 0 J2-8
TOP 8 0.3219686 0.2601574 180 N 439 0 J2-9
TOP 9 0.3554331 0.6735433 180 N 284 198 J2-10
TOP 10 0.7707874 0.6696063 180 N 284 197 J2-S1
TOP 11 0.3219686 0.5042519 180 N 284 196 J2-S2
TOP 12 0.3219686 0.1184252 180 N 284 195 J2-S3
TOP 13 0.8455907 0.0869291 180 N 284 194 J2-S4
#
# CMP 171
CMP 37 3.6210196 0.485 0 N FB2 BLM18EG121SN1D ;0=1,1=0.0461
PRP AEC_Qualified 'No'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.murata.com/en-us/products/productdata/8796747366430/ENFA0021.pdf'
PRP DataSheet 'https://www.murata.com/en-us/products/productdata/8796747366430/ENFA0021.pdf'
PRP Datasheet_Path 'datasheets/FBead-BLM18EG121SN1D.pdf'
PRP DCR_ohm '60m'
PRP Device_Class_L1 'Passive Components'
PRP Device_Class_L2 'EMI / RFI Components'
PRP Device_Class_L3 'Ferrite Beads and Chips'
PRP Digikey_Description 'FERRITE BEAD 120 OHM 0603 1LN'
PRP Digikey_Part_Number '490-3991-1-ND'
PRP helpURL 'https://upverter.com/upn/revision/3e0d9a214349089d/'
PRP Imax_A '2A'
PRP Impedance_At_Frequency '120O @ 100MHz'
PRP Lead_free 'Yes'
PRP Manufacturer 'Murata'
PRP Material 'Ferrite'
PRP Mouser_Description 'Ferrite Beads 120ohms GHz General Usage'
PRP Mouser_Part_Number '81-BLM18EG121SN1D'
PRP Operating_Temperature_Range '-55°C to +125°C'
PRP PackageReference '0603'
PRP Part_Number 'BLM18EG121SN1D'
PRP PartNumber 'BLM18EG121SN1D'
PRP RoHS 'TRUE'
PRP SizeZ_mm '0.95mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 '490-3991-1-ND'
PRP Supplier_Part_Number_2 '81-BLM18EG121SN1D'
PRP Tolerance__ '25%'
TOP 0 3.6475944 0.485 180 N 166 7 FB2-1
TOP 1 3.5944448 0.485 180 N 167 1 FB2-2
#
# CMP 172
CMP 37 4.0000787 0.5647083 0 N FB1 BLM18EG121SN1D ;0=1,1=0.0461
PRP AEC_Qualified 'No'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.murata.com/en-us/products/productdata/8796747366430/ENFA0021.pdf'
PRP DataSheet 'https://www.murata.com/en-us/products/productdata/8796747366430/ENFA0021.pdf'
PRP Datasheet_Path 'datasheets/FBead-BLM18EG121SN1D.pdf'
PRP DCR_ohm '60m'
PRP Device_Class_L1 'Passive Components'
PRP Device_Class_L2 'EMI / RFI Components'
PRP Device_Class_L3 'Ferrite Beads and Chips'
PRP Digikey_Description 'FERRITE BEAD 120 OHM 0603 1LN'
PRP Digikey_Part_Number '490-3991-1-ND'
PRP helpURL 'https://upverter.com/upn/revision/3e0d9a214349089d/'
PRP Imax_A '2A'
PRP Impedance_At_Frequency '120O @ 100MHz'
PRP Lead_free 'Yes'
PRP Manufacturer 'Murata'
PRP Material 'Ferrite'
PRP Mouser_Description 'Ferrite Beads 120ohms GHz General Usage'
PRP Mouser_Part_Number '81-BLM18EG121SN1D'
PRP Operating_Temperature_Range '-55°C to +125°C'
PRP PackageReference '0603'
PRP Part_Number 'BLM18EG121SN1D'
PRP PartNumber 'BLM18EG121SN1D'
PRP RoHS 'TRUE'
PRP SizeZ_mm '0.95mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 '490-3991-1-ND'
PRP Supplier_Part_Number_2 '81-BLM18EG121SN1D'
PRP Tolerance__ '25%'
TOP 0 4.0266535 0.5647083 180 N 159 36 FB1-1
TOP 1 3.9735039 0.5647083 180 N 165 5 FB1-2
#
# CMP 173
CMP 58 1.1475568 0.6780658 90 N D1 SMBJ6.5CA ;0=1,1=0.1043
PRP AEC_Category 'Q101'
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.littelfuse.com/~/media/Electronics_Technical/Datasheets/TVS_Diodes/Littelfuse_TVS_Diode_SMBJ_Datasheet.pdf'
PRP CompType 'TVS'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Ipp ''
PRP Manufacturer 'Littelfuse'
PRP MountType 'SMT'
PRP PackageReference 'SMB'
PRP PartNumber 'SMBJ6.5CA'
PRP Ppk '600W'
PRP RJA_CperW '100'
PRP RoHS 'Y'
PRP SizeArea_mm2 '21.336'
PRP SizeAreaWB_mm2 '44.156'
PRP SizeX_mm '5.6'
PRP SizeY_mm '3.81'
PRP SizeZ_mm '2.6'
PRP Value '6.5V'
PRP Value1 '600W'
PRP Vbr_Max ''
PRP Vbr_Min ''
PRP Vc ''
PRP VRWM '6.5V'
TOP 0 1.1475568 0.7650737 0 N 284 200 D1-1
TOP 1 1.1475568 0.5910579 0 N 177 2 D1-2
#
# CMP 174
CMP 8 0.2278901 1.3730598 90 N C230 GR442QR73D102KW01L ;0=1,1=0.0799
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '1808'
PRP Cap_F '1nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.murata.com/capacitor/product/GR442QR73D102KW01%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '1808'
PRP PartNumber 'GR442QR73D102KW01L'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '9'
PRP SizeAreaWB_mm2 '16.5'
PRP SizeX_mm '4.5'
PRP SizeY_mm '2'
PRP SizeZ_mm '2.03'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-8145-1-ND'
PRP Supplier_Part_Number_2 '31Y1776'
PRP Supplier_Part_Number_3 '81-GR442QR73D102KW01'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '1000pF'
PRP Value1 'Unknown'
PRP Value2 '2000V'
PRP ValueDisplayed '1000pF'
PRP VDC_V '2kV'
TOP 0 0.2278901 1.4557369 180 N 285 17 C230-1
TOP 1 0.2278901 1.2903826 180 N 42 5 C230-2
#
# CMP 175
CMP 6 0.285 0.9066816 180 N C227 GRM21BZ71E106KE15L ;0=1,1=0.0571
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0805'
PRP Cap_F '10µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM21BZ71E106KE15-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'GRM21BZ71E106KE15L'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GRM21BZ71E106KE5L'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '10uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '10uF'
PRP VDC_V '25V'
TOP 0 0.2450001 0.9066816 0 N 176 4 C227-1
TOP 1 0.3250001 0.9066816 0 N 285 9 C227-2
#
# CMP 176
CMP 1 7.1827969 0.136456 90 N C225 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 7.1827969 0.160078 180 N 284 147 C225-1
TOP 1 7.1827969 0.1128339 180 N 157 27 C225-2
#
# CMP 177
CMP 5 5.6420461 0.0934739 0 N C224 GCM188R71H104KA57D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.murata.com/capacitor/product/GCM188R71H104KA57%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm '20m'
PRP IRMS_A '1.84A'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCM188R71H104KA57D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-4779-1-ND'
PRP Supplier_Part_Number_2 '81-GCM188R71H104KA7D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 '0.02 ohm'
PRP Value2 '50V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '50V'
TOP 0 5.6735422 0.0934739 270 N 157 17 C224-1
TOP 1 5.6105501 0.0934739 270 N 284 49 C224-2
#
# CMP 178
CMP 1 5.4836603 0.1400415 270 N C223 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 5.4836603 0.1164195 0 N 284 146 C223-1
TOP 1 5.4836603 0.1636636 0 N 159 44 C223-2
#
# CMP 179
CMP 5 6.4921654 0.2908213 180 N C220 GCM1885C1H102JA16D ;0=1,1=0.0394
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '1nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://psearch.en.murata.com/capacitor/product/GCM1885C1H102JA16%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Incomplete'
PRP IRMS_A ''
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCM1885C1H102JA16D'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'C0G/NP0'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '1000pF'
PRP Value1 ''
PRP Value2 '50V'
PRP ValueDisplayed '1000pF'
PRP VDC_V '50V'
TOP 0 6.4606693 0.2908213 90 N 347 0 C220-1
TOP 1 6.5236614 0.2908213 90 N 284 150 C220-2
#
# CMP 180
CMP 5 6 0.4800002 270 N C219 GCM1885C1H102JA16D ;0=1,1=0.0394
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '1nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://psearch.en.murata.com/capacitor/product/GCM1885C1H102JA16%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Incomplete'
PRP IRMS_A ''
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCM1885C1H102JA16D'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'C0G/NP0'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '1000pF'
PRP Value1 ''
PRP Value2 '50V'
PRP ValueDisplayed '1000pF'
PRP VDC_V '50V'
TOP 0 6 0.4485041 0 N 344 0 C219-1
TOP 1 6 0.5114962 0 N 284 89 C219-2
#
# CMP 181
CMP 5 6.124176 0.48 270 N C218 GRM1885C1H101JA01D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '100pF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM1885C1H101JA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GRM1885C1H101JA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '490-1427-1-ND'
PRP Supplier_Part_Number_2 '81-GRM39C101J50'
PRP Supplier_Part_Number_3 '8819866'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'C0G/NP0'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '100pF'
PRP Value1 'Unknown'
PRP Value2 '50V'
PRP ValueDisplayed '100pF'
PRP VDC_V '50V'
TOP 0 6.124176 0.4485039 0 N 345 0 C218-1
TOP 1 6.124176 0.511496 0 N 284 88 C218-2
#
# CMP 182
CMP 5 6.1991755 0.4799995 270 N C217 GCM1885C1H102JA16D ;0=1,1=0.0394
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '1nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://psearch.en.murata.com/capacitor/product/GCM1885C1H102JA16%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Incomplete'
PRP IRMS_A ''
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCM1885C1H102JA16D'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'C0G/NP0'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '1000pF'
PRP Value1 ''
PRP Value2 '50V'
PRP ValueDisplayed '1000pF'
PRP VDC_V '50V'
TOP 0 6.1991755 0.4485034 0 N 346 0 C217-1
TOP 1 6.1991755 0.5114955 0 N 284 87 C217-2
#
# CMP 183
CMP 5 6 0.2300002 270 N C216 GCM1885C1H102JA16D ;0=1,1=0.0394
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '1nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://psearch.en.murata.com/capacitor/product/GCM1885C1H102JA16%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Incomplete'
PRP IRMS_A ''
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCM1885C1H102JA16D'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'C0G/NP0'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '1000pF'
PRP Value1 ''
PRP Value2 '50V'
PRP ValueDisplayed '1000pF'
PRP VDC_V '50V'
TOP 0 6 0.1985041 0 N 348 1 C216-1
TOP 1 6 0.2614962 0 N 284 85 C216-2
#
# CMP 184
CMP 5 6.124176 0.23 270 N C215 GRM1885C1H101JA01D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '100pF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM1885C1H101JA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GRM1885C1H101JA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '490-1427-1-ND'
PRP Supplier_Part_Number_2 '81-GRM39C101J50'
PRP Supplier_Part_Number_3 '8819866'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'C0G/NP0'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '100pF'
PRP Value1 'Unknown'
PRP Value2 '50V'
PRP ValueDisplayed '100pF'
PRP VDC_V '50V'
TOP 0 6.124176 0.1985039 0 N 349 0 C215-1
TOP 1 6.124176 0.261496 0 N 284 83 C215-2
#
# CMP 185
CMP 5 6.1991755 0.2299995 270 N C214 GCM1885C1H102JA16D ;0=1,1=0.0394
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '1nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://psearch.en.murata.com/capacitor/product/GCM1885C1H102JA16%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Incomplete'
PRP IRMS_A ''
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCM1885C1H102JA16D'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'C0G/NP0'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '1000pF'
PRP Value1 ''
PRP Value2 '50V'
PRP ValueDisplayed '1000pF'
PRP VDC_V '50V'
TOP 0 6.1991755 0.1985034 0 N 350 0 C214-1
TOP 1 6.1991755 0.2614955 0 N 284 84 C214-2
#
# CMP 186
CMP 5 3.89 2.005 90 N C213 GCM188R71H104KA57D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.murata.com/capacitor/product/GCM188R71H104KA57%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm '20m'
PRP IRMS_A '1.84A'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCM188R71H104KA57D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-4779-1-ND'
PRP Supplier_Part_Number_2 '81-GCM188R71H104KA7D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 '0.02 ohm'
PRP Value2 '50V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '50V'
TOP 0 3.89 2.0364961 180 N 159 40 C213-1
TOP 1 3.89 1.973504 180 N 284 140 C213-2
#
# CMP 187
CMP 5 5.88 0.48 270 N C212 GCM188R71H104KA57D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.murata.com/capacitor/product/GCM188R71H104KA57%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm '20m'
PRP IRMS_A '1.84A'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCM188R71H104KA57D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-4779-1-ND'
PRP Supplier_Part_Number_2 '81-GCM188R71H104KA7D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 '0.02 ohm'
PRP Value2 '50V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '50V'
TOP 0 5.88 0.4485039 0 N 157 25 C212-1
TOP 1 5.88 0.511496 0 N 284 90 C212-2
#
# CMP 188
CMP 5 5.88 0.23 270 N C211 GCM188R71H104KA57D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.murata.com/capacitor/product/GCM188R71H104KA57%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm '20m'
PRP IRMS_A '1.84A'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCM188R71H104KA57D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-4779-1-ND'
PRP Supplier_Part_Number_2 '81-GCM188R71H104KA7D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 '0.02 ohm'
PRP Value2 '50V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '50V'
TOP 0 5.88 0.1985039 0 N 157 21 C211-1
TOP 1 5.88 0.261496 0 N 284 86 C211-2
#
# CMP 189
CMP 1 6.67 1.4449999 90 N C208 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 6.67 1.4686219 180 N 159 13 C208-1
TOP 1 6.67 1.4213778 180 N 284 81 C208-2
#
# CMP 190
CMP 1 6.355514 1.6319651 0 N C206 GRM155R70J103KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '10nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J103KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J103KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J103KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J103KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.01uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.01uF'
PRP VDC_V '6.3V'
TOP 0 6.379136 1.6319651 270 N 159 20 C206-1
TOP 1 6.3318919 1.6319651 270 N 284 96 C206-2
#
# CMP 191
CMP 5 6.3513577 1.5712446 0 N C205 GRM188Z71A106MA73D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '10µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GRM188Z71A106MA73%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GRM188Z71A106MA73D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GRM188Z71A106MA3D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '10uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '10uF'
PRP VDC_V '10V'
TOP 0 6.3828538 1.5712446 270 N 159 19 C205-1
TOP 1 6.3198617 1.5712446 270 N 284 95 C205-2
#
# CMP 192
CMP 1 6.870214 1.7389369 180 N C204 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 6.846592 1.7389369 90 N 171 1 C204-1
TOP 1 6.8938361 1.7389369 90 N 284 77 C204-2
#
# CMP 193
CMP 1 6.870214 1.6208269 180 N C202 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 6.846592 1.6208269 90 N 171 2 C202-1
TOP 1 6.8938361 1.6208269 90 N 284 78 C202-2
#
# CMP 194
CMP 1 6.870214 1.6798819 180 N C198 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 6.846592 1.6798819 90 N 172 3 C198-1
TOP 1 6.8938361 1.6798819 90 N 284 76 C198-2
#
# CMP 195
CMP 1 6.556277 1.8950779 270 N C194 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 6.556277 1.8714559 0 N 172 2 C194-1
TOP 1 6.556277 1.9187 0 N 284 71 C194-2
#
# CMP 196
CMP 1 6.648622 1.3699999 180 N C190 GRM1555C1E120JA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '12pF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM1555C1E120JA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM1555C1E120JA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GRM1555C1E120JA1D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'C0G/NP0'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '12pF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '12pF'
PRP VDC_V '25V'
TOP 0 6.625 1.3699999 90 N 287 0 C190-1
TOP 1 6.6722441 1.3699999 90 N 284 74 C190-2
#
# CMP 197
CMP 1 6.541378 1.3699999 0 N C189 GRM1555C1E120JA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '12pF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM1555C1E120JA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM1555C1E120JA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GRM1555C1E120JA1D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'C0G/NP0'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '12pF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '12pF'
PRP VDC_V '25V'
TOP 0 6.565 1.3699999 270 N 288 0 C189-1
TOP 1 6.5177559 1.3699999 270 N 284 75 C189-2
#
# CMP 198
CMP 7 2.6940041 1.5993005 270 N C179 GRM32ER7YA106KA12K ;0=1,1=0.1063
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '1210'
PRP Cap_F '10µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM32ER7YA106KA12-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm '1m'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A '6A'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '1210'
PRP PartNumber 'GRM32ER7YA106KA12K'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '8'
PRP SizeAreaWB_mm2 '14.7'
PRP SizeX_mm '3.2'
PRP SizeY_mm '2.5'
PRP SizeZ_mm '2.7'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM32ER7YA106KA12K-ND'
PRP Supplier_Part_Number_2 '81-GRM32ER7YA106KA2K'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '10uF'
PRP Value1 '0.001 ohm'
PRP Value2 '35V'
PRP ValueDisplayed '10µF'
PRP VDC_V '35V'
TOP 0 2.6940041 1.5422139 0 N 157 15 C179-1
TOP 1 2.6940041 1.6563871 0 N 284 45 C179-2
#
# CMP 199
CMP 1 5.8542457 1.5476225 270 N C178 GRM155R72A272KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '2.7nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R72A272KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R72A272KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R72A272KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R72A272KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '2700pF'
PRP Value1 'Unknown'
PRP Value2 '100V'
PRP ValueDisplayed '2700pF'
PRP VDC_V '100V'
TOP 0 5.8542457 1.5240005 0 N 192 0 C178-1
TOP 1 5.8542457 1.5712446 0 N 284 44 C178-2
#
# CMP 200
CMP 5 5.6641276 1.6462942 270 N C172 GRM188Z71C475KE21D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '4.7µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM188Z71C475KE21-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-06-05'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GRM188Z71C475KE21D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '4.7uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '4.7uF'
PRP VDC_V '16V'
TOP 0 5.6641276 1.6147981 0 N 157 13 C172-1
TOP 1 5.6641276 1.6777902 0 N 284 43 C172-2
#
# CMP 201
CMP 7 2.8220901 1.7593005 0 N C171 GRM32ER71A476ME15L ;0=1,1=0.1063
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '1210'
PRP Cap_F '47µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM32ER71A476ME15-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '1210'
PRP PartNumber 'GRM32ER71A476ME15L'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '8'
PRP SizeAreaWB_mm2 '14.7'
PRP SizeX_mm '3.2'
PRP SizeY_mm '2.5'
PRP SizeZ_mm '2.7'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '490-6543-1-ND'
PRP Supplier_Part_Number_2 '81-GRM32ER71A476ME5L'
PRP Supplier_Part_Number_3 '2362130'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '47uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '47uF'
PRP VDC_V '10V'
TOP 0 2.8791767 1.7593005 270 N 159 9 C171-1
TOP 1 2.7650035 1.7593005 270 N 284 46 C171-2
#
# CMP 202
CMP 7 2.3323308 0.9666816 270 N C168 GRM32ER7YA106KA12K ;0=1,1=0.1063
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '1210'
PRP Cap_F '10µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM32ER7YA106KA12-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm '1m'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A '6A'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '1210'
PRP PartNumber 'GRM32ER7YA106KA12K'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '8'
PRP SizeAreaWB_mm2 '14.7'
PRP SizeX_mm '3.2'
PRP SizeY_mm '2.5'
PRP SizeZ_mm '2.7'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM32ER7YA106KA12K-ND'
PRP Supplier_Part_Number_2 '81-GRM32ER7YA106KA2K'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '10uF'
PRP Value1 '0.001 ohm'
PRP Value2 '35V'
PRP ValueDisplayed '10µF'
PRP VDC_V '35V'
TOP 0 2.3323308 0.909595 0 N 157 11 C168-1
TOP 1 2.3323308 1.0237682 0 N 284 42 C168-2
#
# CMP 203
CMP 1 5.8542455 1.1284338 270 N C166 GRM155R72A272KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '2.7nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R72A272KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R72A272KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R72A272KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R72A272KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '2700pF'
PRP Value1 'Unknown'
PRP Value2 '100V'
PRP ValueDisplayed '2700pF'
PRP VDC_V '100V'
TOP 0 5.8542455 1.1048118 0 N 197 0 C166-1
TOP 1 5.8542455 1.1520559 0 N 284 47 C166-2
#
# CMP 204
CMP 5 5.6640615 1.2271048 270 N C161 GRM188Z71C475KE21D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '4.7µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM188Z71C475KE21-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-06-05'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GRM188Z71C475KE21D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '4.7uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '4.7uF'
PRP VDC_V '16V'
TOP 0 5.6640615 1.1956087 0 N 157 16 C161-1
TOP 1 5.6640615 1.2586008 0 N 284 48 C161-2
#
# CMP 205
CMP 7 2.4604174 1.1266816 0 N C159 GRM32ER71A476ME15L ;0=1,1=0.1063
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '1210'
PRP Cap_F '47µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM32ER71A476ME15-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '1210'
PRP PartNumber 'GRM32ER71A476ME15L'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '8'
PRP SizeAreaWB_mm2 '14.7'
PRP SizeX_mm '3.2'
PRP SizeY_mm '2.5'
PRP SizeZ_mm '2.7'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '490-6543-1-ND'
PRP Supplier_Part_Number_2 '81-GRM32ER71A476ME5L'
PRP Supplier_Part_Number_3 '2362130'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '47uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '47uF'
PRP VDC_V '10V'
TOP 0 2.517504 1.1266816 270 N 175 5 C159-1
TOP 1 2.4033308 1.1266817 270 N 284 41 C159-2
#
# CMP 206
CMP 1 6.67 0.495 90 N C131 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 6.67 0.518622 180 N 159 11 C131-1
TOP 1 6.67 0.4713779 180 N 284 55 C131-2
#
# CMP 207
CMP 1 6.355514 0.6819651 0 N C129 GRM155R70J103KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '10nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J103KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J103KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J103KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J103KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.01uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.01uF'
PRP VDC_V '6.3V'
TOP 0 6.379136 0.6819651 270 N 159 17 C129-1
TOP 1 6.3318919 0.6819651 270 N 284 93 C129-2
#
# CMP 208
CMP 5 6.3513577 0.6212443 0 N C128 GRM188Z71A106MA73D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '10µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GRM188Z71A106MA73%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GRM188Z71A106MA73D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GRM188Z71A106MA3D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '10uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '10uF'
PRP VDC_V '10V'
TOP 0 6.3828538 0.6212443 270 N 159 18 C128-1
TOP 1 6.3198617 0.6212443 270 N 284 94 C128-2
#
# CMP 209
CMP 1 6.870214 0.7889371 180 N C127 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 6.846592 0.7889371 90 N 173 4 C127-1
TOP 1 6.8938361 0.7889371 90 N 284 54 C127-2
#
# CMP 210
CMP 1 6.870214 0.6708269 180 N C125 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 6.846592 0.6708269 90 N 173 3 C125-1
TOP 1 6.8938361 0.6708269 90 N 284 53 C125-2
#
# CMP 211
CMP 1 6.870214 0.729882 180 N C121 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 6.846592 0.729882 90 N 174 6 C121-1
TOP 1 6.8938361 0.729882 90 N 284 52 C121-2
#
# CMP 212
CMP 1 6.5562769 0.945078 270 N C117 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 6.5562769 0.921456 0 N 174 5 C117-1
TOP 1 6.5562769 0.9687001 0 N 284 51 C117-2
#
# CMP 213
CMP 1 6.72801 0.4891201 270 N C113 GRM1555C1E120JA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '12pF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM1555C1E120JA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM1555C1E120JA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GRM1555C1E120JA1D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'C0G/NP0'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '12pF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '12pF'
PRP VDC_V '25V'
TOP 0 6.72801 0.4654981 0 N 305 1 C113-1
TOP 1 6.72801 0.5127422 0 N 284 56 C113-2
#
# CMP 214
CMP 1 6.72801 0.3818761 90 N C112 GRM1555C1E120JA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '12pF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM1555C1E120JA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM1555C1E120JA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GRM1555C1E120JA1D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'C0G/NP0'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '12pF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '12pF'
PRP VDC_V '25V'
TOP 0 6.72801 0.4054981 180 N 306 1 C112-1
TOP 1 6.72801 0.358254 180 N 284 57 C112-2
#
# CMP 215
CMP 7 1.755653 0.835 270 N C107 GRM32ER7YA106KA12K ;0=1,1=0.1063
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '1210'
PRP Cap_F '10µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM32ER7YA106KA12-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm '1m'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A '6A'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '1210'
PRP PartNumber 'GRM32ER7YA106KA12K'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '8'
PRP SizeAreaWB_mm2 '14.7'
PRP SizeX_mm '3.2'
PRP SizeY_mm '2.5'
PRP SizeZ_mm '2.7'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM32ER7YA106KA12K-ND'
PRP Supplier_Part_Number_2 '81-GRM32ER7YA106KA2K'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '10uF'
PRP Value1 '0.001 ohm'
PRP Value2 '35V'
PRP ValueDisplayed '10µF'
PRP VDC_V '35V'
TOP 0 1.755653 0.7779134 0 N 157 26 C107-1
TOP 1 1.755653 0.8920866 0 N 284 119 C107-2
#
# CMP 216
CMP 7 1.55 0.835 270 N C105 GRM32ER7YA106KA12K ;0=1,1=0.1063
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '1210'
PRP Cap_F '10µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM32ER7YA106KA12-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm '1m'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A '6A'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '1210'
PRP PartNumber 'GRM32ER7YA106KA12K'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '8'
PRP SizeAreaWB_mm2 '14.7'
PRP SizeX_mm '3.2'
PRP SizeY_mm '2.5'
PRP SizeZ_mm '2.7'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM32ER7YA106KA12K-ND'
PRP Supplier_Part_Number_2 '81-GRM32ER7YA106KA2K'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '10uF'
PRP Value1 '0.001 ohm'
PRP Value2 '35V'
PRP ValueDisplayed '10µF'
PRP VDC_V '35V'
TOP 0 1.55 0.7779134 0 N 152 4 C105-1
TOP 1 1.55 0.8920866 0 N 284 118 C105-2
#
# CMP 217
CMP 1 4.735 1.1520559 180 N C100 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 4.711378 1.1520559 90 N 284 145 C100-1
TOP 1 4.7586221 1.1520559 90 N 159 43 C100-2
#
# CMP 218
CMP 1 3.595 0.594909 90 N C90 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 3.595 0.618531 180 N 351 0 C90-1
TOP 1 3.595 0.5712869 180 N 284 120 C90-2
#
# CMP 219
CMP 5 3.015 0.66 270 N C89 GRM188Z71A475ME15D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '4.7µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM188Z71A475ME15-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GRM188Z71A475ME15D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 '81-GRM188Z71A475ME5D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '4.7uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '4.7uF'
PRP VDC_V '10V'
TOP 0 3.015 0.6285039 0 N 351 1 C89-1
TOP 1 3.015 0.691496 0 N 284 149 C89-2
#
# CMP 220
CMP 1 3.9486221 0.7899363 0 N C80 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 3.9722441 0.7899363 270 N 564 1 C80-1
TOP 1 3.925 0.7899363 270 N 563 1 C80-2
#
# CMP 221
CMP 1 3.8448104 0.7899363 180 N C79 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 3.8211884 0.7899363 90 N 564 0 C79-1
TOP 1 3.8684325 0.7899363 90 N 563 0 C79-2
#
# CMP 222
CMP 1 3.7203614 0.7899363 180 N C78 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 3.6967394 0.7899363 90 N 24 0 C78-1
TOP 1 3.7439835 0.7899363 90 N 23 0 C78-2
#
# CMP 223
CMP 1 0.5877952 0.7854326 0 N C71 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 0.6114172 0.7854326 270 N 284 144 C71-1
TOP 1 0.5641731 0.7854326 270 N 161 2 C71-2
#
# CMP 224
CMP 1 2.1493875 1.5 0 N C70 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 2.1730095 1.5 270 N 284 143 C70-1
TOP 1 2.1257654 1.5 270 N 159 42 C70-2
#
# CMP 225
CMP 1 3.7136911 0.0819746 270 N C62 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 3.7136911 0.0583526 0 N 284 142 C62-1
TOP 1 3.7136911 0.1055967 0 N 159 41 C62-2
#
# CMP 226
CMP 1 3.6536912 0.0819746 270 N C61 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 3.6536912 0.0583526 0 N 284 141 C61-1
TOP 1 3.6536912 0.1055967 0 N 153 12 C61-2
#
# CMP 227
CMP 0 3.673 1.0043754 270 N C56 GRM033Z71C104KE14D ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0201'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033Z71C104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-06-05'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'GRM033Z71C104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.18'
PRP SizeAreaWB_mm2 '2.08'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GRM033Z71C104KE4D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '16V'
TOP 0 3.673 0.9913833 0 N 175 32 C56-1
TOP 1 3.673 1.0173675 0 N 284 201 C56-2
#
# CMP 228
CMP 0 3.99 1.1150787 0 N C55 GRM033Z71C104KE14D ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0201'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033Z71C104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-06-05'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'GRM033Z71C104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.18'
PRP SizeAreaWB_mm2 '2.08'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GRM033Z71C104KE4D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '16V'
TOP 0 4.0029921 1.1150787 270 N 175 15 C55-1
TOP 1 3.9770079 1.1150787 270 N 284 139 C55-2
#
# CMP 229
CMP 0 3.6547796 1.1151039 270 N C54 GRM033Z71C104KE14D ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0201'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033Z71C104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-06-05'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'GRM033Z71C104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.18'
PRP SizeAreaWB_mm2 '2.08'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GRM033Z71C104KE4D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '16V'
TOP 0 3.6547796 1.1021118 0 N 175 14 C54-1
TOP 1 3.6547796 1.128096 0 N 284 138 C54-2
#
# CMP 230
CMP 5 3.21 1.3647586 270 N C53 C1608X7S1A335K080AC ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '3.3µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=C1608X7S1A335K080AC'
PRP CompType 'Capacitor'
PRP ESR_ohm '4.796m'
PRP IRMS_A '2.3752A'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'C1608X7S1A335K080AC'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '445-14256-1-ND'
PRP Supplier_Part_Number_2 '52X3755'
PRP Supplier_Part_Number_3 '810-C1608X7S1A335K0C'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7S'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '3.3uF'
PRP Value1 '0.004796 ohm'
PRP Value2 '10V'
PRP ValueDisplayed '3.3uF'
PRP VDC_V '10V'
TOP 0 3.21 1.3332625 0 N 175 9 C53-1
TOP 1 3.21 1.3962546 0 N 284 133 C53-2
#
# CMP 231
CMP 5 3.295 1.1266065 270 N C52 C1608X7S1A335K080AC ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '3.3µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=C1608X7S1A335K080AC'
PRP CompType 'Capacitor'
PRP ESR_ohm '4.796m'
PRP IRMS_A '2.3752A'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'C1608X7S1A335K080AC'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '445-14256-1-ND'
PRP Supplier_Part_Number_2 '52X3755'
PRP Supplier_Part_Number_3 '810-C1608X7S1A335K0C'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7S'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '3.3uF'
PRP Value1 '0.004796 ohm'
PRP Value2 '10V'
PRP ValueDisplayed '3.3uF'
PRP VDC_V '10V'
TOP 0 3.295 1.0951104 0 N 175 10 C52-1
TOP 1 3.295 1.1581025 0 N 284 134 C52-2
#
# CMP 232
CMP 0 3.8929628 1.2573709 180 N C51 GRM033Z71C104KE14D ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0201'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033Z71C104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-06-05'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'GRM033Z71C104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.18'
PRP SizeAreaWB_mm2 '2.08'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GRM033Z71C104KE4D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '16V'
TOP 0 3.8799707 1.2573709 90 N 175 13 C51-1
TOP 1 3.9059549 1.2573709 90 N 284 137 C51-2
#
# CMP 233
CMP 0 3.8148496 0.9461023 270 N C50 GRM033Z71C104KE14D ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0201'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033Z71C104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-06-05'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'GRM033Z71C104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.18'
PRP SizeAreaWB_mm2 '2.08'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GRM033Z71C104KE4D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '16V'
TOP 0 3.8148496 0.9331102 0 N 175 12 C50-1
TOP 1 3.8148496 0.9590944 0 N 284 136 C50-2
#
# CMP 234
CMP 0 3.4458408 1.3522891 270 N C49 GRM033Z71C104KE14D ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0201'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033Z71C104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-06-05'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'GRM033Z71C104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.18'
PRP SizeAreaWB_mm2 '2.08'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GRM033Z71C104KE4D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '16V'
TOP 0 3.4458408 1.339297 0 N 175 11 C49-1
TOP 1 3.4458408 1.3652812 0 N 284 135 C49-2
#
# CMP 235
CMP 39 3.9565821 1.0608955 270 N C47 GRM033C80J105ME05D ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.murata.com/en-us/products/productdetail?partno=GRM033C80J105ME05%23'
PRP DataSheet 'https://www.murata.com/en-us/products/productdetail?partno=GRM033C80J105ME05%23'
PRP Datasheet_Path 'datasheets/Cap-GRM033C80J105ME05D.pdf'
PRP helpURL 'https://upverter.com/upn/revision/64a3db239e8cbfc8/'
PRP Lead_free 'Yes'
PRP Manufacturer 'Murata'
PRP Operating_Temperature_Range '-55°C to +105°C'
PRP PackageReference '0201'
PRP Part_Number 'GRM033C80J105ME05D'
PRP PartNumber 'GRM033C80J105ME05D'
PRP RoHS 'TRUE'
PRP SizeZ_mm '0.39mm'
PRP TempCo '22%'
PRP Temperature_Characteristic 'X6S'
PRP Tolerance__ '20%'
PRP Value '1µF'
PRP ValueDisplayed '1.0uF'
PRP VDC_V '6.3V'
TOP 0 3.9565821 1.0497735 270 N 284 165 C47-1
TOP 1 3.9565821 1.0720175 270 N 175 30 C47-2
#
# CMP 236
CMP 39 3.693174 1.1151039 90 N C46 GRM033C80J105ME05D ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.murata.com/en-us/products/productdetail?partno=GRM033C80J105ME05%23'
PRP DataSheet 'https://www.murata.com/en-us/products/productdetail?partno=GRM033C80J105ME05%23'
PRP Datasheet_Path 'datasheets/Cap-GRM033C80J105ME05D.pdf'
PRP helpURL 'https://upverter.com/upn/revision/64a3db239e8cbfc8/'
PRP Lead_free 'Yes'
PRP Manufacturer 'Murata'
PRP Operating_Temperature_Range '-55°C to +105°C'
PRP PackageReference '0201'
PRP Part_Number 'GRM033C80J105ME05D'
PRP PartNumber 'GRM033C80J105ME05D'
PRP RoHS 'TRUE'
PRP SizeZ_mm '0.39mm'
PRP TempCo '22%'
PRP Temperature_Characteristic 'X6S'
PRP Tolerance__ '20%'
PRP Value '1µF'
PRP ValueDisplayed '1.0uF'
PRP VDC_V '6.3V'
TOP 0 3.693174 1.1262259 90 N 284 164 C46-1
TOP 1 3.693174 1.1039819 90 N 175 29 C46-2
#
# CMP 237
CMP 39 3.3958409 0.9945607 270 N C45 GRM033C80J105ME05D ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.murata.com/en-us/products/productdetail?partno=GRM033C80J105ME05%23'
PRP DataSheet 'https://www.murata.com/en-us/products/productdetail?partno=GRM033C80J105ME05%23'
PRP Datasheet_Path 'datasheets/Cap-GRM033C80J105ME05D.pdf'
PRP helpURL 'https://upverter.com/upn/revision/64a3db239e8cbfc8/'
PRP Lead_free 'Yes'
PRP Manufacturer 'Murata'
PRP Operating_Temperature_Range '-55°C to +105°C'
PRP PackageReference '0201'
PRP Part_Number 'GRM033C80J105ME05D'
PRP PartNumber 'GRM033C80J105ME05D'
PRP RoHS 'TRUE'
PRP SizeZ_mm '0.39mm'
PRP TempCo '22%'
PRP Temperature_Characteristic 'X6S'
PRP Tolerance__ '20%'
PRP Value '1µF'
PRP ValueDisplayed '1.0uF'
PRP VDC_V '6.3V'
TOP 0 3.3958409 0.9834387 270 N 284 163 C45-1
TOP 1 3.3958409 1.0056827 270 N 175 28 C45-2
#
# CMP 238
CMP 39 3.3958412 1.2340552 270 N C44 GRM033C80J105ME05D ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.murata.com/en-us/products/productdetail?partno=GRM033C80J105ME05%23'
PRP DataSheet 'https://www.murata.com/en-us/products/productdetail?partno=GRM033C80J105ME05%23'
PRP Datasheet_Path 'datasheets/Cap-GRM033C80J105ME05D.pdf'
PRP helpURL 'https://upverter.com/upn/revision/64a3db239e8cbfc8/'
PRP Lead_free 'Yes'
PRP Manufacturer 'Murata'
PRP Operating_Temperature_Range '-55°C to +105°C'
PRP PackageReference '0201'
PRP Part_Number 'GRM033C80J105ME05D'
PRP PartNumber 'GRM033C80J105ME05D'
PRP RoHS 'TRUE'
PRP SizeZ_mm '0.39mm'
PRP TempCo '22%'
PRP Temperature_Characteristic 'X6S'
PRP Tolerance__ '20%'
PRP Value '1µF'
PRP ValueDisplayed '1.0uF'
PRP VDC_V '6.3V'
TOP 0 3.3958412 1.2229332 270 N 284 162 C44-1
TOP 1 3.3958412 1.2451772 270 N 175 27 C44-2
#
# CMP 239
CMP 39 3.3482444 1.3522891 90 N C42 GRM033C80J105ME05D ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.murata.com/en-us/products/productdetail?partno=GRM033C80J105ME05%23'
PRP DataSheet 'https://www.murata.com/en-us/products/productdetail?partno=GRM033C80J105ME05%23'
PRP Datasheet_Path 'datasheets/Cap-GRM033C80J105ME05D.pdf'
PRP helpURL 'https://upverter.com/upn/revision/64a3db239e8cbfc8/'
PRP Lead_free 'Yes'
PRP Manufacturer 'Murata'
PRP Operating_Temperature_Range '-55°C to +105°C'
PRP PackageReference '0201'
PRP Part_Number 'GRM033C80J105ME05D'
PRP PartNumber 'GRM033C80J105ME05D'
PRP RoHS 'TRUE'
PRP SizeZ_mm '0.39mm'
PRP TempCo '22%'
PRP Temperature_Characteristic 'X6S'
PRP Tolerance__ '20%'
PRP Value '1µF'
PRP ValueDisplayed '1.0uF'
PRP VDC_V '6.3V'
TOP 0 3.3482444 1.3634111 90 N 284 161 C42-1
TOP 1 3.3482444 1.3411671 90 N 175 26 C42-2
#
# CMP 240
CMP 39 3.673 1.1930667 270 N C41 GRM033C80J105ME05D ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.murata.com/en-us/products/productdetail?partno=GRM033C80J105ME05%23'
PRP DataSheet 'https://www.murata.com/en-us/products/productdetail?partno=GRM033C80J105ME05%23'
PRP Datasheet_Path 'datasheets/Cap-GRM033C80J105ME05D.pdf'
PRP helpURL 'https://upverter.com/upn/revision/64a3db239e8cbfc8/'
PRP Lead_free 'Yes'
PRP Manufacturer 'Murata'
PRP Operating_Temperature_Range '-55°C to +105°C'
PRP PackageReference '0201'
PRP Part_Number 'GRM033C80J105ME05D'
PRP PartNumber 'GRM033C80J105ME05D'
PRP RoHS 'TRUE'
PRP SizeZ_mm '0.39mm'
PRP TempCo '22%'
PRP Temperature_Characteristic 'X6S'
PRP Tolerance__ '20%'
PRP Value '1µF'
PRP ValueDisplayed '1.0uF'
PRP VDC_V '6.3V'
TOP 0 3.673 1.1819447 270 N 284 160 C41-1
TOP 1 3.673 1.2041887 270 N 175 25 C41-2
#
# CMP 241
CMP 39 3.3958412 1.1089091 90 N C40 GRM033C80J105ME05D ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.murata.com/en-us/products/productdetail?partno=GRM033C80J105ME05%23'
PRP DataSheet 'https://www.murata.com/en-us/products/productdetail?partno=GRM033C80J105ME05%23'
PRP Datasheet_Path 'datasheets/Cap-GRM033C80J105ME05D.pdf'
PRP helpURL 'https://upverter.com/upn/revision/64a3db239e8cbfc8/'
PRP Lead_free 'Yes'
PRP Manufacturer 'Murata'
PRP Operating_Temperature_Range '-55°C to +105°C'
PRP PackageReference '0201'
PRP Part_Number 'GRM033C80J105ME05D'
PRP PartNumber 'GRM033C80J105ME05D'
PRP RoHS 'TRUE'
PRP SizeZ_mm '0.39mm'
PRP TempCo '22%'
PRP Temperature_Characteristic 'X6S'
PRP Tolerance__ '20%'
PRP Value '1µF'
PRP ValueDisplayed '1.0uF'
PRP VDC_V '6.3V'
TOP 0 3.3958412 1.1200311 90 N 284 159 C40-1
TOP 1 3.3958412 1.0977871 90 N 175 24 C40-2
#
# CMP 242
CMP 39 3.9565821 0.973 270 N C39 GRM033C80J105ME05D ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.murata.com/en-us/products/productdetail?partno=GRM033C80J105ME05%23'
PRP DataSheet 'https://www.murata.com/en-us/products/productdetail?partno=GRM033C80J105ME05%23'
PRP Datasheet_Path 'datasheets/Cap-GRM033C80J105ME05D.pdf'
PRP helpURL 'https://upverter.com/upn/revision/64a3db239e8cbfc8/'
PRP Lead_free 'Yes'
PRP Manufacturer 'Murata'
PRP Operating_Temperature_Range '-55°C to +105°C'
PRP PackageReference '0201'
PRP Part_Number 'GRM033C80J105ME05D'
PRP PartNumber 'GRM033C80J105ME05D'
PRP RoHS 'TRUE'
PRP SizeZ_mm '0.39mm'
PRP TempCo '22%'
PRP Temperature_Characteristic 'X6S'
PRP Tolerance__ '20%'
PRP Value '1µF'
PRP ValueDisplayed '1.0uF'
PRP VDC_V '6.3V'
TOP 0 3.9565821 0.961878 270 N 284 158 C39-1
TOP 1 3.9565821 0.984122 270 N 175 23 C39-2
#
# CMP 243
CMP 1 3.531385 0.5096456 270 N C38 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 3.531385 0.4860236 0 N 167 2 C38-1
TOP 1 3.531385 0.5332677 0 N 284 132 C38-2
#
# CMP 244
CMP 1 3.7396119 0.4929997 180 N C37 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 3.7159899 0.4929997 90 N 166 5 C37-1
TOP 1 3.763234 0.4929997 90 N 284 130 C37-2
#
# CMP 245
CMP 1 3.7363779 0.7089685 180 N C36 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 3.7127559 0.7089685 90 N 166 2 C36-1
TOP 1 3.76 0.7089685 90 N 284 127 C36-2
#
# CMP 246
CMP 1 4.139437 0.7171307 90 N C35 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 4.139437 0.7407527 180 N 166 4 C35-1
TOP 1 4.139437 0.6935086 180 N 284 129 C35-2
#
# CMP 247
CMP 1 3.7363779 0.6589683 180 N C34 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 3.7127559 0.6589683 90 N 166 3 C34-1
TOP 1 3.76 0.6589683 90 N 284 128 C34-2
#
# CMP 248
CMP 5 3.7388819 0.5690823 180 N C33 GRM188Z71A475ME15D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '4.7µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM188Z71A475ME15-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GRM188Z71A475ME15D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 '81-GRM188Z71A475ME5D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '4.7uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '4.7uF'
PRP VDC_V '10V'
TOP 0 3.7073858 0.5690823 90 N 166 6 C33-1
TOP 1 3.7703779 0.5690823 90 N 284 131 C33-2
#
# CMP 249
CMP 39 3.4458408 1.2343185 270 N C32 GRM033C80J105ME05D ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.murata.com/en-us/products/productdetail?partno=GRM033C80J105ME05%23'
PRP DataSheet 'https://www.murata.com/en-us/products/productdetail?partno=GRM033C80J105ME05%23'
PRP Datasheet_Path 'datasheets/Cap-GRM033C80J105ME05D.pdf'
PRP helpURL 'https://upverter.com/upn/revision/64a3db239e8cbfc8/'
PRP Lead_free 'Yes'
PRP Manufacturer 'Murata'
PRP Operating_Temperature_Range '-55°C to +105°C'
PRP PackageReference '0201'
PRP Part_Number 'GRM033C80J105ME05D'
PRP PartNumber 'GRM033C80J105ME05D'
PRP RoHS 'TRUE'
PRP SizeZ_mm '0.39mm'
PRP TempCo '22%'
PRP Temperature_Characteristic 'X6S'
PRP Tolerance__ '20%'
PRP Value '1µF'
PRP ValueDisplayed '1.0uF'
PRP VDC_V '6.3V'
TOP 0 3.4458408 1.2231965 270 N 284 157 C32-1
TOP 1 3.4458408 1.2454405 270 N 175 22 C32-2
#
# CMP 250
CMP 39 3.8148496 1.239567 0 N C31 GRM033C80J105ME05D ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.murata.com/en-us/products/productdetail?partno=GRM033C80J105ME05%23'
PRP DataSheet 'https://www.murata.com/en-us/products/productdetail?partno=GRM033C80J105ME05%23'
PRP Datasheet_Path 'datasheets/Cap-GRM033C80J105ME05D.pdf'
PRP helpURL 'https://upverter.com/upn/revision/64a3db239e8cbfc8/'
PRP Lead_free 'Yes'
PRP Manufacturer 'Murata'
PRP Operating_Temperature_Range '-55°C to +105°C'
PRP PackageReference '0201'
PRP Part_Number 'GRM033C80J105ME05D'
PRP PartNumber 'GRM033C80J105ME05D'
PRP RoHS 'TRUE'
PRP SizeZ_mm '0.39mm'
PRP TempCo '22%'
PRP Temperature_Characteristic 'X6S'
PRP Tolerance__ '20%'
PRP Value '1µF'
PRP ValueDisplayed '1.0uF'
PRP VDC_V '6.3V'
TOP 0 3.8259716 1.239567 180 N 284 156 C31-1
TOP 1 3.8037276 1.239567 180 N 175 21 C31-2
#
# CMP 251
CMP 39 3.4458408 1.1089091 90 N C29 GRM033C80J105ME05D ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.murata.com/en-us/products/productdetail?partno=GRM033C80J105ME05%23'
PRP DataSheet 'https://www.murata.com/en-us/products/productdetail?partno=GRM033C80J105ME05%23'
PRP Datasheet_Path 'datasheets/Cap-GRM033C80J105ME05D.pdf'
PRP helpURL 'https://upverter.com/upn/revision/64a3db239e8cbfc8/'
PRP Lead_free 'Yes'
PRP Manufacturer 'Murata'
PRP Operating_Temperature_Range '-55°C to +105°C'
PRP PackageReference '0201'
PRP Part_Number 'GRM033C80J105ME05D'
PRP PartNumber 'GRM033C80J105ME05D'
PRP RoHS 'TRUE'
PRP SizeZ_mm '0.39mm'
PRP TempCo '22%'
PRP Temperature_Characteristic 'X6S'
PRP Tolerance__ '20%'
PRP Value '1µF'
PRP ValueDisplayed '1.0uF'
PRP VDC_V '6.3V'
TOP 0 3.4458408 1.1200311 90 N 284 155 C29-1
TOP 1 3.4458408 1.0977871 90 N 175 20 C29-2
#
# CMP 252
CMP 1 3.8753087 0.7089689 0 N C28 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 3.8989307 0.7089689 270 N 165 3 C28-1
TOP 1 3.8516866 0.7089689 270 N 284 123 C28-2
#
# CMP 253
CMP 1 3.8753087 0.6589687 0 N C27 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 3.8989307 0.6589687 270 N 165 2 C27-1
TOP 1 3.8516866 0.6589687 270 N 284 122 C27-2
#
# CMP 254
CMP 1 3.8753087 0.6089685 0 N C26 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 3.8989307 0.6089685 270 N 165 1 C26-1
TOP 1 3.8516866 0.6089685 270 N 284 121 C26-2
#
# CMP 255
CMP 5 3.875 0.5404529 0 N C25 C1608X7S1A335K080AC ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '3.3µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=C1608X7S1A335K080AC'
PRP CompType 'Capacitor'
PRP ESR_ohm '4.796m'
PRP IRMS_A '2.3752A'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'C1608X7S1A335K080AC'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '445-14256-1-ND'
PRP Supplier_Part_Number_2 '52X3755'
PRP Supplier_Part_Number_3 '810-C1608X7S1A335K0C'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7S'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '3.3uF'
PRP Value1 '0.004796 ohm'
PRP Value2 '10V'
PRP ValueDisplayed '3.3uF'
PRP VDC_V '10V'
TOP 0 3.9064961 0.5404529 270 N 165 4 C25-1
TOP 1 3.843504 0.5404529 270 N 284 124 C25-2
#
# CMP 256
CMP 1 4.1009588 0.5542595 180 N C24 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 4.0773368 0.5542595 90 N 159 37 C24-1
TOP 1 4.1245809 0.5542595 90 N 284 125 C24-2
#
# CMP 257
CMP 39 3.9160924 1.1150787 180 N C22 GRM033C80J105ME05D ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.murata.com/en-us/products/productdetail?partno=GRM033C80J105ME05%23'
PRP DataSheet 'https://www.murata.com/en-us/products/productdetail?partno=GRM033C80J105ME05%23'
PRP Datasheet_Path 'datasheets/Cap-GRM033C80J105ME05D.pdf'
PRP helpURL 'https://upverter.com/upn/revision/64a3db239e8cbfc8/'
PRP Lead_free 'Yes'
PRP Manufacturer 'Murata'
PRP Operating_Temperature_Range '-55°C to +105°C'
PRP PackageReference '0201'
PRP Part_Number 'GRM033C80J105ME05D'
PRP PartNumber 'GRM033C80J105ME05D'
PRP RoHS 'TRUE'
PRP SizeZ_mm '0.39mm'
PRP TempCo '22%'
PRP Temperature_Characteristic 'X6S'
PRP Tolerance__ '20%'
PRP Value '1µF'
PRP ValueDisplayed '1.0uF'
PRP VDC_V '6.3V'
TOP 0 3.9049704 1.1150787 0 N 284 154 C22-1
TOP 1 3.9272144 1.1150787 0 N 175 19 C22-2
#
# CMP 258
CMP 39 3.3958412 1.3522891 90 N C21 GRM033C80J105ME05D ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.murata.com/en-us/products/productdetail?partno=GRM033C80J105ME05%23'
PRP DataSheet 'https://www.murata.com/en-us/products/productdetail?partno=GRM033C80J105ME05%23'
PRP Datasheet_Path 'datasheets/Cap-GRM033C80J105ME05D.pdf'
PRP helpURL 'https://upverter.com/upn/revision/64a3db239e8cbfc8/'
PRP Lead_free 'Yes'
PRP Manufacturer 'Murata'
PRP Operating_Temperature_Range '-55°C to +105°C'
PRP PackageReference '0201'
PRP Part_Number 'GRM033C80J105ME05D'
PRP PartNumber 'GRM033C80J105ME05D'
PRP RoHS 'TRUE'
PRP SizeZ_mm '0.39mm'
PRP TempCo '22%'
PRP Temperature_Characteristic 'X6S'
PRP Tolerance__ '20%'
PRP Value '1µF'
PRP ValueDisplayed '1.0uF'
PRP VDC_V '6.3V'
TOP 0 3.3958412 1.3634111 90 N 284 153 C21-1
TOP 1 3.3958412 1.3411671 90 N 175 18 C21-2
#
# CMP 259
CMP 39 3.4458408 0.9945605 270 N C20 GRM033C80J105ME05D ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.murata.com/en-us/products/productdetail?partno=GRM033C80J105ME05%23'
PRP DataSheet 'https://www.murata.com/en-us/products/productdetail?partno=GRM033C80J105ME05%23'
PRP Datasheet_Path 'datasheets/Cap-GRM033C80J105ME05D.pdf'
PRP helpURL 'https://upverter.com/upn/revision/64a3db239e8cbfc8/'
PRP Lead_free 'Yes'
PRP Manufacturer 'Murata'
PRP Operating_Temperature_Range '-55°C to +105°C'
PRP PackageReference '0201'
PRP Part_Number 'GRM033C80J105ME05D'
PRP PartNumber 'GRM033C80J105ME05D'
PRP RoHS 'TRUE'
PRP SizeZ_mm '0.39mm'
PRP TempCo '22%'
PRP Temperature_Characteristic 'X6S'
PRP Tolerance__ '20%'
PRP Value '1µF'
PRP ValueDisplayed '1.0uF'
PRP VDC_V '6.3V'
TOP 0 3.4458408 0.9834385 270 N 284 152 C20-1
TOP 1 3.4458408 1.0056825 270 N 175 17 C20-2
#
# CMP 260
CMP 39 3.9565821 1.1930667 270 N C19 GRM033C80J105ME05D ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.murata.com/en-us/products/productdetail?partno=GRM033C80J105ME05%23'
PRP DataSheet 'https://www.murata.com/en-us/products/productdetail?partno=GRM033C80J105ME05%23'
PRP Datasheet_Path 'datasheets/Cap-GRM033C80J105ME05D.pdf'
PRP helpURL 'https://upverter.com/upn/revision/64a3db239e8cbfc8/'
PRP Lead_free 'Yes'
PRP Manufacturer 'Murata'
PRP Operating_Temperature_Range '-55°C to +105°C'
PRP PackageReference '0201'
PRP Part_Number 'GRM033C80J105ME05D'
PRP PartNumber 'GRM033C80J105ME05D'
PRP RoHS 'TRUE'
PRP SizeZ_mm '0.39mm'
PRP TempCo '22%'
PRP Temperature_Characteristic 'X6S'
PRP Tolerance__ '20%'
PRP Value '1µF'
PRP ValueDisplayed '1.0uF'
PRP VDC_V '6.3V'
TOP 0 3.9565821 1.1819447 270 N 284 151 C19-1
TOP 1 3.9565821 1.2041887 270 N 175 16 C19-2
#
# CMP 261
CMP 1 4.186181 1.2540556 180 N C18 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 4.162559 1.2540556 90 N 162 7 C18-1
TOP 1 4.2098031 1.2540556 90 N 284 108 C18-2
#
# CMP 262
CMP 1 4.1908525 1.0133221 180 N C17 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 4.1672305 1.0133221 90 N 162 10 C17-1
TOP 1 4.2144746 1.0133221 90 N 284 112 C17-2
#
# CMP 263
CMP 1 3.6888654 1.4999057 270 N C16 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 3.6888654 1.4762837 0 N 162 9 C16-1
TOP 1 3.6888654 1.5235278 0 N 284 111 C16-2
#
# CMP 264
CMP 5 3.435 0.8247231 0 N C14 C1608X7S1A335K080AC ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '3.3µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=C1608X7S1A335K080AC'
PRP CompType 'Capacitor'
PRP ESR_ohm '4.796m'
PRP IRMS_A '2.3752A'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'C1608X7S1A335K080AC'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '445-14256-1-ND'
PRP Supplier_Part_Number_2 '52X3755'
PRP Supplier_Part_Number_3 '810-C1608X7S1A335K0C'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7S'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '3.3uF'
PRP Value1 '0.004796 ohm'
PRP Value2 '10V'
PRP ValueDisplayed '3.3uF'
PRP VDC_V '10V'
TOP 0 3.4664961 0.8247231 270 N 162 11 C14-1
TOP 1 3.403504 0.8247231 270 N 284 114 C14-2
#
# CMP 265
CMP 1 4.1861813 1.3170738 180 N C13 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 4.1625593 1.3170738 90 N 159 22 C13-1
TOP 1 4.2098034 1.3170738 90 N 284 101 C13-2
#
# CMP 266
CMP 1 4.1006718 1.4982207 270 N C12 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 4.1006718 1.4745987 0 N 159 23 C12-1
TOP 1 4.1006718 1.5218428 0 N 284 102 C12-2
#
# CMP 267
CMP 1 3.831661 1.499906 270 N C11 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 3.831661 1.476284 0 N 159 24 C11-1
TOP 1 3.831661 1.5235281 0 N 284 103 C11-2
#
# CMP 268
CMP 1 3.7560823 1.4999057 270 N C10 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 3.7560823 1.4762837 0 N 159 25 C10-1
TOP 1 3.7560823 1.5235278 0 N 284 104 C10-2
#
# CMP 269
CMP 1 4.1936718 0.89 180 N C9 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 4.1700498 0.89 90 N 159 30 C9-1
TOP 1 4.2172939 0.89 90 N 284 113 C9-2
#
# CMP 270
CMP 1 4.1921806 0.9529706 180 N C8 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 4.1685586 0.9529706 90 N 159 21 C8-1
TOP 1 4.2158027 0.9529706 90 N 284 100 C8-2
#
# CMP 271
CMP 5 3.6191288 1.5014965 270 N C6 C1608X7S1A335K080AC ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '3.3µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=C1608X7S1A335K080AC'
PRP CompType 'Capacitor'
PRP ESR_ohm '4.796m'
PRP IRMS_A '2.3752A'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'C1608X7S1A335K080AC'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '445-14256-1-ND'
PRP Supplier_Part_Number_2 '52X3755'
PRP Supplier_Part_Number_3 '810-C1608X7S1A335K0C'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7S'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '3.3uF'
PRP Value1 '0.004796 ohm'
PRP Value2 '10V'
PRP ValueDisplayed '3.3uF'
PRP VDC_V '10V'
TOP 0 3.6191288 1.4700004 0 N 159 26 C6-1
TOP 1 3.6191288 1.5329925 0 N 284 105 C6-2
#
# CMP 272
CMP 5 3.896573 1.5014965 270 N C5 C1608X7S1A335K080AC ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '3.3µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=C1608X7S1A335K080AC'
PRP CompType 'Capacitor'
PRP ESR_ohm '4.796m'
PRP IRMS_A '2.3752A'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'C1608X7S1A335K080AC'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '445-14256-1-ND'
PRP Supplier_Part_Number_2 '52X3755'
PRP Supplier_Part_Number_3 '810-C1608X7S1A335K0C'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7S'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '3.3uF'
PRP Value1 '0.004796 ohm'
PRP Value2 '10V'
PRP ValueDisplayed '3.3uF'
PRP VDC_V '10V'
TOP 0 3.896573 1.4700004 0 N 159 27 C5-1
TOP 1 3.896573 1.5329925 0 N 284 106 C5-2
#
# CMP 273
CMP 5 4.2000008 1.3818104 180 N C4 C1608X7S1A335K080AC ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '3.3µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=C1608X7S1A335K080AC'
PRP CompType 'Capacitor'
PRP ESR_ohm '4.796m'
PRP IRMS_A '2.3752A'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'C1608X7S1A335K080AC'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '445-14256-1-ND'
PRP Supplier_Part_Number_2 '52X3755'
PRP Supplier_Part_Number_3 '810-C1608X7S1A335K0C'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7S'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '3.3uF'
PRP Value1 '0.004796 ohm'
PRP Value2 '10V'
PRP ValueDisplayed '3.3uF'
PRP VDC_V '10V'
TOP 0 4.1685047 1.3818104 90 N 159 28 C4-1
TOP 1 4.2314968 1.3818104 90 N 284 107 C4-2
#
# CMP 274
CMP 5 3.2885079 1.3647586 270 N C3 C1608X7S1A335K080AC ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '3.3µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=C1608X7S1A335K080AC'
PRP CompType 'Capacitor'
PRP ESR_ohm '4.796m'
PRP IRMS_A '2.3752A'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'C1608X7S1A335K080AC'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '445-14256-1-ND'
PRP Supplier_Part_Number_2 '52X3755'
PRP Supplier_Part_Number_3 '810-C1608X7S1A335K0C'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7S'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '3.3uF'
PRP Value1 '0.004796 ohm'
PRP Value2 '10V'
PRP ValueDisplayed '3.3uF'
PRP VDC_V '10V'
TOP 0 3.2885079 1.3332625 0 N 175 6 C3-1
TOP 1 3.2885079 1.3962546 0 N 284 97 C3-2
#
# CMP 275
CMP 5 3.2621373 0.9807811 90 N C2 C1608X7S1A335K080AC ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '3.3µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=C1608X7S1A335K080AC'
PRP CompType 'Capacitor'
PRP ESR_ohm '4.796m'
PRP IRMS_A '2.3752A'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'C1608X7S1A335K080AC'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '445-14256-1-ND'
PRP Supplier_Part_Number_2 '52X3755'
PRP Supplier_Part_Number_3 '810-C1608X7S1A335K0C'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7S'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '3.3uF'
PRP Value1 '0.004796 ohm'
PRP Value2 '10V'
PRP ValueDisplayed '3.3uF'
PRP VDC_V '10V'
TOP 0 3.2621373 1.0122772 180 N 175 8 C2-1
TOP 1 3.2621373 0.9492851 180 N 284 99 C2-2
#
# CMP 276
CMP 5 3.3385739 0.9807811 90 N C1 C1608X7S1A335K080AC ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '3.3µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=C1608X7S1A335K080AC'
PRP CompType 'Capacitor'
PRP ESR_ohm '4.796m'
PRP IRMS_A '2.3752A'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'C1608X7S1A335K080AC'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '445-14256-1-ND'
PRP Supplier_Part_Number_2 '52X3755'
PRP Supplier_Part_Number_3 '810-C1608X7S1A335K0C'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7S'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '3.3uF'
PRP Value1 '0.004796 ohm'
PRP Value2 '10V'
PRP ValueDisplayed '3.3uF'
PRP VDC_V '10V'
TOP 0 3.3385739 1.0122772 180 N 175 7 C1-1
TOP 1 3.3385739 0.9492851 180 N 284 98 C1-2
#
