#
#Component attribute names
#
@0 .comp_mount_type
@1 .comp_height

# CMP 0
CMP 1 1.0235 0.5125 0 N R299 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 0.999878 0.5125 270 N 1 2 R299-1
TOP 1 1.0471221 0.5125 270 N 284 539 R299-2
#
# CMP 1
CMP 17 0.8795 0.531 180 N U47 SN74LVC1G08DBVR ;0=1,1=0.0571
PRP 3-State_Output 'No'
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer 'Texas Instruments'
PRP Alternate_PartNumber ''
PRP Bits(#) '1'
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/SN74LVC1G08.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/SN74LVC1G08'
PRP CompType 'IC'
PRP DatasheetVersion 'SCES217Y'
PRP F_@_Nom_Voltage(Max)(Mhz) '150'
PRP Gate_Type 'AND'
PRP Generic_Part_Number 'SN74LVC1G08'
PRP ICC_@_Nom_Voltage(Max)(mA) '0.01'
PRP Input_Type 'CMOS/TTL'
PRP Logic 'True'
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP Operating_Temperature_Range(C) '-40 to 125,-40 to 85'
PRP Output_Drive_(IOL/IOH)(Max)(mA) '32/-32'
PRP Output_Type 'CMOS'
PRP PackageDescription 'SOT-23-5'
PRP PackageReference 'DBV0005A'
PRP PartId '1'
PRP PartNumber 'SN74LVC1G08DBVR'
PRP Rating 'Catalog'
PRP RoHS 'Y'
PRP Schmitt_Trigger 'No'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm ''
PRP Sub-Family 'AND Gate'
PRP Technology_Family 'LVC'
PRP tpd_@_Nom_Voltage(Max)(ns) '4.5,6,4,5'
PRP U/M ''
PRP VCC(Max)(V) '5.5'
PRP VCC(Min)(V) '1.65'
PRP Voltage(Nom)(V) '1.8,2.5,3.3,5'
TOP 0 0.9336339 0.4935984 90 N 1 1 U47-1
TOP 1 0.9336339 0.531 90 N 215 2 U47-2
TOP 2 0.9336339 0.5684015 90 N 284 538 U47-3
TOP 3 0.8253662 0.5684015 90 N 190 2 U47-4
TOP 4 0.8253662 0.4935984 90 N 152 25 U47-5
#
# CMP 2
CMP 20 6.08 0.815 90 N U46 SN74LVC1G04DCKR ;0=1,1=0.0433
PRP 3-State_Output 'No'
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Bits(#) '1'
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/SN74LVC1G04.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/SN74LVC1G04'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/SN74LVC1G04/datasheet'
PRP CompType 'IC'
PRP DatasheetVersion 'SCES214AD'
PRP F_@_Nom_Voltage(Max)(Mhz) '150'
PRP Generic_Part_Number 'SN74LVC1G04'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP ICC_@_Nom_Voltage(Max)(mA) '0.01'
PRP Input_Type 'CMOS/TTL'
PRP Logic 'Inverting'
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP Operating_Temperature_Range(C) '-40 to 125,-40 to 85'
PRP Output_Drive_(IOL/IOH)(Max)(mA) '32/-32'
PRP Output_Type 'CMOS'
PRP PackageDescription 'SOT-SC70-5'
PRP PackageReference 'DCK0005A'
PRP PartId '1'
PRP PartNumber 'SN74LVC1G04DCKR'
PRP Rating 'Catalog'
PRP RoHS ''
PRP Schmitt_Trigger 'No'
PRP SizeArea_mm2 '4.2'
PRP SizeAreaWB_mm2 '9.3'
PRP SizeX_mm '2.1'
PRP SizeY_mm '2.0'
PRP SizeZ_mm '1.1'
PRP Sub-Family 'Inverting Buffer/Driver'
PRP Technology_Family 'LVC'
PRP tpd_@_Nom_Voltage(Max)(ns) '7.5,5.2,4.2,3.7'
PRP VCC(Max)(V) '5.5'
PRP VCC(Min)(V) '1.65'
PRP Voltage(Nom)(V) '1.8,2.5,3.3,5'
TOP 0 6.1055906 0.8592913 0 N 0 130 U46-1
TOP 1 6.08 0.8592913 0 N 99 3 U46-2
TOP 2 6.0544095 0.8592913 0 N 284 410 U46-3
TOP 3 6.0544095 0.7707086 0 N 3 2 U46-4
TOP 4 6.1055906 0.7707086 0 N 159 163 U46-5
#
# CMP 3
CMP 5 0.856862 0.4254104 0 N C249 GCM188R71C104KA37J ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/w_hinm/S0717E.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCM188R71C104KA37J'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-8015-1-ND'
PRP Supplier_Part_Number_2 '81-GCM188R71C104KA7J'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '16V'
TOP 0 0.8253659 0.4254104 270 N 152 18 C249-1
TOP 1 0.888358 0.4254104 270 N 284 411 C249-2
#
# CMP 4
CMP 5 6.0640947 0.6983828 180 N C248 GCM188R71C104KA37J ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/w_hinm/S0717E.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCM188R71C104KA37J'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-8015-1-ND'
PRP Supplier_Part_Number_2 '81-GCM188R71C104KA7J'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '16V'
TOP 0 6.0955908 0.6983828 90 N 159 162 C248-1
TOP 1 6.0325987 0.6983828 90 N 284 409 C248-2
#
# CMP 5
CMP 1 1.6078741 1.21 180 N R327 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 1.6314961 1.21 90 N 364 0 R327-1
TOP 1 1.584252 1.21 90 N 4 1 R327-2
#
# CMP 6
CMP 1 1.6078741 1.39801 180 N R326 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 1.6314961 1.39801 90 N 369 0 R326-1
TOP 1 1.584252 1.39801 90 N 6 0 R326-2
#
# CMP 7
CMP 1 1.6078741 1.5849241 180 N R325 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 1.6314961 1.5849241 90 N 365 0 R325-1
TOP 1 1.584252 1.5849241 90 N 5 0 R325-2
#
# CMP 8
CMP 1 1.6078741 1.6533533 180 N R324 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 1.6314961 1.6533533 90 N 370 0 R324-1
TOP 1 1.584252 1.6533533 90 N 7 0 R324-2
#
# CMP 9
CMP 59 5.6527952 0.5641422 180 N U16 CAT24M01WI-GT3 ;0=1,1=0.0689
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'https://www.mouser.com/datasheet/2/308/1/CAT24C512_D-2310637.pdf'
PRP LatestRevisionDate '09/03/2017'
PRP Manufacturer 'ON Semiconductor'
PRP MountType 'SMT'
PRP PackageReference 'SOIC-8'
PRP PartNumber 'CAT24M01WI-GT3'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '29.351'
PRP SizeAreaWB_mm2 '55.131'
PRP SizeX_mm '5.99'
PRP SizeY_mm '4.9'
PRP SizeZ_mm '1.75'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'CAT24M01WI-GT3OSTR-ND'
PRP Supplier_Part_Number_2 '55T1802'
PRP Supplier_Part_Number_3 '863-CAT24M01WI-GT3'
TOP 0 5.7600787 0.4891422 90 N 22 2 U16-1
TOP 1 5.7600787 0.5391422 90 N 21 2 U16-2
TOP 2 5.7600787 0.5891422 90 N 20 2 U16-3
TOP 3 5.7600787 0.6391422 90 N 284 412 U16-4
TOP 4 5.5455118 0.6391422 90 N 508 2 U16-5
TOP 5 5.5455118 0.5891422 90 N 509 2 U16-6
TOP 6 5.5455118 0.5391422 90 N 19 1 U16-7
TOP 7 5.5455118 0.4891422 90 N 159 164 U16-8
#
# CMP 10
CMP 65 2.9756071 0.6109449 90 N S1 CAS-120TA ;0=1,1=0.0984
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Circuit 'SPDT'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://copal-electronics.info/en/0008e/02462.pdf'
PRP CompType 'Switch'
PRP CurrentRating_mA '100A'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Copal Electronics'
PRP MountType 'SMT'
PRP Orientation 'Top Actuated'
PRP PackageReference 'Switch, 5.4x2.5x2.5mm'
PRP PartNumber 'CAS-120TA'
PRP PositionCount '1'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'CAS120JCT-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP SwitchFunction 'On-On'
PRP VDC_V '6V'
TOP 0 3.0445048 0.6562205 180 N 166 8 S1-1
TOP 1 2.9756072 0.5656693 180 N 351 3 S1-2
TOP 2 2.9067095 0.6562205 180 N 352 1 S1-3
#
# CMP 11
CMP 1 5.8689347 0.6150012 180 N R323 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 5.8925567 0.6150012 90 N 284 402 R323-1
TOP 1 5.8453126 0.6150012 90 N 20 1 R323-2
#
# CMP 12
CMP 1 5.8689347 0.5569912 180 N R321 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 5.8925567 0.5569912 90 N 284 403 R321-1
TOP 1 5.8453126 0.5569912 90 N 22 1 R321-2
#
# CMP 13
CMP 1 5.8689347 0.6767292 180 N R320 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 5.8925567 0.6767292 90 N 159 158 R320-1
TOP 1 5.8453126 0.6767292 90 N 20 0 R320-2
#
# CMP 14
CMP 1 5.8689347 0.4882144 180 N R318 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 5.8925567 0.4882144 90 N 159 157 R318-1
TOP 1 5.8453126 0.4882144 90 N 22 0 R318-2
#
# CMP 15
CMP 3 3.6939377 0.555 0 N R307 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 3.6742527 0.555 270 N 284 413 R307-1
TOP 1 3.7136228 0.555 270 N 23 2 R307-2
#
# CMP 16
CMP 44 -0.0000005 1.0440762 90 N J34 1051640001 ;0=1,1=0.1063
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL 'Y'
PRP Cert_VDE ''
PRP ClassName ''
PRP CNHeader 'FALSE'
PRP Color 'Black'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.molex.com/pdm_docs/sd/1051640001_sd.pdf'
PRP CompType 'USB'
PRP ContactFinish 'Gold'
PRP CT 'TRUE'
PRP Current_A '1.8A'
PRP Gender 'Female'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Molex'
PRP MountType 'SMT'
PRP Note ''
PRP Orientation 'R/A'
PRP PackageReference 'Receptacle, USB 2.0, Micro B, 5 Pos, 0.65mm Pitch, R/A, SMT'
PRP PartNumber '1051640001'
PRP PinCount '5'
PRP Pitch_mm '0.65'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'WM11263CT-ND'
PRP Supplier_Part_Number_2 '99Y3224'
PRP Supplier_Part_Number_3 '538-105164-0001'
PRP Voltage_V '30V'
TOP 0 0.1618106 0.9928951 270 N 176 7 J34-1
TOP 1 0.1618105 1.0184857 270 N 151 1 J34-2
TOP 2 0.1618106 1.0440762 270 N 150 1 J34-3
TOP 3 0.1618105 1.0696666 270 N 149 1 J34-4
TOP 4 0.1618106 1.0952573 270 N 285 51 J34-5
TOP 5 0.1476372 1.141025 270 N 42 9 J34-6
TOP 6 0.0570861 1.199588 0 N 42 7 J34-7
TOP 7 0.0570861 1.0809855 270 N 42 11 J34-8
TOP 8 0.0570861 1.0071668 270 N 42 10 J34-9
TOP 9 0.0570861 0.8885644 0 N 42 6 J34-10
TOP 10 0.1476372 0.9471274 270 N 42 8 J34-11
#
# CMP 17
CMP 1 5.1285403 0.5852952 270 N C95 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 5.1285403 0.5616732 180 N 574 3 C95-1
TOP 1 5.1285403 0.6089173 180 N 284 368 C95-2
#
# CMP 18
CMP 23 1.9977163 0.4851041 180 N D16 TPD1E01B04DPYR ;0=1,1=0.0177
PRP AEC_Category 'Q200'
PRP AEC_Qualified ''
PRP Alternate_Manufacturer 'Texas Instruments'
PRP Alternate_PartNumber 'TPD1E01B04DPYT'
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/tpd1e01b04.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/tpd1e01b04'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/tpd1e01b04/datasheet'
PRP CompType 'IC'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP Operating_Temperature_Range '-40 to 125 C'
PRP PackageDescription 'X1SON-2'
PRP PackageReference 'DPY0002A'
PRP PartNumber 'TPD1E01B04DPYR'
PRP Rating 'Catalog'
PRP RoHS ''
PRP SizeArea_mm2 '0.6'
PRP SizeAreaWB_mm2 '3.2'
PRP SizeX_mm '1.0'
PRP SizeY_mm '0.6'
PRP SizeZ_mm '0.45'
PRP Value ''
TOP 0 2.0105116 0.4851041 180 N 30 2 D16-1
TOP 1 1.984921 0.4851041 180 N 284 414 D16-2
#
# CMP 19
CMP 23 4.3515761 0.4666593 180 N D15 TPD1E01B04DPYR ;0=1,1=0.0177
PRP AEC_Category 'Q200'
PRP AEC_Qualified ''
PRP Alternate_Manufacturer 'Texas Instruments'
PRP Alternate_PartNumber 'TPD1E01B04DPYT'
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/tpd1e01b04.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/tpd1e01b04'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/tpd1e01b04/datasheet'
PRP CompType 'IC'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP Operating_Temperature_Range '-40 to 125 C'
PRP PackageDescription 'X1SON-2'
PRP PackageReference 'DPY0002A'
PRP PartNumber 'TPD1E01B04DPYR'
PRP Rating 'Catalog'
PRP RoHS ''
PRP SizeArea_mm2 '0.6'
PRP SizeAreaWB_mm2 '3.2'
PRP SizeX_mm '1.0'
PRP SizeY_mm '0.6'
PRP SizeZ_mm '0.45'
PRP Value ''
TOP 0 4.3643714 0.4666593 180 N 284 369 D15-1
TOP 1 4.3387808 0.4666593 180 N 25 2 D15-2
#
# CMP 20
CMP 56 4.565 0.67 180 N U52 TS3DDR3812RUAR ;0=1,1=0.0461
PRP -3Db_Bandwith '1.675GHz'
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'No'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/ts3ddr3812.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/GPN'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/GPN/datasheet'
PRP CompType 'IC'
PRP DataSheet 'http://www.ti.com/lit/ds/symlink/ts3ddr3812.pdf'
PRP Datasheet_Path 'datasheets/IC-TS3DDR3812RUAR.pdf'
PRP Digikey_Description 'IC MUX/DEMUX DDR3 1:2 42WQFN'
PRP Digikey_Part_Number '296-28307-1-ND'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP helpURL 'https://upverter.com/upn/revision/ade7f521fbdb6cf8/'
PRP Lead_free 'Yes'
PRP Manufacturer 'Texas Instruments'
PRP Max_Supply_Voltage '3.6V'
PRP Min_Supply_Voltage '3V'
PRP MountType ''
PRP Mouser_Description 'Multiplexer Switch ICs 12-Channel,1:2 MUX/ DEMUX Switch'
PRP Mouser_Part_Number '595-TS3DDR3812RUAR'
PRP Mux_Demux_Ratio '1:2'
PRP Nominal_Supply_Current '300uA'
PRP On_State_Resistance '8O'
PRP Operating_Temperature_Range '-40°C to +85°C'
PRP PackageDescription ''
PRP PackageReference 'WQFN42'
PRP Part_Number 'TS3DDR3812RUAR'
PRP PartNumber 'TS3DDR3812RUAR'
PRP PositionCount '12'
PRP Rating ''
PRP RoHS 'TRUE'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm '0.8mm'
PRP Standoff_Height '0mm'
PRP TaMax_C '+85°C'
PRP TaMin_C '-40°C'
TOP 0 4.6299606 0.5125197 180 N 159 165 U52-1
TOP 1 4.6299606 0.5322047 180 N 102 1 U52-2
TOP 2 4.6299606 0.5518898 180 N 101 1 U52-3
TOP 3 4.6299606 0.5715748 180 N 583 4 U52-4
TOP 4 4.6299606 0.5912598 180 N 582 4 U52-5
TOP 5 4.6299606 0.6109449 180 N 581 4 U52-6
TOP 6 4.6299606 0.6306299 180 N 580 4 U52-7
TOP 7 4.6299606 0.650315 180 N 99 4 U52-8
TOP 8 4.6299606 0.67 180 N 123 2 U52-9
TOP 9 4.6299606 0.689685 180 N 123 3 U52-10
TOP 10 4.6299606 0.7093701 180 N 577 4 U52-11
TOP 11 4.6299606 0.7290551 180 N 576 4 U52-12
TOP 12 4.6299606 0.7487402 180 N 575 4 U52-13
TOP 13 4.6299606 0.7684252 180 N 120 1 U52-14
TOP 14 4.6299606 0.7881102 180 N 0 131 U52-15
TOP 15 4.6299606 0.8077953 180 N 0 132 U52-16
TOP 16 4.6299606 0.8274803 180 N 159 166 U52-17
TOP 17 4.5945276 0.8432283 180 N 81 2 U52-18
TOP 18 4.5748425 0.8432283 180 N 81 3 U52-19
TOP 19 4.5551575 0.8432283 180 N 81 4 U52-20
TOP 20 4.5354724 0.8432283 180 N 81 5 U52-21
TOP 21 4.5000394 0.8274803 180 N 389 0 U52-22
TOP 22 4.5000394 0.8077953 180 N 119 1 U52-23
TOP 23 4.5000394 0.7881102 180 N 387 0 U52-24
TOP 24 4.5000394 0.7684252 180 N 26 0 U52-25
TOP 25 4.5000394 0.7487402 180 N 390 0 U52-26
TOP 26 4.5000394 0.7290551 180 N 28 0 U52-27
TOP 27 4.5000394 0.7093701 180 N 388 0 U52-28
TOP 28 4.5000394 0.689685 180 N 31 0 U52-29
TOP 29 4.5000394 0.67 180 N 159 167 U52-30
TOP 30 4.5000394 0.650315 180 N 453 1 U52-31
TOP 31 4.5000394 0.6306299 180 N 32 0 U52-32
TOP 32 4.5000394 0.6109449 180 N 454 0 U52-33
TOP 33 4.5000394 0.5912598 180 N 571 0 U52-34
TOP 34 4.5000394 0.5715748 180 N 444 1 U52-35
TOP 35 4.5000394 0.5518898 180 N 27 0 U52-36
TOP 36 4.5000394 0.5322047 180 N 446 0 U52-37
TOP 37 4.5000394 0.5125197 180 N 29 0 U52-38
TOP 38 4.5354724 0.4967717 180 N 450 1 U52-39
TOP 39 4.5551575 0.4967717 180 N 64 1 U52-40
TOP 40 4.5748425 0.4967717 180 N 452 0 U52-41
TOP 41 4.5945276 0.4967717 180 N 59 1 U52-42
TOP 42 4.565 0.67 180 N 284 415 U52-43
#
# CMP 21
CMP 49 4.43 1.627913 0 N U51 SN74CB3Q3257PWR ;0=1,1=0.0472
PRP Alternate_Manufacturer 'Texas Instruments'
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/sn74cb3q3257.pdf'
PRP CompType 'IC'
PRP LatestRevisionDate '2017-06-09'
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP PackageDescription 'TSSOP-16'
PRP PackageReference 'PW0016A'
PRP PartNumber 'SN74CB3Q3257PWR'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '32.0'
PRP SizeAreaWB_mm2 '58.8'
PRP SizeX_mm '6.4'
PRP SizeY_mm '5.0'
PRP SizeZ_mm '1.2'
PRP U/M 'EA'
TOP 0 4.3177952 1.7174799 270 N 123 4 U51-1
TOP 1 4.3177952 1.6918893 270 N 381 2 U51-2
TOP 2 4.3177952 1.6662988 270 N 49 1 U51-3
TOP 3 4.3177952 1.6407082 270 N 96 1 U51-4
TOP 4 4.3177952 1.6151177 270 N 371 0 U51-5
TOP 5 4.3177952 1.5895271 270 N 53 1 U51-6
TOP 6 4.3177952 1.5639366 270 N 93 1 U51-7
TOP 7 4.3177952 1.538346 270 N 284 416 U51-8
TOP 8 4.5422046 1.538346 270 N 94 1 U51-9
TOP 9 4.5422046 1.5639366 270 N 55 1 U51-10
TOP 10 4.5422046 1.5895271 270 N 372 1 U51-11
TOP 11 4.5422046 1.6151177 270 N 95 1 U51-12
TOP 12 4.5422046 1.6407082 270 N 66 1 U51-13
TOP 13 4.5422046 1.6662988 270 N 380 0 U51-14
TOP 14 4.5422046 1.6918893 270 N 3 3 U51-15
TOP 15 4.5422046 1.7174799 270 N 159 168 U51-16
#
# CMP 22
CMP 56 5.2383859 1.020036 180 N U50 TS3DDR3812RUAR ;0=1,1=0.0461
PRP -3Db_Bandwith '1.675GHz'
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'No'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/ts3ddr3812.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/GPN'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/GPN/datasheet'
PRP CompType 'IC'
PRP DataSheet 'http://www.ti.com/lit/ds/symlink/ts3ddr3812.pdf'
PRP Datasheet_Path 'datasheets/IC-TS3DDR3812RUAR.pdf'
PRP Digikey_Description 'IC MUX/DEMUX DDR3 1:2 42WQFN'
PRP Digikey_Part_Number '296-28307-1-ND'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP helpURL 'https://upverter.com/upn/revision/ade7f521fbdb6cf8/'
PRP Lead_free 'Yes'
PRP Manufacturer 'Texas Instruments'
PRP Max_Supply_Voltage '3.6V'
PRP Min_Supply_Voltage '3V'
PRP MountType ''
PRP Mouser_Description 'Multiplexer Switch ICs 12-Channel,1:2 MUX/ DEMUX Switch'
PRP Mouser_Part_Number '595-TS3DDR3812RUAR'
PRP Mux_Demux_Ratio '1:2'
PRP Nominal_Supply_Current '300uA'
PRP On_State_Resistance '8O'
PRP Operating_Temperature_Range '-40°C to +85°C'
PRP PackageDescription ''
PRP PackageReference 'WQFN42'
PRP Part_Number 'TS3DDR3812RUAR'
PRP PartNumber 'TS3DDR3812RUAR'
PRP PositionCount '12'
PRP Rating ''
PRP RoHS 'TRUE'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm '0.8mm'
PRP Standoff_Height '0mm'
PRP TaMax_C '+85°C'
PRP TaMin_C '-40°C'
TOP 0 5.3033465 0.8625557 180 N 159 142 U50-1
TOP 1 5.3033465 0.8822407 180 N 333 3 U50-2
TOP 2 5.3033465 0.9019258 180 N 331 3 U50-3
TOP 3 5.3033465 0.9216108 180 N 329 3 U50-4
TOP 4 5.3033465 0.9412958 180 N 327 3 U50-5
TOP 5 5.3033465 0.9609809 180 N 325 3 U50-6
TOP 6 5.3033465 0.9806659 180 N 323 1 U50-7
TOP 7 5.3033465 1.000351 180 N 47 0 U50-8
TOP 8 5.3033465 1.020036 180 N 46 5 U50-9
TOP 9 5.3033465 1.039721 180 N 46 4 U50-10
TOP 10 5.3033465 1.0594061 180 N 322 1 U50-11
TOP 11 5.3033465 1.0790911 180 N 321 1 U50-12
TOP 12 5.3033465 1.0987762 180 N 320 1 U50-13
TOP 13 5.3033465 1.1184612 180 N 319 1 U50-14
TOP 14 5.3033465 1.1381462 180 N 310 1 U50-15
TOP 15 5.3033465 1.1578313 180 N 309 1 U50-16
TOP 16 5.3033465 1.1775163 180 N 159 141 U50-17
TOP 17 5.2679135 1.1932643 180 N 469 1 U50-18
TOP 18 5.2482284 1.1932643 180 N 393 1 U50-19
TOP 19 5.2285434 1.1932643 180 N 459 1 U50-20
TOP 20 5.2088583 1.1932643 180 N 395 1 U50-21
TOP 21 5.1734253 1.1775163 180 N 461 1 U50-22
TOP 22 5.1734253 1.1578313 180 N 397 1 U50-23
TOP 23 5.1734253 1.1381462 180 N 463 1 U50-24
TOP 24 5.1734253 1.1184612 180 N 399 1 U50-25
TOP 25 5.1734253 1.0987762 180 N 465 1 U50-26
TOP 26 5.1734253 1.0790911 180 N 401 1 U50-27
TOP 27 5.1734253 1.0594061 180 N 467 1 U50-28
TOP 28 5.1734253 1.039721 180 N 403 1 U50-29
TOP 29 5.1734253 1.020036 180 N 159 140 U50-30
TOP 30 5.1734253 1.000351 180 N 478 0 U50-31
TOP 31 5.1734253 0.9806659 180 N 405 0 U50-32
TOP 32 5.1734253 0.9609809 180 N 473 0 U50-33
TOP 33 5.1734253 0.9412958 180 N 406 0 U50-34
TOP 34 5.1734253 0.9216108 180 N 474 0 U50-35
TOP 35 5.1734253 0.9019258 180 N 407 0 U50-36
TOP 36 5.1734253 0.8822407 180 N 475 0 U50-37
TOP 37 5.1734253 0.8625557 180 N 408 0 U50-38
TOP 38 5.2088583 0.8468077 180 N 409 0 U50-39
TOP 39 5.2285434 0.8468077 180 N 476 0 U50-40
TOP 40 5.2482284 0.8468077 180 N 410 0 U50-41
TOP 41 5.2679135 0.8468077 180 N 477 0 U50-42
TOP 42 5.2383859 1.020036 180 N 284 390 U50-43
#
# CMP 23
CMP 49 5.765 0.8252282 0 N U49 SN74CB3Q3257PWR ;0=1,1=0.0472
PRP Alternate_Manufacturer 'Texas Instruments'
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/sn74cb3q3257.pdf'
PRP CompType 'IC'
PRP LatestRevisionDate '2017-06-09'
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP PackageDescription 'TSSOP-16'
PRP PackageReference 'PW0016A'
PRP PartNumber 'SN74CB3Q3257PWR'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '32.0'
PRP SizeAreaWB_mm2 '58.8'
PRP SizeX_mm '6.4'
PRP SizeY_mm '5.0'
PRP SizeZ_mm '1.2'
PRP U/M 'EA'
TOP 0 5.6527952 0.9147951 270 N 98 0 U49-1
TOP 1 5.6527952 0.8892045 270 N 492 4 U49-2
TOP 2 5.6527952 0.863614 270 N 70 1 U49-3
TOP 3 5.6527952 0.8380234 270 N 69 0 U49-4
TOP 4 5.6527952 0.8124329 270 N 107 4 U49-5
TOP 5 5.6527952 0.7868423 270 N 66 0 U49-6
TOP 6 5.6527952 0.7612518 270 N 65 0 U49-7
TOP 7 5.6527952 0.7356612 270 N 284 371 U49-8
TOP 8 5.8772046 0.7356612 270 N 63 0 U49-9
TOP 9 5.8772046 0.7612518 270 N 64 0 U49-10
TOP 10 5.8772046 0.7868423 270 N 505 4 U49-11
TOP 11 5.8772046 0.8124329 270 N 60 0 U49-12
TOP 12 5.8772046 0.8380234 270 N 62 1 U49-13
TOP 13 5.8772046 0.863614 270 N 108 0 U49-14
TOP 14 5.8772046 0.8892045 270 N 3 0 U49-15
TOP 15 5.8772046 0.9147951 270 N 159 127 U49-16
#
# CMP 24
CMP 67 1.1588963 0.919 90 N TP30 TESTPOINT ;0=1,1=0.0000
PRP CompType 'Testpoint'
PRP Manufacturer 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 1.1588963 0.919 90 N 39 1 TP30-1
#
# CMP 25
CMP 67 1.1058963 0.919 90 N TP29 TESTPOINT ;0=1,1=0.0000
PRP CompType 'Testpoint'
PRP Manufacturer 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 1.1058963 0.919 90 N 40 1 TP29-1
#
# CMP 26
CMP 67 1.0538963 0.92 90 N TP28 TESTPOINT ;0=1,1=0.0000
PRP CompType 'Testpoint'
PRP Manufacturer 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 1.0538963 0.92 90 N 38 1 TP28-1
#
# CMP 27
CMP 67 1.0038963 0.92 90 N TP27 TESTPOINT ;0=1,1=0.0000
PRP CompType 'Testpoint'
PRP Manufacturer 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 1.0038963 0.92 90 N 41 1 TP27-1
#
# CMP 28
CMP 3 1.8199897 0.127488 0 N R317 ERJ-2GEJ511X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/DMA0000COL9.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP LatestRevisionDate ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GEJ511X'
PRP Power_W '100mW'
PRP Published ''
PRP Publisher ''
PRP Res_ohm '510'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P510JCT-ND'
PRP Supplier_Part_Number_2 '65T8293'
PRP Supplier_Part_Number_3 '667-ERJ-2GEJ511X'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '510'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '510R'
PRP ValueDisplayed '510'
PRP VDC_V '50V'
TOP 0 1.8003047 0.127488 270 N 247 2 R317-1
TOP 1 1.8396748 0.127488 270 N 82 0 R317-2
#
# CMP 29
CMP 1 2.945 0.12 0 N R315 CRCW0402130RFKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW0402130RFKED'
PRP Power_W '63mW'
PRP Res_ohm '130'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-130LCT-ND'
PRP Supplier_Part_Number_2 '52K6679'
PRP Supplier_Part_Number_3 '71-CRCW0402-130-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '130'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '130R'
PRP ValueDisplayed '130'
PRP VDC_V '50V'
TOP 0 2.921378 0.12 270 N 87 1 R315-1
TOP 1 2.9686221 0.12 270 N 153 33 R315-2
#
# CMP 30
CMP 3 2.1035237 0.0818975 270 N R314 ERJ-2GEJ361X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/DMA0000COL9.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP LatestRevisionDate ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GEJ361X'
PRP Power_W '100mW'
PRP Published ''
PRP Publisher ''
PRP Res_ohm '360'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P360JCT-ND'
PRP Supplier_Part_Number_2 '53W4165'
PRP Supplier_Part_Number_3 '667-ERJ-2GEJ361X'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '360'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '360R'
PRP ValueDisplayed '360'
PRP VDC_V '50V'
TOP 0 2.1035237 0.0622125 180 N 88 1 R314-1
TOP 1 2.1035237 0.1015826 180 N 159 143 R314-2
#
# CMP 31
CMP 1 2.7454706 2.2201184 90 N R313 CRCW0402130RFKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW0402130RFKED'
PRP Power_W '63mW'
PRP Res_ohm '130'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-130LCT-ND'
PRP Supplier_Part_Number_2 '52K6679'
PRP Supplier_Part_Number_3 '71-CRCW0402-130-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '130'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '130R'
PRP ValueDisplayed '130'
PRP VDC_V '50V'
TOP 0 2.7454706 2.2437404 0 N 90 1 R313-1
TOP 1 2.7454706 2.1964963 0 N 159 146 R313-2
#
# CMP 32
CMP 3 0.7720658 1.6276302 90 N R312 CRCW04021K00FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04021K00FKED'
PRP Power_W '63mW'
PRP Res_ohm '1k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-1.00KLCT-ND'
PRP Supplier_Part_Number_2 '52K6545'
PRP Supplier_Part_Number_3 '71-CRCW0402-1.0K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '1.00k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '1k00'
PRP ValueDisplayed '1.00k'
PRP VDC_V '50V'
TOP 0 0.7720658 1.6473152 0 N 35 1 R312-1
TOP 1 0.7720658 1.6079451 0 N 168 39 R312-2
#
# CMP 33
CMP 3 0.645 1.625 90 N R311 CRCW04021K00FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04021K00FKED'
PRP Power_W '63mW'
PRP Res_ohm '1k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-1.00KLCT-ND'
PRP Supplier_Part_Number_2 '52K6545'
PRP Supplier_Part_Number_3 '71-CRCW0402-1.0K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '1.00k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '1k00'
PRP ValueDisplayed '1.00k'
PRP VDC_V '50V'
TOP 0 0.645 1.644685 0 N 36 1 R311-1
TOP 1 0.645 1.6053149 0 N 168 38 R311-2
#
# CMP 34
CMP 3 1.1845965 1.6563871 0 N R310 CRCW04021K00FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04021K00FKED'
PRP Power_W '63mW'
PRP Res_ohm '1k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-1.00KLCT-ND'
PRP Supplier_Part_Number_2 '52K6545'
PRP Supplier_Part_Number_3 '71-CRCW0402-1.0K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '1.00k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '1k00'
PRP ValueDisplayed '1.00k'
PRP VDC_V '50V'
TOP 0 1.1649115 1.6563871 270 N 131 2 R310-1
TOP 1 1.2042816 1.6563871 270 N 285 50 R310-2
#
# CMP 35
CMP 3 1.0958902 1.65 90 N R309 CRCW04021K00FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04021K00FKED'
PRP Power_W '63mW'
PRP Res_ohm '1k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-1.00KLCT-ND'
PRP Supplier_Part_Number_2 '52K6545'
PRP Supplier_Part_Number_3 '71-CRCW0402-1.0K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '1.00k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '1k00'
PRP ValueDisplayed '1.00k'
PRP VDC_V '50V'
TOP 0 1.0958902 1.669685 0 N 132 2 R309-1
TOP 1 1.0958902 1.6303149 0 N 285 49 R309-2
#
# CMP 36
CMP 3 1.0169934 1.65 90 N R308 CRCW04021K00FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04021K00FKED'
PRP Power_W '63mW'
PRP Res_ohm '1k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-1.00KLCT-ND'
PRP Supplier_Part_Number_2 '52K6545'
PRP Supplier_Part_Number_3 '71-CRCW0402-1.0K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '1.00k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '1k00'
PRP ValueDisplayed '1.00k'
PRP VDC_V '50V'
TOP 0 1.0169934 1.669685 0 N 133 2 R308-1
TOP 1 1.0169934 1.6303149 0 N 285 48 R308-2
#
# CMP 37
CMP 1 6.6200002 1.9000779 90 N R306 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 6.6200002 1.9236999 0 N 159 161 R306-1
TOP 1 6.6200002 1.8764558 0 N 300 1 R306-2
#
# CMP 38
CMP 1 6.62 0.95 90 N R305 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 6.62 0.973622 0 N 159 160 R305-1
TOP 1 6.62 0.9263779 0 N 336 1 R305-2
#
# CMP 39
CMP 1 5.695315 2.0086405 270 N R304 ERJ-2GEJ102X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/DMA0000COL9.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS 'Passed with Exemption'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GEJ102X'
PRP Power_W '100mW'
PRP Published ''
PRP Publisher ''
PRP Res_ohm '1k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P1.0KJCT-ND'
PRP Supplier_Part_Number_2 '65T8247'
PRP Supplier_Part_Number_3 '667-ERJ-2GEJ102X'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '1.0k'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '1k00'
PRP ValueDisplayed '1.0k'
PRP VDC_V '50V'
TOP 0 5.695315 1.9850185 180 N 284 395 R304-1
TOP 1 5.695315 2.0322626 180 N 104 0 R304-2
#
# CMP 40
CMP 3 5.715 2.0908591 0 N R303 ERJ-2GEJ511X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/DMA0000COL9.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP LatestRevisionDate ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GEJ511X'
PRP Power_W '100mW'
PRP Published ''
PRP Publisher ''
PRP Res_ohm '510'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P510JCT-ND'
PRP Supplier_Part_Number_2 '65T8293'
PRP Supplier_Part_Number_3 '667-ERJ-2GEJ511X'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '510'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '510R'
PRP ValueDisplayed '510'
PRP VDC_V '50V'
TOP 0 5.695315 2.0908591 270 N 104 1 R303-1
TOP 1 5.7346851 2.0908591 270 N 83 1 R303-2
#
# CMP 41
CMP 3 6 2.1042686 90 N R302 ERJ-2GEJ361X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/DMA0000COL9.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP LatestRevisionDate ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GEJ361X'
PRP Power_W '100mW'
PRP Published ''
PRP Publisher ''
PRP Res_ohm '360'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P360JCT-ND'
PRP Supplier_Part_Number_2 '53W4165'
PRP Supplier_Part_Number_3 '667-ERJ-2GEJ361X'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '360'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '360R'
PRP ValueDisplayed '360'
PRP VDC_V '50V'
TOP 0 6 2.1239536 0 N 85 1 R302-1
TOP 1 6 2.0845835 0 N 157 52 R302-2
#
# CMP 42
CMP 3 3.8109997 1.6129228 90 N R297 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 3.8109997 1.6326078 0 N 453 0 R297-1
TOP 1 3.8109997 1.5932377 0 N 103 0 R297-2
#
# CMP 43
CMP 1 2.1764112 1.365 0 N R296 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 2.1527892 1.365 270 N 246 1 R296-1
TOP 1 2.2000333 1.365 270 N 159 145 R296-2
#
# CMP 44
CMP 1 1.99 1.1635867 0 N R295 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 1.966378 1.1635867 270 N 247 3 R295-1
TOP 1 2.0136221 1.1635867 270 N 159 144 R295-2
#
# CMP 45
CMP 1 5.501378 0.9920163 180 N R294 ERJ-2GEJ102X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/DMA0000COL9.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS 'Passed with Exemption'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GEJ102X'
PRP Power_W '100mW'
PRP Published ''
PRP Publisher ''
PRP Res_ohm '1k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P1.0KJCT-ND'
PRP Supplier_Part_Number_2 '65T8247'
PRP Supplier_Part_Number_3 '667-ERJ-2GEJ102X'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '1.0k'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '1k00'
PRP ValueDisplayed '1.0k'
PRP VDC_V '50V'
TOP 0 5.525 0.9920163 90 N 284 399 R294-1
TOP 1 5.4777559 0.9920163 90 N 47 2 R294-2
#
# CMP 46
CMP 1 5.501378 1.0570163 180 N R292 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 5.525 1.0570163 90 N 159 153 R292-1
TOP 1 5.4777559 1.0570163 90 N 47 1 R292-2
#
# CMP 47
CMP 1 4.5817319 1.367932 0 N R290 ERJ-2GEJ102X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/DMA0000COL9.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS 'Passed with Exemption'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GEJ102X'
PRP Power_W '100mW'
PRP Published ''
PRP Publisher ''
PRP Res_ohm '1k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P1.0KJCT-ND'
PRP Supplier_Part_Number_2 '65T8247'
PRP Supplier_Part_Number_3 '667-ERJ-2GEJ102X'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '1.0k'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '1k00'
PRP ValueDisplayed '1.0k'
PRP VDC_V '50V'
TOP 0 4.5581099 1.367932 270 N 284 392 R290-1
TOP 1 4.605354 1.367932 270 N 99 1 R290-2
#
# CMP 48
CMP 1 5.465315 0.9115457 270 N R289 ERJ-2GEJ102X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/DMA0000COL9.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS 'Passed with Exemption'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GEJ102X'
PRP Power_W '100mW'
PRP Published ''
PRP Publisher ''
PRP Res_ohm '1k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P1.0KJCT-ND'
PRP Supplier_Part_Number_2 '65T8247'
PRP Supplier_Part_Number_3 '667-ERJ-2GEJ102X'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '1.0k'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '1k00'
PRP ValueDisplayed '1.0k'
PRP VDC_V '50V'
TOP 0 5.465315 0.8879237 180 N 284 397 R289-1
TOP 1 5.465315 0.9351678 180 N 98 3 R289-2
#
# CMP 49
CMP 1 4.5817319 1.4309026 0 N R288 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 4.5581099 1.4309026 270 N 159 148 R288-1
TOP 1 4.605354 1.4309026 270 N 99 2 R288-2
#
# CMP 50
CMP 1 5.53 0.9115457 270 N R287 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 5.53 0.8879237 180 N 159 152 R287-1
TOP 1 5.53 0.9351678 180 N 98 4 R287-2
#
# CMP 51
CMP 3 4.312252 1.2317945 180 N R286 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 4.331937 1.2317945 90 N 60 1 R286-1
TOP 1 4.2925669 1.2317945 90 N 61 0 R286-2
#
# CMP 52
CMP 3 4.2364666 0.6746845 270 N R285 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 4.2364666 0.6549995 180 N 528 1 R285-1
TOP 1 4.2364666 0.6943696 180 N 109 0 R285-2
#
# CMP 53
CMP 3 4.143 0.674685 270 N R282 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 4.143 0.655 180 N 531 1 R282-1
TOP 1 4.143 0.6943701 180 N 112 0 R282-2
#
# CMP 54
CMP 3 3.0747737 1.0319426 0 N R280 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 3.0550887 1.0319426 270 N 537 1 R280-1
TOP 1 3.0944588 1.0319426 270 N 114 0 R280-2
#
# CMP 55
CMP 3 3.5751898 0.4685293 270 N R3 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 3.5751898 0.4488443 180 N 119 0 R3-1
TOP 1 3.5751898 0.4882144 180 N 558 1 R3-2
#
# CMP 56
CMP 61 1.93 0.1233935 0 N Q13 BSS123W-7-F ;0=1,1=0.0433
PRP AEC_Category 'Q101'
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer 'None'
PRP Alternate_PartNumber ''
PRP ChType 'N'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.diodes.com/datasheets/ds30368.pdf'
PRP CompType 'MOSFET'
PRP IdsMax_A '170mA'
PRP LatestRevisionDate '2017-03-09'
PRP LatestRevisionNote 'Added parts.'
PRP Manufacturer 'Diodes Inc.'
PRP MountType 'SMT'
PRP PackageReference 'SOT-323'
PRP PartNumber 'BSS123W-7-F'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP QgTyp_nC ''
PRP Rdson45_ohm '10'
PRP RoHS 'Y'
PRP SizeArea_mm2 '4.84'
PRP SizeAreaWB_mm2 '10.24'
PRP SizeX_mm '2.2'
PRP SizeY_mm '2.2'
PRP SizeZ_mm '1.1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'BSS123W-FDICT-ND'
PRP Supplier_Part_Number_2 '621-BSS123W-F'
PRP Supplier_Part_Number_3 ''
PRP U/M 'EA'
PRP Value '100V'
PRP Value1 '1'
PRP Value2 ''
PRP Vault_Folder ''
PRP VdsMax_V '100V'
PRP Vgs_V '20V'
TOP 0 1.8925983 0.148984 90 N 82 1 Q13-1
TOP 1 1.8925983 0.0978029 90 N 284 417 Q13-2
TOP 2 1.9674014 0.1233934 90 N 89 1 Q13-3
#
# CMP 57
CMP 61 5.828 2.0652686 0 N Q11 BSS123W-7-F ;0=1,1=0.0433
PRP AEC_Category 'Q101'
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer 'None'
PRP Alternate_PartNumber ''
PRP ChType 'N'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.diodes.com/datasheets/ds30368.pdf'
PRP CompType 'MOSFET'
PRP IdsMax_A '170mA'
PRP LatestRevisionDate '2017-03-09'
PRP LatestRevisionNote 'Added parts.'
PRP Manufacturer 'Diodes Inc.'
PRP MountType 'SMT'
PRP PackageReference 'SOT-323'
PRP PartNumber 'BSS123W-7-F'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP QgTyp_nC ''
PRP Rdson45_ohm '10'
PRP RoHS 'Y'
PRP SizeArea_mm2 '4.84'
PRP SizeAreaWB_mm2 '10.24'
PRP SizeX_mm '2.2'
PRP SizeY_mm '2.2'
PRP SizeZ_mm '1.1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'BSS123W-FDICT-ND'
PRP Supplier_Part_Number_2 '621-BSS123W-F'
PRP Supplier_Part_Number_3 ''
PRP U/M 'EA'
PRP Value '100V'
PRP Value1 '1'
PRP Value2 ''
PRP Vault_Folder ''
PRP VdsMax_V '100V'
PRP Vgs_V '20V'
TOP 0 5.7905983 2.0908591 90 N 83 0 Q11-1
TOP 1 5.7905983 2.039678 90 N 284 370 Q11-2
TOP 2 5.8654014 2.0652685 90 N 86 1 Q11-3
#
# CMP 58
CMP 71 0.165 1.6144121 0 N DS3 150060RS75000 ;0=1,1=0.0315
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Angle '140'
PRP Color 'Red'
PRP ColorTemperature ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://katalog.we-online.de/led/datasheet/150060RS75000.pdf'
PRP CompType 'LED'
PRP DynamicResistance ''
PRP Family_Io ''
PRP FamilyName ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Io_A '30mA'
PRP Ir_A ''
PRP LambdaD ''
PRP LambdaP ''
PRP Luminance_Lv ''
PRP LuminousFlux_PhiV ''
PRP LuminousIntensity_IV ''
PRP Manufacturer 'Wurth Elektronik'
PRP MountType 'SMT'
PRP NumParallelLEDs ''
PRP NumSeriesLEDs ''
PRP PackageReference 'LED_0603'
PRP PartNumber '150060RS75000'
PRP Power_TotalModule '72mW'
PRP RJC_CperW ''
PRP RoHS 'Y'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm ''
PRP TJmax_C '85°C'
PRP TYPE 'AlInGaP'
PRP Value 'Red'
PRP Value1 '0.072W'
PRP Value2 '2V'
PRP Vf_V '2V'
PRP Vr_V '5V'
TOP 0 0.133504 1.6144121 0 N 285 52 DS3-1
TOP 1 0.1964961 1.6144121 0 N 84 1 DS3-2
#
# CMP 59
CMP 71 5.930687 2.0908591 270 N DS2 150060RS75000 ;0=1,1=0.0315
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Angle '140'
PRP Color 'Red'
PRP ColorTemperature ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://katalog.we-online.de/led/datasheet/150060RS75000.pdf'
PRP CompType 'LED'
PRP DynamicResistance ''
PRP Family_Io ''
PRP FamilyName ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Io_A '30mA'
PRP Ir_A ''
PRP LambdaD ''
PRP LambdaP ''
PRP Luminance_Lv ''
PRP LuminousFlux_PhiV ''
PRP LuminousIntensity_IV ''
PRP Manufacturer 'Wurth Elektronik'
PRP MountType 'SMT'
PRP NumParallelLEDs ''
PRP NumSeriesLEDs ''
PRP PackageReference 'LED_0603'
PRP PartNumber '150060RS75000'
PRP Power_TotalModule '72mW'
PRP RJC_CperW ''
PRP RoHS 'Y'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm ''
PRP TJmax_C '85°C'
PRP TYPE 'AlInGaP'
PRP Value 'Red'
PRP Value1 '0.072W'
PRP Value2 '2V'
PRP Vf_V '2V'
PRP Vr_V '5V'
TOP 0 5.930687 2.0593631 270 N 86 0 DS2-1
TOP 1 5.930687 2.1223552 270 N 85 0 DS2-2
#
# CMP 60
CMP 8 7.185155 2.1069687 0 N C247 GR442QR73D102KW01L ;0=1,1=0.0799
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '1808'
PRP Cap_F '1nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.murata.com/capacitor/product/GR442QR73D102KW01%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '1808'
PRP PartNumber 'GR442QR73D102KW01L'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '9'
PRP SizeAreaWB_mm2 '16.5'
PRP SizeX_mm '4.5'
PRP SizeY_mm '2'
PRP SizeZ_mm '2.03'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-8145-1-ND'
PRP Supplier_Part_Number_2 '31Y1776'
PRP Supplier_Part_Number_3 '81-GR442QR73D102KW01'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '1000pF'
PRP Value1 'Unknown'
PRP Value2 '2000V'
PRP ValueDisplayed '1000pF'
PRP VDC_V '2kV'
TOP 0 7.1024779 2.1069687 270 N 284 418 C247-1
TOP 1 7.2678322 2.1069687 270 N 43 9 C247-2
#
# CMP 61
CMP 1 4.64 1.7124799 180 N C246 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 4.663622 1.7124799 90 N 284 394 C246-1
TOP 1 4.6163779 1.7124799 90 N 159 150 C246-2
#
# CMP 62
CMP 1 4.715 0.8411811 90 N C245 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 4.715 0.8648031 0 N 284 401 C245-1
TOP 1 4.715 0.817559 0 N 159 156 C245-2
#
# CMP 63
CMP 1 5.0363821 1.4519545 180 N C242 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 5.0600041 1.4519545 90 N 284 396 C242-1
TOP 1 5.01276 1.4519545 90 N 159 151 C242-2
#
# CMP 64
CMP 1 4.6366549 1.5883887 270 N C241 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 4.6366549 1.5647667 180 N 284 393 C241-1
TOP 1 4.6366549 1.6120108 180 N 159 149 C241-2
#
# CMP 65
CMP 1 4.6703837 1.2368466 270 N C240 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 4.6703837 1.2132246 180 N 284 391 C240-1
TOP 1 4.6703837 1.2604687 180 N 159 147 C240-2
#
# CMP 66
CMP 1 5.3398765 0.7647682 270 N C239 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 5.3398765 0.7411462 180 N 284 398 C239-1
TOP 1 5.3398765 0.7883903 180 N 159 154 C239-2
#
# CMP 67
CMP 1 5.425 1.178691 180 N C238 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 5.448622 1.178691 90 N 284 400 C238-1
TOP 1 5.4013779 1.178691 90 N 159 155 C238-2
#
# CMP 68
CMP 1 5.975 0.9147951 180 N C43 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 5.998622 0.9147951 90 N 284 404 C43-1
TOP 1 5.9513779 0.9147951 90 N 159 159 C43-2
#
# CMP 69
CMP 1 1.6078741 1.1172304 180 N C136 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 1.6314961 1.1172304 90 N 284 380 C136-1
TOP 1 1.584252 1.1172304 90 N 159 131 C136-2
#
# CMP 70
CMP 1 1.6078741 1.34 180 N C137 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 1.6314961 1.34 90 N 284 381 C137-1
TOP 1 1.584252 1.34 90 N 159 132 C137-2
#
# CMP 71
CMP 1 1.6078741 1.7238633 180 N C138 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 1.6314961 1.7238633 90 N 284 382 C138-1
TOP 1 1.584252 1.7238633 90 N 159 133 C138-2
#
# CMP 72
CMP 1 1.1997933 1.115266 0 N C139 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 1.1761713 1.115266 270 N 285 40 C139-1
TOP 1 1.2234154 1.115266 270 N 168 31 C139-2
#
# CMP 73
CMP 1 1.1997932 1.3400004 0 N C140 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 1.1761712 1.3400004 270 N 285 41 C140-1
TOP 1 1.2234153 1.3400004 270 N 168 32 C140-2
#
# CMP 74
CMP 1 1.1869291 1.723863 0 N C141 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 1.1633071 1.723863 270 N 285 42 C141-1
TOP 1 1.2105512 1.723863 270 N 168 33 C141-2
#
# CMP 75
CMP 1 0.4953149 1.1884673 0 N C145 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 0.4716929 1.1884673 270 N 285 43 C145-1
TOP 1 0.518937 1.1884673 270 N 168 34 C145-2
#
# CMP 76
CMP 2 0.9774887 1.0253231 90 N C146 GCM155C71A105KE38D ;0=1,1=0.0276
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM155C71A105KE38%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155C71A105KE38D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.7'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GCM155C71A105KE8D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7S'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '1uF'
PRP VDC_V '10V'
TOP 0 0.9774887 1.0453231 0 N 168 40 C146-1
TOP 1 0.9774887 1.0053231 0 N 285 53 C146-2
#
# CMP 77
CMP 1 0.7876264 1.0212204 270 N C147 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 0.7876264 0.9975984 180 N 285 44 C147-1
TOP 1 0.7876264 1.0448425 180 N 168 35 C147-2
#
# CMP 78
CMP 2 0.8508059 1.6276302 270 N C148 GCM155C71A105KE38D ;0=1,1=0.0276
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM155C71A105KE38%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155C71A105KE38D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.7'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GCM155C71A105KE8D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7S'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '1uF'
PRP VDC_V '10V'
TOP 0 0.8508059 1.6076302 180 N 168 29 C148-1
TOP 1 0.8508059 1.6476302 180 N 285 36 C148-2
#
# CMP 79
CMP 1 0.4805004 1.5056598 0 N C150 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 0.4568784 1.5056598 270 N 285 45 C150-1
TOP 1 0.5041225 1.5056598 270 N 168 36 C150-2
#
# CMP 80
CMP 1 1.105 1.2215749 180 N C153 GRM155C81C225KE11D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '2.2µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155C81C225KE11-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155C81C225KE11D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155C81C225KE11D-ND'
PRP Supplier_Part_Number_2 '81-GRM155C81C225KE1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '105°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X6S'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '2.2uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '2.2uF'
PRP VDC_V '16V'
TOP 0 1.128622 1.2215749 90 N 285 39 C153-1
TOP 1 1.0813779 1.2215749 90 N 130 4 C153-2
#
# CMP 81
CMP 1 0.7749811 0.9418502 180 N C155 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 0.7986031 0.9418502 90 N 285 46 C155-1
TOP 1 0.751359 0.9418502 90 N 130 5 C155-2
#
# CMP 82
CMP 2 1.105 1.27 0 N C156 GCM155C71A105KE38D ;0=1,1=0.0276
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM155C71A105KE38%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155C71A105KE38D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.7'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GCM155C71A105KE8D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7S'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '1uF'
PRP VDC_V '10V'
TOP 0 1.085 1.27 270 N 130 3 C156-1
TOP 1 1.125 1.27 270 N 285 35 C156-2
#
# CMP 83
CMP 70 0.165 1.5313854 0 N D3 150060VS75000 ;0=1,1=0.0315
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Angle ''
PRP Color 'green'
PRP ColorTemperature ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://katalog.we-online.de/led/datasheet/150060VS75000.pdf'
PRP CompType 'LED'
PRP DynamicResistance ''
PRP Family_Io ''
PRP FamilyName ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Io_A '20mA'
PRP Ir_A ''
PRP LambdaD ''
PRP LambdaP ''
PRP Luminance_Lv ''
PRP LuminousFlux_PhiV ''
PRP LuminousIntensity_IV ''
PRP Manufacturer 'Wurth Elektronik'
PRP MountType 'SMT'
PRP NumParallelLEDs ''
PRP NumSeriesLEDs ''
PRP PackageReference 'LED_0603'
PRP PartNumber '150060VS75000'
PRP Power_TotalModule ''
PRP RJC_CperW ''
PRP RoHS 'Y'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm ''
PRP TJmax_C ''
PRP TYPE 'AlInGaP'
PRP Value 'Green'
PRP Value1 'W'
PRP Value2 '2V'
PRP Vf_V '2V'
PRP Vr_V ''
TOP 0 0.133504 1.5313854 0 N 285 54 D3-1
TOP 1 0.1964961 1.5313854 0 N 91 1 D3-2
#
# CMP 84
CMP 3 0.395315 1.2041156 180 N R144 CRCW04021K00FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04021K00FKED'
PRP Power_W '63mW'
PRP Res_ohm '1k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-1.00KLCT-ND'
PRP Supplier_Part_Number_2 '52K6545'
PRP Supplier_Part_Number_3 '71-CRCW0402-1.0K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '1.00k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '1k00'
PRP ValueDisplayed '1.00k'
PRP VDC_V '50V'
TOP 0 0.415 1.2041156 90 N 147 3 R144-1
TOP 1 0.3756299 1.2041156 90 N 168 28 R144-2
#
# CMP 85
CMP 3 0.27 1.53 0 N R259 ERJ-2GEJ361X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/DMA0000COL9.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP LatestRevisionDate ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GEJ361X'
PRP Power_W '100mW'
PRP Published ''
PRP Publisher ''
PRP Res_ohm '360'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P360JCT-ND'
PRP Supplier_Part_Number_2 '53W4165'
PRP Supplier_Part_Number_3 '667-ERJ-2GEJ361X'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '360'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '360R'
PRP ValueDisplayed '360'
PRP VDC_V '50V'
TOP 0 0.250315 1.53 270 N 91 0 R259-1
TOP 1 0.2896851 1.53 270 N 34 1 R259-2
#
# CMP 86
CMP 3 0.275 1.6 0 N R260 ERJ-2GEJ361X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/DMA0000COL9.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP LatestRevisionDate ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GEJ361X'
PRP Power_W '100mW'
PRP Published ''
PRP Publisher ''
PRP Res_ohm '360'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P360JCT-ND'
PRP Supplier_Part_Number_2 '53W4165'
PRP Supplier_Part_Number_3 '667-ERJ-2GEJ361X'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '360'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '360R'
PRP ValueDisplayed '360'
PRP VDC_V '50V'
TOP 0 0.255315 1.6 270 N 84 0 R260-1
TOP 1 0.2946851 1.6 270 N 33 1 R260-2
#
# CMP 87
CMP 3 0.965 1.65 90 N R261 CRCW04021K00FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04021K00FKED'
PRP Power_W '63mW'
PRP Res_ohm '1k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-1.00KLCT-ND'
PRP Supplier_Part_Number_2 '52K6545'
PRP Supplier_Part_Number_3 '71-CRCW0402-1.0K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '1.00k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '1k00'
PRP ValueDisplayed '1.00k'
PRP VDC_V '50V'
TOP 0 0.965 1.669685 0 N 134 2 R261-1
TOP 1 0.965 1.6303149 0 N 285 37 R261-2
#
# CMP 88
CMP 15 1.3938583 1.6488633 0 N U25 ISO7220CDR ;0=1,1=0.0689
PRP #_of_TX/RX ''
PRP Channel_Configuration '2/01/2000'
PRP ComponentLink1Description 'Manufacturer URL'
PRP ComponentLink1URL 'http://www.ti.com/'
PRP ComponentLink2Description 'Datasheet'
PRP ComponentLink2URL 'http://www.ti.com/general/docs/lit/getliterature.tsp?genericPartNumber=ISO7220C&fileType=pdf'
PRP ComponentLink3Description 'URL Link1'
PRP ComponentLink3URL 'SamplesURL:http://www.ti.com/product/iso7220c#samples'
PRP Datarate(Mbps) '25'
PRP DatasheetVersion 'SLLS755L'
PRP Duplex ''
PRP Eco-Plan 'Green (RoHS & no Sb/Br)'
PRP ESD(kV) ''
PRP Fail_Safe ''
PRP Fault_Protection(V) ''
PRP ICC(Max)(mA) ''
PRP Input_Noise_Filter 'Yes'
PRP Insulation_Rating(VRMS) '2500'
PRP Isolated ''
PRP Manufacturer 'Texas Instruments'
PRP Mounting_Technology 'Surface Mount'
PRP Number_of_Nodes ''
PRP PackageDescription '8-Pin Plastic Small Outline Integrated Circuit, 4.9 x 3.9 mm, Pitch 1.27 mm Pitch'
PRP PackageReference 'D0008B'
PRP PackageVersion 'revM, Jun-2011'
PRP PartNumber 'ISO7220CDR'
PRP Prop_Delay(Max)(ns) '42'
PRP Rating 'Catalog'
PRP Signaling_Rate(Mbps) ''
PRP SubFamily 'Isolator'
PRP Supply_Voltage(s)(V) '3.3, 5'
PRP Thermal_Shutdown 'No'
PRP TTL/CMOS_Input_Threshold 'TTL'
PRP VCC(Max)(V) ''
PRP VCC(Min)(V) ''
TOP 0 1.2853583 1.7238633 270 N 168 41 U25-1
TOP 1 1.2853583 1.6738633 270 N 124 1 U25-2
TOP 2 1.2853583 1.6238633 270 N 127 1 U25-3
TOP 3 1.2853583 1.5738633 270 N 285 55 U25-4
TOP 4 1.5023583 1.5738633 270 N 284 419 U25-5
TOP 5 1.5023583 1.6238633 270 N 5 1 U25-6
TOP 6 1.5023583 1.6738633 270 N 7 1 U25-7
TOP 7 1.5023583 1.7238633 270 N 159 169 U25-8
#
# CMP 89
CMP 14 1.395 1.415 180 N U26 ISO7721DR ;0=1,1=0.0689
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer 'Texas Instruments'
PRP Alternate_PartNumber 'ISO7721D'
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/iso7721.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/iso7721'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/iso7721/datasheet'
PRP CompType 'IC'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP Operating_Temperature_Range '-55 to 125 C'
PRP PackageDescription 'SOIC-8'
PRP PackageReference 'D0008B'
PRP PartNumber 'ISO7721DR'
PRP Rating 'Catalog'
PRP RoHS 'Y'
PRP SizeArea_mm2 '29.4'
PRP SizeAreaWB_mm2 '55.2'
PRP SizeX_mm '6.0'
PRP SizeY_mm '4.9'
PRP SizeZ_mm '1.75'
TOP 0 1.5032677 1.34 90 N 159 170 U26-1
TOP 1 1.5032677 1.39 90 N 6 1 U26-2
TOP 2 1.5032677 1.44 90 N 367 1 U26-3
TOP 3 1.5032677 1.49 90 N 284 420 U26-4
TOP 4 1.2867323 1.49 90 N 285 56 U26-5
TOP 5 1.2867323 1.44 90 N 126 1 U26-6
TOP 6 1.2867323 1.39 90 N 125 1 U26-7
TOP 7 1.2867323 1.34 90 N 168 42 U26-8
#
# CMP 90
CMP 14 1.395 1.1902656 180 N U27 ISO7721DR ;0=1,1=0.0689
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer 'Texas Instruments'
PRP Alternate_PartNumber 'ISO7721D'
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/iso7721.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/iso7721'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/iso7721/datasheet'
PRP CompType 'IC'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP Operating_Temperature_Range '-55 to 125 C'
PRP PackageDescription 'SOIC-8'
PRP PackageReference 'D0008B'
PRP PartNumber 'ISO7721DR'
PRP Rating 'Catalog'
PRP RoHS 'Y'
PRP SizeArea_mm2 '29.4'
PRP SizeAreaWB_mm2 '55.2'
PRP SizeX_mm '6.0'
PRP SizeY_mm '4.9'
PRP SizeZ_mm '1.75'
TOP 0 1.5032677 1.1152656 90 N 159 119 U27-1
TOP 1 1.5032677 1.1652656 90 N 4 0 U27-2
TOP 2 1.5032677 1.2152656 90 N 362 1 U27-3
TOP 3 1.5032677 1.2652656 90 N 284 353 U27-4
TOP 4 1.2867323 1.2652656 90 N 285 34 U27-5
TOP 5 1.2867323 1.2152656 90 N 129 1 U27-6
TOP 6 1.2867323 1.1652656 90 N 128 1 U27-7
TOP 7 1.2867323 1.1152656 90 N 168 27 U27-8
#
# CMP 91
CMP 19 0.3414984 1.3166452 90 N U28 LM4040C25QDBZR ;0=1,1=0.0441
PRP Code_JEDEC 'TO-236'
PRP ComponentLink1Description 'Manufacturer URL'
PRP ComponentLink1URL 'http://www.ti.com/'
PRP ComponentLink2Description 'Datasheet'
PRP ComponentLink2URL 'http://www.ti.com/general/docs/lit/getliterature.tsp?genericPartNumber=LM4040C25&fileType=pdf'
PRP ComponentLink3Description 'Package Specification'
PRP ComponentLink3URL 'http://www.ti.com/litv/pdf/mpds108a'
PRP DatasheetVersion 'SLOS456K'
PRP Eco-Plan 'Green (RoHS & no Sb/Br)'
PRP Initial_Accuracy_@_25/deg_C(_) '0.5'
PRP Iout/Iz(Max)(mA) '15'
PRP Manufacturer 'Texas Instruments'
PRP Min_Iz_for_Regulation(uA) '75'
PRP Mounting_Technology 'Surface Mount'
PRP PackageDescription '3-Pin Plastic Small Outline, Body 2.92 x 1.3 mm, Pitch 0.95 mm'
PRP PackageReference 'DBZ0003A'
PRP PackageVersion '4203227/B'
PRP PartNumber 'LM4040C25QDBZR'
PRP Rating 'Catalog'
PRP SubFamily 'Shunt Voltage Reference'
PRP Temp_Coeff(Max)(ppm/_degree_C) '100'
PRP Temp_Coeff(Typ)(ppm/_degree_C) '15'
PRP VO(V) '2.5'
TOP 0 0.3789 1.3638893 0 N 147 4 U28-1
TOP 1 0.3040969 1.3638893 0 N 285 57 U28-2
TOP 2 0.3414984 1.2694011 0 N 147 5 U28-3
#
# CMP 92
CMP 9 3.27 0.8062143 270 N Y1 ABM10W-25.0000MHZ-4-D1X-T3 ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'https://abracon.com/Resonators/ABM10W.pdf'
PRP CompType 'Crystal'
PRP Frequency_Stability '20 ppm'
PRP Frequency_Tolerance '10 ppm'
PRP Frequency_Fixed '25MHz'
PRP Frequency_Max ''
PRP Frequency_Min ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Load_Capacitance '4 pF'
PRP Manufacturer 'Abracon Corporation'
PRP MountType 'SMT'
PRP PackageReference '2x2.5mm'
PRP PartNumber 'ABM10W-25.0000MHZ-8-K1Z-T3'
PRP REACh ''
PRP RoHS 'Y'
PRP SizeArea_mm2 '5'
PRP SizeAreaWB_mm2 '10.5'
PRP SizeX_mm '2'
PRP SizeY_mm '2.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '85°C'
PRP TaMin_C '-40°C'
TOP 0 3.2380118 0.7825923 0 N 357 1 Y1-1
TOP 1 3.3019882 0.7825923 0 N 284 355 Y1-2
TOP 2 3.3019882 0.8298364 0 N 356 1 Y1-3
TOP 3 3.2380118 0.8298364 0 N 284 356 Y1-4
#
# CMP 93
CMP 16 2.16 1.62 180 N U48 TPIC2810D ;0=1,1=0.0689
PRP DatasheetVersion 'SLIS109A'
PRP Generic_Part_Number 'TPIC2810'
PRP ICC(uA) '620'
PRP IO(CONT)(A) '0.1'
PRP IO(PEAK)(A) '0.21'
PRP Manufacturer 'Texas Instruments'
PRP Operating_Temperature_Range(C) '-40 to 125'
PRP PackageReference 'D0016A'
PRP PartNumber 'TPIC2810D'
PRP Priority_(type_2) '1'
PRP Rating 'Catalog'
PRP rDS(on)(Ohms) '5'
PRP tPLH(ns) '1150'
PRP VDS(Max)(V) '40'
TOP 0 2.2672835 1.445 90 N 159 171 U48-1
TOP 1 2.2672835 1.495 90 N 508 3 U48-2
TOP 2 2.2672835 1.545 90 N 271 1 U48-3
TOP 3 2.2672835 1.595 90 N 270 1 U48-4
TOP 4 2.2672835 1.645 90 N 269 1 U48-5
TOP 5 2.2672835 1.695 90 N 268 1 U48-6
TOP 6 2.2672835 1.745 90 N 280 2 U48-7
TOP 7 2.2672835 1.795 90 N 105 1 U48-8
TOP 8 2.0527166 1.795 90 N 282 2 U48-9
TOP 9 2.0527166 1.745 90 N 281 2 U48-10
TOP 10 2.0527166 1.695 90 N 267 1 U48-11
TOP 11 2.0527166 1.645 90 N 266 1 U48-12
TOP 12 2.0527166 1.595 90 N 265 1 U48-13
TOP 13 2.0527166 1.545 90 N 264 1 U48-14
TOP 14 2.0527166 1.495 90 N 509 3 U48-15
TOP 15 2.0527166 1.445 90 N 284 421 U48-16
#
# CMP 94
CMP 26 0.4686894 0.9983207 270 N U45 TPS79601DRBR ;0=1,1=0.0394
PRP Accuracy(_) '2'
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Manufacturer URL'
PRP ComponentLink1URL 'http://www.ti.com/'
PRP ComponentLink2Description 'Datasheet'
PRP ComponentLink2URL 'http://www.ti.com/general/docs/lit/getliterature.tsp?genericPartNumber=TPS79601&fileType=pdf'
PRP ComponentLink3Description 'Package Specification'
PRP ComponentLink3URL 'http://www.ti.com/litv/pdf/mpds118h'
PRP CompType 'IC'
PRP DatasheetVersion 'SLVS351N'
PRP Eco-Plan 'Green (RoHS & no Sb/Br)'
PRP Iout(Max)(A) '1'
PRP Iq(Typ)(mA) '0.26'
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP PackageDescription 'VSON-8'
PRP PackageReference 'DRB0008B'
PRP PackageVersion '4203482-2/K'
PRP PartNumber 'TPS79601DRBR'
PRP RoHS 'Y'
PRP SizeArea_mm2 '9.0'
PRP SizeAreaWB_mm2 '16.0'
PRP SizeX_mm '3.0'
PRP SizeY_mm '3.0'
PRP SizeZ_mm '1.0'
PRP SubFamily 'Single Channel LDO'
PRP U/M ''
PRP Vdo(Typ)(mV) '250'
PRP Vin(Max)(V) '5.5'
PRP Vin(Min)(V) '2.7'
PRP Vout_Adj(Max)(V) '5.5'
PRP Vout_Adj(Min)(V) '1.2'
TOP 0 0.4303035 0.9432025 180 N 176 8 U45-1
TOP 1 0.4558941 0.9432025 180 N 176 9 U45-2
TOP 2 0.4814846 0.9432025 180 N 168 43 U45-3
TOP 3 0.5070752 0.9432025 180 N 168 44 U45-4
TOP 4 0.5070752 1.0534387 180 N 286 3 U45-5
TOP 5 0.4814846 1.0534387 180 N 285 58 U45-6
TOP 6 0.4558941 1.0534387 180 N 0 133 U45-7
TOP 7 0.4303035 1.0534387 180 N 176 10 U45-8
TOP 8 0.4686894 0.9983207 270 N 285 59 U45-9
#
# CMP 95
CMP 24 0.255 1.0608089 180 N U44 TPD4E02B04DQAR ;0=1,1=0.0217
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer 'Texas Instruments'
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/tpd4e02b04.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/tpd4e02b04'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/tpd4e02b04/datasheet'
PRP CompType 'IC'
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP PackageDescription 'USON-10'
PRP PackageReference 'DQA0010A'
PRP PartNumber 'TPD4E02B04DQAR'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '7.0'
PRP SizeX_mm '1.0'
PRP SizeY_mm '2.5'
PRP SizeZ_mm '0.55'
TOP 0 0.271437 1.0214388 90 N 151 3 U44-1
TOP 1 0.271437 1.0411238 90 N 150 3 U44-2
TOP 2 0.271437 1.0608088 90 N 285 61 U44-3
TOP 3 0.271437 1.0804939 90 N 149 3 U44-4
TOP 4 0.271437 1.1001789 90 N 0 135 U44-5
TOP 5 0.238563 1.1001789 90 N 0 134 U44-6
TOP 6 0.238563 1.0804939 90 N 149 2 U44-7
TOP 7 0.238563 1.0608088 90 N 285 60 U44-8
TOP 8 0.238563 1.0411238 90 N 150 2 U44-9
TOP 9 0.238563 1.0214388 90 N 151 2 U44-10
#
# CMP 96
CMP 25 2.8212205 0.2876551 0 N U36 TPS62177DQCR ;0=1,1=0.0315
PRP Alternate_Manufacturer 'Texas Instruments'
PRP Alternate_PartNumber 'TPS62177DQCT'
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/tps62177.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'www.ti.com/product/tps62177'
PRP CompType 'IC'
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP PackageDescription 'WSON-10'
PRP PackageReference 'DQC0010A'
PRP PartNumber 'TPS62177DQCR'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '6.0'
PRP SizeAreaWB_mm2 '12.0'
PRP SizeX_mm '2.0'
PRP SizeY_mm '3.0'
PRP SizeZ_mm '0.8'
TOP 0 2.7838189 0.3270253 270 N 284 425 U36-1
TOP 1 2.7838189 0.3073402 270 N 152 19 U36-2
TOP 2 2.7838189 0.2876552 270 N 155 1 U36-3
TOP 3 2.7838189 0.2679701 270 N 0 136 U36-4
TOP 4 2.7838189 0.2482851 270 N 284 424 U36-5
TOP 5 2.858622 0.2482851 270 N 284 423 U36-6
TOP 6 2.858622 0.2679701 270 N 37 1 U36-7
TOP 7 2.858622 0.2876552 270 N 154 1 U36-8
TOP 8 2.858622 0.3073402 270 N 257 1 U36-9
TOP 9 2.858622 0.3270253 270 N 153 34 U36-10
TOP 10 2.8212205 0.2876552 0 N 284 422 U36-11
#
# CMP 97
CMP 21 1.7843703 1.55 270 N U35 TCA9617BDGKR ;0=1,1=0.0433
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer 'Texas Instruments'
PRP Alternate_PartNumber ''
PRP Code_JEDEC 'MO-187-AA'
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/tca9617b.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/tca9617b'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/tca9617b/datasheet'
PRP CompType 'IC'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP PackageDescription 'VSSOP-8'
PRP PackageReference 'DGK0008A'
PRP PartNumber 'TCA9617BDGKR'
PRP RoHS 'Y'
PRP SizeArea_mm2 '14.7'
PRP SizeAreaWB_mm2 '23.6'
PRP SizeX_mm '4.9'
PRP SizeY_mm '3'
PRP SizeZ_mm '1.1'
TOP 0 1.7459845 1.4624016 180 N 159 172 U35-1
TOP 1 1.7715751 1.4624016 180 N 507 2 U35-2
TOP 2 1.7971656 1.4624016 180 N 506 2 U35-3
TOP 3 1.8227562 1.4624016 180 N 284 426 U35-4
TOP 4 1.8227562 1.6375985 180 N 159 173 U35-5
TOP 5 1.7971656 1.6375985 180 N 229 2 U35-6
TOP 6 1.7715751 1.6375985 180 N 230 2 U35-7
TOP 7 1.7459845 1.6375985 180 N 153 35 U35-8
#
# CMP 98
CMP 30 0.665 2.1312206 90 N U34 SN74LVC2G17DSF2 ;0=1,1=0.0157
PRP 3-State_Output 'No'
PRP Bits(#) '2'
PRP DatasheetVersion 'SCES381N'
PRP F_@_Nom_Voltage(Max)(Mhz) '150'
PRP Generic_Part_Number 'SN74LVC2G17'
PRP ICC_@_Nom_Voltage(Max)(mA) '0.01'
PRP Input_Type 'CMOS/TTL'
PRP Logic 'True'
PRP Manufacturer 'Texas Instruments'
PRP Operating_Temperature_Range(C) '-40 to 125,-40 to 85'
PRP Output_Drive_(IOL/IOH)(Max)(mA) '32/-32'
PRP Output_Type 'CMOS'
PRP PackageReference 'DSF0006A'
PRP PartNumber 'SN74LVC2G17DSF2'
PRP Rating 'Catalog'
PRP Schmitt_Trigger 'Yes'
PRP Sub-Family 'Non-Inverting Buffer/Driver'
PRP Technology_Family 'LVC'
PRP tpd_@_Nom_Voltage(Max)(ns) '9.3,5.7,5.4,4.3'
PRP VCC(Max)(V) '5.5'
PRP VCC(Min)(V) '1.65'
PRP Voltage(Nom)(V) '1.8,2.5,3.3,5'
TOP 0 0.6787796 2.1469686 90 N 244 4 U34-1
TOP 1 0.6650001 2.1469686 90 N 284 427 U34-2
TOP 2 0.6512206 2.1469686 90 N 283 2 U34-3
TOP 3 0.6512206 2.1154726 270 N 106 0 U34-4
TOP 4 0.6650001 2.1154726 270 N 159 174 U34-5
TOP 5 0.6787796 2.1154726 270 N 425 1 U34-6
#
# CMP 99
CMP 20 0.8633734 2.0281457 180 N U33 SN74LVC1G07DCKT ;0=1,1=0.0433
PRP 3-State_Output 'No'
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Bits(#) '1'
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/sn74lvc1g07.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/sn74lvc1g07'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/sn74lvc1g07/datasheet'
PRP CompType 'IC'
PRP DatasheetVersion 'SCES296AC'
PRP F_@_Nom_Voltage(Max)(Mhz) '150'
PRP Generic_Part_Number 'SN74LVC1G07'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP ICC_@_Nom_Voltage(Max)(mA) '0.01'
PRP Input_Type 'CMOS/TTL'
PRP Logic 'True'
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP Operating_Temperature_Range(C) '-40 to 125,-40 to 85'
PRP Output_Drive_(IOL/IOH)(Max)(mA) '32/-32'
PRP Output_Type 'CMOS'
PRP PackageDescription 'SOT-SC70-5'
PRP PackageReference 'DCK0005A'
PRP PartId '1'
PRP PartNumber 'SN74LVC1G07DCKT'
PRP Rating 'Catalog'
PRP RoHS ''
PRP Schmitt_Trigger 'No'
PRP SizeArea_mm2 '4.2'
PRP SizeAreaWB_mm2 '9.3'
PRP SizeX_mm '2.1'
PRP SizeY_mm '2.0'
PRP SizeZ_mm '1.1'
PRP Sub-Family 'Non-Inverting Buffer/Driver'
PRP Technology_Family 'LVC'
PRP tpd_@_Nom_Voltage(Max)(ns) '8.6,6,4.7,4'
PRP VCC(Max)(V) '5.5'
PRP VCC(Min)(V) '1.65'
PRP Voltage(Nom)(V) '1.8,2.5,3.3,5'
TOP 0 0.9076647 2.0025551 90 N 0 122 U33-1
TOP 1 0.9076647 2.0281457 90 N 241 1 U33-2
TOP 2 0.9076647 2.0537362 90 N 284 255 U33-3
TOP 3 0.819082 2.0537362 90 N 411 1 U33-4
TOP 4 0.819082 2.0025551 90 N 159 72 U33-5
#
# CMP 100
CMP 53 2.8375591 1.5743005 180 N U32 TPS62913RPUR ;0=1,1=0.0461
PRP AEC_Qualified 'No'
PRP Datasheet_Path 'datasheets/IC-TPS62913RPUR.pdf'
PRP helpURL 'https://upverter.com/upn/revision/a05e95a0cb7f20b8/'
PRP Manufacturer 'Texas Instruments'
PRP Max_Duty_Cycle '55%'
PRP Max_Supply_Voltage '17V'
PRP Min_Supply_Voltage '3V'
PRP Nominal_Supply_Current '5mA'
PRP Number_Of_Outputs '1'
PRP Operating_Temperature_Range '-40°C to +150°C'
PRP Output_Type 'AdjustableProgrammable'
PRP Output_Voltage '0.8-5.5V'
PRP PackageReference 'VQFN-HR10'
PRP Part_Number 'TPS62913RPUR'
PRP PartNumber 'TPS62913RPUR'
PRP RoHS 'UNKNOWN'
PRP SizeZ_mm '1mm'
PRP Standoff_Height '0mm'
PRP Switching_Frequency '1/2.2MHz'
PRP Switching_Topology 'Buck'
PRP TJmax_C '+150°C'
TOP 0 2.8720079 1.564458 180 N 206 1 U32-1
TOP 1 2.8651182 1.584143 180 N 202 1 U32-2
TOP 2 2.8720079 1.6038281 180 N 159 175 U32-3
TOP 3 2.81 1.6038281 180 N 284 429 U32-4
TOP 4 2.8031103 1.584143 180 N 246 2 U32-5
TOP 5 2.81 1.564458 180 N 157 55 U32-6
TOP 6 2.8080315 1.5378832 180 N 284 428 U32-7
TOP 7 2.8277166 1.5378832 180 N 204 1 U32-8
TOP 8 2.8474016 1.5378832 180 N 205 2 U32-9
TOP 9 2.8670867 1.5378832 180 N 203 1 U32-10
#
# CMP 101
CMP 28 5.7991276 1.5476225 0 N U31 TPS74801DRCR ;0=1,1=0.0394
PRP Accuracy(_) '2'
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/tps74801.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/tps74801'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/tps74801/datasheet'
PRP CompType 'IC'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Iout(Max)(A) '1.5'
PRP Iq(Typ)(mA) '1'
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP Operating_Temperature_Range '-40 to 125 C'
PRP PackageDescription 'VSON-10'
PRP PackageReference 'DRC0010J'
PRP PartNumber 'TPS74801DRCR'
PRP Power_Good 'TRUE'
PRP Rating 'Catalog'
PRP RoHS 'Y'
PRP SizeArea_mm2 '9'
PRP SizeAreaWB_mm2 '16'
PRP SizeX_mm '3'
PRP SizeY_mm '3'
PRP SizeZ_mm '1'
PRP Vdo(Typ)(mV) '60'
PRP Vin(Max)(V) '5.5'
PRP Vin(Min)(V) '0.8'
PRP Vout_Adj(Max)(V) '3.6'
PRP Vout_Adj(Min)(V) '0.8'
TOP 0 5.7440095 1.5869926 0 N 157 57 U31-1
TOP 1 5.7440095 1.5673076 0 N 157 56 U31-2
TOP 2 5.7440095 1.5476225 0 N 193 1 U31-3
TOP 3 5.7440095 1.5279375 0 N 196 1 U31-4
TOP 4 5.7440095 1.5082524 0 N 195 1 U31-5
TOP 5 5.8542457 1.5082524 0 N 284 431 U31-6
TOP 6 5.8542457 1.5279374 0 N 192 1 U31-7
TOP 7 5.8542457 1.5476225 0 N 194 2 U31-8
TOP 8 5.8542457 1.5673075 0 N 170 8 U31-9
TOP 9 5.8542457 1.5869926 0 N 170 7 U31-10
TOP 10 5.7991276 1.5476225 0 N 284 430 U31-11
#
# CMP 102
CMP 28 5.7991275 1.1284338 0 N U30 TPS74801DRCR ;0=1,1=0.0394
PRP Accuracy(_) '2'
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/tps74801.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/tps74801'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/tps74801/datasheet'
PRP CompType 'IC'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Iout(Max)(A) '1.5'
PRP Iq(Typ)(mA) '1'
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP Operating_Temperature_Range '-40 to 125 C'
PRP PackageDescription 'VSON-10'
PRP PackageReference 'DRC0010J'
PRP PartNumber 'TPS74801DRCR'
PRP Power_Good 'TRUE'
PRP Rating 'Catalog'
PRP RoHS 'Y'
PRP SizeArea_mm2 '9'
PRP SizeAreaWB_mm2 '16'
PRP SizeX_mm '3'
PRP SizeY_mm '3'
PRP SizeZ_mm '1'
PRP Vdo(Typ)(mV) '60'
PRP Vin(Max)(V) '5.5'
PRP Vin(Min)(V) '0.8'
PRP Vout_Adj(Max)(V) '3.6'
PRP Vout_Adj(Min)(V) '0.8'
TOP 0 5.7440094 1.1678039 0 N 157 51 U30-1
TOP 1 5.7440094 1.1481189 0 N 157 50 U30-2
TOP 2 5.7440094 1.1284338 0 N 198 1 U30-3
TOP 3 5.7440094 1.1087488 0 N 201 1 U30-4
TOP 4 5.7440094 1.0890637 0 N 200 1 U30-5
TOP 5 5.8542456 1.0890637 0 N 284 341 U30-6
TOP 6 5.8542456 1.1087487 0 N 197 1 U30-7
TOP 7 5.8542456 1.1284338 0 N 199 2 U30-8
TOP 8 5.8542456 1.1481188 0 N 169 7 U30-9
TOP 9 5.8542456 1.1678039 0 N 169 6 U30-10
TOP 10 5.7991275 1.1284338 0 N 284 340 U30-11
#
# CMP 103
CMP 53 2.475886 0.9416816 180 N U29 TPS62913RPUR ;0=1,1=0.0461
PRP AEC_Qualified 'No'
PRP Datasheet_Path 'datasheets/IC-TPS62913RPUR.pdf'
PRP helpURL 'https://upverter.com/upn/revision/a05e95a0cb7f20b8/'
PRP Manufacturer 'Texas Instruments'
PRP Max_Duty_Cycle '55%'
PRP Max_Supply_Voltage '17V'
PRP Min_Supply_Voltage '3V'
PRP Nominal_Supply_Current '5mA'
PRP Number_Of_Outputs '1'
PRP Operating_Temperature_Range '-40°C to +150°C'
PRP Output_Type 'AdjustableProgrammable'
PRP Output_Voltage '0.8-5.5V'
PRP PackageReference 'VQFN-HR10'
PRP Part_Number 'TPS62913RPUR'
PRP PartNumber 'TPS62913RPUR'
PRP RoHS 'UNKNOWN'
PRP SizeZ_mm '1mm'
PRP Standoff_Height '0mm'
PRP Switching_Frequency '1/2.2MHz'
PRP Switching_Topology 'Buck'
PRP TJmax_C '+150°C'
TOP 0 2.5103349 0.9318391 180 N 211 1 U29-1
TOP 1 2.5034451 0.9515241 180 N 207 2 U29-2
TOP 2 2.5103348 0.9712092 180 N 175 38 U29-3
TOP 3 2.4483269 0.9712092 180 N 284 329 U29-4
TOP 4 2.4414372 0.9515241 180 N 247 1 U29-5
TOP 5 2.4483269 0.9318392 180 N 157 46 U29-6
TOP 6 2.4463585 0.9052643 180 N 284 330 U29-7
TOP 7 2.4660435 0.9052643 180 N 209 1 U29-8
TOP 8 2.4857285 0.9052643 180 N 210 2 U29-9
TOP 9 2.5054136 0.9052643 180 N 208 1 U29-10
#
# CMP 104
CMP 56 4.8272047 1.4564989 0 N U23 TS3DDR3812RUAR ;0=1,1=0.0461
PRP -3Db_Bandwith '1.675GHz'
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'No'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/ts3ddr3812.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/GPN'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/GPN/datasheet'
PRP CompType 'IC'
PRP DataSheet 'http://www.ti.com/lit/ds/symlink/ts3ddr3812.pdf'
PRP Datasheet_Path 'datasheets/IC-TS3DDR3812RUAR.pdf'
PRP Digikey_Description 'IC MUX/DEMUX DDR3 1:2 42WQFN'
PRP Digikey_Part_Number '296-28307-1-ND'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP helpURL 'https://upverter.com/upn/revision/ade7f521fbdb6cf8/'
PRP Lead_free 'Yes'
PRP Manufacturer 'Texas Instruments'
PRP Max_Supply_Voltage '3.6V'
PRP Min_Supply_Voltage '3V'
PRP MountType ''
PRP Mouser_Description 'Multiplexer Switch ICs 12-Channel,1:2 MUX/ DEMUX Switch'
PRP Mouser_Part_Number '595-TS3DDR3812RUAR'
PRP Mux_Demux_Ratio '1:2'
PRP Nominal_Supply_Current '300uA'
PRP On_State_Resistance '8O'
PRP Operating_Temperature_Range '-40°C to +85°C'
PRP PackageDescription ''
PRP PackageReference 'WQFN42'
PRP Part_Number 'TS3DDR3812RUAR'
PRP PartNumber 'TS3DDR3812RUAR'
PRP PositionCount '12'
PRP Rating ''
PRP RoHS 'TRUE'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm '0.8mm'
PRP Standoff_Height '0mm'
PRP TaMax_C '+85°C'
PRP TaMin_C '-40°C'
TOP 0 4.7622441 1.6139792 0 N 159 139 U23-1
TOP 1 4.7622441 1.5942942 0 N 79 0 U23-2
TOP 2 4.7622441 1.5746091 0 N 77 0 U23-3
TOP 3 4.7622441 1.5549241 0 N 75 0 U23-4
TOP 4 4.7622441 1.5352391 0 N 73 0 U23-5
TOP 5 4.7622441 1.515554 0 N 71 0 U23-6
TOP 6 4.7622441 1.495869 0 N 67 0 U23-7
TOP 7 4.7622441 1.4761839 0 N 99 0 U23-8
TOP 8 4.7622441 1.4564989 0 N 98 2 U23-9
TOP 9 4.7622441 1.4368139 0 N 98 1 U23-10
TOP 10 4.7622441 1.4171288 0 N 58 1 U23-11
TOP 11 4.7622441 1.3974438 0 N 56 1 U23-12
TOP 12 4.7622441 1.3777587 0 N 54 1 U23-13
TOP 13 4.7622441 1.3580737 0 N 52 1 U23-14
TOP 14 4.7622441 1.3383887 0 N 50 1 U23-15
TOP 15 4.7622441 1.3187036 0 N 48 1 U23-16
TOP 16 4.7622441 1.2990186 0 N 159 138 U23-17
TOP 17 4.7976771 1.2832706 0 N 49 0 U23-18
TOP 18 4.8173622 1.2832706 0 N 490 1 U23-19
TOP 19 4.8370472 1.2832706 0 N 51 1 U23-20
TOP 20 4.8567323 1.2832706 0 N 480 1 U23-21
TOP 21 4.8921653 1.2990186 0 N 53 0 U23-22
TOP 22 4.8921653 1.3187036 0 N 482 1 U23-23
TOP 23 4.8921653 1.3383887 0 N 55 0 U23-24
TOP 24 4.8921653 1.3580737 0 N 484 1 U23-25
TOP 25 4.8921653 1.3777587 0 N 57 1 U23-26
TOP 26 4.8921653 1.3974438 0 N 486 1 U23-27
TOP 27 4.8921653 1.4171288 0 N 59 0 U23-28
TOP 28 4.8921653 1.4368139 0 N 488 1 U23-29
TOP 29 4.8921653 1.4564989 0 N 159 137 U23-30
TOP 30 4.8921653 1.4761839 0 N 68 1 U23-31
TOP 31 4.8921653 1.495869 0 N 503 1 U23-32
TOP 32 4.8921653 1.515554 0 N 72 1 U23-33
TOP 33 4.8921653 1.5352391 0 N 493 3 U23-34
TOP 34 4.8921653 1.5549241 0 N 74 1 U23-35
TOP 35 4.8921653 1.5746091 0 N 495 3 U23-36
TOP 36 4.8921653 1.5942942 0 N 76 1 U23-37
TOP 37 4.8921653 1.6139792 0 N 497 3 U23-38
TOP 38 4.8567323 1.6297272 0 N 499 3 U23-39
TOP 39 4.8370472 1.6297272 0 N 78 1 U23-40
TOP 40 4.8173622 1.6297272 0 N 501 3 U23-41
TOP 41 4.7976771 1.6297272 0 N 80 1 U23-42
TOP 42 4.8272047 1.4564989 0 N 284 389 U23-43
#
# CMP 105
CMP 29 0.7552962 0.365 270 N U21 SN74AHC1G02DRLR ;0=1,1=0.0236
PRP 3-State_Output 'No'
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer 'Texas Instruments'
PRP Alternate_PartNumber ''
PRP Bits(#) '1'
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/SN74AHC1G02.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/SN74AHC1G02'
PRP CompType 'IC'
PRP DatasheetVersion 'SCLS342M'
PRP F_@_Nom_Voltage(Max)(Mhz) '75'
PRP Gate_Type 'NOR'
PRP Generic_Part_Number 'SN74AHC1G02'
PRP ICC_@_Nom_Voltage(Max)(mA) '0.01'
PRP Input_Type 'CMOS'
PRP Logic 'True'
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP Operating_Temperature_Range(C) '-40 to 125,-40 to 85'
PRP Output_Drive_(IOL/IOH)(Max)(mA) '50/-50'
PRP Output_Type 'CMOS'
PRP PackageDescription 'SOT-OTHER-5'
PRP PackageReference 'DRL0005A'
PRP PartId '1'
PRP PartNumber 'SN74AHC1G02DRLR'
PRP Rating 'Catalog'
PRP RoHS 'Y'
PRP Schmitt_Trigger 'No'
PRP SizeArea_mm2 '2.56'
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm '1.6'
PRP SizeY_mm '1.6'
PRP SizeZ_mm '0.6'
PRP Sub-Family 'NAND Gate'
PRP Technology_Family 'AHC'
PRP tpd_@_Nom_Voltage(Max)(ns) '11.4,7.5'
PRP U/M ''
PRP VCC(Max)(V) '5.5'
PRP VCC(Min)(V) '2'
PRP Voltage(Nom)(V) '3.3,5'
TOP 0 0.7356111 0.3358662 180 N 185 2 U21-1
TOP 1 0.7552961 0.3358662 180 N 183 2 U21-2
TOP 2 0.7749812 0.3358661 180 N 284 432 U21-3
TOP 3 0.7749811 0.394134 180 N 1 0 U21-4
TOP 4 0.7356111 0.3941339 180 N 152 20 U21-5
#
# CMP 106
CMP 24 1.0385372 0.4369927 90 N U20 TPD4E02B04DQAR ;0=1,1=0.0217
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer 'Texas Instruments'
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/tpd4e02b04.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/tpd4e02b04'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/tpd4e02b04/datasheet'
PRP CompType 'IC'
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP PackageDescription 'USON-10'
PRP PackageReference 'DQA0010A'
PRP PartNumber 'TPD4E02B04DQAR'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '7.0'
PRP SizeX_mm '1.0'
PRP SizeY_mm '2.5'
PRP SizeZ_mm '0.55'
TOP 0 1.0779073 0.4534297 0 N 0 123 U20-1
TOP 1 1.0582223 0.4534297 0 N 0 124 U20-2
TOP 2 1.0385373 0.4534297 0 N 284 260 U20-3
TOP 3 1.0188522 0.4534297 0 N 179 0 U20-4
TOP 4 0.9991672 0.4534297 0 N 178 0 U20-5
TOP 5 0.9991672 0.4205557 0 N 178 1 U20-6
TOP 6 1.0188522 0.4205557 0 N 179 1 U20-7
TOP 7 1.0385373 0.4205557 0 N 284 261 U20-8
TOP 8 1.0582223 0.4205557 0 N 0 125 U20-9
TOP 9 1.0779073 0.4205557 0 N 0 126 U20-10
#
# CMP 107
CMP 31 1.6769236 0.7559051 0 N U19 TPS22965TDSGRQ1 ;0=1,1=0.0315
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer 'Texas Instruments'
PRP Alternate_PartNumber 'TPS22965TDSGTQ1'
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/tps22965-q1.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/tps22965-q1'
PRP CompType 'IC'
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP PackageDescription 'WSON-8'
PRP PackageReference 'DSG0008B'
PRP PartNumber 'TPS22965TDSGRQ1'
PRP RoHS 'Y'
PRP SizeArea_mm2 '4.0'
PRP SizeAreaWB_mm2 '9.0'
PRP SizeX_mm '2.0'
PRP SizeY_mm '2.0'
PRP SizeZ_mm '0.8'
PRP U/M 'EA'
TOP 0 1.639522 0.7854326 270 N 152 23 U19-1
TOP 1 1.639522 0.7657476 270 N 152 22 U19-2
TOP 2 1.639522 0.7460625 270 N 190 1 U19-3
TOP 3 1.639522 0.7263775 270 N 152 21 U19-4
TOP 4 1.7143252 0.7263775 270 N 284 434 U19-5
TOP 5 1.7143252 0.7460625 270 N 191 1 U19-6
TOP 6 1.7143252 0.7657476 270 N 157 59 U19-7
TOP 7 1.7143252 0.7854326 270 N 157 58 U19-8
TOP 8 1.6769236 0.7559051 0 N 284 433 U19-9
#
# CMP 108
CMP 57 0.5001972 0.3450849 0 N U18 TUSB320LIRWBR ;0=1,1=0.0157
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer 'Texas Instruments'
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/tusb320li.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/tusb320li'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/tusb320li/datasheet'
PRP CompType 'IC'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP Operating_Temperature_Range '-40 to 85 C'
PRP PackageDescription 'X2QFN-12'
PRP PackageReference 'RWB0012A'
PRP PartNumber 'TUSB320LIRWBR'
PRP Rating 'Catalog'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.56'
PRP SizeAreaWB_mm2 '6.76'
PRP SizeX_mm '1.6'
PRP SizeY_mm '1.6'
PRP SizeZ_mm '0.4'
TOP 0 0.4746065 0.3529589 0 N 179 2 U18-1
TOP 1 0.4746065 0.3372109 0 N 178 2 U18-2
TOP 2 0.4765752 0.3155573 270 N 181 1 U18-3
TOP 3 0.492323 0.3155573 270 N 180 1 U18-4
TOP 4 0.5080711 0.3155573 270 N 189 1 U18-5
TOP 5 0.5238191 0.3155573 270 N 182 1 U18-6
TOP 6 0.5257877 0.3372109 180 N 186 1 U18-7
TOP 7 0.5257877 0.3529589 180 N 184 1 U18-8
TOP 8 0.5238191 0.3746125 90 N 187 1 U18-9
TOP 9 0.5080711 0.3746125 90 N 284 435 U18-10
TOP 10 0.492323 0.3746125 90 N 188 1 U18-11
TOP 11 0.476575 0.3746125 90 N 152 24 U18-12
#
# CMP 109
CMP 24 5.0354046 0.4842577 270 N U15 TPD4E02B04DQAR ;0=1,1=0.0217
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer 'Texas Instruments'
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/tpd4e02b04.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/tpd4e02b04'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/tpd4e02b04/datasheet'
PRP CompType 'IC'
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP PackageDescription 'USON-10'
PRP PackageReference 'DQA0010A'
PRP PartNumber 'TPD4E02B04DQAR'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '7.0'
PRP SizeX_mm '1.0'
PRP SizeY_mm '2.5'
PRP SizeZ_mm '0.55'
TOP 0 4.9960345 0.4678207 180 N 577 1 U15-1
TOP 1 5.0157195 0.4678207 180 N 576 1 U15-2
TOP 2 5.0354045 0.4678207 180 N 284 282 U15-3
TOP 3 5.0550896 0.4678207 180 N 575 1 U15-4
TOP 4 5.0747746 0.4678207 180 N 574 1 U15-5
TOP 5 5.0747746 0.5006947 180 N 574 2 U15-6
TOP 6 5.0550896 0.5006947 180 N 575 2 U15-7
TOP 7 5.0354045 0.5006947 180 N 284 283 U15-8
TOP 8 5.0157195 0.5006947 180 N 576 2 U15-9
TOP 9 4.9960345 0.5006947 180 N 577 2 U15-10
#
# CMP 110
CMP 24 4.825 0.4841169 270 N U14 TPD4E02B04DQAR ;0=1,1=0.0217
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer 'Texas Instruments'
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/tpd4e02b04.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/tpd4e02b04'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/tpd4e02b04/datasheet'
PRP CompType 'IC'
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP PackageDescription 'USON-10'
PRP PackageReference 'DQA0010A'
PRP PartNumber 'TPD4E02B04DQAR'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '7.0'
PRP SizeX_mm '1.0'
PRP SizeY_mm '2.5'
PRP SizeZ_mm '0.55'
TOP 0 4.7856299 0.4676799 180 N 583 2 U14-1
TOP 1 4.8053149 0.4676799 180 N 582 2 U14-2
TOP 2 4.8249999 0.4676799 180 N 284 290 U14-3
TOP 3 4.844685 0.4676799 180 N 581 2 U14-4
TOP 4 4.86437 0.4676799 180 N 580 2 U14-5
TOP 5 4.86437 0.5005539 180 N 580 3 U14-6
TOP 6 4.844685 0.5005539 180 N 581 3 U14-7
TOP 7 4.8249999 0.5005539 180 N 284 291 U14-8
TOP 8 4.8053149 0.5005539 180 N 582 3 U14-9
TOP 9 4.7856299 0.5005539 180 N 583 3 U14-10
#
# CMP 111
CMP 24 2.18 0.465 270 N U13 TPD4E02B04DQAR ;0=1,1=0.0217
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer 'Texas Instruments'
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/tpd4e02b04.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/tpd4e02b04'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/tpd4e02b04/datasheet'
PRP CompType 'IC'
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP PackageDescription 'USON-10'
PRP PackageReference 'DQA0010A'
PRP PartNumber 'TPD4E02B04DQAR'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '7.0'
PRP SizeX_mm '1.0'
PRP SizeY_mm '2.5'
PRP SizeZ_mm '0.55'
TOP 0 2.1406299 0.448563 180 N 589 2 U13-1
TOP 1 2.1603149 0.448563 180 N 588 2 U13-2
TOP 2 2.1799999 0.448563 180 N 284 307 U13-3
TOP 3 2.199685 0.448563 180 N 587 2 U13-4
TOP 4 2.21937 0.448563 180 N 586 2 U13-5
TOP 5 2.21937 0.481437 180 N 586 3 U13-6
TOP 6 2.199685 0.481437 180 N 587 3 U13-7
TOP 7 2.1799999 0.481437 180 N 284 308 U13-8
TOP 8 2.1603149 0.481437 180 N 588 3 U13-9
TOP 9 2.1406299 0.481437 180 N 589 3 U13-10
#
# CMP 112
CMP 24 1.835 0.464476 270 N U12 TPD4E02B04DQAR ;0=1,1=0.0217
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer 'Texas Instruments'
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/tpd4e02b04.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/tpd4e02b04'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/tpd4e02b04/datasheet'
PRP CompType 'IC'
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP PackageDescription 'USON-10'
PRP PackageReference 'DQA0010A'
PRP PartNumber 'TPD4E02B04DQAR'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '7.0'
PRP SizeX_mm '1.0'
PRP SizeY_mm '2.5'
PRP SizeZ_mm '0.55'
TOP 0 1.7956299 0.448039 180 N 595 1 U12-1
TOP 1 1.8153149 0.448039 180 N 594 1 U12-2
TOP 2 1.8349999 0.448039 180 N 284 301 U12-3
TOP 3 1.854685 0.448039 180 N 593 1 U12-4
TOP 4 1.87437 0.448039 180 N 592 1 U12-5
TOP 5 1.87437 0.480913 180 N 592 2 U12-6
TOP 6 1.854685 0.480913 180 N 593 2 U12-7
TOP 7 1.8349999 0.480913 180 N 284 302 U12-8
TOP 8 1.8153149 0.480913 180 N 594 2 U12-9
TOP 9 1.7956299 0.480913 180 N 595 2 U12-10
#
# CMP 113
CMP 54 0.4881971 0.62 90 N U11 TPD6E001RSER ;0=1,1=0.0236
PRP 1394_/_Firewire 'TRUE'
PRP Breakdown_Voltage(Min)(V) '11'
PRP ComponentLink1Description 'Manufacturer URL'
PRP ComponentLink1URL 'http://www.ti.com/'
PRP ComponentLink2Description 'Datasheet'
PRP ComponentLink2URL 'http://www.ti.com/general/docs/lit/getliterature.tsp?genericPartNumber=TPD6E001&fileType=pdf'
PRP ComponentLink3Description 'URL Link1'
PRP ComponentLink3URL 'SamplesURL:http://www.ti.com/product/tpd6e001#samples'
PRP Ctotal(Typ)(pF) ''
PRP DatasheetVersion 'SLLS685C'
PRP Differential_Capacitance(pF) ''
PRP Eco-Plan 'Green (RoHS & no Sb/Br)'
PRP HDMI ''
PRP IEC_61000-4-2_Air-Gap(+/-_kV) '15'
PRP IEC_61000-4-2_Air-Gap(Typ)(+/-_kV) ''
PRP IEC_61000-4-2_Contact(+/-_kV) '8'
PRP IEC_61000-4-2_Contact(Typ)(+/-_kV) ''
PRP IO_Capacitance(Typ)(pF) '1.5'
PRP IO_Leakage_Current(nA) '1'
PRP Manufacturer 'Texas Instruments'
PRP Mounting_Technology 'Surface Mount'
PRP Number_of_Channels ''
PRP PackageDescription '10-Leads Plastic Quad Flatpack No-Lead, 2 x 1.5 x 0.55 mm Body, 0.5 mm Pitch'
PRP PackageReference 'RSE0010A'
PRP PackageVersion 'revD, Jan-2011'
PRP PartNumber 'TPD6E001RSER'
PRP Serial_ATA_/_eSATA 'TRUE'
PRP SubFamily 'ESD Solution'
PRP USB_Full_Speed ''
PRP USB_High_Speed 'TRUE'
PRP USB_Super_Speed ''
TOP 0 0.5177247 0.6465748 0 N 437 2 U11-1
TOP 1 0.4980396 0.6465748 0 N 435 2 U11-2
TOP 2 0.4783546 0.6465748 0 N 433 2 U11-3
TOP 3 0.4586696 0.6465748 0 N 0 138 U11-4
TOP 4 0.452764 0.6199999 90 N 248 1 U11-5
TOP 5 0.4586696 0.5934252 0 N 431 2 U11-6
TOP 6 0.4783546 0.5934252 0 N 429 2 U11-7
TOP 7 0.4980396 0.5934252 0 N 427 2 U11-8
TOP 8 0.5177247 0.5934252 0 N 0 137 U11-9
TOP 9 0.5236302 0.6199999 90 N 161 6 U11-10
#
# CMP 114
CMP 29 0.2927818 0.6142126 0 N U10 TPD2E001DRLR ;0=1,1=0.0236
PRP 1394_/_Firewire ''
PRP Breakdown_Voltage(Min)(V) '11'
PRP ComponentLink1Description 'Manufacturer URL'
PRP ComponentLink1URL 'http://www.ti.com/'
PRP ComponentLink2Description 'Datasheet'
PRP ComponentLink2URL 'http://www.ti.com/general/docs/lit/getliterature.tsp?genericPartNumber=TPD2E001&fileType=pdf'
PRP ComponentLink3Description 'URL Link1'
PRP ComponentLink3URL 'SamplesURL:http://www.ti.com/product/tpd2e001#samples'
PRP Ctotal(Typ)(pF) ''
PRP DatasheetVersion 'SLLS684F'
PRP Differential_Capacitance(pF) ''
PRP Eco-Plan 'Green (RoHS & no Sb/Br)'
PRP HDMI ''
PRP IEC_61000-4-2_Air-Gap(+/-_kV) '15'
PRP IEC_61000-4-2_Air-Gap(Typ)(+/-_kV) ''
PRP IEC_61000-4-2_Contact(+/-_kV) '8'
PRP IEC_61000-4-2_Contact(Typ)(+/-_kV) ''
PRP IO_Capacitance(Typ)(pF) '1.5'
PRP IO_Leakage_Current(nA) '1'
PRP Manufacturer 'Texas Instruments'
PRP Mounting_Technology 'Surface Mount'
PRP Number_of_Channels ''
PRP PackageDescription '5-Pin Plastic Small Outline, Flat Lead 0.5 mm Pitch'
PRP PackageReference 'DRL0005A'
PRP PackageVersion 'revD, Aug-2007'
PRP PartNumber 'TPD2E001DRLR'
PRP Serial_ATA_/_eSATA ''
PRP SubFamily 'ESD Solution'
PRP USB_Full_Speed ''
PRP USB_High_Speed 'TRUE'
PRP USB_Super_Speed ''
TOP 0 0.2636479 0.6338977 270 N 161 5 U10-1
TOP 1 0.2636479 0.6142127 270 N 0 127 U10-2
TOP 2 0.2636479 0.5945276 270 N 439 1 U10-3
TOP 3 0.3219157 0.5945276 270 N 248 0 U10-4
TOP 4 0.3219157 0.6338977 270 N 0 128 U10-5
#
# CMP 115
CMP 18 0.7410262 0.6785954 180 N U8 TPS22918TDBVTQ1 ;0=1,1=0.0571
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer 'Texas Instruments'
PRP Alternate_PartNumber 'TPS22918TDBVRQ1'
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/tps22918-q1.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/tps22918-q1'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/tps22918-q1/datasheet'
PRP CompType 'IC'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP Operating_Temperature_Range '-40 to 105 C'
PRP PackageDescription 'SOT-23-6'
PRP PackageReference 'DBV0006A'
PRP PartNumber 'TPS22918TDBVTQ1'
PRP Rating 'Automotive'
PRP RoHS 'Y'
PRP SizeArea_mm2 '8.12'
PRP SizeAreaWB_mm2 '14.82'
PRP SizeX_mm '2.8'
PRP SizeY_mm '2.9'
PRP SizeZ_mm '1.45'
TOP 0 0.7951601 0.6411938 90 N 159 176 U8-1
TOP 1 0.7951601 0.6785954 90 N 284 436 U8-2
TOP 2 0.7951601 0.7159969 90 N 231 2 U8-3
TOP 3 0.6868924 0.7159969 90 N 0 139 U8-4
TOP 4 0.6868924 0.6785954 90 N 161 8 U8-5
TOP 5 0.6868924 0.6411938 90 N 161 7 U8-6
#
# CMP 116
CMP 42 2.875 1.0794998 90 N U7 S25FL128SAGNFI000 ;0=1,1=0.0000
PRP Access_Time '8ns'
PRP AEC_Qualified 'No'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.cypress.com/file/448601/download'
PRP DataSheet 'https://www.cypress.com/file/448601/download'
PRP Datasheet_Path 'datasheets/IC-S25FL128SAGNFI000.pdf'
PRP Digikey_Description 'IC FLASH 128MBIT SPI/QUAD 8WSON'
PRP Digikey_Part_Number '1274-1178-ND'
PRP Frequency_Fixed '133MHz'
PRP helpURL 'https://upverter.com/upn/revision/39782ed3cd62795d/'
PRP Interface 'SPI'
PRP Lead_free 'Yes'
PRP Manufacturer 'Cypress Semiconductor'
PRP Max_Supply_Voltage '3.6V'
PRP Memory_Size '128Mbits'
PRP Memory_Type 'FLASH'
PRP Min_Supply_Voltage '1.65V'
PRP Mouser_Part_Number '797-25FL128SAGNFI000'
PRP Nominal_Supply_Current '16-100mA'
PRP Operating_Temperature_Range '-40°C to +85°C'
PRP PackageReference 'WSON8'
PRP Part_Number 'S25FL128SAGNFI000'
PRP PartNumber 'S25FL128SAGNFI000'
PRP RoHS 'TRUE'
PRP SizeZ_mm '0.8mm'
PRP Standoff_Height '0mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 '1274-1178-ND'
PRP Supplier_Part_Number_2 '797-25FL128SAGNFI000'
PRP TaMax_C '+85°C'
PRP TaMin_C '-40°C'
TOP 0 2.95 1.2320798 90 N 416 1 U7-1
TOP 1 2.9 1.2320798 90 N 242 1 U7-2
TOP 2 2.85 1.2320798 90 N 18 1 U7-3
TOP 3 2.8 1.2320798 90 N 284 437 U7-4
TOP 4 2.8 0.9269198 90 N 243 1 U7-5
TOP 5 2.85 0.9269198 90 N 417 1 U7-6
TOP 6 2.9 0.9269198 90 N 17 1 U7-7
TOP 7 2.95 0.9269198 90 N 159 177 U7-8
TOP 8 2.875 1.0794998 90 N 284 438 U7-9
#
# CMP 117
CMP 20 2.1086709 0.7523875 180 N U6 SN74LVC1G17DCKR ;0=1,1=0.0433
PRP 3-State_Output 'No'
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Bits(#) '1'
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/sn74lvc1g17.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/sn74lvc1g17'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/sn74lvc1g17/datasheet'
PRP CompType 'IC'
PRP DatasheetVersion 'SCES351V'
PRP F_@_Nom_Voltage(Max)(Mhz) '150'
PRP Generic_Part_Number 'SN74LVC1G17'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP ICC_@_Nom_Voltage(Max)(mA) '0.01'
PRP Input_Type 'CMOS/TTL'
PRP Logic 'True'
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP Operating_Temperature_Range(C) '-40 to 125,-40 to 85'
PRP Output_Drive_(IOL/IOH)(Max)(mA) '32/-32'
PRP Output_Type 'CMOS'
PRP PackageDescription 'SOT-SC70-5'
PRP PackageReference 'DCK0005A'
PRP PartId '1'
PRP PartNumber 'SN74LVC1G17DCKR'
PRP Rating 'Catalog'
PRP RoHS 'Y'
PRP Schmitt_Trigger 'Yes'
PRP SizeArea_mm2 '4.2'
PRP SizeAreaWB_mm2 '9.3'
PRP SizeX_mm '2.1'
PRP SizeY_mm '2.0'
PRP SizeZ_mm '1.1'
PRP Sub-Family 'Non-Inverting Buffer/Driver'
PRP Technology_Family 'LVC'
PRP tpd_@_Nom_Voltage(Max)(ns) '11,6.5,5.5,5'
PRP VCC(Max)(V) '5.5'
PRP VCC(Min)(V) '1.65'
PRP Voltage(Nom)(V) '1.8,2.5,3.3,5'
TOP 0 2.1529622 0.7267969 90 N 0 129 U6-1
TOP 1 2.1529622 0.7523875 90 N 424 2 U6-2
TOP 2 2.1529622 0.777978 90 N 284 316 U6-3
TOP 3 2.0643795 0.777978 90 N 245 0 U6-4
TOP 4 2.0643795 0.7267969 90 N 153 24 U6-5
#
# CMP 118
CMP 17 2.0813112 0.911401 270 N U5 SN74LVC1G08DBVR ;0=1,1=0.0571
PRP 3-State_Output 'No'
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer 'Texas Instruments'
PRP Alternate_PartNumber ''
PRP Bits(#) '1'
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/SN74LVC1G08.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/SN74LVC1G08'
PRP CompType 'IC'
PRP DatasheetVersion 'SCES217Y'
PRP F_@_Nom_Voltage(Max)(Mhz) '150'
PRP Gate_Type 'AND'
PRP Generic_Part_Number 'SN74LVC1G08'
PRP ICC_@_Nom_Voltage(Max)(mA) '0.01'
PRP Input_Type 'CMOS/TTL'
PRP Logic 'True'
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP Operating_Temperature_Range(C) '-40 to 125,-40 to 85'
PRP Output_Drive_(IOL/IOH)(Max)(mA) '32/-32'
PRP Output_Type 'CMOS'
PRP PackageDescription 'SOT-23-5'
PRP PackageReference 'DBV0005A'
PRP PartId '1'
PRP PartNumber 'SN74LVC1G08DBVR'
PRP Rating 'Catalog'
PRP RoHS 'Y'
PRP Schmitt_Trigger 'No'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm ''
PRP Sub-Family 'AND Gate'
PRP Technology_Family 'LVC'
PRP tpd_@_Nom_Voltage(Max)(ns) '4.5,6,4,5'
PRP U/M ''
PRP VCC(Max)(V) '5.5'
PRP VCC(Min)(V) '1.65'
PRP Voltage(Nom)(V) '1.8,2.5,3.3,5'
TOP 0 2.0439096 0.8572671 180 N 220 3 U5-1
TOP 1 2.0813112 0.8572671 180 N 245 1 U5-2
TOP 2 2.1187127 0.8572671 180 N 284 317 U5-3
TOP 3 2.1187127 0.9655348 180 N 224 1 U5-4
TOP 4 2.0439096 0.9655348 180 N 153 25 U5-5
#
# CMP 119
CMP 50 3.3480537 0.4187008 270 N U3 TCA6408ARGTR ;0=1,1=0.0394
PRP 5V_Tolerant_I/O 'Yes'
PRP #_of_I/Os '8'
PRP Channel_Width ''
PRP Code_JEDEC 'MO-220'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'http://www.ti.com/general/docs/lit/getliterature.tsp?genericPartNumber=TCA6408A&fileType=pdf'
PRP ComponentLink2Description 'Package Specification'
PRP ComponentLink2URL 'http://www.ti.com/litv/pdf/mpds361'
PRP Configuration_Registers 'Yes'
PRP DatasheetVersion 'SCPS192C'
PRP Eco-Plan 'Green (RoHS & no Sb/Br)'
PRP Enable_Pin ''
PRP EXP_Pin ''
PRP fSCLK(Max)(MHz) '400'
PRP Function ''
PRP I2C_Address '0100 00x'
PRP Interrupt_Output 'Yes'
PRP Low_Power 'Yes'
PRP Manufacturer 'Texas Instruments'
PRP Master_Side_I2C_Bus_Capacitance_Supported(pF) ''
PRP Max_Frequency(kHz) '400'
PRP Mounting_Technology 'Surface Mount'
PRP No._of_Outputs '8'
PRP On-Chip_Power-on-Reset ''
PRP Open_Drain_I/O_Type ''
PRP PackageDescription '16-Pin Plastic Quad Flat No-Lead, 3 x 3 mm Body, 0.5 mm Pitch, 1.45 x 1.45 mm Exposed Pad'
PRP PackageReference 'RGT0016A'
PRP PackageVersion 'revH, Oct-2011'
PRP PartNumber 'TCA6408ARGTR'
PRP Push-Pull_I/O_Type 'Yes'
PRP Rating ''
PRP Reset_Input 'Yes'
PRP Simultaneously_Active_Channels ''
PRP Slave_Side_I2C_Bus_Capacitance_Supported(pF) ''
PRP SubFamily 'I2C IO Expander'
PRP Technology_Family ''
PRP tpd_max(ns) ''
PRP Vcc_range(V) '1.65 to 5.5'
PRP VCC(Max)(V) '5.5'
PRP VCC(Min)(V) '1.65'
PRP Voltage_Nodes(V) ''
TOP 0 3.3185261 0.3635827 180 N 219 2 U3-1
TOP 1 3.3382111 0.3635827 180 N 228 2 U3-2
TOP 2 3.3578962 0.3635827 180 N 227 2 U3-3
TOP 3 3.3775812 0.3635827 180 N 226 2 U3-4
TOP 4 3.4031718 0.3891733 270 N 225 2 U3-5
TOP 5 3.4031718 0.4088583 270 N 284 439 U3-6
TOP 6 3.4031718 0.4285434 270 N 0 140 U3-7
TOP 7 3.4031718 0.4482284 270 N 0 141 U3-8
TOP 8 3.3775812 0.4738189 180 N 0 142 U3-9
TOP 9 3.3578962 0.4738189 180 N 0 143 U3-10
TOP 10 3.3382111 0.4738189 180 N 212 1 U3-11
TOP 11 3.3185261 0.4738189 180 N 218 2 U3-12
TOP 12 3.2929356 0.4482284 270 N 217 2 U3-13
TOP 13 3.2929356 0.4285434 270 N 153 36 U3-14
TOP 14 3.2929356 0.4088583 270 N 153 37 U3-15
TOP 15 3.2929356 0.3891733 270 N 213 1 U3-16
TOP 16 3.3480537 0.4187009 270 N 284 440 U3-17
#
# CMP 120
CMP 18 2.0212399 1.279447 0 N U2 SN74LVC1G11DBVR ;0=1,1=0.0571
PRP 3-State_Output 'No'
PRP Bits(#) '1'
PRP DatasheetVersion 'SCES487F'
PRP F_@_Nom_Voltage(Max)(Mhz) '150'
PRP Gate_Type 'AND'
PRP Generic_Part_Number 'SN74LVC1G11'
PRP ICC_@_Nom_Voltage(Max)(mA) '0.01'
PRP Input_Type 'CMOS/TTL'
PRP Logic 'True'
PRP Manufacturer 'Texas Instruments'
PRP Operating_Temperature_Range(C) '-40 to 125,-40 to 85'
PRP Output_Drive_(IOL/IOH)(Max)(mA) '32/-32'
PRP Output_Type 'CMOS'
PRP PackageReference 'DBV0006A'
PRP PartId '1'
PRP Rating 'Catalog'
PRP Schmitt_Trigger 'No'
PRP Sub-Family 'AND Gate'
PRP Technology_Family 'LVC'
PRP tpd_@_Nom_Voltage(Max)(ns) '20,7.8,6.2,4.6'
PRP VCC(Max)(V) '5.5'
PRP VCC(Min)(V) '1.65'
PRP Voltage(Nom)(V) '1.8,2.5,3.3,5'
TOP 0 1.967106 1.3168486 270 N 425 0 U2-1
TOP 1 1.967106 1.279447 270 N 284 309 U2-2
TOP 2 1.967106 1.2420455 270 N 247 0 U2-3
TOP 3 2.0753737 1.2420455 270 N 423 0 U2-4
TOP 4 2.0753737 1.279447 270 N 159 97 U2-5
TOP 5 2.0753737 1.3168486 270 N 246 0 U2-6
#
# CMP 121
CMP 67 1.265 0.9298935 0 N TP26 TESTPOINT ;0=1,1=0.0461
PRP CompType 'Testpoint'
PRP Manufacturer 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 1.265 0.9298935 0 N 285 31 TP26-1
#
# CMP 122
CMP 67 0.6747462 0.9345294 90 N TP25 TESTPOINT ;0=1,1=0.0461
PRP CompType 'Testpoint'
PRP Manufacturer 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 0.6747462 0.9345294 90 N 168 25 TP25-1
#
# CMP 123
CMP 67 0.7484786 1.1603547 0 N TP24 TESTPOINT ;0=1,1=0.0461
PRP CompType 'Testpoint'
PRP Manufacturer 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 0.7484786 1.1603547 0 N 285 32 TP24-1
#
# CMP 124
CMP 67 0.258563 0.915 0 N TP23 TESTPOINT ;0=1,1=0.0461
PRP CompType 'Testpoint'
PRP Manufacturer 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 0.258563 0.915 0 N 176 5 TP23-1
#
# CMP 125
CMP 67 7.165 0.225 270 N TP22 TESTPOINT ;0=1,1=0.0461
PRP CompType 'Testpoint'
PRP Manufacturer 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 7.165 0.225 270 N 236 3 TP22-1
#
# CMP 126
CMP 67 6.975 1.3454505 270 N TP21 TESTPOINT ;0=1,1=0.0461
PRP CompType 'Testpoint'
PRP Manufacturer 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 6.975 1.3454505 270 N 236 2 TP21-1
#
# CMP 127
CMP 67 6.555 1.797094 90 N TP20 TESTPOINT ;0=1,1=0.0461
PRP CompType 'Testpoint'
PRP Manufacturer 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 6.555 1.797094 90 N 304 1 TP20-1
#
# CMP 128
CMP 67 6.779033 1.5139083 0 N TP19 TESTPOINT ;0=1,1=0.0461
PRP CompType 'Testpoint'
PRP Manufacturer 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 6.779033 1.5139083 0 N 163 2 TP19-1
#
# CMP 129
CMP 67 1.03 1.905 270 N TP18 TESTPOINT ;0=1,1=0.0461
PRP CompType 'Testpoint'
PRP Manufacturer 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 1.03 1.905 270 N 221 1 TP18-1
#
# CMP 130
CMP 67 5.82 1.32371 270 N TP17 TESTPOINT ;0=1,1=0.0461
PRP CompType 'Testpoint'
PRP Manufacturer 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 5.82 1.32371 270 N 284 238 TP17-1
#
# CMP 131
CMP 67 6.471651 1.3081312 270 N TP16 TESTPOINT ;0=1,1=0.0461
PRP CompType 'Testpoint'
PRP Manufacturer 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 6.471651 1.3081312 270 N 284 239 TP16-1
#
# CMP 132
CMP 67 2.445 1.228071 270 N TP15 TESTPOINT ;0=1,1=0.0461
PRP CompType 'Testpoint'
PRP Manufacturer 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 2.445 1.228071 270 N 284 240 TP15-1
#
# CMP 133
CMP 67 2.802405 1.8605118 270 N TP14 TESTPOINT ;0=1,1=0.0461
PRP CompType 'Testpoint'
PRP Manufacturer 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 2.802405 1.8605118 270 N 284 241 TP14-1
#
# CMP 134
CMP 67 1.715 0.11 270 N TP13 TESTPOINT ;0=1,1=0.0461
PRP CompType 'Testpoint'
PRP Manufacturer 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 1.715 0.11 270 N 284 242 TP13-1
#
# CMP 135
CMP 67 6.1284121 1.0947196 270 N TP12 TESTPOINT ;0=1,1=0.0461
PRP CompType 'Testpoint'
PRP Manufacturer 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 6.1284121 1.0947196 270 N 169 1 TP12-1
#
# CMP 136
CMP 67 6.0881376 1.5130412 270 N TP11 TESTPOINT ;0=1,1=0.0461
PRP CompType 'Testpoint'
PRP Manufacturer 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 6.0881376 1.5130412 270 N 170 2 TP11-1
#
# CMP 137
CMP 67 2.52 1.228071 270 N TP10 TESTPOINT ;0=1,1=0.0461
PRP CompType 'Testpoint'
PRP Manufacturer 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 2.52 1.228071 270 N 175 35 TP10-1
#
# CMP 138
CMP 67 2.8772539 1.865 270 N TP9 TESTPOINT ;0=1,1=0.0461
PRP CompType 'Testpoint'
PRP Manufacturer 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 2.8772539 1.865 270 N 159 65 TP9-1
#
# CMP 139
CMP 67 1.86 0.8489623 270 N TP8 TESTPOINT ;0=1,1=0.0461
PRP CompType 'Testpoint'
PRP Manufacturer 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 1.86 0.8489623 270 N 157 39 TP8-1
#
# CMP 140
CMP 67 6.7005666 0.6114983 180 N TP7 TESTPOINT ;0=1,1=0.0461
PRP CompType 'Testpoint'
PRP Manufacturer 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 6.7005666 0.6114983 180 N 164 2 TP7-1
#
# CMP 141
CMP 67 2.6668507 0.48 270 N TP6 TESTPOINT ;0=1,1=0.0461
PRP CompType 'Testpoint'
PRP Manufacturer 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 2.6668507 0.48 270 N 284 256 TP6-1
#
# CMP 142
CMP 67 0.5075065 0.2593054 270 N TP5 TESTPOINT ;0=1,1=0.0461
PRP CompType 'Testpoint'
PRP Manufacturer 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 0.5075065 0.2593054 270 N 189 0 TP5-1
#
# CMP 143
CMP 67 1.44 0.5488498 180 N TP4 TESTPOINT ;0=1,1=0.0461
PRP CompType 'Testpoint'
PRP Manufacturer 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 1.44 0.5488498 180 N 152 7 TP4-1
#
# CMP 144
CMP 67 0.6215522 0.5054488 270 N TP3 TESTPOINT ;0=1,1=0.0461
PRP CompType 'Testpoint'
PRP Manufacturer 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 0.6215522 0.5054488 270 N 187 0 TP3-1
#
# CMP 145
CMP 68 3.0617855 0.8644343 270 N TP2 TP_SM_1MM ;0=1,1=0.0461
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ClassName ''
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'https://sps06.itg.ti.com/sites/KMS/crossdivteams/altium/docs/ComponentDatasheets/PROBE_TEST_POINT.png'
PRP CompType 'Test Point'
PRP Key 'TP_SM_1MM'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Any'
PRP MountType 'SMT'
PRP Note ''
PRP PackageReference '1mm Test Point, SMT'
PRP PartNumber 'TP_SM_1MM'
PRP Publisher 'Texas Instruments'
PRP RoHS ''
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Value ''
TOP 0 3.0617855 0.8644343 270 N 519 0 TP2-1
#
# CMP 146
CMP 68 3.0988659 0.9227513 270 N TP1 TP_SM_1MM ;0=1,1=0.0461
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ClassName ''
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'https://sps06.itg.ti.com/sites/KMS/crossdivteams/altium/docs/ComponentDatasheets/PROBE_TEST_POINT.png'
PRP CompType 'Test Point'
PRP Key 'TP_SM_1MM'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Any'
PRP MountType 'SMT'
PRP Note ''
PRP PackageReference '1mm Test Point, SMT'
PRP PartNumber 'TP_SM_1MM'
PRP Publisher 'Texas Instruments'
PRP RoHS ''
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Value ''
TOP 0 3.0988659 0.9227513 270 N 559 1 TP1-1
#
# CMP 147
CMP 35 1.375 2.2188184 180 N SW4 434351045816 ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP Circuit 'SPST-NO'
PRP Coil_Resistance_ohm '100mO'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.we-online.com/catalog/datasheet/434351045816.pdf'
PRP Contact_Current_Rating '50mA'
PRP DataSheet 'https://www.we-online.com/catalog/datasheet/434351045816.pdf'
PRP Datasheet_Path 'datasheets/Switch-434351045816.pdf'
PRP Digikey_Description 'SWITCH TACTILE SPST-NO 0.05A 12V'
PRP Digikey_Part_Number '732-7057-1-ND'
PRP Electromechanical_Life '200000Cycles'
PRP helpURL 'https://upverter.com/upn/revision/bab06782c464a9f5/'
PRP Lead_free 'Yes'
PRP Manufacturer 'Wurth Electronics'
PRP MountType 'Surface Mount'
PRP Mouser_Part_Number '710-434351045816'
PRP Operating_Force '160gf'
PRP Operating_Temperature_Range '-40°C to +85°C'
PRP PackageReference 'SMT_SW_4MM7_4MM5'
PRP Part_Number '434351045816'
PRP PartNumber '434351045816'
PRP RoHS 'TRUE'
PRP SizeZ_mm '1.75mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 '732-7057-1-ND'
PRP Supplier_Part_Number_2 '710-434351045816'
PRP VDC_V '12V'
TOP 0 1.2647638 2.1853538 180 N 284 442 SW4-1
TOP 1 1.2647638 2.252283 180 N 283 4 SW4-2
TOP 2 1.4852362 2.1853538 180 N 284 441 SW4-3
TOP 3 1.4852362 2.252283 180 N 283 3 SW4-4
#
# CMP 148
CMP 35 0.95 2.2188189 180 N SW3 434351045816 ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP Circuit 'SPST-NO'
PRP Coil_Resistance_ohm '100mO'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.we-online.com/catalog/datasheet/434351045816.pdf'
PRP Contact_Current_Rating '50mA'
PRP DataSheet 'https://www.we-online.com/catalog/datasheet/434351045816.pdf'
PRP Datasheet_Path 'datasheets/Switch-434351045816.pdf'
PRP Digikey_Description 'SWITCH TACTILE SPST-NO 0.05A 12V'
PRP Digikey_Part_Number '732-7057-1-ND'
PRP Electromechanical_Life '200000Cycles'
PRP helpURL 'https://upverter.com/upn/revision/bab06782c464a9f5/'
PRP Lead_free 'Yes'
PRP Manufacturer 'Wurth Electronics'
PRP MountType 'Surface Mount'
PRP Mouser_Part_Number '710-434351045816'
PRP Operating_Force '160gf'
PRP Operating_Temperature_Range '-40°C to +85°C'
PRP PackageReference 'SMT_SW_4MM7_4MM5'
PRP Part_Number '434351045816'
PRP PartNumber '434351045816'
PRP RoHS 'TRUE'
PRP SizeZ_mm '1.75mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 '732-7057-1-ND'
PRP Supplier_Part_Number_2 '710-434351045816'
PRP VDC_V '12V'
TOP 0 0.8397638 2.1853543 180 N 284 366 SW3-1
TOP 1 0.8397638 2.2522835 180 N 241 3 SW3-2
TOP 2 1.0602362 2.1853543 180 N 284 367 SW3-3
TOP 3 1.0602362 2.2522835 180 N 241 4 SW3-4
#
# CMP 149
CMP 35 0.477559 2.218819 180 N SW2 434351045816 ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP Circuit 'SPST-NO'
PRP Coil_Resistance_ohm '100mO'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.we-online.com/catalog/datasheet/434351045816.pdf'
PRP Contact_Current_Rating '50mA'
PRP DataSheet 'https://www.we-online.com/catalog/datasheet/434351045816.pdf'
PRP Datasheet_Path 'datasheets/Switch-434351045816.pdf'
PRP Digikey_Description 'SWITCH TACTILE SPST-NO 0.05A 12V'
PRP Digikey_Part_Number '732-7057-1-ND'
PRP Electromechanical_Life '200000Cycles'
PRP helpURL 'https://upverter.com/upn/revision/bab06782c464a9f5/'
PRP Lead_free 'Yes'
PRP Manufacturer 'Wurth Electronics'
PRP MountType 'Surface Mount'
PRP Mouser_Part_Number '710-434351045816'
PRP Operating_Force '160gf'
PRP Operating_Temperature_Range '-40°C to +85°C'
PRP PackageReference 'SMT_SW_4MM7_4MM5'
PRP Part_Number '434351045816'
PRP PartNumber '434351045816'
PRP RoHS 'TRUE'
PRP SizeZ_mm '1.75mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 '732-7057-1-ND'
PRP Supplier_Part_Number_2 '710-434351045816'
PRP VDC_V '12V'
TOP 0 0.3673228 2.1853544 180 N 284 364 SW2-1
TOP 1 0.3673228 2.2522836 180 N 244 2 SW2-2
TOP 2 0.5877952 2.1853544 180 N 284 365 SW2-3
TOP 3 0.5877952 2.2522836 180 N 244 3 SW2-4
#
# CMP 150
CMP 34 3.6622994 0.194508 270 N SW1 416131160804 ;0=1,1=0.0461
PRP AEC_Qualified 'No'
PRP Circuit '4PST'
PRP Coil_Resistance_ohm '100mO'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.we-online.com/catalog/datasheet/416131160804.pdf'
PRP Contact_Current_Rating '25mA'
PRP DataSheet 'https://www.we-online.com/catalog/datasheet/416131160804.pdf'
PRP Datasheet_Path 'datasheets/Switch-416131160804.pdf'
PRP Digikey_Description 'SWITCH SLIDE DIP SPST 25MA 24V'
PRP Digikey_Part_Number '732-3854-1-ND'
PRP Electromechanical_Life '1000Cycles'
PRP helpURL 'https://upverter.com/upn/revision/a00acd1291e2c884/'
PRP Lead_free 'Yes'
PRP Manufacturer 'Wurth'
PRP Mouser_Description 'DIP Switches / SIP Switches WS-DISV DIP 4p SMT 1.27mm Hrztl HP'
PRP Mouser_Part_Number '710-416131160804'
PRP Operating_Temperature_Range '-40°C to +85°C'
PRP PackageReference 'SMT_SW'
PRP Part_Number '416131160804'
PRP PartNumber '416131160804'
PRP PositionCount '4'
PRP RoHS 'TRUE'
PRP SizeZ_mm '2.65mm'
PRP Standoff_Height '0mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 '732-3854-1-ND'
PRP Supplier_Part_Number_2 '710-416131160804'
PRP VDC_V '24V'
TOP 0 3.8122994 0.119508 270 N 254 1 SW1-1
TOP 1 3.8122994 0.169508 270 N 253 1 SW1-2
TOP 2 3.8122994 0.219508 270 N 252 1 SW1-3
TOP 3 3.8122994 0.269508 270 N 251 1 SW1-4
TOP 4 3.5122994 0.269508 270 N 225 3 SW1-5
TOP 5 3.5122994 0.219508 270 N 226 3 SW1-6
TOP 6 3.5122994 0.169508 270 N 227 3 SW1-7
TOP 7 3.5122994 0.119508 270 N 228 3 SW1-8
#
# CMP 151
CMP 1 1.6178741 2.2161811 90 N R279 ERJ-2RKF2200X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C86.pdf'
PRP CompType 'Resistor'
PRP EIA_Code ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF2200X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '220'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P220LCT-ND'
PRP Supplier_Part_Number_2 '64R5267'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF2200X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '220'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '220R'
PRP ValueDisplayed '220'
PRP VDC_V '50V'
TOP 0 1.6178741 2.2398031 0 N 272 1 R279-1
TOP 1 1.6178741 2.192559 0 N 159 70 R279-2
#
# CMP 152
CMP 1 2.385 1.795 180 N R278 ERJ-2GEJ102X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/DMA0000COL9.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS 'Passed with Exemption'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GEJ102X'
PRP Power_W '100mW'
PRP Published ''
PRP Publisher ''
PRP Res_ohm '1k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P1.0KJCT-ND'
PRP Supplier_Part_Number_2 '65T8247'
PRP Supplier_Part_Number_3 '667-ERJ-2GEJ102X'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '1.0k'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '1k00'
PRP ValueDisplayed '1.0k'
PRP VDC_V '50V'
TOP 0 2.408622 1.795 90 N 284 252 R278-1
TOP 1 2.3613779 1.795 90 N 105 0 R278-2
#
# CMP 153
CMP 1 1.737874 2.2161812 90 N R277 ERJ-2RKF2200X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C86.pdf'
PRP CompType 'Resistor'
PRP EIA_Code ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF2200X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '220'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P220LCT-ND'
PRP Supplier_Part_Number_2 '64R5267'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF2200X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '220'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '220R'
PRP ValueDisplayed '220'
PRP VDC_V '50V'
TOP 0 1.737874 2.2398032 0 N 273 1 R277-1
TOP 1 1.737874 2.1925591 0 N 159 69 R277-2
#
# CMP 154
CMP 1 1.9309306 1.6165686 0 N R276 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 1.9073086 1.6165686 270 N 284 243 R276-1
TOP 1 1.9545527 1.6165686 270 N 281 0 R276-2
#
# CMP 155
CMP 1 2.388009 1.676555 180 N R275 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 2.411631 1.676555 90 N 284 244 R275-1
TOP 1 2.3643869 1.676555 90 N 280 0 R275-2
#
# CMP 156
CMP 1 1.9309306 1.7398517 0 N R274 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 1.9073086 1.7398517 270 N 284 245 R274-1
TOP 1 1.9545527 1.7398517 270 N 282 0 R274-2
#
# CMP 157
CMP 1 1.8778739 2.2161813 90 N R273 ERJ-2RKF2200X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C86.pdf'
PRP CompType 'Resistor'
PRP EIA_Code ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF2200X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '220'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P220LCT-ND'
PRP Supplier_Part_Number_2 '64R5267'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF2200X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '220'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '220R'
PRP ValueDisplayed '220'
PRP VDC_V '50V'
TOP 0 1.8778739 2.2398033 0 N 274 0 R273-1
TOP 1 1.8778739 2.1925592 0 N 159 66 R273-2
#
# CMP 158
CMP 3 2.955 1.923347 180 N R272 ERJ-2GEJ511X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/DMA0000COL9.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP LatestRevisionDate ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GEJ511X'
PRP Power_W '100mW'
PRP Published ''
PRP Publisher ''
PRP Res_ohm '510'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P510JCT-ND'
PRP Supplier_Part_Number_2 '65T8293'
PRP Supplier_Part_Number_3 '667-ERJ-2GEJ511X'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '510'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '510R'
PRP ValueDisplayed '510'
PRP VDC_V '50V'
TOP 0 2.974685 1.923347 90 N 392 0 R272-1
TOP 1 2.9353149 1.923347 90 N 256 0 R272-2
#
# CMP 159
CMP 1 1.9309306 1.8045396 0 N R271 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 1.9073086 1.8045396 270 N 159 82 R271-1
TOP 1 1.9545527 1.8045396 270 N 282 1 R271-2
#
# CMP 160
CMP 1 1.9309306 1.6768811 0 N R270 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 1.9073086 1.6768811 270 N 159 83 R270-1
TOP 1 1.9545527 1.6768811 270 N 281 1 R270-2
#
# CMP 161
CMP 1 2.388009 1.7315547 180 N R269 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 2.411631 1.7315547 90 N 159 84 R269-1
TOP 1 2.3643869 1.7315547 90 N 280 1 R269-2
#
# CMP 162
CMP 1 3.065 1.9154575 0 N R268 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 3.041378 1.9154575 270 N 392 2 R268-1
TOP 1 3.0886221 1.9154575 270 N 159 81 R268-2
#
# CMP 163
CMP 1 2.0178738 2.2161814 90 N R267 ERJ-2RKF2200X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C86.pdf'
PRP CompType 'Resistor'
PRP EIA_Code ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF2200X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '220'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P220LCT-ND'
PRP Supplier_Part_Number_2 '64R5267'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF2200X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '220'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '220R'
PRP ValueDisplayed '220'
PRP VDC_V '50V'
TOP 0 2.0178738 2.2398034 0 N 275 1 R267-1
TOP 1 2.0178738 2.1925593 0 N 159 85 R267-2
#
# CMP 164
CMP 1 2.1892913 2.2161813 90 N R266 ERJ-2RKF2200X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C86.pdf'
PRP CompType 'Resistor'
PRP EIA_Code ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF2200X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '220'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P220LCT-ND'
PRP Supplier_Part_Number_2 '64R5267'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF2200X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '220'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '220R'
PRP ValueDisplayed '220'
PRP VDC_V '50V'
TOP 0 2.1892913 2.2398033 0 N 276 1 R266-1
TOP 1 2.1892913 2.1925592 0 N 159 80 R266-2
#
# CMP 165
CMP 3 2.6360889 1.9171245 180 N R265 ERJ-2GEJ361X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/DMA0000COL9.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP LatestRevisionDate ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GEJ361X'
PRP Power_W '100mW'
PRP Published ''
PRP Publisher ''
PRP Res_ohm '360'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P360JCT-ND'
PRP Supplier_Part_Number_2 '53W4165'
PRP Supplier_Part_Number_3 '667-ERJ-2GEJ361X'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '360'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '360R'
PRP ValueDisplayed '360'
PRP VDC_V '50V'
TOP 0 2.6557739 1.9171245 90 N 258 0 R265-1
TOP 1 2.6164038 1.9171245 90 N 157 41 R265-2
#
# CMP 166
CMP 1 2.3292912 2.2161814 90 N R264 ERJ-2RKF2200X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C86.pdf'
PRP CompType 'Resistor'
PRP EIA_Code ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF2200X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '220'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P220LCT-ND'
PRP Supplier_Part_Number_2 '64R5267'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF2200X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '220'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '220R'
PRP ValueDisplayed '220'
PRP VDC_V '50V'
TOP 0 2.3292912 2.2398034 0 N 277 1 R264-1
TOP 1 2.3292912 2.1925593 0 N 159 79 R264-2
#
# CMP 167
CMP 1 2.4692911 2.2161815 90 N R263 ERJ-2RKF2200X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C86.pdf'
PRP CompType 'Resistor'
PRP EIA_Code ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF2200X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '220'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P220LCT-ND'
PRP Supplier_Part_Number_2 '64R5267'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF2200X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '220'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '220R'
PRP ValueDisplayed '220'
PRP VDC_V '50V'
TOP 0 2.4692911 2.2398035 0 N 278 1 R263-1
TOP 1 2.4692911 2.1925594 0 N 159 77 R263-2
#
# CMP 168
CMP 1 2.609291 2.2161815 90 N R262 ERJ-2RKF2200X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C86.pdf'
PRP CompType 'Resistor'
PRP EIA_Code ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF2200X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '220'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P220LCT-ND'
PRP Supplier_Part_Number_2 '64R5267'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF2200X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '220'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '220R'
PRP ValueDisplayed '220'
PRP VDC_V '50V'
TOP 0 2.609291 2.2398035 0 N 279 0 R262-1
TOP 1 2.609291 2.1925594 0 N 159 76 R262-2
#
# CMP 169
CMP 1 2.9745294 2.0055656 270 N R258 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 2.9745294 1.9819436 180 N 392 1 R258-1
TOP 1 2.9745294 2.0291877 180 N 159 78 R258-2
#
# CMP 170
CMP 1 1.9182675 0.87901 90 N R257 ERJ-2RKF5100X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF5100X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '510'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P510LCT-ND'
PRP Supplier_Part_Number_2 '53W4394'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF5100X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '510'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '510R'
PRP ValueDisplayed '510'
PRP VDC_V '50V'
TOP 0 1.9182675 0.902632 0 N 260 0 R257-1
TOP 1 1.9182675 0.8553879 0 N 157 42 R257-2
#
# CMP 171
CMP 1 4.8167748 0.8380235 270 N R256 ERJ-2GEJ102X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/DMA0000COL9.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS 'Passed with Exemption'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GEJ102X'
PRP Power_W '100mW'
PRP Published ''
PRP Publisher ''
PRP Res_ohm '1k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P1.0KJCT-ND'
PRP Supplier_Part_Number_2 '65T8247'
PRP Supplier_Part_Number_3 '667-ERJ-2GEJ102X'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '1.0k'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '1k00'
PRP ValueDisplayed '1.0k'
PRP VDC_V '50V'
TOP 0 4.8167748 0.8144015 180 N 284 281 R256-1
TOP 1 4.8167748 0.8616456 180 N 81 1 R256-2
#
# CMP 172
CMP 6 7.364165 2.1469686 270 N R255 ERJ-6ENF1004V ;0=1,1=0.0571
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'ERJ-6ENF1004V'
PRP Power_W '125mW'
PRP Res_ohm '1M'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 'P1.00MCCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-6ENF1004V'
PRP Supplier_Part_Number_3 '1748405'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '1.00Meg'
PRP Value1 '1%'
PRP Value2 '0.125W'
PRP Value_Code '1M00'
PRP ValueDisplayed '1.00M'
PRP VDC_V ''
TOP 0 7.364165 2.1069687 270 N 43 10 R255-1
TOP 1 7.364165 2.1869687 270 N 284 443 R255-2
#
# CMP 173
CMP 6 7.4305651 1.155 270 N R254 ERJ-6ENF1004V ;0=1,1=0.0571
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'ERJ-6ENF1004V'
PRP Power_W '125mW'
PRP Res_ohm '1M'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 'P1.00MCCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-6ENF1004V'
PRP Supplier_Part_Number_3 '1748405'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '1.00Meg'
PRP Value1 '1%'
PRP Value2 '0.125W'
PRP Value_Code '1M00'
PRP ValueDisplayed '1.00M'
PRP VDC_V ''
TOP 0 7.4305651 1.1150001 270 N 44 9 R254-1
TOP 1 7.4305651 1.1950001 270 N 284 359 R254-2
#
# CMP 174
CMP 1 0.6919686 1.2171658 90 N R252 CRCW040230K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code ''
PRP Green_EU_RoHS 'Passed with Exemption'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040230K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '30k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-30.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6953'
PRP Supplier_Part_Number_3 '71-CRCW0402-30K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '30.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '30k0'
PRP ValueDisplayed '30.0k'
PRP VDC_V '50V'
TOP 0 0.6919686 1.2407878 0 N 285 33 R252-1
TOP 1 0.6919686 1.1935437 0 N 286 0 R252-2
#
# CMP 175
CMP 1 0.6319686 1.2152309 270 N R251 CRCW040251K1FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040251K1FKED'
PRP Power_W '63mW'
PRP Res_ohm '51.1k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-51.1KLCT-ND'
PRP Supplier_Part_Number_2 '52K7131'
PRP Supplier_Part_Number_3 '71-CRCW0402-51.1K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '51.1k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '51k1'
PRP ValueDisplayed '51.1k'
PRP VDC_V '50V'
TOP 0 0.6319686 1.1916089 180 N 286 1 R251-1
TOP 1 0.6319686 1.238853 180 N 168 26 R251-2
#
# CMP 176
CMP 1 6.205 0.5782014 180 N R243 ERJ-2RKF4992X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF4992X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '49.9k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P49.9KLCT-ND'
PRP Supplier_Part_Number_2 '73T6530'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF4992X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '49.9k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '49k9'
PRP ValueDisplayed '49.9k'
PRP VDC_V '50V'
TOP 0 6.228622 0.5782014 90 N 343 3 R243-1
TOP 1 6.1813779 0.5782014 90 N 157 44 R243-2
#
# CMP 177
CMP 1 7.300378 0.221456 180 N R226 CRCW0402220RJNED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW0402220RJNED'
PRP Power_W '63mW'
PRP Res_ohm '220'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-220JCT-ND'
PRP Supplier_Part_Number_2 '59M6718'
PRP Supplier_Part_Number_3 '71-CRCW0402J-220-E3'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP Value '220'
PRP Value1 '5%'
PRP Value2 '0.063W'
PRP Value_Code '220R'
PRP ValueDisplayed '220'
PRP VDC_V '50V'
TOP 0 7.324 0.221456 90 N 238 2 R226-1
TOP 1 7.2767559 0.221456 90 N 159 120 R226-2
#
# CMP 178
CMP 1 6.5709716 1.4448823 270 N R221 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 6.5709716 1.4212603 180 N 284 360 R221-1
TOP 1 6.5709716 1.4685044 180 N 303 2 R221-2
#
# CMP 179
CMP 1 6.848 1.8996849 90 N R218 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 6.848 1.9233069 0 N 284 361 R218-1
TOP 1 6.848 1.8760628 0 N 492 3 R218-2
#
# CMP 180
CMP 1 6.443006 2.0129704 270 N R211 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 6.443006 1.9893484 180 N 495 2 R211-1
TOP 1 6.443006 2.0365925 180 N 159 117 R211-2
#
# CMP 181
CMP 1 6.383005 2.0129704 270 N R210 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 6.383005 1.9893484 180 N 497 2 R210-1
TOP 1 6.383005 2.0365925 180 N 159 116 R210-2
#
# CMP 182
CMP 1 6.520001 1.444999 90 N R209 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 6.520001 1.468621 0 N 303 1 R209-1
TOP 1 6.520001 1.4213769 0 N 159 115 R209-2
#
# CMP 183
CMP 1 6.729387 1.9000779 270 N R208 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 6.729387 1.8764559 180 N 107 3 R208-1
TOP 1 6.729387 1.9237 180 N 159 114 R208-2
#
# CMP 184
CMP 1 6.674387 1.9000779 270 N R207 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 6.674387 1.8764559 180 N 505 3 R207-1
TOP 1 6.674387 1.9237 180 N 159 113 R207-2
#
# CMP 185
CMP 1 6.796277 1.8996849 270 N R206 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 6.796277 1.8760629 180 N 492 2 R206-1
TOP 1 6.796277 1.923307 180 N 159 112 R206-2
#
# CMP 186
CMP 1 6.506277 2.0130484 270 N R205 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 6.506277 1.9894264 180 N 493 2 R205-1
TOP 1 6.506277 2.0366705 180 N 159 111 R205-2
#
# CMP 187
CMP 1 6.251378 1.8309624 180 N R204 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 6.275 1.8309624 90 N 499 2 R204-1
TOP 1 6.2277559 1.8309624 90 N 159 110 R204-2
#
# CMP 188
CMP 1 6.251378 1.7526528 180 N R203 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 6.275 1.7526528 90 N 501 2 R203-1
TOP 1 6.2277559 1.7526528 90 N 159 122 R203-2
#
# CMP 189
CMP 1 2.9450005 0.1952532 0 N R195 ERJ-2RKF1003X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Yes'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1003X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '100k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '100k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '100k'
PRP ValueDisplayed '100k'
PRP VDC_V '50V'
TOP 0 2.9213785 0.1952532 270 N 37 0 R195-1
TOP 1 2.9686226 0.1952532 270 N 153 22 R195-2
#
# CMP 190
CMP 1 2.9450005 0.2502535 0 N R194 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 2.9213785 0.2502535 270 N 154 0 R194-1
TOP 1 2.9686226 0.2502535 270 N 153 17 R194-2
#
# CMP 191
CMP 3 2.7350005 0.2266316 90 N R193 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 2.7350005 0.2463166 0 N 155 0 R193-1
TOP 1 2.7350005 0.2069465 0 N 152 5 R193-2
#
# CMP 192
CMP 1 1.758279 1.7483441 270 N R192 CRCW04024K70JNED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04024K70JNED'
PRP Power_W '63mW'
PRP Res_ohm '4.7k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-4.7KJCT-ND'
PRP Supplier_Part_Number_2 '59M6733'
PRP Supplier_Part_Number_3 '71-CRCW0402J-4.7K-E3'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP Value '4.7k'
PRP Value1 '5%'
PRP Value2 '0.063W'
PRP Value_Code '4k70'
PRP ValueDisplayed '4.7k'
PRP VDC_V '50V'
TOP 0 1.758279 1.7247221 180 N 230 1 R192-1
TOP 1 1.758279 1.7719662 180 N 153 18 R192-2
#
# CMP 193
CMP 1 1.8132786 1.7483442 270 N R190 CRCW04024K70JNED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04024K70JNED'
PRP Power_W '63mW'
PRP Res_ohm '4.7k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-4.7KJCT-ND'
PRP Supplier_Part_Number_2 '59M6733'
PRP Supplier_Part_Number_3 '71-CRCW0402J-4.7K-E3'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP Value '4.7k'
PRP Value1 '5%'
PRP Value2 '0.063W'
PRP Value_Code '4k70'
PRP ValueDisplayed '4.7k'
PRP VDC_V '50V'
TOP 0 1.8132786 1.7247222 180 N 229 1 R190-1
TOP 1 1.8132786 1.7719663 180 N 153 19 R190-2
#
# CMP 194
CMP 1 1.094864 1.88 270 N R184 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 1.094864 1.856378 180 N 153 23 R184-1
TOP 1 1.094864 1.9036221 180 N 221 2 R184-2
#
# CMP 195
CMP 1 1.1515018 2.17 270 N R181 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 1.1515018 2.146378 180 N 283 0 R181-1
TOP 1 1.1515018 2.1936221 180 N 159 71 R181-2
#
# CMP 196
CMP 1 0.7690927 2.0773585 270 N R179 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 0.7690927 2.0537365 180 N 411 2 R179-1
TOP 1 0.7690927 2.1009806 180 N 159 75 R179-2
#
# CMP 197
CMP 1 0.968084 2.0045241 90 N R178 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 0.968084 2.0281461 0 N 241 2 R178-1
TOP 1 0.968084 1.980902 0 N 159 74 R178-2
#
# CMP 198
CMP 1 5.0041718 0.1360277 90 N R176 CRCW04024K70JNED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04024K70JNED'
PRP Power_W '63mW'
PRP Res_ohm '4.7k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-4.7KJCT-ND'
PRP Supplier_Part_Number_2 '59M6733'
PRP Supplier_Part_Number_3 '71-CRCW0402J-4.7K-E3'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP Value '4.7k'
PRP Value1 '5%'
PRP Value2 '0.063W'
PRP Value_Code '4k70'
PRP ValueDisplayed '4.7k'
PRP VDC_V '50V'
TOP 0 5.0041718 0.1596497 0 N 508 1 R176-1
TOP 1 5.0041718 0.1124056 0 N 159 125 R176-2
#
# CMP 199
CMP 1 4.9033144 0.1360277 90 N R175 CRCW04024K70JNED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04024K70JNED'
PRP Power_W '63mW'
PRP Res_ohm '4.7k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-4.7KJCT-ND'
PRP Supplier_Part_Number_2 '59M6733'
PRP Supplier_Part_Number_3 '71-CRCW0402J-4.7K-E3'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP Value '4.7k'
PRP Value1 '5%'
PRP Value2 '0.063W'
PRP Value_Code '4k70'
PRP ValueDisplayed '4.7k'
PRP VDC_V '50V'
TOP 0 4.9033144 0.1596497 0 N 509 1 R175-1
TOP 1 4.9033144 0.1124056 0 N 159 126 R175-2
#
# CMP 200
CMP 1 3.7954439 1.7866522 180 N R174 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 3.8190659 1.7866522 90 N 378 1 R174-1
TOP 1 3.7718218 1.7866522 90 N 382 1 R174-2
#
# CMP 201
CMP 1 3.9105906 1.7026188 180 N R173 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 3.9342126 1.7026188 90 N 381 0 R173-1
TOP 1 3.8869685 1.7026188 90 N 383 1 R173-2
#
# CMP 202
CMP 3 3.8570004 1.6124809 90 N R172 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 3.8570004 1.6321659 0 N 372 0 R172-1
TOP 1 3.8570004 1.5927958 0 N 373 0 R172-2
#
# CMP 203
CMP 3 3.897 1.612481 90 N R171 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 3.897 1.632166 0 N 375 1 R171-1
TOP 1 3.897 1.5927959 0 N 376 0 R171-2
#
# CMP 204
CMP 3 3.8933084 1.7866522 0 N R170 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 3.8736234 1.7866522 270 N 378 2 R170-1
TOP 1 3.9129935 1.7866522 270 N 379 0 R170-2
#
# CMP 205
CMP 3 3.9350001 1.6124806 90 N R169 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 3.9350001 1.6321656 0 N 381 1 R169-1
TOP 1 3.9350001 1.5927955 0 N 8 0 R169-2
#
# CMP 206
CMP 3 3.209685 1.072379 0 N R168 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 3.19 1.072379 270 N 444 0 R168-1
TOP 1 3.2293701 1.072379 270 N 445 0 R168-2
#
# CMP 207
CMP 3 3.209685 1.0243795 0 N R167 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 3.19 1.0243795 270 N 447 1 R167-1
TOP 1 3.2293701 1.0243795 270 N 448 0 R167-2
#
# CMP 208
CMP 3 3.7729997 1.6124811 90 N R166 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 3.7729997 1.6321661 0 N 450 0 R166-1
TOP 1 3.7729997 1.592796 0 N 451 0 R166-2
#
# CMP 209
CMP 3 3.7070003 1.6124811 90 N R164 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 3.7070003 1.6321661 0 N 362 0 R164-1
TOP 1 3.7070003 1.592796 0 N 363 0 R164-2
#
# CMP 210
CMP 1 2.8340041 1.4393005 270 N R163 CRCW04024K99FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04024K99FKED'
PRP Power_W '63mW'
PRP Res_ohm '4.99k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-4.99KLCT-ND'
PRP Supplier_Part_Number_2 '52K7048'
PRP Supplier_Part_Number_3 '71-CRCW0402-4.99K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '4.99k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '4k99'
PRP ValueDisplayed '4.99k'
PRP VDC_V '50V'
TOP 0 2.8340041 1.4156785 180 N 284 334 R163-1
TOP 1 2.8340041 1.4629226 180 N 205 1 R163-2
#
# CMP 211
CMP 1 2.8840041 1.4393005 90 N R162 CRCW040215K4FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040215K4FKED'
PRP Power_W '63mW'
PRP Res_ohm '15.4k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-15.4KLCT-ND'
PRP Supplier_Part_Number_2 '52K6710'
PRP Supplier_Part_Number_3 '71-CRCW0402-15.4K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '15.4k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '15k4'
PRP ValueDisplayed '15.4k'
PRP VDC_V '50V'
TOP 0 2.8840041 1.4629225 0 N 205 0 R162-1
TOP 1 2.8840041 1.4156784 0 N 159 103 R162-2
#
# CMP 212
CMP 1 5.9141276 1.4815468 270 N R161 CRCW04024K99FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04024K99FKED'
PRP Power_W '63mW'
PRP Res_ohm '4.99k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-4.99KLCT-ND'
PRP Supplier_Part_Number_2 '52K7048'
PRP Supplier_Part_Number_3 '71-CRCW0402-4.99K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '4.99k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '4k99'
PRP ValueDisplayed '4.99k'
PRP VDC_V '50V'
TOP 0 5.9141276 1.4579248 180 N 284 236 R161-1
TOP 1 5.9141276 1.5051689 180 N 194 0 R161-2
#
# CMP 213
CMP 6 2.9564747 1.4108457 270 N R160 ERJ-6ENF1822V ;0=1,1=0.0571
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'ERJ-6ENF1822V'
PRP Power_W '125mW'
PRP Res_ohm '18.2k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 'P18.2KCCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-6ENF1822V'
PRP Supplier_Part_Number_3 '2057612'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '18.2k'
PRP Value1 '1%'
PRP Value2 '0.125W'
PRP Value_Code '18k2'
PRP ValueDisplayed '18.2k'
PRP VDC_V ''
TOP 0 2.9564747 1.3708458 270 N 284 333 R160-1
TOP 1 2.9564747 1.4508458 270 N 203 0 R160-2
#
# CMP 214
CMP 1 6.0041276 1.5051689 0 N R159 CRCW04021K87FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04021K87FKED'
PRP Power_W '63mW'
PRP Res_ohm '1.87k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-1.87KLCT-ND'
PRP Supplier_Part_Number_2 '52K6590'
PRP Supplier_Part_Number_3 '71-CRCW0402-1.87K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '1.87k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '1k87'
PRP ValueDisplayed '1.87k'
PRP VDC_V '50V'
TOP 0 5.9805056 1.5051689 270 N 194 1 R159-1
TOP 1 6.0277497 1.5051689 270 N 170 4 R159-2
#
# CMP 215
CMP 1 5.6541276 1.4868225 0 N R158 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 5.6305056 1.4868225 270 N 157 38 R158-1
TOP 1 5.6777497 1.4868225 270 N 196 0 R158-2
#
# CMP 216
CMP 1 5.6541276 1.4368225 0 N R157 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 5.6305056 1.4368225 270 N 157 37 R157-1
TOP 1 5.6777497 1.4368225 270 N 195 0 R157-2
#
# CMP 217
CMP 1 5.6541276 1.5368224 180 N R155 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 5.6777496 1.5368224 90 N 193 0 R155-1
TOP 1 5.6305055 1.5368224 90 N 159 73 R155-2
#
# CMP 218
CMP 1 2.4723308 0.8066816 270 N R154 CRCW04024K99FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04024K99FKED'
PRP Power_W '63mW'
PRP Res_ohm '4.99k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-4.99KLCT-ND'
PRP Supplier_Part_Number_2 '52K7048'
PRP Supplier_Part_Number_3 '71-CRCW0402-4.99K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '4.99k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '4k99'
PRP ValueDisplayed '4.99k'
PRP VDC_V '50V'
TOP 0 2.4723308 0.7830596 180 N 284 328 R154-1
TOP 1 2.4723308 0.8303036 180 N 210 1 R154-2
#
# CMP 219
CMP 1 2.5223308 0.8066816 90 N R153 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 2.5223308 0.8303037 0 N 210 0 R153-1
TOP 1 2.5223308 0.7830596 0 N 175 37 R153-2
#
# CMP 220
CMP 1 5.9141275 1.0623578 270 N R152 CRCW04021K69FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04021K69FKED'
PRP Power_W '63mW'
PRP Res_ohm '1.69k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-1.69KLCT-ND'
PRP Supplier_Part_Number_2 '52K6583'
PRP Supplier_Part_Number_3 '71-CRCW0402-1.69K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '1.69k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '1k69'
PRP ValueDisplayed '1.69k'
PRP VDC_V '50V'
TOP 0 5.9141275 1.0387358 180 N 284 339 R152-1
TOP 1 5.9141275 1.0859799 180 N 199 1 R152-2
#
# CMP 221
CMP 1 6.0041275 1.0859798 0 N R151 CRCW04023K57FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04023K57FKED'
PRP Power_W '63mW'
PRP Res_ohm '3.57k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-3.57KLCT-ND'
PRP Supplier_Part_Number_2 '52K6946'
PRP Supplier_Part_Number_3 '71-CRCW0402-3.57K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '3.57k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '3k57'
PRP ValueDisplayed '3.57k'
PRP VDC_V '50V'
TOP 0 5.9805055 1.0859798 270 N 199 0 R151-1
TOP 1 6.0277496 1.0859798 270 N 169 5 R151-2
#
# CMP 222
CMP 1 5.6541275 1.0676338 0 N R150 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 5.6305055 1.0676338 270 N 157 49 R150-1
TOP 1 5.6777496 1.0676338 270 N 201 0 R150-2
#
# CMP 223
CMP 1 5.6541275 1.0176338 0 N R149 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 5.6305055 1.0176338 270 N 157 48 R149-1
TOP 1 5.6777496 1.0176338 270 N 200 0 R149-2
#
# CMP 224
CMP 6 2.6373307 0.8446816 180 N R148 ERJ-6ENF1822V ;0=1,1=0.0571
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'ERJ-6ENF1822V'
PRP Power_W '125mW'
PRP Res_ohm '18.2k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 'P18.2KCCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-6ENF1822V'
PRP Supplier_Part_Number_3 '2057612'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '18.2k'
PRP Value1 '1%'
PRP Value2 '0.125W'
PRP Value_Code '18k2'
PRP ValueDisplayed '18.2k'
PRP VDC_V ''
TOP 0 2.6773306 0.8446816 180 N 284 327 R148-1
TOP 1 2.5973307 0.8446816 180 N 208 0 R148-2
#
# CMP 225
CMP 1 5.6541275 1.1176328 180 N R147 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 5.6777495 1.1176328 90 N 198 0 R147-1
TOP 1 5.6305054 1.1176328 90 N 159 105 R147-2
#
# CMP 226
CMP 1 6.5708545 0.4949989 270 N R126 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 6.5708545 0.4713769 180 N 284 362 R126-1
TOP 1 6.5708545 0.518621 180 N 340 2 R126-2
#
# CMP 227
CMP 1 6.848 0.9496849 90 N R123 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 6.848 0.9733069 0 N 284 363 R123-1
TOP 1 6.848 0.9260628 0 N 472 3 R123-2
#
# CMP 228
CMP 1 6.443006 1.0629703 270 N R116 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 6.443006 1.0393483 180 N 327 2 R116-1
TOP 1 6.443006 1.0865924 180 N 159 86 R116-2
#
# CMP 229
CMP 1 6.38301 1.0629598 270 N R115 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 6.38301 1.0393378 180 N 329 2 R115-1
TOP 1 6.38301 1.0865819 180 N 159 87 R115-2
#
# CMP 230
CMP 1 6.520001 0.494999 90 N R114 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 6.520001 0.518621 0 N 340 1 R114-1
TOP 1 6.520001 0.4713769 0 N 159 88 R114-2
#
# CMP 231
CMP 1 6.506277 1.0596849 270 N R113 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 6.506277 1.0360629 180 N 325 2 R113-1
TOP 1 6.506277 1.083307 180 N 159 89 R113-2
#
# CMP 232
CMP 1 6.6743876 0.9500779 270 N R112 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 6.6743876 0.9264559 180 N 479 3 R112-1
TOP 1 6.6743876 0.9737 180 N 159 90 R112-2
#
# CMP 233
CMP 1 6.796277 0.9496849 270 N R111 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 6.796277 0.9260629 180 N 472 2 R111-1
TOP 1 6.796277 0.973307 180 N 159 91 R111-2
#
# CMP 234
CMP 1 6.729387 0.9500778 270 N R110 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 6.729387 0.9264558 180 N 471 3 R110-1
TOP 1 6.729387 0.9736999 180 N 159 106 R110-2
#
# CMP 235
CMP 1 6.2513778 0.8809623 180 N R109 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 6.2749998 0.8809623 90 N 331 2 R109-1
TOP 1 6.2277557 0.8809623 90 N 159 123 R109-2
#
# CMP 236
CMP 1 6.2512998 0.8026527 180 N R108 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 6.2749218 0.8026527 90 N 333 2 R108-1
TOP 1 6.2276777 0.8026527 90 N 159 124 R108-2
#
# CMP 237
CMP 1 6.4933065 0.9404404 270 N R106 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 6.4933065 0.9168184 180 N 342 1 R106-1
TOP 1 6.4933065 0.9640625 180 N 341 1 R106-2
#
# CMP 238
CMP 3 3.0747737 1.0796157 0 N R99 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 3.0550887 1.0796157 270 N 538 1 R99-1
TOP 1 3.0944588 1.0796157 270 N 115 0 R99-2
#
# CMP 239
CMP 1 1.645 0.663273 0 N R98 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 1.621378 0.663273 270 N 190 0 R98-1
TOP 1 1.6686221 0.663273 270 N 284 264 R98-2
#
# CMP 240
CMP 1 0.5232942 0.4634126 90 N R97 ERJ-2GEJ102X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/DMA0000COL9.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS 'Passed with Exemption'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GEJ102X'
PRP Power_W '100mW'
PRP Published ''
PRP Publisher ''
PRP Res_ohm '1k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P1.0KJCT-ND'
PRP Supplier_Part_Number_2 '65T8247'
PRP Supplier_Part_Number_3 '667-ERJ-2GEJ102X'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '1.0k'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '1k00'
PRP ValueDisplayed '1.0k'
PRP VDC_V '50V'
TOP 0 0.5232942 0.4870346 0 N 284 325 R97-1
TOP 1 0.5232942 0.4397906 0 N 188 0 R97-2
#
# CMP 241
CMP 1 5.9865 0.82 90 N R96 ERJ-2GEJ102X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/DMA0000COL9.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS 'Passed with Exemption'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GEJ102X'
PRP Power_W '100mW'
PRP Published ''
PRP Publisher ''
PRP Res_ohm '1k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P1.0KJCT-ND'
PRP Supplier_Part_Number_2 '65T8247'
PRP Supplier_Part_Number_3 '667-ERJ-2GEJ102X'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '1.0k'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '1k00'
PRP ValueDisplayed '1.0k'
PRP VDC_V '50V'
TOP 0 5.9865 0.843622 0 N 284 408 R96-1
TOP 1 5.9865 0.7963779 0 N 3 1 R96-2
#
# CMP 242
CMP 1 0.3964038 0.3126046 0 N R95 CRCW04024K70JNED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04024K70JNED'
PRP Power_W '63mW'
PRP Res_ohm '4.7k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-4.7KJCT-ND'
PRP Supplier_Part_Number_2 '59M6733'
PRP Supplier_Part_Number_3 '71-CRCW0402J-4.7K-E3'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP Value '4.7k'
PRP Value1 '5%'
PRP Value2 '0.063W'
PRP Value_Code '4k70'
PRP ValueDisplayed '4.7k'
PRP VDC_V '50V'
TOP 0 0.3727818 0.3126046 270 N 284 322 R95-1
TOP 1 0.4200259 0.3126046 270 N 181 0 R95-2
#
# CMP 243
CMP 1 0.4278465 0.2600849 180 N R94 CRCW0402909KFKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW0402909KFKED'
PRP Power_W '63mW'
PRP Res_ohm '909k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-909KLCT-ND'
PRP Supplier_Part_Number_2 '52K7340'
PRP Supplier_Part_Number_3 '71-CRCW0402909KFKED'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '909k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '909k'
PRP ValueDisplayed '909k'
PRP VDC_V '50V'
TOP 0 0.4514685 0.2600849 90 N 180 0 R94-1
TOP 1 0.4042244 0.2600849 90 N 152 14 R94-2
#
# CMP 244
CMP 1 0.6699475 0.2943054 270 N R93 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 0.6699475 0.2706834 180 N 152 10 R93-1
TOP 1 0.6699475 0.3179274 180 N 185 0 R93-2
#
# CMP 245
CMP 1 0.6699475 0.4046872 90 N R92 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 0.6699475 0.4283093 0 N 152 11 R92-1
TOP 1 0.6699475 0.3810652 0 N 183 0 R92-2
#
# CMP 246
CMP 1 0.5875065 0.2636873 0 N R91 CRCW0402200KJNED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW0402200KJNED'
PRP Power_W '63mW'
PRP Res_ohm '200k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-200KJCT-ND'
PRP Supplier_Part_Number_2 '89M6629'
PRP Supplier_Part_Number_3 '71-CRCW0402J-200K-E3'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP Value '200k'
PRP Value1 '5%'
PRP Value2 '0.063W'
PRP Value_Code '200k'
PRP ValueDisplayed '200k'
PRP VDC_V '50V'
TOP 0 0.5638845 0.2636873 270 N 182 0 R91-1
TOP 1 0.6111286 0.2636873 270 N 152 13 R91-2
#
# CMP 247
CMP 3 0.5928214 0.3644117 0 N R90 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 0.5731363 0.3644117 270 N 184 0 R90-1
TOP 1 0.6125065 0.3644117 270 N 183 1 R90-2
#
# CMP 248
CMP 3 0.5928214 0.3243054 0 N R89 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 0.5731364 0.3243054 270 N 186 0 R89-1
TOP 1 0.6125065 0.3243054 270 N 185 1 R89-2
#
# CMP 249
CMP 3 4.1109995 1.6124805 90 N R86 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 4.1109995 1.6321655 0 N 469 0 R86-1
TOP 1 4.1109995 1.5927954 0 N 470 0 R86-2
#
# CMP 250
CMP 3 4.1489993 1.6124805 90 N R85 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 4.1489993 1.6321655 0 N 459 0 R85-1
TOP 1 4.1489993 1.5927954 0 N 460 0 R85-2
#
# CMP 251
CMP 3 4.312252 1.4107552 180 N R84 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 4.331937 1.4107552 90 N 461 0 R84-1
TOP 1 4.2925669 1.4107552 90 N 462 0 R84-2
#
# CMP 252
CMP 3 4.32 1.3332972 180 N R83 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 4.339685 1.3332972 90 N 463 0 R83-1
TOP 1 4.3003149 1.3332972 90 N 464 0 R83-2
#
# CMP 253
CMP 3 4.1869991 1.6124805 90 N R82 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 4.1869991 1.6321655 0 N 465 0 R82-1
TOP 1 4.1869991 1.5927954 0 N 466 0 R82-2
#
# CMP 254
CMP 3 4.312252 1.450755 180 N R81 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 4.331937 1.450755 90 N 467 0 R81-1
TOP 1 4.2925669 1.450755 90 N 468 0 R81-2
#
# CMP 255
CMP 3 4.312252 1.1513281 180 N R80 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 4.331937 1.1513281 90 N 48 0 R80-1
TOP 1 4.2925669 1.1513281 90 N 491 0 R80-2
#
# CMP 256
CMP 3 4.5571622 1.3132134 180 N R78 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 4.5768472 1.3132134 90 N 52 0 R78-1
TOP 1 4.5374771 1.3132134 90 N 483 0 R78-2
#
# CMP 257
CMP 3 4.312252 1.1913279 180 N R77 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 4.331937 1.1913279 90 N 54 0 R77-1
TOP 1 4.2925669 1.1913279 90 N 485 0 R77-2
#
# CMP 258
CMP 3 4.4522433 1.0298714 180 N R76 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 4.4719283 1.0298714 90 N 56 0 R76-1
TOP 1 4.4325582 1.0298714 90 N 487 0 R76-2
#
# CMP 259
CMP 3 4.4516133 1.0867287 180 N R72 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 4.4712983 1.0867287 90 N 419 2 R72-1
TOP 1 4.4319282 1.0867287 90 N 420 0 R72-2
#
# CMP 260
CMP 3 4.312252 1.071647 180 N R71 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 4.331937 1.071647 90 N 421 2 R71-1
TOP 1 4.2925669 1.071647 90 N 422 0 R71-2
#
# CMP 261
CMP 3 4.312252 0.989818 180 N R70 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 4.331937 0.989818 90 N 393 0 R70-1
TOP 1 4.2925669 0.989818 90 N 394 0 R70-2
#
# CMP 262
CMP 3 4.312252 1.0308178 180 N R69 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 4.331937 1.0308178 90 N 395 0 R69-1
TOP 1 4.2925669 1.0308178 90 N 396 0 R69-2
#
# CMP 263
CMP 3 4.312252 0.9528182 180 N R68 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 4.331937 0.9528182 90 N 397 0 R68-1
TOP 1 4.2925669 0.9528182 90 N 398 0 R68-2
#
# CMP 264
CMP 3 4.312252 0.9168184 180 N R67 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 4.331937 0.9168184 90 N 399 0 R67-1
TOP 1 4.2925669 0.9168184 90 N 400 0 R67-2
#
# CMP 265
CMP 3 4.3122521 0.8788186 180 N R66 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 4.3319371 0.8788186 90 N 401 0 R66-1
TOP 1 4.2925669 0.8788186 90 N 402 0 R66-2
#
# CMP 266
CMP 3 4.3122521 0.8408188 180 N R65 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 4.3319371 0.8408188 90 N 403 0 R65-1
TOP 1 4.2925669 0.8408188 90 N 404 0 R65-2
#
# CMP 267
CMP 3 3.209685 1.2312617 0 N R58 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 3.19 1.2312617 270 N 510 1 R58-1
TOP 1 3.2293701 1.2312617 270 N 511 0 R58-2
#
# CMP 268
CMP 3 3.209685 1.2742614 0 N R57 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 3.19 1.2742614 270 N 512 1 R57-1
TOP 1 3.2293701 1.2742614 270 N 513 0 R57-2
#
# CMP 269
CMP 1 2.5041738 0.146378 90 N R56 CRCW04024K70JNED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04024K70JNED'
PRP Power_W '63mW'
PRP Res_ohm '4.7k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-4.7KJCT-ND'
PRP Supplier_Part_Number_2 '59M6733'
PRP Supplier_Part_Number_3 '71-CRCW0402J-4.7K-E3'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP Value '4.7k'
PRP Value1 '5%'
PRP Value2 '0.063W'
PRP Value_Code '4k70'
PRP ValueDisplayed '4.7k'
PRP VDC_V '50V'
TOP 0 2.5041738 0.17 0 N 506 1 R56-1
TOP 1 2.5041738 0.1227559 0 N 159 93 R56-2
#
# CMP 270
CMP 1 2.4041738 0.1463777 90 N R55 CRCW04024K70JNED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04024K70JNED'
PRP Power_W '63mW'
PRP Res_ohm '4.7k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-4.7KJCT-ND'
PRP Supplier_Part_Number_2 '59M6733'
PRP Supplier_Part_Number_3 '71-CRCW0402J-4.7K-E3'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP Value '4.7k'
PRP Value1 '5%'
PRP Value2 '0.063W'
PRP Value_Code '4k70'
PRP ValueDisplayed '4.7k'
PRP VDC_V '50V'
TOP 0 2.4041738 0.1699997 0 N 507 1 R55-1
TOP 1 2.4041738 0.1227556 0 N 159 94 R55-2
#
# CMP 271
CMP 3 3.209685 1.3172611 0 N R54 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 3.19 1.3172611 270 N 514 1 R54-1
TOP 1 3.2293701 1.3172611 270 N 515 0 R54-2
#
# CMP 272
CMP 3 3.2105005 1.391922 90 N R52 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 3.2105005 1.411607 0 N 544 1 R52-1
TOP 1 3.2105005 1.3722369 0 N 545 0 R52-2
#
# CMP 273
CMP 3 3.355 1.4535 0 N R51 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 3.335315 1.4535 270 N 546 1 R51-1
TOP 1 3.3746851 1.4535 270 N 547 0 R51-2
#
# CMP 274
CMP 3 3.355 1.4935 0 N R50 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 3.335315 1.4935 270 N 548 1 R50-1
TOP 1 3.3746851 1.4935 270 N 549 0 R50-2
#
# CMP 275
CMP 3 3.2975 1.4155 0 N R49 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 3.277815 1.4155 270 N 550 1 R49-1
TOP 1 3.3171851 1.4155 270 N 551 0 R49-2
#
# CMP 276
CMP 3 3.355 1.534 0 N R47 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 3.335315 1.534 270 N 554 1 R47-1
TOP 1 3.3746851 1.534 270 N 555 0 R47-2
#
# CMP 277
CMP 3 3.3441576 1.600481 90 N R46 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 3.3441576 1.620166 0 N 556 1 R46-1
TOP 1 3.3441576 1.5807959 0 N 557 0 R46-2
#
# CMP 278
CMP 3 3.5287232 0.4699213 270 N R45 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 3.5287232 0.4502363 180 N 121 1 R45-1
TOP 1 3.5287232 0.4896064 180 N 558 0 R45-2
#
# CMP 279
CMP 3 3.8726292 0.6115192 270 N R44 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 3.8726292 0.5918342 180 N 284 298 R44-1
TOP 1 3.8726292 0.6312043 180 N 563 2 R44-2
#
# CMP 280
CMP 1 3.1645294 0.914795 90 N R42 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 3.1645294 0.938417 0 N 415 1 R42-1
TOP 1 3.1645294 0.8911729 0 N 385 1 R42-2
#
# CMP 281
CMP 3 0.185 0.5945275 180 N R40 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 0.204685 0.5945275 90 N 439 2 R40-1
TOP 1 0.1653149 0.5945275 90 N 159 121 R40-2
#
# CMP 282
CMP 3 0.8672375 0.7547997 180 N R39 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 0.8869225 0.7547997 90 N 284 279 R39-1
TOP 1 0.8475524 0.7547997 90 N 231 1 R39-2
#
# CMP 283
CMP 3 3.4490015 1.6124813 270 N R38 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 3.4490015 1.5927963 180 N 428 0 R38-1
TOP 1 3.4490015 1.6321664 180 N 427 1 R38-2
#
# CMP 284
CMP 3 3.4970012 1.6124813 270 N R37 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 3.4970012 1.5927963 180 N 430 0 R37-1
TOP 1 3.4970012 1.6321664 180 N 429 1 R37-2
#
# CMP 285
CMP 3 3.5350009 1.6124813 270 N R36 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 3.5350009 1.5927963 180 N 432 0 R36-1
TOP 1 3.5350009 1.6321664 180 N 431 1 R36-2
#
# CMP 286
CMP 3 3.6110003 1.6124813 270 N R35 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 3.6110003 1.5927963 180 N 434 0 R35-1
TOP 1 3.6110003 1.6321664 180 N 433 1 R35-2
#
# CMP 287
CMP 3 3.5730006 1.6124813 270 N R34 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 3.5730006 1.5927963 180 N 436 0 R34-1
TOP 1 3.5730006 1.6321664 180 N 435 1 R34-2
#
# CMP 288
CMP 3 3.6690003 1.612481 270 N R33 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 3.6690003 1.592796 180 N 438 0 R33-1
TOP 1 3.6690003 1.6321661 180 N 437 1 R33-2
#
# CMP 289
CMP 6 0.7495495 0.0739312 180 N R32 ERJ-6ENF1004V ;0=1,1=0.0571
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'ERJ-6ENF1004V'
PRP Power_W '125mW'
PRP Res_ohm '1M'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 'P1.00MCCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-6ENF1004V'
PRP Supplier_Part_Number_3 '1748405'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '1.00Meg'
PRP Value1 '1%'
PRP Value2 '0.125W'
PRP Value_Code '1M00'
PRP ValueDisplayed '1.00M'
PRP VDC_V ''
TOP 0 0.7895494 0.0739312 180 N 45 11 R32-1
TOP 1 0.7095494 0.0739312 180 N 284 354 R32-2
#
# CMP 290
CMP 1 3.255 0.8935314 180 N R31 CRCW040247K5FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040247K5FKED'
PRP Power_W '63mW'
PRP Res_ohm '47.5k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-47.5KLCT-ND'
PRP Supplier_Part_Number_2 '52K7100'
PRP Supplier_Part_Number_3 '71-CRCW0402-47.5K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '47.5k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '47k5'
PRP ValueDisplayed '47.5k'
PRP VDC_V '50V'
TOP 0 3.278622 0.8935314 90 N 416 0 R31-1
TOP 1 3.2313779 0.8935314 90 N 159 95 R31-2
#
# CMP 291
CMP 3 2.86 0.8289632 90 N R30 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 2.86 0.8486482 0 N 17 0 R30-1
TOP 1 2.86 0.8092781 0 N 412 0 R30-2
#
# CMP 292
CMP 3 2.83 1.2935432 180 N R29 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 2.849685 1.2935432 90 N 18 0 R29-1
TOP 1 2.8103149 1.2935432 90 N 413 0 R29-2
#
# CMP 293
CMP 3 2.83 1.3392674 180 N R28 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 2.849685 1.3392674 90 N 242 0 R28-1
TOP 1 2.8103149 1.3392674 90 N 414 1 R28-2
#
# CMP 294
CMP 3 2.76 0.8289633 90 N R27 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 2.76 0.8486483 0 N 243 0 R27-1
TOP 1 2.76 0.8092782 0 N 415 0 R27-2
#
# CMP 295
CMP 3 2.8100006 0.8289632 90 N R26 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 2.8100006 0.8486482 0 N 417 0 R26-1
TOP 1 2.8100006 0.8092781 0 N 418 0 R26-2
#
# CMP 296
CMP 1 3.92 0.2695077 180 N R25 ERJ-2GEJ102X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/DMA0000COL9.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS 'Passed with Exemption'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GEJ102X'
PRP Power_W '100mW'
PRP Published ''
PRP Publisher ''
PRP Res_ohm '1k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P1.0KJCT-ND'
PRP Supplier_Part_Number_2 '65T8247'
PRP Supplier_Part_Number_3 '667-ERJ-2GEJ102X'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '1.0k'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '1k00'
PRP ValueDisplayed '1.0k'
PRP VDC_V '50V'
TOP 0 3.943622 0.2695077 90 N 284 318 R25-1
TOP 1 3.8963779 0.2695077 90 N 251 0 R25-2
#
# CMP 297
CMP 1 3.92 0.2195079 180 N R24 ERJ-2GEJ102X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/DMA0000COL9.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS 'Passed with Exemption'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GEJ102X'
PRP Power_W '100mW'
PRP Published ''
PRP Publisher ''
PRP Res_ohm '1k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P1.0KJCT-ND'
PRP Supplier_Part_Number_2 '65T8247'
PRP Supplier_Part_Number_3 '667-ERJ-2GEJ102X'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '1.0k'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '1k00'
PRP ValueDisplayed '1.0k'
PRP VDC_V '50V'
TOP 0 3.943622 0.2195079 90 N 284 319 R24-1
TOP 1 3.8963779 0.2195079 90 N 252 0 R24-2
#
# CMP 298
CMP 1 3.92 0.169508 180 N R23 ERJ-2GEJ102X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/DMA0000COL9.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS 'Passed with Exemption'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GEJ102X'
PRP Power_W '100mW'
PRP Published ''
PRP Publisher ''
PRP Res_ohm '1k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P1.0KJCT-ND'
PRP Supplier_Part_Number_2 '65T8247'
PRP Supplier_Part_Number_3 '667-ERJ-2GEJ102X'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '1.0k'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '1k00'
PRP ValueDisplayed '1.0k'
PRP VDC_V '50V'
TOP 0 3.943622 0.169508 90 N 284 321 R23-1
TOP 1 3.8963779 0.169508 90 N 253 0 R23-2
#
# CMP 299
CMP 1 3.92 0.119508 180 N R22 ERJ-2GEJ102X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/DMA0000COL9.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS 'Passed with Exemption'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GEJ102X'
PRP Power_W '100mW'
PRP Published ''
PRP Publisher ''
PRP Res_ohm '1k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P1.0KJCT-ND'
PRP Supplier_Part_Number_2 '65T8247'
PRP Supplier_Part_Number_3 '667-ERJ-2GEJ102X'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '1.0k'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '1k00'
PRP ValueDisplayed '1.0k'
PRP VDC_V '50V'
TOP 0 3.943622 0.119508 90 N 284 320 R22-1
TOP 1 3.8963779 0.119508 90 N 254 0 R22-2
#
# CMP 300
CMP 1 1.545 1.8296251 270 N R21 ERJ-2GEJ102X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/DMA0000COL9.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS 'Passed with Exemption'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GEJ102X'
PRP Power_W '100mW'
PRP Published ''
PRP Publisher ''
PRP Res_ohm '1k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P1.0KJCT-ND'
PRP Supplier_Part_Number_2 '65T8247'
PRP Supplier_Part_Number_3 '667-ERJ-2GEJ102X'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '1.0k'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '1k00'
PRP ValueDisplayed '1.0k'
PRP VDC_V '50V'
TOP 0 1.545 1.8060031 180 N 284 314 R21-1
TOP 1 1.545 1.8532472 180 N 2 1 R21-2
#
# CMP 301
CMP 1 2.1408032 1.0940723 180 N R20 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 2.1644252 1.0940723 90 N 223 3 R20-1
TOP 1 2.1171811 1.0940723 90 N 284 315 R20-2
#
# CMP 302
CMP 1 2.2628442 0.7673875 90 N R19 ERJ-2RKF49R9X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/lecs/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF49R9X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '49.9'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P49.9LCT-ND'
PRP Supplier_Part_Number_2 '73T6527'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF49R9X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '49.9'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '49R9'
PRP ValueDisplayed '49.9'
PRP VDC_V '50V'
TOP 0 2.2628442 0.7910095 0 N 423 2 R19-1
TOP 1 2.2628442 0.7437654 0 N 424 1 R19-2
#
# CMP 303
CMP 1 2.1408034 1.0390723 0 N R18 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 2.1171814 1.0390723 270 N 224 0 R18-1
TOP 1 2.1644255 1.0390723 270 N 223 2 R18-2
#
# CMP 304
CMP 1 3.4119288 0.269508 0 N R17 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 3.3883068 0.269508 270 N 159 100 R17-1
TOP 1 3.4355509 0.269508 270 N 225 1 R17-2
#
# CMP 305
CMP 1 3.4119288 0.219508 0 N R16 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 3.3883068 0.219508 270 N 159 101 R16-1
TOP 1 3.4355509 0.219508 270 N 226 1 R16-2
#
# CMP 306
CMP 1 3.4119288 0.169508 0 N R15 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 3.3883068 0.169508 270 N 159 99 R15-1
TOP 1 3.4355509 0.169508 270 N 227 1 R15-2
#
# CMP 307
CMP 1 3.4119288 0.119508 0 N R14 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 3.3883068 0.119508 270 N 159 98 R14-1
TOP 1 3.4355509 0.119508 270 N 228 1 R14-2
#
# CMP 308
CMP 3 3.0747737 1.181642 0 N R13 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 3.0550887 1.181642 270 N 539 1 R13-1
TOP 1 3.0944588 1.181642 270 N 116 0 R13-2
#
# CMP 309
CMP 3 3.0747737 1.1350452 0 N R12 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 3.0550887 1.1350452 270 N 540 1 R12-1
TOP 1 3.0944588 1.1350452 270 N 117 0 R12-2
#
# CMP 310
CMP 1 3.27 0.5307619 0 N R11 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 3.246378 0.5307619 270 N 153 26 R11-1
TOP 1 3.2936221 0.5307619 270 N 212 0 R11-2
#
# CMP 311
CMP 1 3.215 0.3585827 0 N R10 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 3.191378 0.3585827 270 N 153 27 R10-1
TOP 1 3.2386221 0.3585827 270 N 213 0 R10-2
#
# CMP 312
CMP 3 3.0747737 1.2381086 0 N R9 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 3.0550887 1.2381086 270 N 541 1 R9-1
TOP 1 3.0944588 1.2381086 270 N 118 0 R9-2
#
# CMP 313
CMP 3 3.41 1.612481 270 N R7 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 3.41 1.592796 180 N 368 0 R7-1
TOP 1 3.41 1.6321661 180 N 367 0 R7-2
#
# CMP 314
CMP 1 2.1627168 1.2291301 180 N R6 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 2.1863388 1.2291301 90 N 284 310 R6-1
TOP 1 2.1390947 1.2291301 90 N 423 1 R6-2
#
# CMP 315
CMP 3 3.2409016 0.9690625 180 N R4 ERJ-2GE0R00X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '65T8307'
PRP Supplier_Part_Number_3 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP TempCo '600 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '50V'
TOP 0 3.2605866 0.9690625 90 N 560 0 R4-1
TOP 1 3.2212165 0.9690625 90 N 559 2 R4-2
#
# CMP 316
CMP 1 3.337655 0.6332438 270 N R2 CRCW04022K67FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K67FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.67k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.67KLCT-ND'
PRP Supplier_Part_Number_2 '52K6808'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.67K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.67k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k67'
PRP ValueDisplayed '2.67k'
PRP VDC_V '50V'
TOP 0 3.337655 0.6096218 180 N 284 269 R2-1
TOP 1 3.337655 0.6568659 180 N 156 1 R2-2
#
# CMP 317
CMP 1 3.2374746 0.6332442 90 N R1 ERJ-2RKF1002X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF1002X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '10k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P10.0KLCT-ND'
PRP Supplier_Part_Number_2 '90W2949'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF1002X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 3.2374746 0.6568662 0 N 156 2 R1-1
TOP 1 3.2374746 0.6096221 0 N 157 43 R1-2
#
# CMP 318
CMP 61 2.848 1.981 90 N Q10 BSS223PWH6327 ;0=1,1=0.0433
PRP AEC_Category 'Q101'
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer 'None'
PRP Alternate_PartNumber ''
PRP ChMode 'Enhancement'
PRP ChType 'P'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.infineon.com/dgdl?folderId=db3a304314dca38901154a72e3951a65&fileId=db3a3043321e49940132481523b6245f'
PRP CompType 'MOSFET'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IdsMax_A '-390mA'
PRP Manufacturer 'Infineon Technologies'
PRP MountType 'SMT'
PRP PackageReference 'SOT-323'
PRP PartNumber 'BSS223PWH6327'
PRP QgTyp_nC '-0.5'
PRP Rdson45_ohm '1.2'
PRP RoHS 'Y'
PRP SizeArea_mm2 '4.84'
PRP SizeAreaWB_mm2 '10.24'
PRP SizeX_mm '2.2'
PRP SizeY_mm '2.2'
PRP SizeZ_mm '1.1'
PRP Value '-20V'
PRP Value1 '1'
PRP Value2 ''
PRP VdsMax_V '-20V'
PRP Vgs_V '-12V'
TOP 0 2.8735905 2.0184017 180 N 256 1 Q10-1
TOP 1 2.8224094 2.0184017 180 N 259 1 Q10-2
TOP 2 2.8479999 1.9435986 180 N 284 357 Q10-3
#
# CMP 319
CMP 60 7.324 0.1136601 270 N Q5 BSS123 ;0=1,1=0.0433
PRP AEC_Category 'Q101'
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer 'None'
PRP Alternate_PartNumber ''
PRP ChType 'N'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.fairchildsemi.com/ds/BS/BSS123.pdf'
PRP CompType 'MOSFET'
PRP IdsMax_A '1.7dA'
PRP LatestRevisionDate '2017-03-09'
PRP LatestRevisionNote 'Added parts.'
PRP Manufacturer 'Fairchild Semiconductor'
PRP MountType 'SMT'
PRP PackageReference 'SOT-23'
PRP PartNumber 'BSS123'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP QgTyp_nC '1.8'
PRP Rdson45_ohm '10'
PRP RoHS 'Y'
PRP SizeArea_mm2 '7.5'
PRP SizeAreaWB_mm2 '14'
PRP SizeX_mm '2.5'
PRP SizeY_mm '3'
PRP SizeZ_mm '1.1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'BSS123NCT-ND'
PRP Supplier_Part_Number_2 '58K8768'
PRP Supplier_Part_Number_3 '512-BSS123'
PRP U/M 'EA'
PRP Value '100V'
PRP Value1 '1'
PRP Value2 '1.8 nC'
PRP Vault_Folder ''
PRP VdsMax_V '100V'
PRP Vgs_V '20V'
TOP 0 7.2865984 0.066416 180 N 339 1 Q5-1
TOP 1 7.3614015 0.066416 180 N 284 358 Q5-2
TOP 2 7.324 0.1609042 180 N 238 1 Q5-3
#
# CMP 320
CMP 60 1.2011207 2.0170245 90 N Q3 IRLML6401TRPBF ;0=1,1=0.0433
PRP AEC_Category 'Q101'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer 'None'
PRP Alternate_PartNumber ''
PRP ChMode 'Enhancement'
PRP ChType 'P'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://www.infineon.com/dgdl/irlml6401pbf.pdf?fileId=5546d462533600a401535668b96d2634'
PRP CompType 'MOSFET'
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP IdsMax_A '-4.3A'
PRP Manufacturer 'Infineon Technologies'
PRP MountType 'SMT'
PRP PackageReference 'SOT-23'
PRP PartNumber 'IRLML6401TRPBF'
PRP QgTyp_nC '10'
PRP Rdson45_ohm '50m'
PRP RoHS 'Y'
PRP SizeArea_mm2 '7.5'
PRP SizeAreaWB_mm2 '14'
PRP SizeX_mm '2.5'
PRP SizeY_mm '3'
PRP SizeZ_mm '1.1'
PRP Value '-12V'
PRP Value1 '0.05 ohm'
PRP Value2 '10 nC'
PRP VdsMax_V '-12V'
PRP Vgs_V '-8V'
TOP 0 1.2385223 2.0642686 0 N 222 2 Q3-1
TOP 1 1.1637192 2.0642686 0 N 283 1 Q3-2
TOP 2 1.2011207 1.9697804 0 N 284 254 Q3-3
#
# CMP 321
CMP 60 1.0622533 2.0170245 90 N Q2 IRLML6401TRPBF ;0=1,1=0.0433
PRP AEC_Category 'Q101'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer 'None'
PRP Alternate_PartNumber ''
PRP ChMode 'Enhancement'
PRP ChType 'P'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://www.infineon.com/dgdl/irlml6401pbf.pdf?fileId=5546d462533600a401535668b96d2634'
PRP CompType 'MOSFET'
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP IdsMax_A '-4.3A'
PRP Manufacturer 'Infineon Technologies'
PRP MountType 'SMT'
PRP PackageReference 'SOT-23'
PRP PartNumber 'IRLML6401TRPBF'
PRP QgTyp_nC '10'
PRP Rdson45_ohm '50m'
PRP RoHS 'Y'
PRP SizeArea_mm2 '7.5'
PRP SizeAreaWB_mm2 '14'
PRP SizeX_mm '2.5'
PRP SizeY_mm '3'
PRP SizeZ_mm '1.1'
PRP Value '-12V'
PRP Value1 '0.05 ohm'
PRP Value2 '10 nC'
PRP VdsMax_V '-12V'
PRP Vgs_V '-8V'
TOP 0 1.0996549 2.0642686 0 N 214 2 Q2-1
TOP 1 1.0248518 2.0642686 0 N 241 0 Q2-2
TOP 2 1.0622533 1.9697804 0 N 284 253 Q2-3
#
# CMP 322
CMP 36 2.9350005 0.3388362 270 N L4 74405020100 ;0=1,1=0.0461
PRP AEC_Qualified 'No'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://katalog.we-online.de/pbs/datasheet/74405020100.pdf'
PRP Imax_A '580mA'
PRP Irms '0.58A'
PRP Isat '0.95A'
PRP Manufacturer 'Wurth Electronics'
PRP Material 'Ferrite'
PRP PackageReference 'SMT_IND_2MM0_1MM6'
PRP PartNumber '74405020100'
PRP RoHS 'TRUE'
PRP SizeZ_mm '1mm'
PRP Symbol_Name 'SYM-74405020100'
PRP Technology 'Wirewound'
TOP 0 2.9350005 0.3073401 270 N 257 2 L4-1
TOP 1 2.9350005 0.3703323 270 N 153 38 L4-2
#
# CMP 323
CMP 69 3.0074261 1.6333565 270 N L3 74438356022 ;0=1,1=0.0827
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://katalog.we-online.com/pbs/datasheet/74438356022.pdf'
PRP CompType 'Inductor'
PRP DCR_ohm '29m'
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP Imax_A '4.7A'
PRP Ind_H '2.2µH'
PRP Irms '4.7A @ 40C rise'
PRP Isat '6.2A @ 20% inductance drop'
PRP LatestRevisionDate '2017-06-02'
PRP Manufacturer 'Wurth Elektronik'
PRP Material '?'
PRP MountType 'SMT'
PRP PackageReference '4.1x4.1mm'
PRP PartNumber '74438356022'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '16.81'
PRP SizeAreaWB_mm2 '26.01'
PRP SizeX_mm '4.1'
PRP SizeY_mm '4.1'
PRP SizeZ_mm '2.1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '732-8232-1-ND'
PRP Supplier_Part_Number_2 '710-74438356022'
PRP Supplier_Part_Number_3 ''
PRP Technology 'Shielded'
PRP Value '2.2uH'
PRP Value1 '0.029 ohm'
PRP Value2 '4.7A'
PRP ValueDisplayed '2.2uH'
TOP 0 3.0074261 1.586703 270 N 202 2 L3-1
TOP 1 3.0074261 1.68001 270 N 159 178 L3-2
#
# CMP 324
CMP 69 2.6457533 1.0007368 270 N L2 74438356022 ;0=1,1=0.0827
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://katalog.we-online.com/pbs/datasheet/74438356022.pdf'
PRP CompType 'Inductor'
PRP DCR_ohm '29m'
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP Imax_A '4.7A'
PRP Ind_H '2.2µH'
PRP Irms '4.7A @ 40C rise'
PRP Isat '6.2A @ 20% inductance drop'
PRP LatestRevisionDate '2017-06-02'
PRP Manufacturer 'Wurth Elektronik'
PRP Material '?'
PRP MountType 'SMT'
PRP PackageReference '4.1x4.1mm'
PRP PartNumber '74438356022'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '16.81'
PRP SizeAreaWB_mm2 '26.01'
PRP SizeX_mm '4.1'
PRP SizeY_mm '4.1'
PRP SizeZ_mm '2.1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '732-8232-1-ND'
PRP Supplier_Part_Number_2 '710-74438356022'
PRP Supplier_Part_Number_3 ''
PRP Technology 'Shielded'
PRP Value '2.2uH'
PRP Value1 '0.029 ohm'
PRP Value2 '4.7A'
PRP ValueDisplayed '2.2uH'
TOP 0 2.6457533 0.9540833 270 N 207 1 L2-1
TOP 1 2.6457533 1.0473902 270 N 175 36 L2-2
#
# CMP 325
CMP 6 1.322441 0.5476535 0 N L1 BLM21PG300SH1D ;0=1,1=0.0571
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.murata.com/en-us/api/pdfdownloadapi?cate=luNoiseSupprFilteChipFerriBead&partno=BLM21PG300SH1%23'
PRP CompType 'Ferrite Bead'
PRP DCR_ohm '14m'
PRP Imax_A '4A'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'BLM21PG300SH1D'
PRP Published '2014-04-30'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-11049-1-ND'
PRP Supplier_Part_Number_2 '87X8590'
PRP Supplier_Part_Number_3 '81-BLM21PG300SH1D'
PRP Value '30 ohm'
PRP Value1 '0.014 ohm'
PRP Value2 '4A'
PRP ValueDisplayed '30 ohm'
PRP Ztyp@1GHz_Ohm ''
PRP ZTyp@100MHz_Ohm '30'
TOP 0 1.2824411 0.5476535 0 N 177 5 L1-1
TOP 1 1.3624411 0.5476535 0 N 152 16 L1-2
#
# CMP 326
CMP 46 6.6541747 0.183858 0 N J33 OSTTE030161 ;0=2,1=0.3346
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA 'Y'
PRP Cert_CULUS ''
PRP Cert_UL 'Y'
PRP Cert_VDE ''
PRP ClassName ''
PRP CNHeader 'False'
PRP Color 'Blue'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.on-shore.com/wp-content/uploads/2015/09/osttexx0161.pdf'
PRP CompType 'Terminal Block'
PRP ContactFinish 'Tin'
PRP CT 'True'
PRP Current_A '10A'
PRP Gender 'Female'
PRP Green_EU_RoHS 'Incomplete'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Not Set'
PRP Green_REACh 'Incomplete'
PRP LatestRevisionDate '2017-07-12'
PRP Manufacturer 'On-Shore Technology'
PRP MountType 'TH'
PRP Note ''
PRP Orientation 'R/A'
PRP PackageReference 'Terminal Block, 3.5mm, 3x1, TH'
PRP PartNumber 'OSTTE030161'
PRP PinCount '3'
PRP Pitch_mm '3.5'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count '1'
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'ED2636-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Voltage_V '125V'
TOP 0 6.5163795 0.1838581 0 N 354 2 J33-1
TOP 1 6.6541748 0.1838581 0 N 284 213 J33-2
TOP 2 6.79197 0.1838581 0 N 353 2 J33-3
#
# CMP 327
CMP 63 5.9991755 0.365 180 N J25 PEC05SAAN ;0=2,1=0.3575
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL 'Y'
PRP Cert_VDE ''
PRP ClassName 'Header'
PRP CNHeader 'TRUE'
PRP Color 'Black'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.sullinscorp.com/catalogs/77_PAGE108-109_.100_MALE_HDR.pdf'
PRP CompType 'Header'
PRP ContactFinish 'Tin'
PRP CT 'FALSE'
PRP Current_A '3A'
PRP Gender 'Male'
PRP Green_EU_RoHS 'Incomplete'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Not Set'
PRP Green_REACh 'Incomplete'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Sullins Connector Solutions'
PRP MountType 'TH'
PRP Note ''
PRP Orientation 'Vertical'
PRP PackageReference 'Header, 2.54mm, 5x1, TH'
PRP PartNumber 'PEC05SAAN'
PRP PinCount '5'
PRP Pitch_mm '2.54'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count '1'
PRP RowSpacing_mm ''
PRP Shrouded 'N'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'S1012E-05-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Voltage_V '1.8kV'
TOP 0 6.1991755 0.365 180 N 346 3 J25-1
TOP 1 6.0991755 0.365 180 N 345 3 J25-2
TOP 2 5.9991755 0.365 180 N 344 3 J25-3
TOP 3 5.8991755 0.365 180 N 157 35 J25-4
TOP 4 5.7991755 0.365 180 N 284 214 J25-5
#
# CMP 328
CMP 63 5.9991755 0.115 180 N J24 PEC05SAAN ;0=2,1=0.3575
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL 'Y'
PRP Cert_VDE ''
PRP ClassName 'Header'
PRP CNHeader 'TRUE'
PRP Color 'Black'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.sullinscorp.com/catalogs/77_PAGE108-109_.100_MALE_HDR.pdf'
PRP CompType 'Header'
PRP ContactFinish 'Tin'
PRP CT 'FALSE'
PRP Current_A '3A'
PRP Gender 'Male'
PRP Green_EU_RoHS 'Incomplete'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Not Set'
PRP Green_REACh 'Incomplete'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Sullins Connector Solutions'
PRP MountType 'TH'
PRP Note ''
PRP Orientation 'Vertical'
PRP PackageReference 'Header, 2.54mm, 5x1, TH'
PRP PartNumber 'PEC05SAAN'
PRP PinCount '5'
PRP Pitch_mm '2.54'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count '1'
PRP RowSpacing_mm ''
PRP Shrouded 'N'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'S1012E-05-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Voltage_V '1.8kV'
TOP 0 6.1991755 0.115 180 N 350 3 J24-1
TOP 1 6.0991755 0.115 180 N 349 3 J24-2
TOP 2 5.9991755 0.115 180 N 348 3 J24-3
TOP 3 5.8991755 0.115 180 N 157 34 J24-4
TOP 4 5.7991755 0.115 180 N 284 208 J24-5
#
# CMP 329
CMP 64 3.604174 2 270 N J23 PRPC005DAAN-RC ;0=2,1=0.3441
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL 'Y'
PRP Cert_VDE ''
PRP ClassName 'Header'
PRP Color 'Black'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://sullinscorp.com/drawings/294___R__C_____D___N-RC,_11636.pdf'
PRP CompType 'Header'
PRP ContactFinish 'Gold'
PRP Current_A '3A'
PRP Gender 'Male'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Sullins Connector Solutions'
PRP MountType 'TH'
PRP Note ''
PRP Orientation 'Vertical'
PRP PackageReference 'Header, 2.54mm, 5x2, TH'
PRP PartNumber 'PRPC005DAAN-RC'
PRP PinCount '10'
PRP Pitch_mm '2.54'
PRP RoHS 'Y'
PRP Row_Count '2'
PRP RowSpacing_mm '2.54'
PRP Shrouded 'N'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'S2011EC-05-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Voltage_V '1kV'
TOP 0 3.404174 1.95 270 N 518 0 J23-1
TOP 1 3.404174 2.05 270 N 514 0 J23-2
TOP 2 3.504174 1.95 270 N 284 215 J23-3
TOP 3 3.504174 2.05 270 N 284 216 J23-4
TOP 4 3.604174 1.9500001 270 N 517 0 J23-5
TOP 5 3.604174 2.0499999 270 N 512 0 J23-6
TOP 6 3.704174 1.95 270 N 516 0 J23-7
TOP 7 3.704174 2.05 270 N 510 0 J23-8
TOP 8 3.804174 1.95 270 N 284 217 J23-9
TOP 9 3.804174 2.05 270 N 159 61 J23-10
#
# CMP 330
CMP 62 2.695 0.634465 0 N J18 PBC02SAAN ;0=2,1=0.3300
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL 'Y'
PRP Cert_VDE ''
PRP ClassName 'Header'
PRP CNHeader 'TRUE'
PRP Color 'Black'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.sullinscorp.com/catalogs/77_PAGE108-109_.100_MALE_HDR.pdf'
PRP CompType 'Header'
PRP ContactFinish 'Gold'
PRP CT 'FALSE'
PRP Current_A '3A'
PRP Gender 'Male'
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Sullins Connector Solutions'
PRP MountType 'TH'
PRP Note ''
PRP Orientation 'Vertical'
PRP PackageReference 'Sullins 100mil, 1x2, 230 mil above insulator'
PRP PartNumber 'PBC02SAAN'
PRP PinCount '2'
PRP Pitch_mm '2.54'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count '1'
PRP RowSpacing_mm ''
PRP Shrouded 'N'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'S1011E-02-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Voltage_V '1.8kV'
TOP 0 2.695 0.684465 90 N 284 218 J18-1
TOP 1 2.695 0.584465 90 N 352 0 J18-2
#
# CMP 331
CMP 62 1.6686221 1.023768 270 N J17 PBC02SAAN ;0=2,1=0.3300
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL 'Y'
PRP Cert_VDE ''
PRP ClassName 'Header'
PRP CNHeader 'TRUE'
PRP Color 'Black'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.sullinscorp.com/catalogs/77_PAGE108-109_.100_MALE_HDR.pdf'
PRP CompType 'Header'
PRP ContactFinish 'Gold'
PRP CT 'FALSE'
PRP Current_A '3A'
PRP Gender 'Male'
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Sullins Connector Solutions'
PRP MountType 'TH'
PRP Note ''
PRP Orientation 'Vertical'
PRP PackageReference 'Sullins 100mil, 1x2, 230 mil above insulator'
PRP PartNumber 'PBC02SAAN'
PRP PinCount '2'
PRP Pitch_mm '2.54'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count '1'
PRP RowSpacing_mm ''
PRP Shrouded 'N'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'S1011E-02-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Voltage_V '1.8kV'
TOP 0 1.6186221 1.023768 0 N 284 207 J17-1
TOP 1 1.7186221 1.023768 0 N 596 2 J17-2
#
# CMP 332
CMP 62 6.3270598 0.4150001 180 N J16 PBC02SAAN ;0=2,1=0.3300
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL 'Y'
PRP Cert_VDE ''
PRP ClassName 'Header'
PRP CNHeader 'TRUE'
PRP Color 'Black'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.sullinscorp.com/catalogs/77_PAGE108-109_.100_MALE_HDR.pdf'
PRP CompType 'Header'
PRP ContactFinish 'Gold'
PRP CT 'FALSE'
PRP Current_A '3A'
PRP Gender 'Male'
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Sullins Connector Solutions'
PRP MountType 'TH'
PRP Note ''
PRP Orientation 'Vertical'
PRP PackageReference 'Sullins 100mil, 1x2, 230 mil above insulator'
PRP PartNumber 'PBC02SAAN'
PRP PinCount '2'
PRP Pitch_mm '2.54'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count '1'
PRP RowSpacing_mm ''
PRP Shrouded 'N'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'S1011E-02-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Voltage_V '1.8kV'
TOP 0 6.3270598 0.3650001 270 N 343 1 J16-1
TOP 1 6.3270598 0.4650001 270 N 284 206 J16-2
#
# CMP 333
CMP 62 6.3270598 0.1650004 180 N J15 PBC02SAAN ;0=2,1=0.3300
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL 'Y'
PRP Cert_VDE ''
PRP ClassName 'Header'
PRP CNHeader 'TRUE'
PRP Color 'Black'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.sullinscorp.com/catalogs/77_PAGE108-109_.100_MALE_HDR.pdf'
PRP CompType 'Header'
PRP ContactFinish 'Gold'
PRP CT 'FALSE'
PRP Current_A '3A'
PRP Gender 'Male'
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Sullins Connector Solutions'
PRP MountType 'TH'
PRP Note ''
PRP Orientation 'Vertical'
PRP PackageReference 'Sullins 100mil, 1x2, 230 mil above insulator'
PRP PartNumber 'PBC02SAAN'
PRP PinCount '2'
PRP Pitch_mm '2.54'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count '1'
PRP RowSpacing_mm ''
PRP Shrouded 'N'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'S1011E-02-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Voltage_V '1.8kV'
TOP 0 6.3270598 0.1150004 270 N 347 3 J15-1
TOP 1 6.3270598 0.2150004 270 N 284 205 J15-2
#
# CMP 334
CMP 62 5.3671057 0.5432509 0 N J14 PBC02SAAN ;0=2,1=0.3300
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL 'Y'
PRP Cert_VDE ''
PRP ClassName 'Header'
PRP CNHeader 'TRUE'
PRP Color 'Black'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.sullinscorp.com/catalogs/77_PAGE108-109_.100_MALE_HDR.pdf'
PRP CompType 'Header'
PRP ContactFinish 'Gold'
PRP CT 'FALSE'
PRP Current_A '3A'
PRP Gender 'Male'
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Sullins Connector Solutions'
PRP MountType 'TH'
PRP Note ''
PRP Orientation 'Vertical'
PRP PackageReference 'Sullins 100mil, 1x2, 230 mil above insulator'
PRP PartNumber 'PBC02SAAN'
PRP PinCount '2'
PRP Pitch_mm '2.54'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count '1'
PRP RowSpacing_mm ''
PRP Shrouded 'N'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'S1011E-02-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Voltage_V '1.8kV'
TOP 0 5.3671057 0.5932509 90 N 157 33 J14-1
TOP 1 5.3671057 0.4932509 90 N 158 1 J14-2
#
# CMP 335
CMP 62 5.2358266 0.5432509 0 N J13 PBC02SAAN ;0=2,1=0.3300
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL 'Y'
PRP Cert_VDE ''
PRP ClassName 'Header'
PRP CNHeader 'TRUE'
PRP Color 'Black'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.sullinscorp.com/catalogs/77_PAGE108-109_.100_MALE_HDR.pdf'
PRP CompType 'Header'
PRP ContactFinish 'Gold'
PRP CT 'FALSE'
PRP Current_A '3A'
PRP Gender 'Male'
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Sullins Connector Solutions'
PRP MountType 'TH'
PRP Note ''
PRP Orientation 'Vertical'
PRP PackageReference 'Sullins 100mil, 1x2, 230 mil above insulator'
PRP PartNumber 'PBC02SAAN'
PRP PinCount '2'
PRP Pitch_mm '2.54'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count '1'
PRP RowSpacing_mm ''
PRP Shrouded 'N'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'S1011E-02-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Voltage_V '1.8kV'
TOP 0 5.2358266 0.5932509 90 N 159 60 J13-1
TOP 1 5.2358266 0.4932509 90 N 160 1 J13-2
#
# CMP 336
CMP 47 5.304172 2.0499998 180 N J12 PBC03SAAN ;0=2,1=0.3300
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName 'Header'
PRP CNHeader 'TRUE'
PRP Color ''
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.sullinscorp.com/catalogs/77_Page78-79_HEADER_.100_2.54mm_MALE_BREAKAWAY.pdf'
PRP CompType 'Header'
PRP ContactFinish ''
PRP CT 'FALSE'
PRP Current_A ''
PRP Gender ''
PRP Green_EU_RoHS 'Incomplete'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Not Set'
PRP Green_REACh 'Incomplete'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Sullins Connector Solutions'
PRP MountType 'TH'
PRP Note ''
PRP Orientation ''
PRP PackageReference 'PBC03SAAN'
PRP PartNumber 'PBC03SAAN'
PRP PinCount ''
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'S1011E-03-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Voltage_V ''
TOP 0 5.404172 2.0499998 180 N 159 62 J12-1
TOP 1 5.304172 2.0499998 180 N 284 219 J12-2
TOP 2 5.204172 2.0499998 180 N 284 220 J12-3
#
# CMP 337
CMP 47 5.304172 0.2499991 180 N J11 PBC03SAAN ;0=2,1=0.3300
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName 'Header'
PRP CNHeader 'TRUE'
PRP Color ''
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.sullinscorp.com/catalogs/77_Page78-79_HEADER_.100_2.54mm_MALE_BREAKAWAY.pdf'
PRP CompType 'Header'
PRP ContactFinish ''
PRP CT 'FALSE'
PRP Current_A ''
PRP Gender ''
PRP Green_EU_RoHS 'Incomplete'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Not Set'
PRP Green_REACh 'Incomplete'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Sullins Connector Solutions'
PRP MountType 'TH'
PRP Note ''
PRP Orientation ''
PRP PackageReference 'PBC03SAAN'
PRP PartNumber 'PBC03SAAN'
PRP PinCount ''
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'S1011E-03-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Voltage_V ''
TOP 0 5.404172 0.2499991 180 N 157 31 J11-1
TOP 1 5.304172 0.2499991 180 N 284 204 J11-2
TOP 2 5.204172 0.2499991 180 N 284 203 J11-3
#
# CMP 338
CMP 62 1.445 0.36 0 N J10 PBC02SAAN ;0=2,1=0.3300
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL 'Y'
PRP Cert_VDE ''
PRP ClassName 'Header'
PRP CNHeader 'TRUE'
PRP Color 'Black'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.sullinscorp.com/catalogs/77_PAGE108-109_.100_MALE_HDR.pdf'
PRP CompType 'Header'
PRP ContactFinish 'Gold'
PRP CT 'FALSE'
PRP Current_A '3A'
PRP Gender 'Male'
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Sullins Connector Solutions'
PRP MountType 'TH'
PRP Note ''
PRP Orientation 'Vertical'
PRP PackageReference 'Sullins 100mil, 1x2, 230 mil above insulator'
PRP PartNumber 'PBC02SAAN'
PRP PinCount '2'
PRP Pitch_mm '2.54'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count '1'
PRP RowSpacing_mm ''
PRP Shrouded 'N'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'S1011E-02-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Voltage_V '1.8kV'
TOP 0 1.445 0.41 90 N 157 32 J10-1
TOP 1 1.445 0.31 90 N 158 0 J10-2
#
# CMP 339
CMP 62 1.4449999 0.1360528 180 N J9 PBC02SAAN ;0=2,1=0.3300
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL 'Y'
PRP Cert_VDE ''
PRP ClassName 'Header'
PRP CNHeader 'TRUE'
PRP Color 'Black'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.sullinscorp.com/catalogs/77_PAGE108-109_.100_MALE_HDR.pdf'
PRP CompType 'Header'
PRP ContactFinish 'Gold'
PRP CT 'FALSE'
PRP Current_A '3A'
PRP Gender 'Male'
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Sullins Connector Solutions'
PRP MountType 'TH'
PRP Note ''
PRP Orientation 'Vertical'
PRP PackageReference 'Sullins 100mil, 1x2, 230 mil above insulator'
PRP PartNumber 'PBC02SAAN'
PRP PinCount '2'
PRP Pitch_mm '2.54'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count '1'
PRP RowSpacing_mm ''
PRP Shrouded 'N'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'S1011E-02-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Voltage_V '1.8kV'
TOP 0 1.4449999 0.0860528 270 N 159 59 J9-1
TOP 1 1.4449999 0.1860528 270 N 160 0 J9-2
#
# CMP 340
CMP 40 7.444 1.645 270 N J8 LPJG16314A4NL ;0=2,1=0.0000
PRP AEC_Qualified 'No'
PRP Conn_Gender 'Female'
PRP Conn_Orientation 'Horizontal'
PRP ContactFinish 'Gold'
PRP Datasheet_Path 'datasheets/Conn-LPJG16314A4NL.pdf'
PRP DUT-Pitch_mm '1.27mm'
PRP helpURL 'https://upverter.com/upn/revision/9003bcdaf47dd8ae/'
PRP Is_Female 'yes'
PRP Lead_free 'Yes'
PRP Manufacturer 'Link-PP'
PRP Operating_Temperature_Range '0°C to +70°C'
PRP PackageReference 'CONN_RJ45'
PRP Part_Number 'LPJG16314A4NL'
PRP PartNumber 'LPJG16314A4NL'
PRP PinCount '8'
PRP RoHS 'TRUE'
PRP SizeZ_mm '13.7mm'
TOP 0 7.0890787 1.42 270 N 284 221 J8-1
TOP 1 7.1890787 1.47 270 N 236 1 J8-2
TOP 2 7.0890787 1.52 270 N 291 3 J8-3
TOP 3 7.1890787 1.57 270 N 292 3 J8-4
TOP 4 7.0890787 1.62 270 N 293 3 J8-5
TOP 5 7.1890787 1.67 270 N 294 3 J8-6
TOP 6 7.0890787 1.72 270 N 295 3 J8-7
TOP 7 7.1890787 1.77 270 N 296 3 J8-8
TOP 8 7.0890787 1.82 270 N 297 3 J8-9
TOP 9 7.1890787 1.87 270 N 298 3 J8-10
TOP 10 7.5390787 1.9097638 270 N 235 1 J8-11
TOP 11 7.619 1.9097638 270 N 234 1 J8-12
TOP 12 7.5390787 1.3802362 270 N 233 2 J8-13
TOP 13 7.619 1.3802362 270 N 232 2 J8-14
TOP 14 7.319 1.3349606 270 N 43 8 J8-15
TOP 15 7.319 1.9550394 270 N 43 7 J8-16
TOP 16 7.4390787 1.42 270 N 0 119 J8-empty-1
TOP 17 7.4390787 1.87 270 N 0 118 J8-empty-2
#
# CMP 341
CMP 41 7.444 0.655 270 N J7 LPJG16314A4NL ;0=2,1=0.0000
PRP AEC_Qualified 'No'
PRP Conn_Gender 'Female'
PRP Conn_Orientation 'Horizontal'
PRP ContactFinish 'Gold'
PRP Datasheet_Path 'datasheets/Conn-LPJG16314A4NL.pdf'
PRP DUT-Pitch_mm '1.27mm'
PRP helpURL 'https://upverter.com/upn/revision/9003bcdaf47dd8ae/'
PRP Is_Female 'yes'
PRP Lead_free 'Yes'
PRP Manufacturer 'Link-PP'
PRP Operating_Temperature_Range '0°C to +70°C'
PRP PackageReference 'CONN_RJ45'
PRP Part_Number 'LPJG16314A4NL'
PRP PartNumber 'LPJG16314A4NL'
PRP PinCount '8'
PRP RoHS 'TRUE'
PRP SizeZ_mm '13.7mm'
TOP 0 7.0890787 0.43 270 N 284 202 J7-1
TOP 1 7.1890787 0.48 270 N 236 0 J7-2
TOP 2 7.0890787 0.53 270 N 311 3 J7-3
TOP 3 7.1890787 0.58 270 N 312 3 J7-4
TOP 4 7.0890787 0.63 270 N 313 3 J7-5
TOP 5 7.1890787 0.68 270 N 314 3 J7-6
TOP 6 7.0890787 0.73 270 N 315 3 J7-7
TOP 7 7.1890787 0.78 270 N 316 3 J7-8
TOP 8 7.0890787 0.83 270 N 317 3 J7-9
TOP 9 7.1890787 0.88 270 N 318 3 J7-10
TOP 10 7.5390787 0.9197638 270 N 240 1 J7-11
TOP 11 7.619 0.9197638 270 N 239 1 J7-12
TOP 12 7.5390787 0.3902362 270 N 238 0 J7-13
TOP 13 7.619 0.3902362 270 N 237 2 J7-14
TOP 14 7.319 0.3449606 270 N 44 7 J7-15
TOP 15 7.319 0.9650394 270 N 44 8 J7-16
TOP 16 7.4390787 0.88 270 N 0 111 J7-empty-1
TOP 17 7.4390787 0.43 270 N 0 110 J7-empty-2
#
# CMP 342
CMP 33 1.118346 0.1545273 0 N J5 2012670005 ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.molex.com/webdocs/datasheets/pdf/en-us/2012670005_IO_CONNECTORS.pdf'
PRP Conn_Orientation 'Right Angle'
PRP ContactFinish 'Gold,Nickel'
PRP DataSheet 'https://www.molex.com/webdocs/datasheets/pdf/en-us/2012670005_IO_CONNECTORS.pdf'
PRP Datasheet_Path 'datasheets/Conn-2012670005.pdf'
PRP Digikey_Description 'CONN RCP USB3.1 TYPEC 24P SMD RA'
PRP Digikey_Part_Number 'WM17992CT-ND'
PRP DUT-Pitch_mm '0.5mm'
PRP helpURL 'https://upverter.com/upn/revision/a684ef3764071fb6/'
PRP Is_Female 'yes'
PRP Lead_free 'Yes'
PRP Manufacturer 'Molex'
PRP Mouser_Part_Number '538-201267-0005'
PRP Operating_Temperature_Range '-40°C to +105°C'
PRP PackageReference 'CONN_USB_9MM39_8MM21'
PRP PartId '1'
PRP Part_Number '2012670005'
PRP PartNumber '2012670005'
PRP PinCount '24'
PRP RoHS 'TRUE'
PRP Shrouded 'true'
PRP SizeZ_mm '3.86mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'WM17992CT-ND'
PRP Supplier_Part_Number_2 '538-201267-0005'
PRP Usb_Standard 'USB 3.1'
PRP Voltage_V '30V'
TOP 0 0.9482673 0.2807084 0 N 45 7 J5-1
TOP 1 1.2884247 0.2807084 0 N 45 8 J5-2
TOP 2 0.9364562 0.0893698 0 N 45 5 J5-3
TOP 3 0.9364562 0.0696848 0 N 45 9 J5-3
TOP 4 0.9364562 0.0893698 0 N 45 13 J5-3
TOP 5 1.3002358 0.0893698 0 N 45 6 J5-4
TOP 6 1.3002358 0.0696848 0 N 45 10 J5-4
TOP 7 1.3002358 0.0893698 0 N 45 14 J5-4
TOP 8 1.0002358 0.3125982 0 N 284 444 J5-A1
TOP 9 1.0199208 0.3125982 0 N 0 144 J5-A2
TOP 10 1.0396058 0.3125982 0 N 0 145 J5-A3
TOP 11 1.0592909 0.3125982 0 N 177 6 J5-A4
TOP 12 1.0789759 0.3125982 0 N 179 3 J5-A5
TOP 13 1.098661 0.3125982 0 N 0 146 J5-A6
TOP 14 1.138031 0.3125982 0 N 0 147 J5-A7
TOP 15 1.1577161 0.3125982 0 N 0 148 J5-A8
TOP 16 1.1774011 0.3125982 0 N 177 7 J5-A9
TOP 17 1.1970862 0.3125982 0 N 0 149 J5-A10
TOP 18 1.2167712 0.3125982 0 N 0 150 J5-A11
TOP 19 1.2364562 0.3125982 0 N 284 445 J5-A12
TOP 20 1.2384247 0.245669 0 N 284 446 J5-B1
TOP 21 1.2069287 0.245669 0 N 0 151 J5-B2
TOP 22 1.1872436 0.245669 0 N 0 152 J5-B3
TOP 23 1.1675586 0.245669 0 N 177 8 J5-B4
TOP 24 1.1478736 0.245669 0 N 178 3 J5-B5
TOP 25 1.1281885 0.245669 0 N 0 153 J5-B6
TOP 26 1.1085035 0.245669 0 N 0 154 J5-B7
TOP 27 1.0888184 0.245669 0 N 0 155 J5-B8
TOP 28 1.0691334 0.245669 0 N 177 9 J5-B9
TOP 29 1.0494484 0.245669 0 N 0 156 J5-B10
TOP 30 1.0297633 0.245669 0 N 0 157 J5-B11
TOP 31 0.9982673 0.245669 0 N 284 447 J5-B12
#
# CMP 343
CMP 62 1.3955401 1.975 180 N J1 PBC02SAAN ;0=2,1=0.3300
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL 'Y'
PRP Cert_VDE ''
PRP ClassName 'Header'
PRP CNHeader 'TRUE'
PRP Color 'Black'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.sullinscorp.com/catalogs/77_PAGE108-109_.100_MALE_HDR.pdf'
PRP CompType 'Header'
PRP ContactFinish 'Gold'
PRP CT 'FALSE'
PRP Current_A '3A'
PRP Gender 'Male'
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Sullins Connector Solutions'
PRP MountType 'TH'
PRP Note ''
PRP Orientation 'Vertical'
PRP PackageReference 'Sullins 100mil, 1x2, 230 mil above insulator'
PRP PartNumber 'PBC02SAAN'
PRP PinCount '2'
PRP Pitch_mm '2.54'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count '1'
PRP RowSpacing_mm ''
PRP Shrouded 'N'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'S1011E-02-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Voltage_V '1.8kV'
TOP 0 1.3955401 1.925 270 N 2 0 J1-1
TOP 1 1.3955401 2.025 270 N 220 2 J1-2
#
# CMP 344
CMP 37 6.1886756 1.1886383 0 N FB6 BLM18EG121SN1D ;0=1,1=0.0461
PRP AEC_Qualified 'No'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.murata.com/en-us/products/productdata/8796747366430/ENFA0021.pdf'
PRP DataSheet 'https://www.murata.com/en-us/products/productdata/8796747366430/ENFA0021.pdf'
PRP Datasheet_Path 'datasheets/FBead-BLM18EG121SN1D.pdf'
PRP DCR_ohm '60m'
PRP Device_Class_L1 'Passive Components'
PRP Device_Class_L2 'EMI / RFI Components'
PRP Device_Class_L3 'Ferrite Beads and Chips'
PRP Digikey_Description 'FERRITE BEAD 120 OHM 0603 1LN'
PRP Digikey_Part_Number '490-3991-1-ND'
PRP helpURL 'https://upverter.com/upn/revision/3e0d9a214349089d/'
PRP Imax_A '2A'
PRP Impedance_At_Frequency '120O @ 100MHz'
PRP Lead_free 'Yes'
PRP Manufacturer 'Murata'
PRP Material 'Ferrite'
PRP Mouser_Description 'Ferrite Beads 120ohms GHz General Usage'
PRP Mouser_Part_Number '81-BLM18EG121SN1D'
PRP Operating_Temperature_Range '-55°C to +125°C'
PRP PackageReference '0603'
PRP Part_Number 'BLM18EG121SN1D'
PRP PartNumber 'BLM18EG121SN1D'
PRP RoHS 'TRUE'
PRP SizeZ_mm '0.95mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 '490-3991-1-ND'
PRP Supplier_Part_Number_2 '81-BLM18EG121SN1D'
PRP Tolerance__ '25%'
TOP 0 6.1621008 1.1886383 0 N 169 8 FB6-1
TOP 1 6.2152504 1.1886383 0 N 171 9 FB6-2
#
# CMP 345
CMP 37 6.1886756 1.4494371 0 N FB5 BLM18EG121SN1D ;0=1,1=0.0461
PRP AEC_Qualified 'No'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.murata.com/en-us/products/productdata/8796747366430/ENFA0021.pdf'
PRP DataSheet 'https://www.murata.com/en-us/products/productdata/8796747366430/ENFA0021.pdf'
PRP Datasheet_Path 'datasheets/FBead-BLM18EG121SN1D.pdf'
PRP DCR_ohm '60m'
PRP Device_Class_L1 'Passive Components'
PRP Device_Class_L2 'EMI / RFI Components'
PRP Device_Class_L3 'Ferrite Beads and Chips'
PRP Digikey_Description 'FERRITE BEAD 120 OHM 0603 1LN'
PRP Digikey_Part_Number '490-3991-1-ND'
PRP helpURL 'https://upverter.com/upn/revision/3e0d9a214349089d/'
PRP Imax_A '2A'
PRP Impedance_At_Frequency '120O @ 100MHz'
PRP Lead_free 'Yes'
PRP Manufacturer 'Murata'
PRP Material 'Ferrite'
PRP Mouser_Description 'Ferrite Beads 120ohms GHz General Usage'
PRP Mouser_Part_Number '81-BLM18EG121SN1D'
PRP Operating_Temperature_Range '-55°C to +125°C'
PRP PackageReference '0603'
PRP Part_Number 'BLM18EG121SN1D'
PRP PartNumber 'BLM18EG121SN1D'
PRP RoHS 'TRUE'
PRP SizeZ_mm '0.95mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 '490-3991-1-ND'
PRP Supplier_Part_Number_2 '81-BLM18EG121SN1D'
PRP Tolerance__ '25%'
TOP 0 6.1621008 1.4494371 0 N 170 5 FB5-1
TOP 1 6.2152504 1.4494371 0 N 172 9 FB5-2
#
# CMP 346
CMP 37 6.1159169 0.9708987 0 N FB4 BLM18EG121SN1D ;0=1,1=0.0461
PRP AEC_Qualified 'No'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.murata.com/en-us/products/productdata/8796747366430/ENFA0021.pdf'
PRP DataSheet 'https://www.murata.com/en-us/products/productdata/8796747366430/ENFA0021.pdf'
PRP Datasheet_Path 'datasheets/FBead-BLM18EG121SN1D.pdf'
PRP DCR_ohm '60m'
PRP Device_Class_L1 'Passive Components'
PRP Device_Class_L2 'EMI / RFI Components'
PRP Device_Class_L3 'Ferrite Beads and Chips'
PRP Digikey_Description 'FERRITE BEAD 120 OHM 0603 1LN'
PRP Digikey_Part_Number '490-3991-1-ND'
PRP helpURL 'https://upverter.com/upn/revision/3e0d9a214349089d/'
PRP Imax_A '2A'
PRP Impedance_At_Frequency '120O @ 100MHz'
PRP Lead_free 'Yes'
PRP Manufacturer 'Murata'
PRP Material 'Ferrite'
PRP Mouser_Description 'Ferrite Beads 120ohms GHz General Usage'
PRP Mouser_Part_Number '81-BLM18EG121SN1D'
PRP Operating_Temperature_Range '-55°C to +125°C'
PRP PackageReference '0603'
PRP Part_Number 'BLM18EG121SN1D'
PRP PartNumber 'BLM18EG121SN1D'
PRP RoHS 'TRUE'
PRP SizeZ_mm '0.95mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 '490-3991-1-ND'
PRP Supplier_Part_Number_2 '81-BLM18EG121SN1D'
PRP Tolerance__ '25%'
TOP 0 6.0893421 0.9708987 0 N 169 2 FB4-1
TOP 1 6.1424917 0.9708987 0 N 173 5 FB4-2
#
# CMP 347
CMP 37 6.1886756 1.3105458 0 N FB3 BLM18EG121SN1D ;0=1,1=0.0461
PRP AEC_Qualified 'No'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.murata.com/en-us/products/productdata/8796747366430/ENFA0021.pdf'
PRP DataSheet 'https://www.murata.com/en-us/products/productdata/8796747366430/ENFA0021.pdf'
PRP Datasheet_Path 'datasheets/FBead-BLM18EG121SN1D.pdf'
PRP DCR_ohm '60m'
PRP Device_Class_L1 'Passive Components'
PRP Device_Class_L2 'EMI / RFI Components'
PRP Device_Class_L3 'Ferrite Beads and Chips'
PRP Digikey_Description 'FERRITE BEAD 120 OHM 0603 1LN'
PRP Digikey_Part_Number '490-3991-1-ND'
PRP helpURL 'https://upverter.com/upn/revision/3e0d9a214349089d/'
PRP Imax_A '2A'
PRP Impedance_At_Frequency '120O @ 100MHz'
PRP Lead_free 'Yes'
PRP Manufacturer 'Murata'
PRP Material 'Ferrite'
PRP Mouser_Description 'Ferrite Beads 120ohms GHz General Usage'
PRP Mouser_Part_Number '81-BLM18EG121SN1D'
PRP Operating_Temperature_Range '-55°C to +125°C'
PRP PackageReference '0603'
PRP Part_Number 'BLM18EG121SN1D'
PRP PartNumber 'BLM18EG121SN1D'
PRP RoHS 'TRUE'
PRP SizeZ_mm '0.95mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 '490-3991-1-ND'
PRP Supplier_Part_Number_2 '81-BLM18EG121SN1D'
PRP Tolerance__ '25%'
TOP 0 6.1621008 1.3105458 0 N 170 6 FB3-1
TOP 1 6.2152504 1.3105458 0 N 174 10 FB3-2
#
# CMP 348
CMP 71 2.703 1.992402 180 N DS1 150060RS75000 ;0=1,1=0.0315
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Angle '140'
PRP Color 'Red'
PRP ColorTemperature ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://katalog.we-online.de/led/datasheet/150060RS75000.pdf'
PRP CompType 'LED'
PRP DynamicResistance ''
PRP Family_Io ''
PRP FamilyName ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Io_A '30mA'
PRP Ir_A ''
PRP LambdaD ''
PRP LambdaP ''
PRP Luminance_Lv ''
PRP LuminousFlux_PhiV ''
PRP LuminousIntensity_IV ''
PRP Manufacturer 'Wurth Elektronik'
PRP MountType 'SMT'
PRP NumParallelLEDs ''
PRP NumSeriesLEDs ''
PRP PackageReference 'LED_0603'
PRP PartNumber '150060RS75000'
PRP Power_TotalModule '72mW'
PRP RJC_CperW ''
PRP RoHS 'Y'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm ''
PRP TJmax_C '85°C'
PRP TYPE 'AlInGaP'
PRP Value 'Red'
PRP Value1 '0.072W'
PRP Value2 '2V'
PRP Vf_V '2V'
PRP Vr_V '5V'
TOP 0 2.734496 1.992402 180 N 259 0 DS1-1
TOP 1 2.6715039 1.992402 180 N 258 1 DS1-2
#
# CMP 349
CMP 70 1.6778741 2.208307 270 N D14 150060VS75000 ;0=1,1=0.0315
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Angle ''
PRP Color 'green'
PRP ColorTemperature ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://katalog.we-online.de/led/datasheet/150060VS75000.pdf'
PRP CompType 'LED'
PRP DynamicResistance ''
PRP Family_Io ''
PRP FamilyName ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Io_A '20mA'
PRP Ir_A ''
PRP LambdaD ''
PRP LambdaP ''
PRP Luminance_Lv ''
PRP LuminousFlux_PhiV ''
PRP LuminousIntensity_IV ''
PRP Manufacturer 'Wurth Elektronik'
PRP MountType 'SMT'
PRP NumParallelLEDs ''
PRP NumSeriesLEDs ''
PRP PackageReference 'LED_0603'
PRP PartNumber '150060VS75000'
PRP Power_TotalModule ''
PRP RJC_CperW ''
PRP RoHS 'Y'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm ''
PRP TJmax_C ''
PRP TYPE 'AlInGaP'
PRP Value 'Green'
PRP Value1 'W'
PRP Value2 '2V'
PRP Vf_V '2V'
PRP Vr_V ''
TOP 0 1.6778741 2.176811 270 N 264 0 D14-1
TOP 1 1.6778741 2.2398031 270 N 272 0 D14-2
#
# CMP 350
CMP 70 1.797874 2.2083071 270 N D13 150060VS75000 ;0=1,1=0.0315
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Angle ''
PRP Color 'green'
PRP ColorTemperature ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://katalog.we-online.de/led/datasheet/150060VS75000.pdf'
PRP CompType 'LED'
PRP DynamicResistance ''
PRP Family_Io ''
PRP FamilyName ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Io_A '20mA'
PRP Ir_A ''
PRP LambdaD ''
PRP LambdaP ''
PRP Luminance_Lv ''
PRP LuminousFlux_PhiV ''
PRP LuminousIntensity_IV ''
PRP Manufacturer 'Wurth Elektronik'
PRP MountType 'SMT'
PRP NumParallelLEDs ''
PRP NumSeriesLEDs ''
PRP PackageReference 'LED_0603'
PRP PartNumber '150060VS75000'
PRP Power_TotalModule ''
PRP RJC_CperW ''
PRP RoHS 'Y'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm ''
PRP TJmax_C ''
PRP TYPE 'AlInGaP'
PRP Value 'Green'
PRP Value1 'W'
PRP Value2 '2V'
PRP Vf_V '2V'
PRP Vr_V ''
TOP 0 1.797874 2.1768111 270 N 265 0 D13-1
TOP 1 1.797874 2.2398032 270 N 273 0 D13-2
#
# CMP 351
CMP 70 1.9378739 2.2083072 270 N D12 150060VS75000 ;0=1,1=0.0315
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Angle ''
PRP Color 'green'
PRP ColorTemperature ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://katalog.we-online.de/led/datasheet/150060VS75000.pdf'
PRP CompType 'LED'
PRP DynamicResistance ''
PRP Family_Io ''
PRP FamilyName ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Io_A '20mA'
PRP Ir_A ''
PRP LambdaD ''
PRP LambdaP ''
PRP Luminance_Lv ''
PRP LuminousFlux_PhiV ''
PRP LuminousIntensity_IV ''
PRP Manufacturer 'Wurth Elektronik'
PRP MountType 'SMT'
PRP NumParallelLEDs ''
PRP NumSeriesLEDs ''
PRP PackageReference 'LED_0603'
PRP PartNumber '150060VS75000'
PRP Power_TotalModule ''
PRP RJC_CperW ''
PRP RoHS 'Y'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm ''
PRP TJmax_C ''
PRP TYPE 'AlInGaP'
PRP Value 'Green'
PRP Value1 'W'
PRP Value2 '2V'
PRP Vf_V '2V'
PRP Vr_V ''
TOP 0 1.9378739 2.1768112 270 N 266 0 D12-1
TOP 1 1.9378739 2.2398033 270 N 274 1 D12-2
#
# CMP 352
CMP 70 2.0778738 2.2083073 270 N D11 150060VS75000 ;0=1,1=0.0315
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Angle ''
PRP Color 'green'
PRP ColorTemperature ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://katalog.we-online.de/led/datasheet/150060VS75000.pdf'
PRP CompType 'LED'
PRP DynamicResistance ''
PRP Family_Io ''
PRP FamilyName ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Io_A '20mA'
PRP Ir_A ''
PRP LambdaD ''
PRP LambdaP ''
PRP Luminance_Lv ''
PRP LuminousFlux_PhiV ''
PRP LuminousIntensity_IV ''
PRP Manufacturer 'Wurth Elektronik'
PRP MountType 'SMT'
PRP NumParallelLEDs ''
PRP NumSeriesLEDs ''
PRP PackageReference 'LED_0603'
PRP PartNumber '150060VS75000'
PRP Power_TotalModule ''
PRP RJC_CperW ''
PRP RoHS 'Y'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm ''
PRP TJmax_C ''
PRP TYPE 'AlInGaP'
PRP Value 'Green'
PRP Value1 'W'
PRP Value2 '2V'
PRP Vf_V '2V'
PRP Vr_V ''
TOP 0 2.0778738 2.1768113 270 N 267 0 D11-1
TOP 1 2.0778738 2.2398034 270 N 275 0 D11-2
#
# CMP 353
CMP 70 2.2492913 2.2083072 270 N D10 150060VS75000 ;0=1,1=0.0315
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Angle ''
PRP Color 'green'
PRP ColorTemperature ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://katalog.we-online.de/led/datasheet/150060VS75000.pdf'
PRP CompType 'LED'
PRP DynamicResistance ''
PRP Family_Io ''
PRP FamilyName ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Io_A '20mA'
PRP Ir_A ''
PRP LambdaD ''
PRP LambdaP ''
PRP Luminance_Lv ''
PRP LuminousFlux_PhiV ''
PRP LuminousIntensity_IV ''
PRP Manufacturer 'Wurth Elektronik'
PRP MountType 'SMT'
PRP NumParallelLEDs ''
PRP NumSeriesLEDs ''
PRP PackageReference 'LED_0603'
PRP PartNumber '150060VS75000'
PRP Power_TotalModule ''
PRP RJC_CperW ''
PRP RoHS 'Y'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm ''
PRP TJmax_C ''
PRP TYPE 'AlInGaP'
PRP Value 'Green'
PRP Value1 'W'
PRP Value2 '2V'
PRP Vf_V '2V'
PRP Vr_V ''
TOP 0 2.2492913 2.1768112 270 N 268 0 D10-1
TOP 1 2.2492913 2.2398033 270 N 276 0 D10-2
#
# CMP 354
CMP 70 2.3892912 2.2083073 270 N D9 150060VS75000 ;0=1,1=0.0315
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Angle ''
PRP Color 'green'
PRP ColorTemperature ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://katalog.we-online.de/led/datasheet/150060VS75000.pdf'
PRP CompType 'LED'
PRP DynamicResistance ''
PRP Family_Io ''
PRP FamilyName ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Io_A '20mA'
PRP Ir_A ''
PRP LambdaD ''
PRP LambdaP ''
PRP Luminance_Lv ''
PRP LuminousFlux_PhiV ''
PRP LuminousIntensity_IV ''
PRP Manufacturer 'Wurth Elektronik'
PRP MountType 'SMT'
PRP NumParallelLEDs ''
PRP NumSeriesLEDs ''
PRP PackageReference 'LED_0603'
PRP PartNumber '150060VS75000'
PRP Power_TotalModule ''
PRP RJC_CperW ''
PRP RoHS 'Y'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm ''
PRP TJmax_C ''
PRP TYPE 'AlInGaP'
PRP Value 'Green'
PRP Value1 'W'
PRP Value2 '2V'
PRP Vf_V '2V'
PRP Vr_V ''
TOP 0 2.3892912 2.1768113 270 N 269 0 D9-1
TOP 1 2.3892912 2.2398034 270 N 277 0 D9-2
#
# CMP 355
CMP 70 2.5292911 2.2083075 270 N D8 150060VS75000 ;0=1,1=0.0315
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Angle ''
PRP Color 'green'
PRP ColorTemperature ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://katalog.we-online.de/led/datasheet/150060VS75000.pdf'
PRP CompType 'LED'
PRP DynamicResistance ''
PRP Family_Io ''
PRP FamilyName ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Io_A '20mA'
PRP Ir_A ''
PRP LambdaD ''
PRP LambdaP ''
PRP Luminance_Lv ''
PRP LuminousFlux_PhiV ''
PRP LuminousIntensity_IV ''
PRP Manufacturer 'Wurth Elektronik'
PRP MountType 'SMT'
PRP NumParallelLEDs ''
PRP NumSeriesLEDs ''
PRP PackageReference 'LED_0603'
PRP PartNumber '150060VS75000'
PRP Power_TotalModule ''
PRP RJC_CperW ''
PRP RoHS 'Y'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm ''
PRP TJmax_C ''
PRP TYPE 'AlInGaP'
PRP Value 'Green'
PRP Value1 'W'
PRP Value2 '2V'
PRP Vf_V '2V'
PRP Vr_V ''
TOP 0 2.5292911 2.1768115 270 N 270 0 D8-1
TOP 1 2.5292911 2.2398036 270 N 278 0 D8-2
#
# CMP 356
CMP 70 2.669291 2.2083075 270 N D7 150060VS75000 ;0=1,1=0.0315
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Angle ''
PRP Color 'green'
PRP ColorTemperature ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://katalog.we-online.de/led/datasheet/150060VS75000.pdf'
PRP CompType 'LED'
PRP DynamicResistance ''
PRP Family_Io ''
PRP FamilyName ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Io_A '20mA'
PRP Ir_A ''
PRP LambdaD ''
PRP LambdaP ''
PRP Luminance_Lv ''
PRP LuminousFlux_PhiV ''
PRP LuminousIntensity_IV ''
PRP Manufacturer 'Wurth Elektronik'
PRP MountType 'SMT'
PRP NumParallelLEDs ''
PRP NumSeriesLEDs ''
PRP PackageReference 'LED_0603'
PRP PartNumber '150060VS75000'
PRP Power_TotalModule ''
PRP RJC_CperW ''
PRP RoHS 'Y'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm ''
PRP TJmax_C ''
PRP TYPE 'AlInGaP'
PRP Value 'Green'
PRP Value1 'W'
PRP Value2 '2V'
PRP Vf_V '2V'
PRP Vr_V ''
TOP 0 2.669291 2.1768115 270 N 271 0 D7-1
TOP 1 2.669291 2.2398036 270 N 279 1 D7-2
#
# CMP 357
CMP 70 2.835 0.1197471 0 N D6 150060VS75000 ;0=1,1=0.0315
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Angle ''
PRP Color 'green'
PRP ColorTemperature ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://katalog.we-online.de/led/datasheet/150060VS75000.pdf'
PRP CompType 'LED'
PRP DynamicResistance ''
PRP Family_Io ''
PRP FamilyName ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Io_A '20mA'
PRP Ir_A ''
PRP LambdaD ''
PRP LambdaP ''
PRP Luminance_Lv ''
PRP LuminousFlux_PhiV ''
PRP LuminousIntensity_IV ''
PRP Manufacturer 'Wurth Elektronik'
PRP MountType 'SMT'
PRP NumParallelLEDs ''
PRP NumSeriesLEDs ''
PRP PackageReference 'LED_0603'
PRP PartNumber '150060VS75000'
PRP Power_TotalModule ''
PRP RJC_CperW ''
PRP RoHS 'Y'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm ''
PRP TJmax_C ''
PRP TYPE 'AlInGaP'
PRP Value 'Green'
PRP Value1 'W'
PRP Value2 '2V'
PRP Vf_V '2V'
PRP Vr_V ''
TOP 0 2.803504 0.1197471 0 N 284 266 D6-1
TOP 1 2.8664961 0.1197471 0 N 87 0 D6-2
#
# CMP 358
CMP 70 2.0362695 0.0918975 90 N D5 150060VS75000 ;0=1,1=0.0315
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Angle ''
PRP Color 'green'
PRP ColorTemperature ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://katalog.we-online.de/led/datasheet/150060VS75000.pdf'
PRP CompType 'LED'
PRP DynamicResistance ''
PRP Family_Io ''
PRP FamilyName ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Io_A '20mA'
PRP Ir_A ''
PRP LambdaD ''
PRP LambdaP ''
PRP Luminance_Lv ''
PRP LuminousFlux_PhiV ''
PRP LuminousIntensity_IV ''
PRP Manufacturer 'Wurth Elektronik'
PRP MountType 'SMT'
PRP NumParallelLEDs ''
PRP NumSeriesLEDs ''
PRP PackageReference 'LED_0603'
PRP PartNumber '150060VS75000'
PRP Power_TotalModule ''
PRP RJC_CperW ''
PRP RoHS 'Y'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm ''
PRP TJmax_C ''
PRP TYPE 'AlInGaP'
PRP Value 'Green'
PRP Value1 'W'
PRP Value2 '2V'
PRP Vf_V '2V'
PRP Vr_V ''
TOP 0 2.0362695 0.1233935 90 N 89 0 D5-1
TOP 1 2.0362695 0.0604014 90 N 88 0 D5-2
#
# CMP 359
CMP 70 2.812725 2.2122444 270 N D4 150060VS75000 ;0=1,1=0.0315
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Angle ''
PRP Color 'green'
PRP ColorTemperature ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://katalog.we-online.de/led/datasheet/150060VS75000.pdf'
PRP CompType 'LED'
PRP DynamicResistance ''
PRP Family_Io ''
PRP FamilyName ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Io_A '20mA'
PRP Ir_A ''
PRP LambdaD ''
PRP LambdaP ''
PRP Luminance_Lv ''
PRP LuminousFlux_PhiV ''
PRP LuminousIntensity_IV ''
PRP Manufacturer 'Wurth Elektronik'
PRP MountType 'SMT'
PRP NumParallelLEDs ''
PRP NumSeriesLEDs ''
PRP PackageReference 'LED_0603'
PRP PartNumber '150060VS75000'
PRP Power_TotalModule ''
PRP RJC_CperW ''
PRP RoHS 'Y'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm ''
PRP TJmax_C ''
PRP TYPE 'AlInGaP'
PRP Value 'Green'
PRP Value1 'W'
PRP Value2 '2V'
PRP Vf_V '2V'
PRP Vr_V ''
TOP 0 2.812725 2.1807484 270 N 284 267 D4-1
TOP 1 2.812725 2.2437405 270 N 90 0 D4-2
#
# CMP 360
CMP 70 1.8982675 1.0017011 90 N D2 150060VS75000 ;0=1,1=0.0315
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Angle ''
PRP Color 'green'
PRP ColorTemperature ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://katalog.we-online.de/led/datasheet/150060VS75000.pdf'
PRP CompType 'LED'
PRP DynamicResistance ''
PRP Family_Io ''
PRP FamilyName ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Io_A '20mA'
PRP Ir_A ''
PRP LambdaD ''
PRP LambdaP ''
PRP Luminance_Lv ''
PRP LuminousFlux_PhiV ''
PRP LuminousIntensity_IV ''
PRP Manufacturer 'Wurth Elektronik'
PRP MountType 'SMT'
PRP NumParallelLEDs ''
PRP NumSeriesLEDs ''
PRP PackageReference 'LED_0603'
PRP PartNumber '150060VS75000'
PRP Power_TotalModule ''
PRP RJC_CperW ''
PRP RoHS 'Y'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm ''
PRP TJmax_C ''
PRP TYPE 'AlInGaP'
PRP Value 'Green'
PRP Value1 'W'
PRP Value2 '2V'
PRP Vf_V '2V'
PRP Vr_V ''
TOP 0 1.8982675 1.0331971 90 N 284 265 D2-1
TOP 1 1.8982675 0.970205 90 N 260 1 D2-2
#
# CMP 361
CMP 1 2.3459447 1.4213783 90 N C237 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 2.3459447 1.4450003 0 N 159 67 C237-1
TOP 1 2.3459447 1.3977562 0 N 284 246 C237-2
#
# CMP 362
CMP 5 2.405945 1.4135039 90 N C236 C1608X7S1A335K080AC ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '3.3µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=C1608X7S1A335K080AC'
PRP CompType 'Capacitor'
PRP ESR_ohm '4.796m'
PRP IRMS_A '2.3752A'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'C1608X7S1A335K080AC'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '445-14256-1-ND'
PRP Supplier_Part_Number_2 '52X3755'
PRP Supplier_Part_Number_3 '810-C1608X7S1A335K0C'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7S'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '3.3uF'
PRP Value1 '0.004796 ohm'
PRP Value2 '10V'
PRP ValueDisplayed '3.3uF'
PRP VDC_V '10V'
TOP 0 2.405945 1.445 0 N 159 68 C236-1
TOP 1 2.405945 1.3820079 0 N 284 247 C236-2
#
# CMP 363
CMP 8 7.235 1.115 0 N C235 GR442QR73D102KW01L ;0=1,1=0.0799
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '1808'
PRP Cap_F '1nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.murata.com/capacitor/product/GR442QR73D102KW01%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '1808'
PRP PartNumber 'GR442QR73D102KW01L'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '9'
PRP SizeAreaWB_mm2 '16.5'
PRP SizeX_mm '4.5'
PRP SizeY_mm '2'
PRP SizeZ_mm '2.03'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-8145-1-ND'
PRP Supplier_Part_Number_2 '31Y1776'
PRP Supplier_Part_Number_3 '81-GR442QR73D102KW01'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '1000pF'
PRP Value1 'Unknown'
PRP Value2 '2000V'
PRP ValueDisplayed '1000pF'
PRP VDC_V '2kV'
TOP 0 7.1523229 1.115 270 N 284 372 C235-1
TOP 1 7.3176772 1.115 270 N 44 10 C235-2
#
# CMP 364
CMP 1 0.5775647 0.9622677 90 N C233 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 0.5775647 0.9858897 0 N 285 47 C233-1
TOP 1 0.5775647 0.9386456 0 N 168 37 C233-2
#
# CMP 365
CMP 2 0.66 1.0401492 270 N C232 GCM155C71A105KE38D ;0=1,1=0.0276
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM155C71A105KE38%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155C71A105KE38D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.7'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GCM155C71A105KE8D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7S'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '1uF'
PRP VDC_V '10V'
TOP 0 0.66 1.0201492 180 N 168 24 C232-1
TOP 1 0.66 1.0601492 180 N 285 30 C232-2
#
# CMP 366
CMP 1 0.352829 0.9622677 270 N C231 GRM155C81C225KE11D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '2.2µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155C81C225KE11-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155C81C225KE11D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155C81C225KE11D-ND'
PRP Supplier_Part_Number_2 '81-GRM155C81C225KE1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '105°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X6S'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '2.2uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '2.2uF'
PRP VDC_V '16V'
TOP 0 0.352829 0.9386457 180 N 176 6 C231-1
TOP 1 0.352829 0.9858898 180 N 285 38 C231-2
#
# CMP 367
CMP 8 0.7314568 0.1801183 0 N C229 GR442QR73D102KW01L ;0=1,1=0.0799
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '1808'
PRP Cap_F '1nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.murata.com/capacitor/product/GR442QR73D102KW01%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '1808'
PRP PartNumber 'GR442QR73D102KW01L'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '9'
PRP SizeAreaWB_mm2 '16.5'
PRP SizeX_mm '4.5'
PRP SizeY_mm '2'
PRP SizeZ_mm '2.03'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-8145-1-ND'
PRP Supplier_Part_Number_2 '31Y1776'
PRP Supplier_Part_Number_3 '81-GR442QR73D102KW01'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '1000pF'
PRP Value1 'Unknown'
PRP Value2 '2000V'
PRP ValueDisplayed '1000pF'
PRP VDC_V '2kV'
TOP 0 0.6487797 0.1801183 270 N 284 388 C229-1
TOP 1 0.814134 0.1801183 270 N 45 12 C229-2
#
# CMP 368
CMP 1 0.6586481 1.1247603 180 N C228 GRM1555C1H150JA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '15pF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM1555C1H150JA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM1555C1H150JA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GRM1555C1H150JA1D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'C0G/NP0'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '15pF'
PRP Value1 'Unknown'
PRP Value2 '50V'
PRP ValueDisplayed '15pF'
PRP VDC_V '50V'
TOP 0 0.6822701 1.1247603 90 N 168 30 C228-1
TOP 1 0.635026 1.1247603 90 N 286 2 C228-2
#
# CMP 369
CMP 1 7.01 0.0604014 180 N C226 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 7.033622 0.0604014 90 N 284 387 C226-1
TOP 1 6.9863779 0.0604014 90 N 159 136 C226-2
#
# CMP 370
CMP 1 6.94 0.265 270 N C222 GCM155R71H472KA37D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '4.7nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.murata.com/capacitor/product/GCM155R71H472KA37%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71H472KA37D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-4915-1-ND'
PRP Supplier_Part_Number_2 '81-GCM155R71H472K37D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '4700pF'
PRP Value1 'Unknown'
PRP Value2 '50V'
PRP ValueDisplayed '4700pF'
PRP VDC_V '50V'
TOP 0 6.94 0.241378 180 N 261 2 C222-1
TOP 1 6.94 0.2886221 180 N 284 270 C222-2
#
# CMP 371
CMP 5 6.1971254 0.494672 180 N C221 GCM1885C1H102JA16D ;0=1,1=0.0394
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '1nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://psearch.en.murata.com/capacitor/product/GCM1885C1H102JA16%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Incomplete'
PRP IRMS_A ''
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCM1885C1H102JA16D'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'C0G/NP0'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '1000pF'
PRP Value1 ''
PRP Value2 '50V'
PRP ValueDisplayed '1000pF'
PRP VDC_V '50V'
TOP 0 6.2286215 0.494672 90 N 343 2 C221-1
TOP 1 6.1656294 0.494672 90 N 284 222 C221-2
#
# CMP 372
CMP 1 6.379136 1.6450379 180 N C210 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 6.402758 1.6450379 90 N 159 109 C210-1
TOP 1 6.3555139 1.6450379 90 N 284 350 C210-2
#
# CMP 373
CMP 1 6.498938 1.6450389 0 N C209 GRM155R70J105MA12D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GRM155R70J105MA12%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J105MA12D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-9665-1-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J105MA2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '1uF'
PRP VDC_V '6.3V'
TOP 0 6.475316 1.6450389 270 N 159 108 C209-1
TOP 1 6.5225601 1.6450389 270 N 284 349 C209-2
#
# CMP 374
CMP 1 6.6250002 1.5704724 270 N C207 GRM155R70J105MA12D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GRM155R70J105MA12%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J105MA12D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-9665-1-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J105MA2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '1uF'
PRP VDC_V '6.3V'
TOP 0 6.6250002 1.5468504 180 N 159 107 C207-1
TOP 1 6.6250002 1.5940945 180 N 284 348 C207-2
#
# CMP 375
CMP 1 6.751411 1.7389359 180 N C203 GRM155R70J105MA12D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GRM155R70J105MA12%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J105MA12D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-9665-1-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J105MA2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '1uF'
PRP VDC_V '6.3V'
TOP 0 6.775033 1.7389359 90 N 171 8 C203-1
TOP 1 6.7277889 1.7389359 90 N 284 347 C203-2
#
# CMP 376
CMP 1 6.755411 1.6208259 180 N C201 GRM155R70J105MA12D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GRM155R70J105MA12%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J105MA12D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-9665-1-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J105MA2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '1uF'
PRP VDC_V '6.3V'
TOP 0 6.779033 1.6208259 90 N 171 7 C201-1
TOP 1 6.7317889 1.6208259 90 N 284 346 C201-2
#
# CMP 377
CMP 1 6.3340004 1.1549855 90 N C200 GRM155R70J103KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '10nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J103KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J103KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J103KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J103KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.01uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.01uF'
PRP VDC_V '6.3V'
TOP 0 6.3340004 1.1786075 0 N 171 5 C200-1
TOP 1 6.3340004 1.1313634 0 N 284 250 C200-2
#
# CMP 378
CMP 5 6.2789344 1.1569712 90 N C199 GRM188Z71A106MA73D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '10µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GRM188Z71A106MA73%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GRM188Z71A106MA73D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GRM188Z71A106MA3D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '10uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '10uF'
PRP VDC_V '10V'
TOP 0 6.2789344 1.1884673 0 N 171 6 C199-1
TOP 1 6.2789344 1.1254752 0 N 284 251 C199-2
#
# CMP 379
CMP 1 6.751411 1.6798809 180 N C197 GRM155R70J105MA12D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GRM155R70J105MA12%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J105MA12D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-9665-1-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J105MA2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '1uF'
PRP VDC_V '6.3V'
TOP 0 6.775033 1.6798809 90 N 172 12 C197-1
TOP 1 6.7277889 1.6798809 90 N 284 345 C197-2
#
# CMP 380
CMP 1 6.3791361 1.6950379 180 N C196 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 6.4027581 1.6950379 90 N 172 13 C196-1
TOP 1 6.355514 1.6950379 90 N 284 351 C196-2
#
# CMP 381
CMP 1 6.498938 1.6950389 0 N C195 GRM155R70J105MA12D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GRM155R70J105MA12%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J105MA12D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-9665-1-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J105MA2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '1uF'
PRP VDC_V '6.3V'
TOP 0 6.475316 1.6950389 270 N 172 11 C195-1
TOP 1 6.5225601 1.6950389 270 N 284 344 C195-2
#
# CMP 382
CMP 1 6.556277 1.8917143 270 N C193 GRM155R70J105MA12D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GRM155R70J105MA12%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J105MA12D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-9665-1-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J105MA2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '1uF'
PRP VDC_V '6.3V'
TOP 0 6.556277 1.8680923 180 N 172 10 C193-1
TOP 1 6.556277 1.9153364 180 N 284 343 C193-2
#
# CMP 383
CMP 1 6.3440004 1.4813773 270 N C192 GRM155R70J103KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '10nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J103KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J103KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J103KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J103KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.01uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.01uF'
PRP VDC_V '6.3V'
TOP 0 6.3440004 1.4577553 180 N 172 7 C192-1
TOP 1 6.3440004 1.5049994 180 N 284 248 C192-2
#
# CMP 384
CMP 5 6.2790004 1.4852121 270 N C191 GRM188Z71A106MA73D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '10µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GRM188Z71A106MA73%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GRM188Z71A106MA73D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GRM188Z71A106MA3D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '10uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '10uF'
PRP VDC_V '10V'
TOP 0 6.2790004 1.453716 180 N 172 8 C191-1
TOP 1 6.2790004 1.5167081 180 N 284 249 C191-2
#
# CMP 385
CMP 1 2.7269271 0.3376552 270 N C188 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 2.7269271 0.3140332 180 N 152 6 C188-1
TOP 1 2.7269271 0.3612773 180 N 284 225 C188-2
#
# CMP 386
CMP 2 2.6668507 0.3401152 270 N C187 GCM155C71A105KE38D ;0=1,1=0.0276
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM155C71A105KE38%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155C71A105KE38D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.7'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GCM155C71A105KE8D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7S'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '1uF'
PRP VDC_V '10V'
TOP 0 2.6668507 0.3201152 180 N 152 17 C187-1
TOP 1 2.6668507 0.3601152 180 N 284 407 C187-2
#
# CMP 387
CMP 1 2.8350005 0.3859623 180 N C186 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 2.8586225 0.3859623 90 N 153 20 C186-1
TOP 1 2.8113784 0.3859623 90 N 284 223 C186-2
#
# CMP 388
CMP 6 2.8350005 0.4589865 180 N C185 GRM21BZ71A226ME15L ;0=1,1=0.0571
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0805'
PRP Cap_F '22µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GRM21BZ71A226ME15%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'GRM21BZ71A226ME15L'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GRM21BZ71A226ME5L'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '22uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '22uF'
PRP VDC_V '10V'
TOP 0 2.8750004 0.4589865 180 N 153 21 C185-1
TOP 1 2.7950004 0.4589865 180 N 284 224 C185-2
#
# CMP 389
CMP 1 0.4947355 2.015 0 N C184 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 0.4711135 2.015 270 N 284 386 C184-1
TOP 1 0.5183576 2.015 270 N 153 32 C184-2
#
# CMP 390
CMP 1 0.4953149 1.965 0 N C183 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 0.4716929 1.965 270 N 284 385 C183-1
TOP 1 0.518937 1.965 270 N 153 31 C183-2
#
# CMP 391
CMP 1 0.769302 1.9778733 270 N C182 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 0.769302 1.9542513 180 N 284 384 C182-1
TOP 1 0.769302 2.0014954 180 N 159 135 C182-2
#
# CMP 392
CMP 1 0.680931 2.065 180 N C181 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 0.704553 2.065 90 N 284 383 C181-1
TOP 1 0.6573089 2.065 90 N 159 134 C181-2
#
# CMP 393
CMP 7 2.6940041 1.5993005 270 N C180 GRM32ER7YA106KA12K ;0=1,1=0.1063
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '1210'
PRP Cap_F '10µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM32ER7YA106KA12-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm '1m'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A '6A'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '1210'
PRP PartNumber 'GRM32ER7YA106KA12K'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '8'
PRP SizeAreaWB_mm2 '14.7'
PRP SizeX_mm '3.2'
PRP SizeY_mm '2.5'
PRP SizeZ_mm '2.7'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM32ER7YA106KA12K-ND'
PRP Supplier_Part_Number_2 '81-GRM32ER7YA106KA2K'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '10uF'
PRP Value1 '0.001 ohm'
PRP Value2 '35V'
PRP ValueDisplayed '10µF'
PRP VDC_V '35V'
TOP 0 2.6940041 1.5422139 180 N 157 60 C180-1
TOP 1 2.6940041 1.6563871 180 N 284 448 C180-2
#
# CMP 394
CMP 5 2.7745111 1.4343005 90 N C177 GRM188R71E474KA12D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '470nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM188R71E474KA12D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GRM188R71E474KA12D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '490-3291-1-ND'
PRP Supplier_Part_Number_2 '81-GRM188R71E474KA12'
PRP Supplier_Part_Number_3 '1828901'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.47uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.47uF'
PRP VDC_V '25V'
TOP 0 2.7745111 1.4657966 0 N 204 0 C177-1
TOP 1 2.7745111 1.4028045 0 N 284 332 C177-2
#
# CMP 395
CMP 1 5.9091276 1.6412939 270 N C176 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 5.9091276 1.6176719 180 N 170 3 C176-1
TOP 1 5.9091276 1.664916 180 N 284 237 C176-2
#
# CMP 396
CMP 7 6.0041276 1.6426225 270 N C175 GRM32ER7YA106KA12K ;0=1,1=0.1063
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '1210'
PRP Cap_F '10µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM32ER7YA106KA12-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm '1m'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A '6A'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '1210'
PRP PartNumber 'GRM32ER7YA106KA12K'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '8'
PRP SizeAreaWB_mm2 '14.7'
PRP SizeX_mm '3.2'
PRP SizeY_mm '2.5'
PRP SizeZ_mm '2.7'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM32ER7YA106KA12K-ND'
PRP Supplier_Part_Number_2 '81-GRM32ER7YA106KA2K'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '10uF'
PRP Value1 '0.001 ohm'
PRP Value2 '35V'
PRP ValueDisplayed '10µF'
PRP VDC_V '35V'
TOP 0 6.0041276 1.5855359 180 N 170 1 C175-1
TOP 1 6.0041276 1.6997091 180 N 284 234 C175-2
#
# CMP 397
CMP 1 5.69521 1.6432942 270 N C174 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 5.69521 1.6196722 180 N 157 36 C174-1
TOP 1 5.69521 1.6669163 180 N 284 235 C174-2
#
# CMP 398
CMP 2 5.6355843 1.6430705 270 N C173 GCM155C71A105KE38D ;0=1,1=0.0276
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM155C71A105KE38%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155C71A105KE38D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.7'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GCM155C71A105KE8D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7S'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '1uF'
PRP VDC_V '10V'
TOP 0 5.6355843 1.6230705 180 N 157 54 C173-1
TOP 1 5.6355843 1.6630705 180 N 284 406 C173-2
#
# CMP 399
CMP 6 2.8390041 1.7843015 180 N C170 GRM21BZ71A226ME15L ;0=1,1=0.0571
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0805'
PRP Cap_F '22µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GRM21BZ71A226ME15%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'GRM21BZ71A226ME15L'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GRM21BZ71A226ME5L'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '22uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '22uF'
PRP VDC_V '10V'
TOP 0 2.879004 1.7843015 180 N 159 102 C170-1
TOP 1 2.799004 1.7843015 180 N 284 331 C170-2
#
# CMP 400
CMP 6 2.8390041 1.6943005 180 N C169 GRM21BZ71A226ME15L ;0=1,1=0.0571
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0805'
PRP Cap_F '22µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GRM21BZ71A226ME15%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'GRM21BZ71A226ME15L'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GRM21BZ71A226ME5L'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '22uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '22uF'
PRP VDC_V '10V'
TOP 0 2.879004 1.6943005 180 N 159 104 C169-1
TOP 1 2.799004 1.6943005 180 N 284 335 C169-2
#
# CMP 401
CMP 7 2.3323308 0.9666816 270 N C167 GRM32ER7YA106KA12K ;0=1,1=0.1063
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '1210'
PRP Cap_F '10µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM32ER7YA106KA12-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm '1m'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A '6A'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '1210'
PRP PartNumber 'GRM32ER7YA106KA12K'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '8'
PRP SizeAreaWB_mm2 '14.7'
PRP SizeX_mm '3.2'
PRP SizeY_mm '2.5'
PRP SizeZ_mm '2.7'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM32ER7YA106KA12K-ND'
PRP Supplier_Part_Number_2 '81-GRM32ER7YA106KA2K'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '10uF'
PRP Value1 '0.001 ohm'
PRP Value2 '35V'
PRP ValueDisplayed '10µF'
PRP VDC_V '35V'
TOP 0 2.3323308 0.909595 180 N 157 45 C167-1
TOP 1 2.3323308 1.0237682 180 N 284 326 C167-2
#
# CMP 402
CMP 1 5.9091275 1.2221048 270 N C165 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 5.9091275 1.1984828 180 N 169 4 C165-1
TOP 1 5.9091275 1.2457269 180 N 284 338 C165-2
#
# CMP 403
CMP 7 6.0041275 1.2234338 270 N C164 GRM32ER7YA106KA12K ;0=1,1=0.1063
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '1210'
PRP Cap_F '10µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM32ER7YA106KA12-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm '1m'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A '6A'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '1210'
PRP PartNumber 'GRM32ER7YA106KA12K'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '8'
PRP SizeAreaWB_mm2 '14.7'
PRP SizeX_mm '3.2'
PRP SizeY_mm '2.5'
PRP SizeZ_mm '2.7'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM32ER7YA106KA12K-ND'
PRP Supplier_Part_Number_2 '81-GRM32ER7YA106KA2K'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '10uF'
PRP Value1 '0.001 ohm'
PRP Value2 '35V'
PRP ValueDisplayed '10µF'
PRP VDC_V '35V'
TOP 0 6.0041275 1.1663472 180 N 169 3 C164-1
TOP 1 6.0041275 1.2805204 180 N 284 337 C164-2
#
# CMP 404
CMP 1 5.6952095 1.2221048 270 N C163 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 5.6952095 1.1984828 180 N 157 47 C163-1
TOP 1 5.6952095 1.2457269 180 N 284 336 C163-2
#
# CMP 405
CMP 2 5.6355843 1.227038 270 N C162 GCM155C71A105KE38D ;0=1,1=0.0276
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM155C71A105KE38%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155C71A105KE38D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.7'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GCM155C71A105KE8D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7S'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '1uF'
PRP VDC_V '10V'
TOP 0 5.6355843 1.207038 180 N 157 53 C162-1
TOP 1 5.6355843 1.247038 180 N 284 405 C162-2
#
# CMP 406
CMP 5 2.4128386 0.8016816 90 N C160 GRM188R71E474KA12D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '470nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM188R71E474KA12D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GRM188R71E474KA12D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '490-3291-1-ND'
PRP Supplier_Part_Number_2 '81-GRM188R71E474KA12'
PRP Supplier_Part_Number_3 '1828901'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.47uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.47uF'
PRP VDC_V '25V'
TOP 0 2.4128386 0.8331777 0 N 209 0 C160-1
TOP 1 2.4128386 0.7701856 0 N 284 233 C160-2
#
# CMP 407
CMP 6 2.4773308 1.1516817 180 N C158 GRM21BZ71A226ME15L ;0=1,1=0.0571
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0805'
PRP Cap_F '22µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GRM21BZ71A226ME15%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'GRM21BZ71A226ME15L'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GRM21BZ71A226ME5L'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '22uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '22uF'
PRP VDC_V '10V'
TOP 0 2.5173307 1.1516817 180 N 175 33 C158-1
TOP 1 2.4373307 1.1516816 180 N 284 231 C158-2
#
# CMP 408
CMP 6 2.4773309 1.0616816 180 N C157 GRM21BZ71A226ME15L ;0=1,1=0.0571
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0805'
PRP Cap_F '22µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GRM21BZ71A226ME15%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'GRM21BZ71A226ME15L'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GRM21BZ71A226ME5L'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '22uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '22uF'
PRP VDC_V '10V'
TOP 0 2.5173308 1.0616816 180 N 175 34 C157-1
TOP 1 2.4373307 1.0616816 180 N 284 232 C157-2
#
# CMP 409
CMP 1 6.3791361 0.695038 180 N C133 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 6.4027581 0.695038 90 N 159 118 C133-1
TOP 1 6.355514 0.695038 90 N 284 352 C133-2
#
# CMP 410
CMP 1 6.4939387 0.695039 0 N C132 GRM155R70J105MA12D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GRM155R70J105MA12%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J105MA12D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-9665-1-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J105MA2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '1uF'
PRP VDC_V '6.3V'
TOP 0 6.4703167 0.695039 270 N 159 63 C132-1
TOP 1 6.5175608 0.695039 270 N 284 229 C132-2
#
# CMP 411
CMP 1 6.625 0.6221346 270 N C130 GRM155R70J105MA12D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GRM155R70J105MA12%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J105MA12D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-9665-1-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J105MA2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '1uF'
PRP VDC_V '6.3V'
TOP 0 6.625 0.5985126 180 N 159 64 C130-1
TOP 1 6.625 0.6457567 180 N 284 230 C130-2
#
# CMP 412
CMP 1 6.7554113 0.7889366 180 N C126 GRM155R70J105MA12D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GRM155R70J105MA12%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J105MA12D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-9665-1-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J105MA2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '1uF'
PRP VDC_V '6.3V'
TOP 0 6.7790333 0.7889366 90 N 173 6 C126-1
TOP 1 6.7317892 0.7889366 90 N 284 273 C126-2
#
# CMP 413
CMP 1 6.7554113 0.6708264 180 N C124 GRM155R70J105MA12D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GRM155R70J105MA12%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J105MA12D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-9665-1-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J105MA2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '1uF'
PRP VDC_V '6.3V'
TOP 0 6.7790333 0.6708264 90 N 173 7 C124-1
TOP 1 6.7317892 0.6708264 90 N 284 274 C124-2
#
# CMP 414
CMP 1 6.2800877 0.9871459 270 N C123 GRM155R70J103KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '10nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J103KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J103KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J103KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J103KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.01uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.01uF'
PRP VDC_V '6.3V'
TOP 0 6.2800877 0.9635239 180 N 173 8 C123-1
TOP 1 6.2800877 1.010768 180 N 284 275 C123-2
#
# CMP 415
CMP 5 6.21 1.0036532 270 N C122 GRM188Z71A106MA73D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '10µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GRM188Z71A106MA73%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GRM188Z71A106MA73D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GRM188Z71A106MA3D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '10uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '10uF'
PRP VDC_V '10V'
TOP 0 6.21 0.9721571 180 N 173 9 C122-1
TOP 1 6.21 1.0351492 180 N 284 276 C122-2
#
# CMP 416
CMP 1 6.7554113 0.7298815 180 N C120 GRM155R70J105MA12D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GRM155R70J105MA12%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J105MA12D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-9665-1-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J105MA2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '1uF'
PRP VDC_V '6.3V'
TOP 0 6.7790333 0.7298815 90 N 174 11 C120-1
TOP 1 6.7317892 0.7298815 90 N 284 271 C120-2
#
# CMP 417
CMP 1 6.374136 0.7450385 180 N C119 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 6.397758 0.7450385 90 N 174 13 C119-1
TOP 1 6.3505139 0.7450385 90 N 284 342 C119-2
#
# CMP 418
CMP 1 6.4939387 0.745039 0 N C118 GRM155R70J105MA12D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GRM155R70J105MA12%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J105MA12D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-9665-1-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J105MA2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '1uF'
PRP VDC_V '6.3V'
TOP 0 6.4703167 0.745039 270 N 174 12 C118-1
TOP 1 6.5175608 0.745039 270 N 284 272 C118-2
#
# CMP 419
CMP 1 6.5562771 0.9417143 270 N C116 GRM155R70J105MA12D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GRM155R70J105MA12%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J105MA12D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-9665-1-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J105MA2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '1uF'
PRP VDC_V '6.3V'
TOP 0 6.5562771 0.9180923 180 N 174 7 C116-1
TOP 1 6.5562771 0.9653364 180 N 284 226 C116-2
#
# CMP 420
CMP 1 6.3440004 1.3432771 270 N C115 GRM155R70J103KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '10nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J103KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J103KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J103KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J103KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.01uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.01uF'
PRP VDC_V '6.3V'
TOP 0 6.3440004 1.3196551 180 N 174 8 C115-1
TOP 1 6.3440004 1.3668992 180 N 284 227 C115-2
#
# CMP 421
CMP 5 6.2790004 1.3432771 270 N C114 GRM188Z71A106MA73D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '10µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GRM188Z71A106MA73%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GRM188Z71A106MA73D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GRM188Z71A106MA3D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '10uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '10uF'
PRP VDC_V '10V'
TOP 0 6.2790004 1.311781 180 N 174 9 C114-1
TOP 1 6.2790004 1.3747731 180 N 284 228 C114-2
#
# CMP 422
CMP 1 5.009 0.992818 0 N C111 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 4.985378 0.992818 270 N 284 379 C111-1
TOP 1 5.0326221 0.992818 270 N 159 130 C111-2
#
# CMP 423
CMP 5 0.74 0.4935434 270 N C110 GCM188R71C104KA37J ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/w_hinm/S0717E.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCM188R71C104KA37J'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-8015-1-ND'
PRP Supplier_Part_Number_2 '81-GCM188R71C104KA7J'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '16V'
TOP 0 0.7400001 0.4620472 180 N 152 15 C110-1
TOP 1 0.7400001 0.5250394 180 N 284 324 C110-2
#
# CMP 424
CMP 1 1.7715751 0.71 90 N C109 GRM155R71C102KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '1nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R71C102KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71C102KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R71C102KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R71C102KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '1000pF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '1000pF'
PRP VDC_V '16V'
TOP 0 1.7715751 0.733622 0 N 191 0 C109-1
TOP 1 1.7715751 0.6863779 0 N 284 378 C109-2
#
# CMP 425
CMP 5 1.7769122 0.844067 270 N C108 GCM188R71C104KA37J ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/w_hinm/S0717E.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCM188R71C104KA37J'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-8015-1-ND'
PRP Supplier_Part_Number_2 '81-GCM188R71C104KA7J'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '16V'
TOP 0 1.7769122 0.8125709 180 N 157 40 C108-1
TOP 1 1.7769122 0.875563 180 N 284 258 C108-2
#
# CMP 426
CMP 5 1.5796736 0.844067 270 N C106 GCM188R71C104KA37J ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/w_hinm/S0717E.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCM188R71C104KA37J'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-8015-1-ND'
PRP Supplier_Part_Number_2 '81-GCM188R71C104KA7J'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '16V'
TOP 0 1.5796736 0.8125709 180 N 152 8 C106-1
TOP 1 1.5796736 0.875563 180 N 284 259 C106-2
#
# CMP 427
CMP 7 1.3908942 0.7008241 270 N C104 GRM32ER7YA106KA12K ;0=1,1=0.1063
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '1210'
PRP Cap_F '10µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM32ER7YA106KA12-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm '1m'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A '6A'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '1210'
PRP PartNumber 'GRM32ER7YA106KA12K'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '8'
PRP SizeAreaWB_mm2 '14.7'
PRP SizeX_mm '3.2'
PRP SizeY_mm '2.5'
PRP SizeZ_mm '2.7'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM32ER7YA106KA12K-ND'
PRP Supplier_Part_Number_2 '81-GRM32ER7YA106KA2K'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '10uF'
PRP Value1 '0.001 ohm'
PRP Value2 '35V'
PRP ValueDisplayed '10µF'
PRP VDC_V '35V'
TOP 0 1.3908942 0.6437375 180 N 152 9 C104-1
TOP 1 1.3908942 0.7579107 180 N 284 262 C104-2
#
# CMP 428
CMP 5 1.26 0.6696063 270 N C103 GRM188R72A104KA35J ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM188R72A104KA35-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GRM188R72A104KA35J'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-6439-1-ND'
PRP Supplier_Part_Number_2 '81-GRM188R72A104KA5J'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '100V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '100V'
TOP 0 1.26 0.6381102 180 N 177 3 C103-1
TOP 1 1.26 0.7011023 180 N 284 257 C103-2
#
# CMP 429
CMP 7 1.1490398 0.6896107 270 N C102 GRM32ER7YA106KA12K ;0=1,1=0.1063
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '1210'
PRP Cap_F '10µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM32ER7YA106KA12-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm '1m'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A '6A'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '1210'
PRP PartNumber 'GRM32ER7YA106KA12K'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '8'
PRP SizeAreaWB_mm2 '14.7'
PRP SizeX_mm '3.2'
PRP SizeY_mm '2.5'
PRP SizeZ_mm '2.7'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM32ER7YA106KA12K-ND'
PRP Supplier_Part_Number_2 '81-GRM32ER7YA106KA2K'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '10uF'
PRP Value1 '0.001 ohm'
PRP Value2 '35V'
PRP ValueDisplayed '10µF'
PRP VDC_V '35V'
TOP 0 1.1490398 0.6325241 180 N 177 4 C102-1
TOP 1 1.1490398 0.7466973 180 N 284 263 C102-2
#
# CMP 430
CMP 5 0.4207877 0.4541072 180 N C101 GCM188R71C104KA37J ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/w_hinm/S0717E.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCM188R71C104KA37J'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-8015-1-ND'
PRP Supplier_Part_Number_2 '81-GCM188R71C104KA7J'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '16V'
TOP 0 0.4522838 0.4541072 90 N 152 12 C101-1
TOP 1 0.3892917 0.4541071 90 N 284 323 C101-2
#
# CMP 431
CMP 1 2.01 0.5713779 270 N C97 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 2.01 0.5477559 180 N 30 1 C97-1
TOP 1 2.01 0.595 180 N 284 293 C97-2
#
# CMP 432
CMP 1 4.3397235 0.5499331 270 N C96 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 4.3397235 0.5263111 180 N 25 1 C96-1
TOP 1 4.3397235 0.5735552 180 N 284 292 C96-2
#
# CMP 433
CMP 1 5.073 0.5852952 270 N C94 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 5.073 0.5616732 180 N 575 3 C94-1
TOP 1 5.073 0.6089173 180 N 284 296 C94-2
#
# CMP 434
CMP 1 5.0179706 0.5852952 270 N C93 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 5.0179706 0.5616732 180 N 576 3 C93-1
TOP 1 5.0179706 0.6089173 180 N 284 295 C93-2
#
# CMP 435
CMP 1 4.965 0.5859974 270 N C92 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 4.965 0.5623754 180 N 577 3 C92-1
TOP 1 4.965 0.6096195 180 N 284 294 C92-2
#
# CMP 436
CMP 1 3.59 0.595 90 N C91 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 3.59 0.618622 0 N 351 2 C91-1
TOP 1 3.59 0.5713779 0 N 284 297 C91-2
#
# CMP 437
CMP 1 4.9111087 0.5851544 270 N C88 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 4.9111087 0.5615324 180 N 580 1 C88-1
TOP 1 4.9111087 0.6087765 180 N 284 285 C88-2
#
# CMP 438
CMP 1 4.8566969 0.5851544 270 N C87 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 4.8566969 0.5615324 180 N 581 1 C87-1
TOP 1 4.8566969 0.6087765 180 N 284 287 C87-2
#
# CMP 439
CMP 1 4.8021089 0.5851544 270 N C86 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 4.8021089 0.5615324 180 N 582 1 C86-1
TOP 1 4.8021089 0.6087765 180 N 284 286 C86-2
#
# CMP 440
CMP 1 4.747109 0.5851544 270 N C85 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 4.747109 0.5615324 180 N 583 1 C85-1
TOP 1 4.747109 0.6087765 180 N 284 284 C85-2
#
# CMP 441
CMP 1 2.2689994 0.5724718 270 N C84 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 2.2689994 0.5488498 180 N 586 1 C84-1
TOP 1 2.2689994 0.5960939 180 N 284 299 C84-2
#
# CMP 442
CMP 1 2.2099994 0.5724718 270 N C83 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 2.2099994 0.5488498 180 N 587 1 C83-1
TOP 1 2.2099994 0.5960939 180 N 284 300 C83-2
#
# CMP 443
CMP 1 2.1499994 0.5724718 270 N C82 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 2.1499994 0.5488498 180 N 588 1 C82-1
TOP 1 2.1499994 0.5960939 180 N 284 289 C82-2
#
# CMP 444
CMP 1 2.0899994 0.5724718 270 N C81 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 2.0899994 0.5488498 180 N 589 1 C81-1
TOP 1 2.0899994 0.5960939 180 N 284 288 C81-2
#
# CMP 445
CMP 5 3.855 0.7273736 90 N C77 GRM188Z71A475ME15D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '4.7µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM188Z71A475ME15-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GRM188Z71A475ME15D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 '81-GRM188Z71A475ME5D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '4.7uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '4.7uF'
PRP VDC_V '10V'
TOP 0 3.855 0.7588697 0 N 564 3 C77-1
TOP 1 3.855 0.6958776 0 N 563 3 C77-2
#
# CMP 446
CMP 5 3.713174 0.6665042 90 N C76 GRM188Z71A475ME15D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '4.7µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM188Z71A475ME15-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GRM188Z71A475ME15D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 '81-GRM188Z71A475ME5D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '4.7uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '4.7uF'
PRP VDC_V '10V'
TOP 0 3.713174 0.6980003 0 N 24 2 C76-1
TOP 1 3.713174 0.6350082 0 N 23 1 C76-2
#
# CMP 447
CMP 1 1.9239994 0.5719478 270 N C75 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 1.9239994 0.5483258 180 N 592 3 C75-1
TOP 1 1.9239994 0.5955699 180 N 284 304 C75-2
#
# CMP 448
CMP 1 1.8649994 0.5719478 270 N C74 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 1.8649994 0.5483258 180 N 593 3 C74-1
TOP 1 1.8649994 0.5955699 180 N 284 305 C74-2
#
# CMP 449
CMP 1 1.8049994 0.5719478 270 N C73 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 1.8049994 0.5483258 180 N 594 3 C73-1
TOP 1 1.8049994 0.5955699 180 N 284 303 C73-2
#
# CMP 450
CMP 1 1.7449994 0.5719478 270 N C72 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 1.7449994 0.5483258 180 N 595 3 C72-1
TOP 1 1.7449994 0.5955699 180 N 284 306 C72-2
#
# CMP 451
CMP 1 0.862101 0.6617863 270 N C69 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 0.862101 0.6381643 180 N 159 96 C69-1
TOP 1 0.862101 0.6854084 180 N 284 280 C69-2
#
# CMP 452
CMP 5 0.9247572 0.6696601 270 N C68 C1608X7S1A335K080AC ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '3.3µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=C1608X7S1A335K080AC'
PRP CompType 'Capacitor'
PRP ESR_ohm '4.796m'
PRP IRMS_A '2.3752A'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'C1608X7S1A335K080AC'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '445-14256-1-ND'
PRP Supplier_Part_Number_2 '52X3755'
PRP Supplier_Part_Number_3 '810-C1608X7S1A335K0C'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7S'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '3.3uF'
PRP Value1 '0.004796 ohm'
PRP Value2 '10V'
PRP ValueDisplayed '3.3uF'
PRP VDC_V '10V'
TOP 0 0.9247572 0.638164 180 N 159 92 C68-1
TOP 1 0.9247572 0.7011561 180 N 284 277 C68-2
#
# CMP 453
CMP 5 0.6110262 0.6726902 270 N C67 GRM188Z71C475KE21D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '4.7µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM188Z71C475KE21-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-06-05'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GRM188Z71C475KE21D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '4.7uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '4.7uF'
PRP VDC_V '16V'
TOP 0 0.6110262 0.6411941 180 N 161 4 C67-1
TOP 1 0.6110262 0.7041862 180 N 284 278 C67-2
#
# CMP 454
CMP 1 2.973622 0.8541486 180 N C66 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 2.997244 0.8541486 90 N 284 377 C66-1
TOP 1 2.9499999 0.8541486 90 N 159 129 C66-2
#
# CMP 455
CMP 1 2.0292244 1.0248626 0 N C65 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 2.0056024 1.0248626 270 N 284 376 C65-1
TOP 1 2.0528465 1.0248626 270 N 153 30 C65-2
#
# CMP 456
CMP 1 2.0175682 0.7464815 90 N C64 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 2.0175682 0.7701035 0 N 284 375 C64-1
TOP 1 2.0175682 0.7228594 0 N 153 29 C64-2
#
# CMP 457
CMP 1 2.2078442 0.7673875 270 N C63 GRM155R71E103KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '10nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R71E103KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E103KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '490-1312-1-ND'
PRP Supplier_Part_Number_2 '81-GRM36X103K25'
PRP Supplier_Part_Number_3 '8819734'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.01uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.01uF'
PRP VDC_V '25V'
TOP 0 2.2078442 0.7437655 180 N 424 0 C63-1
TOP 1 2.2078442 0.7910096 180 N 284 313 C63-2
#
# CMP 458
CMP 1 3.215 0.4183263 0 N C60 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 3.191378 0.4183263 270 N 284 374 C60-1
TOP 1 3.2386221 0.4183263 270 N 153 28 C60-2
#
# CMP 459
CMP 1 3.355 0.8543332 270 N C59 GRM1555C1E120JA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '12pF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM1555C1E120JA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM1555C1E120JA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GRM1555C1E120JA1D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'C0G/NP0'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '12pF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '12pF'
PRP VDC_V '25V'
TOP 0 3.355 0.8307112 180 N 356 0 C59-1
TOP 1 3.355 0.8779553 180 N 284 312 C59-2
#
# CMP 460
CMP 1 3.355 0.7412143 90 N C58 GRM1555C1E120JA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '12pF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM1555C1E120JA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM1555C1E120JA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GRM1555C1E120JA1D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'C0G/NP0'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '12pF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '12pF'
PRP VDC_V '25V'
TOP 0 3.355 0.7648363 0 N 357 0 C58-1
TOP 1 3.355 0.7175922 0 N 284 311 C58-2
#
# CMP 461
CMP 1 2.1624018 1.279447 180 N C57 GRM155R71E104KE14D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71E104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10698-1-ND'
PRP Supplier_Part_Number_2 '31Y1751'
PRP Supplier_Part_Number_3 '81-GRM155R71E104KE4D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '25V'
TOP 0 2.1860238 1.279447 90 N 284 373 C57-1
TOP 1 2.1387797 1.279447 90 N 159 128 C57-2
#
# CMP 462
CMP 1 3.287475 0.6332437 90 N C48 GRM155R70J104KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R70J104KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J104KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'GRM155R70J104KA01D-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J104KA1D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '6.3V'
TOP 0 3.287475 0.6568657 0 N 156 0 C48-1
TOP 1 3.287475 0.6096216 0 N 284 268 C48-2
#
# CMP 463
CMP 72 3.5471328 1.3827956 0 N U1 AM263x_0p96 ;0=1,1=0.0551
PRP Manufacturer 'Texas Instruments'
PRP PartNumber 'XAM2634AOLFGMZCZQ'
TOP 0 3.5471328 1.3827956 0 N 284 537 U1-A1
TOP 1 3.5786289 1.3827956 0 N 428 1 U1-A2
TOP 2 3.610125 1.3827956 0 N 430 1 U1-A3
TOP 3 3.6416211 1.3827956 0 N 436 1 U1-A4
TOP 4 3.6731172 1.3827956 0 N 439 3 U1-A5
TOP 5 3.7046133 1.3827956 0 N 363 1 U1-A6
TOP 6 3.7361094 1.3827956 0 N 364 1 U1-A7
TOP 7 3.7676055 1.3827956 0 N 451 1 U1-A8
TOP 8 3.7991016 1.3827956 0 N 454 1 U1-A9
TOP 9 3.8305977 1.3827956 0 N 376 1 U1-A10
TOP 10 3.8620938 1.3827956 0 N 8 1 U1-A11
TOP 11 3.8935899 1.3827956 0 N 521 1 U1-A12
TOP 12 3.925086 1.3827956 0 N 522 1 U1-A13
TOP 13 3.9565821 1.3827956 0 N 526 1 U1-A14
TOP 14 3.9880782 1.3827956 0 N 389 1 U1-A15
TOP 15 4.0195743 1.3827956 0 N 391 1 U1-A16
TOP 16 4.0510704 1.3827956 0 N 460 1 U1-A17
TOP 17 4.0825665 1.3827956 0 N 284 450 U1-A18
TOP 18 3.5471328 1.3512995 0 N 555 1 U1-B1
TOP 19 3.5786289 1.3512995 0 N 557 1 U1-B2
TOP 20 3.610125 1.3512995 0 N 370 1 U1-B3
TOP 21 3.6416211 1.3512995 0 N 432 1 U1-B4
TOP 22 3.6731172 1.3512995 0 N 434 1 U1-B5
TOP 23 3.7046133 1.3512995 0 N 438 1 U1-B6
TOP 24 3.7361094 1.3512995 0 N 104 2 U1-B7
TOP 25 3.7676055 1.3512995 0 N 452 1 U1-B8
TOP 26 3.7991016 1.3512995 0 N 103 1 U1-B9
TOP 27 3.8305977 1.3512995 0 N 373 1 U1-B10
TOP 28 3.8620938 1.3512995 0 N 377 1 U1-B11
TOP 29 3.8935899 1.3512995 0 N 520 1 U1-B12
TOP 30 3.925086 1.3512995 0 N 523 1 U1-B13
TOP 31 3.9565821 1.3512995 0 N 527 1 U1-B14
TOP 32 3.9880782 1.3512995 0 N 390 1 U1-B15
TOP 33 4.0195743 1.3512995 0 N 97 1 U1-B16
TOP 34 4.0510704 1.3512995 0 N 466 1 U1-B17
TOP 35 4.0825665 1.3512995 0 N 468 1 U1-B18
TOP 36 3.5471328 1.3198034 0 N 547 1 U1-C1
TOP 37 3.5786289 1.3198034 0 N 549 1 U1-C2
TOP 38 3.610125 1.3198034 0 N 358 4 U1-C3
TOP 39 3.6416211 1.3198034 0 N 368 1 U1-C4
TOP 40 3.6731172 1.3198034 0 N 369 1 U1-C5
TOP 41 3.7046133 1.3198034 0 N 426 1 U1-C6
TOP 42 3.7361094 1.3198034 0 N 105 2 U1-C7
TOP 43 3.7676055 1.3198034 0 N 508 4 U1-C8
TOP 44 3.7991016 1.3198034 0 N 374 1 U1-C9
TOP 45 3.8305977 1.3198034 0 N 379 1 U1-C10
TOP 46 3.8620938 1.3198034 0 N 380 1 U1-C11
TOP 47 3.8935899 1.3198034 0 N 524 1 U1-C12
TOP 48 3.925086 1.3198034 0 N 388 1 U1-C13
TOP 49 3.9565821 1.3198034 0 N 387 1 U1-C14
TOP 50 3.9880782 1.3198034 0 N 456 1 U1-C15
TOP 51 4.0195743 1.3198034 0 N 470 1 U1-C16
TOP 52 4.0510704 1.3198034 0 N 462 1 U1-C17
TOP 53 4.0825665 1.3198034 0 N 479 4 U1-C18
TOP 54 3.5471328 1.2883073 0 N 122 1 U1-D1
TOP 55 3.5786289 1.2883073 0 N 551 1 U1-D2
TOP 56 3.610125 1.2883073 0 N 553 1 U1-D3
TOP 57 3.6416211 1.2883073 0 N 392 3 U1-D4
TOP 58 3.6731172 1.2883073 0 N 365 1 U1-D5
TOP 59 3.7046133 1.2883073 0 N 162 15 U1-D6
TOP 60 3.7361094 1.2883073 0 N 509 4 U1-D7
TOP 61 3.7676055 1.2883073 0 N 159 183 U1-D8
TOP 62 3.7991016 1.2883073 0 N 371 1 U1-D9
TOP 63 3.8305977 1.2883073 0 N 175 49 U1-D10
TOP 64 3.8620938 1.2883073 0 N 525 1 U1-D11
TOP 65 3.8935899 1.2883073 0 N 159 182 U1-D12
TOP 66 3.925086 1.2883073 0 N 386 1 U1-D13
TOP 67 3.9565821 1.2883073 0 N 106 1 U1-D14
TOP 68 3.9880782 1.2883073 0 N 458 1 U1-D15
TOP 69 4.0195743 1.2883073 0 N 464 1 U1-D16
TOP 70 4.0510704 1.2883073 0 N 46 6 U1-D17
TOP 71 4.0825665 1.2883073 0 N 471 4 U1-D18
TOP 72 3.5471328 1.2568112 0 N 518 1 U1-E1
TOP 73 3.5786289 1.2568112 0 N 545 1 U1-E2
TOP 74 3.610125 1.2568112 0 N 543 1 U1-E3
TOP 75 3.6416211 1.2568112 0 N 515 1 U1-E4
TOP 76 3.6731172 1.2568112 0 N 284 534 U1-E5
TOP 77 3.7046133 1.2568112 0 N 284 526 U1-E6
TOP 78 3.7361094 1.2568112 0 N 284 519 U1-E7
TOP 79 3.7676055 1.2568112 0 N 284 510 U1-E8
TOP 80 3.7991016 1.2568112 0 N 175 52 U1-E9
TOP 81 3.8305977 1.2568112 0 N 284 493 U1-E10
TOP 82 3.8620938 1.2568112 0 N 175 48 U1-E11
TOP 83 3.8935899 1.2568112 0 N 284 476 U1-E12
TOP 84 3.925086 1.2568112 0 N 284 466 U1-E13
TOP 85 3.9565821 1.2568112 0 N 284 458 U1-E14
TOP 86 3.9880782 1.2568112 0 N 162 14 U1-E15
TOP 87 4.0195743 1.2568112 0 N 478 1 U1-E16
TOP 88 4.0510704 1.2568112 0 N 475 1 U1-E17
TOP 89 4.0825665 1.2568112 0 N 474 1 U1-E18
TOP 90 3.5471328 1.2253151 0 N 99 5 U1-F1
TOP 91 3.5786289 1.2253151 0 N 513 1 U1-F2
TOP 92 3.610125 1.2253151 0 N 517 1 U1-F3
TOP 93 3.6416211 1.2253151 0 N 516 1 U1-F4
TOP 94 3.6731172 1.2253151 0 N 284 533 U1-F5
TOP 95 3.7046133 1.2253151 0 N 284 525 U1-F6
TOP 96 3.7361094 1.2253151 0 N 284 518 U1-F7
TOP 97 3.7676055 1.2253151 0 N 284 509 U1-F8
TOP 98 3.7991016 1.2253151 0 N 175 51 U1-F9
TOP 99 3.8305977 1.2253151 0 N 284 492 U1-F10
TOP 100 3.8620938 1.2253151 0 N 175 47 U1-F11
TOP 101 3.8935899 1.2253151 0 N 284 475 U1-F12
TOP 102 3.925086 1.2253151 0 N 284 465 U1-F13
TOP 103 3.9565821 1.2253151 0 N 284 457 U1-F14
TOP 104 3.9880782 1.2253151 0 N 472 4 U1-F15
TOP 105 4.0195743 1.2253151 0 N 473 1 U1-F16
TOP 106 4.0510704 1.2253151 0 N 63 1 U1-F17
TOP 107 4.0825665 1.2253151 0 N 477 1 U1-F18
TOP 108 3.5471328 1.193819 0 N 118 1 U1-G1
TOP 109 3.5786289 1.193819 0 N 511 1 U1-G2
TOP 110 3.610125 1.193819 0 N 506 3 U1-G3
TOP 111 3.6416211 1.193819 0 N 123 5 U1-G4
TOP 112 3.6731172 1.193819 0 N 175 58 U1-G5
TOP 113 3.7046133 1.193819 0 N 175 55 U1-G6
TOP 114 3.7361094 1.193819 0 N 284 517 U1-G7
TOP 115 3.7676055 1.193819 0 N 284 508 U1-G8
TOP 116 3.7991016 1.193819 0 N 284 500 U1-G9
TOP 117 3.8305977 1.193819 0 N 284 491 U1-G10
TOP 118 3.8620938 1.193819 0 N 284 483 U1-G11
TOP 119 3.8935899 1.193819 0 N 284 474 U1-G12
TOP 120 3.925086 1.193819 0 N 175 46 U1-G13
TOP 121 3.9565821 1.193819 0 N 175 43 U1-G14
TOP 122 3.9880782 1.193819 0 N 65 1 U1-G15
TOP 123 4.0195743 1.193819 0 N 476 1 U1-G16
TOP 124 4.0510704 1.193819 0 N 69 1 U1-G17
TOP 125 4.0825665 1.193819 0 N 61 1 U1-G18
TOP 126 3.5471328 1.1623229 0 N 116 1 U1-H1
TOP 127 3.5786289 1.1623229 0 N 507 3 U1-H2
TOP 128 3.610125 1.1623229 0 N 175 60 U1-H3
TOP 129 3.6416211 1.1623229 0 N 159 185 U1-H4
TOP 130 3.6731172 1.1623229 0 N 284 532 U1-H5
TOP 131 3.7046133 1.1623229 0 N 284 524 U1-H6
TOP 132 3.7361094 1.1623229 0 N 284 516 U1-H7
TOP 133 3.7676055 1.1623229 0 N 284 507 U1-H8
TOP 134 3.7991016 1.1623229 0 N 284 499 U1-H9
TOP 135 3.8305977 1.1623229 0 N 284 490 U1-H10
TOP 136 3.8620938 1.1623229 0 N 284 482 U1-H11
TOP 137 3.8935899 1.1623229 0 N 284 473 U1-H12
TOP 138 3.925086 1.1623229 0 N 284 464 U1-H13
TOP 139 3.9565821 1.1623229 0 N 284 456 U1-H14
TOP 140 3.9880782 1.1623229 0 N 159 181 U1-H15
TOP 141 4.0195743 1.1623229 0 N 483 1 U1-H16
TOP 142 4.0510704 1.1623229 0 N 485 1 U1-H17
TOP 143 4.0825665 1.1623229 0 N 491 1 U1-H18
TOP 144 3.5471328 1.1308268 0 N 115 1 U1-J1
TOP 145 3.5786289 1.1308268 0 N 117 1 U1-J2
TOP 146 3.610125 1.1308268 0 N 98 5 U1-J3
TOP 147 3.6416211 1.1308268 0 N 113 1 U1-J4
TOP 148 3.6731172 1.1308268 0 N 284 531 U1-J5
TOP 149 3.7046133 1.1308268 0 N 284 523 U1-J6
TOP 150 3.7361094 1.1308268 0 N 284 515 U1-J7
TOP 151 3.7676055 1.1308268 0 N 284 506 U1-J8
TOP 152 3.7991016 1.1308268 0 N 284 498 U1-J9
TOP 153 3.8305977 1.1308268 0 N 284 489 U1-J10
TOP 154 3.8620938 1.1308268 0 N 284 481 U1-J11
TOP 155 3.8935899 1.1308268 0 N 284 472 U1-J12
TOP 156 3.925086 1.1308268 0 N 284 463 U1-J13
TOP 157 3.9565821 1.1308268 0 N 284 455 U1-J14
TOP 158 3.9880782 1.1308268 0 N 175 40 U1-J15
TOP 159 4.0195743 1.1308268 0 N 175 39 U1-J16
TOP 160 4.0510704 1.1308268 0 N 73 1 U1-J17
TOP 161 4.0825665 1.1308268 0 N 75 1 U1-J18
TOP 162 3.5471328 1.0993307 0 N 445 1 U1-K1
TOP 163 3.5786289 1.0993307 0 N 114 1 U1-K2
TOP 164 3.610125 1.0993307 0 N 533 1 U1-K3
TOP 165 3.6416211 1.0993307 0 N 535 1 U1-K4
TOP 166 3.6731172 1.0993307 0 N 175 57 U1-K5
TOP 167 3.7046133 1.0993307 0 N 175 54 U1-K6
TOP 168 3.7361094 1.0993307 0 N 284 514 U1-K7
TOP 169 3.7676055 1.0993307 0 N 284 505 U1-K8
TOP 170 3.7991016 1.0993307 0 N 284 497 U1-K9
TOP 171 3.8305977 1.0993307 0 N 284 488 U1-K10
TOP 172 3.8620938 1.0993307 0 N 284 480 U1-K11
TOP 173 3.8935899 1.0993307 0 N 284 471 U1-K12
TOP 174 3.925086 1.0993307 0 N 175 45 U1-K13
TOP 175 3.9565821 1.0993307 0 N 175 42 U1-K14
TOP 176 3.9880782 1.0993307 0 N 67 1 U1-K15
TOP 177 4.0195743 1.0993307 0 N 71 1 U1-K16
TOP 178 4.0510704 1.0993307 0 N 79 1 U1-K17
TOP 179 4.0825665 1.0993307 0 N 77 1 U1-K18
TOP 180 3.5471328 1.0678346 0 N 448 1 U1-L1
TOP 181 3.5786289 1.0678346 0 N 446 1 U1-L2
TOP 182 3.610125 1.0678346 0 N 361 1 U1-L3
TOP 183 3.6416211 1.0678346 0 N 162 16 U1-L4
TOP 184 3.6731172 1.0678346 0 N 284 530 U1-L5
TOP 185 3.7046133 1.0678346 0 N 284 522 U1-L6
TOP 186 3.7361094 1.0678346 0 N 284 513 U1-L7
TOP 187 3.7676055 1.0678346 0 N 284 504 U1-L8
TOP 188 3.7991016 1.0678346 0 N 284 496 U1-L9
TOP 189 3.8305977 1.0678346 0 N 284 487 U1-L10
TOP 190 3.8620938 1.0678346 0 N 284 479 U1-L11
TOP 191 3.8935899 1.0678346 0 N 284 470 U1-L12
TOP 192 3.925086 1.0678346 0 N 284 462 U1-L13
TOP 193 3.9565821 1.0678346 0 N 284 454 U1-L14
TOP 194 3.9880782 1.0678346 0 N 159 180 U1-L15
TOP 195 4.0195743 1.0678346 0 N 481 1 U1-L16
TOP 196 4.0510704 1.0678346 0 N 420 1 U1-L17
TOP 197 4.0825665 1.0678346 0 N 422 1 U1-L18
TOP 198 3.5471328 1.0363385 0 N 100 1 U1-M1
TOP 199 3.5786289 1.0363385 0 N 560 1 U1-M2
TOP 200 3.610125 1.0363385 0 N 360 1 U1-M3
TOP 201 3.6416211 1.0363385 0 N 413 1 U1-M4
TOP 202 3.6731172 1.0363385 0 N 284 529 U1-M5
TOP 203 3.7046133 1.0363385 0 N 284 521 U1-M6
TOP 204 3.7361094 1.0363385 0 N 284 512 U1-M7
TOP 205 3.7676055 1.0363385 0 N 284 503 U1-M8
TOP 206 3.7991016 1.0363385 0 N 284 495 U1-M9
TOP 207 3.8305977 1.0363385 0 N 284 486 U1-M10
TOP 208 3.8620938 1.0363385 0 N 284 478 U1-M11
TOP 209 3.8935899 1.0363385 0 N 284 469 U1-M12
TOP 210 3.925086 1.0363385 0 N 284 461 U1-M13
TOP 211 3.9565821 1.0363385 0 N 284 453 U1-M14
TOP 212 3.9880782 1.0363385 0 N 487 1 U1-M15
TOP 213 4.0195743 1.0363385 0 N 489 1 U1-M16
TOP 214 4.0510704 1.0363385 0 N 443 1 U1-M17
TOP 215 4.0825665 1.0363385 0 N 396 1 U1-M18
TOP 216 3.5471328 1.0048424 0 N 415 2 U1-N1
TOP 217 3.5786289 1.0048424 0 N 418 1 U1-N2
TOP 218 3.610125 1.0048424 0 N 0 158 U1-N3
TOP 219 3.6416211 1.0048424 0 N 414 2 U1-N4
TOP 220 3.6731172 1.0048424 0 N 175 56 U1-N5
TOP 221 3.7046133 1.0048424 0 N 175 53 U1-N6
TOP 222 3.7361094 1.0048424 0 N 284 511 U1-N7
TOP 223 3.7676055 1.0048424 0 N 284 502 U1-N8
TOP 224 3.7991016 1.0048424 0 N 284 494 U1-N9
TOP 225 3.8305977 1.0048424 0 N 284 485 U1-N10
TOP 226 3.8620938 1.0048424 0 N 284 477 U1-N11
TOP 227 3.8935899 1.0048424 0 N 284 468 U1-N12
TOP 228 3.925086 1.0048424 0 N 175 44 U1-N13
TOP 229 3.9565821 1.0048424 0 N 175 41 U1-N14
TOP 230 3.9880782 1.0048424 0 N 162 13 U1-N15
TOP 231 4.0195743 1.0048424 0 N 441 1 U1-N16
TOP 232 4.0510704 1.0048424 0 N 398 1 U1-N17
TOP 233 4.0825665 1.0048424 0 N 394 1 U1-N18
TOP 234 3.5471328 0.9733463 0 N 416 2 U1-P1
TOP 235 3.5786289 0.9733463 0 N 519 1 U1-P2
TOP 236 3.610125 0.9733463 0 N 412 1 U1-P3
TOP 237 3.6416211 0.9733463 0 N 159 184 U1-P4
TOP 238 3.6731172 0.9733463 0 N 284 528 U1-P5
TOP 239 3.7046133 0.9733463 0 N 284 520 U1-P6
TOP 240 3.7361094 0.9733463 0 N 165 8 U1-P7
TOP 241 3.7676055 0.9733463 0 N 284 501 U1-P8
TOP 242 3.7991016 0.9733463 0 N 165 7 U1-P9
TOP 243 3.8305977 0.9733463 0 N 284 484 U1-P10
TOP 244 3.8620938 0.9733463 0 N 165 6 U1-P11
TOP 245 3.8935899 0.9733463 0 N 284 467 U1-P12
TOP 246 3.925086 0.9733463 0 N 284 460 U1-P13
TOP 247 3.9565821 0.9733463 0 N 284 452 U1-P14
TOP 248 3.9880782 0.9733463 0 N 110 1 U1-P15
TOP 249 4.0195743 0.9733463 0 N 404 1 U1-P16
TOP 250 4.0510704 0.9733463 0 N 402 1 U1-P17
TOP 251 4.0825665 0.9733463 0 N 400 1 U1-P18
TOP 252 3.5471328 0.9418502 0 N 356 2 U1-R1
TOP 253 3.5786289 0.9418502 0 N 423 3 U1-R2
TOP 254 3.610125 0.9418502 0 N 47 3 U1-R3
TOP 255 3.6416211 0.9418502 0 N 167 3 U1-R4
TOP 256 3.6731172 0.9418502 0 N 284 527 U1-R5
TOP 257 3.7046133 0.9418502 0 N 166 11 U1-R6
TOP 258 3.7361094 0.9418502 0 N 25 3 U1-R7
TOP 259 3.7676055 0.9418502 0 N 166 10 U1-R8
TOP 260 3.7991016 0.9418502 0 N 175 50 U1-R9
TOP 261 3.8305977 0.9418502 0 N 593 4 U1-R10
TOP 262 3.8620938 0.9418502 0 N 166 9 U1-R11
TOP 263 3.8935899 0.9418502 0 N 584 0 U1-R12
TOP 264 3.925086 0.9418502 0 N 284 459 U1-R13
TOP 265 3.9565821 0.9418502 0 N 590 0 U1-R14
TOP 266 3.9880782 0.9418502 0 N 159 179 U1-R15
TOP 267 4.0195743 0.9418502 0 N 109 1 U1-R16
TOP 268 4.0510704 0.9418502 0 N 405 1 U1-R17
TOP 269 4.0825665 0.9418502 0 N 406 1 U1-R18
TOP 270 3.5471328 0.9103541 0 N 357 2 U1-T1
TOP 271 3.5786289 0.9103541 0 N 284 535 U1-T2
TOP 272 3.610125 0.9103541 0 N 162 17 U1-T3
TOP 273 3.6416211 0.9103541 0 N 175 59 U1-T4
TOP 274 3.6731172 0.9103541 0 N 558 2 U1-T5
TOP 275 3.7046133 0.9103541 0 N 351 5 U1-T6
TOP 276 3.7361094 0.9103541 0 N 26 1 U1-T7
TOP 277 3.7676055 0.9103541 0 N 578 0 U1-T8
TOP 278 3.7991016 0.9103541 0 N 574 4 U1-T9
TOP 279 3.8305977 0.9103541 0 N 29 1 U1-T10
TOP 280 3.8620938 0.9103541 0 N 594 4 U1-T11
TOP 281 3.8935899 0.9103541 0 N 31 1 U1-T12
TOP 282 3.925086 0.9103541 0 N 351 4 U1-T13
TOP 283 3.9565821 0.9103541 0 N 32 1 U1-T14
TOP 284 3.9880782 0.9103541 0 N 565 0 U1-T15
TOP 285 4.0195743 0.9103541 0 N 111 1 U1-T16
TOP 286 4.0510704 0.9103541 0 N 409 1 U1-T17
TOP 287 4.0825665 0.9103541 0 N 407 1 U1-T18
TOP 288 3.5471328 0.878858 0 N 366 0 U1-U1
TOP 289 3.5786289 0.878858 0 N 156 3 U1-U2
TOP 290 3.610125 0.878858 0 N 562 0 U1-U3
TOP 291 3.6416211 0.878858 0 N 567 0 U1-U4
TOP 292 3.6731172 0.878858 0 N 569 0 U1-U5
TOP 293 3.7046133 0.878858 0 N 589 4 U1-U6
TOP 294 3.7361094 0.878858 0 N 592 4 U1-U7
TOP 295 3.7676055 0.878858 0 N 27 1 U1-U8
TOP 296 3.7991016 0.878858 0 N 572 0 U1-U9
TOP 297 3.8305977 0.878858 0 N 28 1 U1-U10
TOP 298 3.8620938 0.878858 0 N 587 4 U1-U11
TOP 299 3.8935899 0.878858 0 N 585 0 U1-U12
TOP 300 3.925086 0.878858 0 N 591 0 U1-U13
TOP 301 3.9565821 0.878858 0 N 586 4 U1-U14
TOP 302 3.9880782 0.878858 0 N 588 4 U1-U15
TOP 303 4.0195743 0.878858 0 N 566 0 U1-U16
TOP 304 4.0510704 0.878858 0 N 410 1 U1-U17
TOP 305 4.0825665 0.878858 0 N 408 1 U1-U18
TOP 306 3.5471328 0.8473619 0 N 284 536 U1-V1
TOP 307 3.5786289 0.8473619 0 N 561 0 U1-V2
TOP 308 3.610125 0.8473619 0 N 568 0 U1-V3
TOP 309 3.6416211 0.8473619 0 N 570 0 U1-V4
TOP 310 3.6731172 0.8473619 0 N 571 1 U1-V5
TOP 311 3.7046133 0.8473619 0 N 24 3 U1-V6
TOP 312 3.7361094 0.8473619 0 N 23 3 U1-V7
TOP 313 3.7676055 0.8473619 0 N 573 0 U1-V8
TOP 314 3.7991016 0.8473619 0 N 579 0 U1-V9
TOP 315 3.8305977 0.8473619 0 N 564 5 U1-V10
TOP 316 3.8620938 0.8473619 0 N 563 5 U1-V11
TOP 317 3.8935899 0.8473619 0 N 30 3 U1-V12
TOP 318 3.925086 0.8473619 0 N 563 4 U1-V13
TOP 319 3.9565821 0.8473619 0 N 564 4 U1-V14
TOP 320 3.9880782 0.8473619 0 N 595 4 U1-V15
TOP 321 4.0195743 0.8473619 0 N 284 451 U1-V16
TOP 322 4.0510704 0.8473619 0 N 112 1 U1-V17
TOP 323 4.0825665 0.8473619 0 N 284 449 U1-V18
#
# CMP 464
CMP 32 0.1137888 1.7718271 270 N FID3 Fiducial ;0=1,1=0.0461
PRP ClassName 'FiducialMark'
PRP CompType 'Fiducial'
PRP Manufacturer 'N/A'
PRP MountType 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 0.1137888 1.7718271 270 N 0 159 FID3-1
#
# CMP 465
CMP 32 0.1137892 0.392065 270 N FID2 Fiducial ;0=1,1=0.0461
PRP ClassName 'FiducialMark'
PRP CompType 'Fiducial'
PRP Manufacturer 'N/A'
PRP MountType 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 0.1137892 0.392065 270 N 0 121 FID2-1
#
# CMP 466
CMP 32 6.99538 2.165 270 N FID1 Fiducial ;0=1,1=0.0461
PRP ClassName 'FiducialMark'
PRP CompType 'Fiducial'
PRP Manufacturer 'N/A'
PRP MountType 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 6.99538 2.165 270 N 0 120 FID1-1
#
