A!LAYER_SORT!LAYER_SUBCLASS!LAYER_ARTWORK!LAYER_USE!LAYER_CONDUCTOR!LAYER_DIELECTRIC_CONSTANT!LAYER_ELECTRICAL_CONDUCTIVITY!LAYER_MATERIAL!LAYER_THERMAL_CONDUCTIVITY!LAYER_THICKNESS!GRAPHIC_DATA_NAME!GRAPHIC_DATA_NUMBER!GRAPHIC_DATA_1!GRAPHIC_DATA_2!GRAPHIC_DATA_3!GRAPHIC_DATA_4!GRAPHIC_DATA_5!GRAPHIC_DATA_6!GRAPHIC_DATA_7!GRAPHIC_DATA_8!GRAPHIC_DATA_9!GRAPHIC_DATA_10!
J!C:/ADW_Projects/lp-em-cc2340r53-rkp-5x5-is24/design/CAD Source/allegro/mcu143a.brd!Wed Mar 20 15:56:07 2024!-100.000!-100.000!14900.001!1400.002!0.001!millimeters!MCU143A!31.496063 mil!2!UP TO DATE!
S!000000!!!!NO!1.000000!0 mho/cm!AIR!!0 mil!!!!!!!!!!!!!
S!000001!TOP!POSITIVE!!YES!1.000000!595900 mho/cm!COPPER!!1.377953 mil!!!!!!!!!!!!!
S!000002!!!!NO!4.200000!0 mho/cm!FR-4!!28.740157 mil!!!!!!!!!!!!!
S!000003!BOTTOM!POSITIVE!!YES!1.000000!595900 mho/cm!COPPER!!1.377953 mil!!!!!!!!!!!!!
S!000004!!!!NO!1.000000!0 mho/cm!AIR!!0 mil!!!!!!!!!!!!!
