#
#Component attribute names
#
@0 .comp_mount_type
@1 .comp_height

# CMP 0
CMP 17 0.1035224 0.5420723 270 N R8 ERJ-3GEY0R00V ;0=1,1=0.0276
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP DataSheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-3GEY0R00V.pdf'
PRP Device_Class_L1 'Passive Components'
PRP Device_Class_L2 'Resistors'
PRP Device_Class_L3 'Chip SMD Resistors'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0603'
PRP Digikey_Part_Number 'P0.0GCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/655dc946655e5dbc/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Resistor, Chip Thick Film, 0 Ohm, 0.1w, Resistor, Chip Thick Film, 0 Ohm, 0.1w, 5%'
PRP Mouser_Part_Number '667-ERJ-3GEY0R00V'
PRP Operating_Temperature_Range '-55¡ãC to +155¡ãC'
PRP PackageReference '0603'
PRP Part_Number 'ERJ-3GEY0R00V'
PRP PartNumber 'ERJ-3GEY0R00V'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.55mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0GCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-3GEY0R00V'
PRP Technology 'Thick Film'
PRP TempCo '-100/+600ppm/¡ãC'
PRP Tolerance__ '5%'
PRP VDC_V '75V'
TOP 0 0.1035224 0.513529 270 N 25 2 1
TOP 1 0.1035224 0.5706156 270 N 27 6 2
#
# CMP 1
CMP 24 0.607479 0.211199 180 N R5 RC0402JR-070RP ;0=1,1=0.0276
PRP AEC_Qualified 'No'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.yageo.com/upload/media/product/productsearch/datasheet/rchip/PYu-RC_51_RoHS_P_2.pdf'
PRP DataSheet 'https://www.yageo.com/upload/media/product/productsearch/datasheet/rchip/PYu-RC_51_RoHS_P_2.pdf'
PRP Datasheet_Path 'datasheets/Res-RC0402JR-070RP.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/16W 0402'
PRP Digikey_Part_Number 'YAG1279CT-ND'
PRP helpURL 'https://upverter.com/upn/revision/1e1ee5977c47aafb/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Yageo'
PRP Mouser_Description 'RC Series 0402 Jumper Thick Film Chip Resistor'
PRP Mouser_Part_Number '603-RC0402JR-070RP'
PRP Operating_Temperature_Range '-55¡ãC to +155¡ãC'
PRP PackageReference '0402'
PRP Part_Number 'RC0402JR-070RP'
PRP PartNumber 'RC0402JR-070RP'
PRP Power_W '63mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'RC_P'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'YAG1279CT-ND'
PRP Supplier_Part_Number_2 '603-RC0402JR-070RP'
PRP Technology 'Thick Film'
PRP Value '0'
PRP VDC_V '50V'
TOP 0 0.627164 0.211199 180 N 8 2 1
TOP 1 0.587794 0.211199 180 N 45 1 2
#
# CMP 2
CMP 5 0.7886744 0.2435912 0 N R172 ERJ-2RKF5100X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF5100X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '510'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P510LCT-ND'
PRP Supplier_Part_Number_2 '53W4394'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF5100X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '510'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '510R'
PRP ValueDisplayed '510'
PRP VDC_V '50V'
TOP 0 0.7689894 0.2435912 270 N 54 12 1
TOP 1 0.8083595 0.2435912 270 N 13 0 2
#
# CMP 3
CMP 19 0.040029 0.687291 180 N C17 GRM155R61A225ME01D ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP Cap_F '2.2¦ÌF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.murata.com/en-us/products/productdetail?partno=GRM155R61A225ME01%23'
PRP DataSheet 'https://www.murata.com/en-us/products/productdetail?partno=GRM155R61A225ME01%23'
PRP Datasheet_Path 'datasheets/Cap-GRM155R61A225ME01D.pdf'
PRP helpURL 'https://upverter.com/upn/revision/9c1060debce10243/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Murata'
PRP Operating_Temperature_Range '-55¡ãC to +85¡ãC'
PRP PackageReference '0402'
PRP Part_Number 'GRM155R61A225ME01D'
PRP PartNumber 'GRM155R61A225ME01D'
PRP RoHS 'TRUE'
PRP SizeZ_mm '0.55mm'
PRP TempCo '15%'
PRP Temperature_Characteristic 'X5R'
PRP Tolerance__ '20%'
PRP Value '2.2¦ÌF'
PRP ValueDisplayed '2.2uF'
PRP VDC_V '10V'
TOP 0 0.055777 0.687291 180 N 11 102 1
TOP 1 0.024281 0.687291 180 N 32 15 2
#
# CMP 4
CMP 29 0.740313 0.8160982 270 N TP5 TESTPOINT ;0=1,1=0.0000
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ClassName ''
PRP ComponentLink1Description ''
PRP ComponentLink1URL ''
PRP CompType 'Testpoint'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'N/A'
PRP MountType ''
PRP Note ''
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
PRP RoHS ''
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Value ''
TOP 0 0.740313 0.8160982 270 N 42 1 1
#
# CMP 5
CMP 25 0.7871354 0.1790012 0 N D3 VLMY1500-GS08 ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP Angle '130¡ã'
PRP Color 'Yellow'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.vishay.com/docs/82554/vlmo1500.pdf'
PRP DataSheet 'https://www.vishay.com/docs/82554/vlmo1500.pdf'
PRP Datasheet_Path 'datasheets/Diode-VLMY1500-GS08.pdf'
PRP Digikey_Description 'LED YELLOW 0402 SMD'
PRP Digikey_Part_Number 'VLMY1500-GS08CT-ND'
PRP Forward_Current '20mA'
PRP helpURL 'https://upverter.com/upn/revision/6fc1d97824805f25/'
PRP LambdaD '590nm'
PRP LambdaP '588nm'
PRP Lead_Free 'Yes'
PRP Led_Orientation 'Top View'
PRP Luminous_Intensity '90mcd'
PRP Manufacturer 'Vishay'
PRP Mounting_Type 'Surface Mount'
PRP Mouser_Description 'VLMY1500-GS08 Yellow LED, 597 nm 1005 (0402), Square Lens SMD package'
PRP Mouser_Part_Number '78-VLMY1500-GS08'
PRP Operating_Temperature_Range '-30¡ãC to +85 ¡ãC'
PRP PackageReference '0402'
PRP Part_Number 'VLMY1500-GS08'
PRP PartNumber 'VLMY1500-GS08'
PRP Power_TotalModule '75mW'
PRP RoHS 'TRUE'
PRP SizeZ_mm '0.35mm'
PRP TaMax_C '+85¡ãC'
PRP TaMin_C '-30¡ãC'
PRP Vf_V '2V'
PRP Vr_V '5V'
TOP 0 0.7684346 0.1790012 0 N 12 0 1
TOP 1 0.8058362 0.1790012 0 N 13 1 2
#
# CMP 6
CMP 24 0.7468588 0.447829 180 N R1 RC0402JR-070RP ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.yageo.com/upload/media/product/productsearch/datasheet/rchip/PYu-RC_51_RoHS_P_2.pdf'
PRP DataSheet 'https://www.yageo.com/upload/media/product/productsearch/datasheet/rchip/PYu-RC_51_RoHS_P_2.pdf'
PRP Datasheet_Path 'datasheets/Res-RC0402JR-070RP.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/16W 0402'
PRP Digikey_Part_Number 'YAG1279CT-ND'
PRP helpURL 'https://upverter.com/upn/revision/1e1ee5977c47aafb/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Yageo'
PRP Mouser_Description 'RC Series 0402 Jumper Thick Film Chip Resistor'
PRP Mouser_Part_Number '603-RC0402JR-070RP'
PRP Operating_Temperature_Range '-55¡ãC to +155¡ãC'
PRP PackageReference '0402'
PRP Part_Number 'RC0402JR-070RP'
PRP PartNumber 'RC0402JR-070RP'
PRP Power_W '63mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'RC_P'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'YAG1279CT-ND'
PRP Supplier_Part_Number_2 '603-RC0402JR-070RP'
PRP Technology 'Thick Film'
PRP Value '0'
PRP VDC_V '50V'
TOP 0 0.7665438 0.447829 180 N 3 2 1
TOP 1 0.7271738 0.447829 180 N 6 6 2
#
# CMP 7
CMP 26 0.6520572 0.6663234 90 N U2 W25Q16JVUXIQ ;0=1,1=0.0000
PRP Access_Time '6ns'
PRP AEC_Qualified 'No'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.winbond.com/resource-files/w25q16jv%20spi%20revh%2004082019%20plus.pdf'
PRP DataSheet 'https://www.winbond.com/resource-files/w25q16jv%20spi%20revh%2004082019%20plus.pdf'
PRP Datasheet_Path 'datasheets/IC-W25Q16JVUXIQ.pdf'
PRP Digikey_Description 'IC FLASH 16MBIT SPI/QUAD 8USON'
PRP Digikey_Part_Number '256-W25Q16JVUXIQTRCT-ND'
PRP Frequency_Fixed '532MHz'
PRP helpURL 'https://upverter.com/upn/revision/f2673167c9b4a4df/'
PRP Interface 'SPI'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Winbond'
PRP Max_Supply_Voltage '3.6V'
PRP Memory_Size '16Mbits'
PRP Memory_Type 'FLASH'
PRP Min_Supply_Voltage '2.7V'
PRP Mouser_Part_Number '454-W25Q16JVUXIQTR'
PRP Nominal_Supply_Current '2-20mA'
PRP Operating_Temperature_Range '-40¡ãC to +85¡ãC'
PRP PackageReference 'USON8'
PRP Part_Number 'W25Q16JVUXIQ'
PRP PartNumber 'W25Q16JVUXIQ'
PRP RoHS 'TRUE'
PRP SizeZ_mm '0.6mm'
PRP Standoff_Height '0mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 '256-W25Q16JVUXIQTRCT-ND'
PRP Supplier_Part_Number_2 '454-W25Q16JVUXIQTR'
PRP TaMax_C '+85¡ãC'
PRP TaMin_C '-40¡ãC'
TOP 0 0.6815848 0.715536 90 N 19 2 1
TOP 1 0.6618997 0.715536 90 N 17 1 2
TOP 2 0.6422147 0.715536 90 N 16 1 3
TOP 3 0.6225296 0.715536 90 N 11 104 4
TOP 4 0.6225296 0.6171108 90 N 18 1 5
TOP 5 0.6422147 0.6171108 90 N 14 1 6
TOP 6 0.6618997 0.6171108 90 N 15 1 7
TOP 7 0.6815848 0.6171108 90 N 32 16 8
TOP 8 0.6520572 0.6663234 90 N 11 103 9
#
# CMP 8
CMP 29 0.038363 0.123508 270 N TP11 TESTPOINT ;0=1,1=0.0000
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ClassName ''
PRP ComponentLink1Description ''
PRP ComponentLink1URL ''
PRP CompType 'Testpoint'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'N/A'
PRP MountType ''
PRP Note ''
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
PRP RoHS ''
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Value ''
TOP 0 0.038363 0.123508 270 N 11 39 1
#
# CMP 9
CMP 4 0.6665166 0.2232294 270 N R244 RC0402FR-071ML ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.yageo.com/NewPortal/yageodocoutput?fileName=/pdf/R-Chip/PYu-RC_Group_51_RoHS_L_0.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Yageo America'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'RC0402FR-071ML'
PRP Power_W '63mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '1M'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '311-1.00MLRCT-ND'
PRP Supplier_Part_Number_2 '66R1086'
PRP Supplier_Part_Number_3 '603-RC0402FR-071ML'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '1.00Meg'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '1M00'
PRP ValueDisplayed '1.00M'
PRP VDC_V ''
TOP 0 0.6665166 0.1996074 180 N 11 105 1
TOP 1 0.6665166 0.2468515 180 N 8 0 2
#
# CMP 10
CMP 8 0.0908282 0.3156568 270 N L7 BLM18KG121TH1D ;0=1,1=0.0394
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.murata.com/en-global/products/productdata/8796737273886/QNFA9101.pdf'
PRP CompType 'Ferrite Bead'
PRP DCR_ohm '0.04'
PRP Imax_A '1.9A'
PRP LatestRevisionDate ''
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'BLM18KG121TH1D'
PRP Published ''
PRP Publisher ''
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1.0'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-13261-1-ND'
PRP Supplier_Part_Number_2 '81-BLM18KG121TH1D'
PRP Supplier_Part_Number_3 ''
PRP Value '120 ohm'
PRP Value1 '0.04 ohm'
PRP Value2 '1.9A'
PRP ValueDisplayed '120 ohm'
PRP Ztyp@1GHz_Ohm ''
PRP ZTyp@100MHz_Ohm '120'
TOP 0 0.0908282 0.2880977 180 N 54 5 1
TOP 1 0.0908282 0.3432158 180 N 32 4 2
#
# CMP 11
CMP 29 0.129294 0.3292266 0 N TP9 TESTPOINT ;0=1,1=0.0354
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ClassName ''
PRP ComponentLink1Description ''
PRP ComponentLink1URL ''
PRP CompType 'Testpoint'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'N/A'
PRP MountType ''
PRP Note ''
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
PRP RoHS ''
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Value ''
TOP 0 0.129294 0.3292266 0 N 32 5 1
#
# CMP 12
CMP 0 0.0362076 0.859219 270 N R86 CRCW02011K00FKED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02011K00FKED'
PRP Power_W '50mW'
PRP Res_ohm '1k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '541-1.00KAABCT-ND'
PRP Supplier_Part_Number_2 '71-CRCW02011K00FKED'
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '1.00k'
PRP Value1 '1%'
PRP Value2 '0.05W'
PRP Value_Code '1k00'
PRP ValueDisplayed '1.00k'
PRP VDC_V '30V'
TOP 0 0.0362076 0.8462269 180 N 28 6 1
TOP 1 0.0362076 0.8722111 180 N 58 0 2
#
# CMP 13
CMP 1 0.0684676 0.8705502 270 N C3 GRM033R60J105MEA2D ;0=1,1=0.0130
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0201'
PRP Cap_F '1¦ÌF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033R60J105MEA2-02.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'GRM033R60J105MEA2D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.18'
PRP SizeAreaWB_mm2 '2.08'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.33'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-7229-1-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '85¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'X5R'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '1uF'
PRP VDC_V '6.3V'
TOP 0 0.0684676 0.8575581 180 N 58 1 1
TOP 1 0.0684676 0.8835423 180 N 11 59 2
#
# CMP 14
CMP 21 0.1805524 0.4667954 270 N C79 GRM31CR70J226ME19K ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP Cap_F '22¦ÌF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.murata.com/en-us/products/productdetail?partno=GRM31CR70J226ME19%23'
PRP DataSheet 'https://www.murata.com/en-us/products/productdetail?partno=GRM31CR70J226ME19%23'
PRP Datasheet_Path 'datasheets/Cap-GRM31CR70J226ME19K.pdf'
PRP helpURL 'https://upverter.com/upn/revision/24953124f7c6a3ae/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Murata'
PRP Operating_Temperature_Range '-55¡ãC to +125¡ãC'
PRP PackageReference '1206'
PRP Part_Number 'GRM31CR70J226ME19K'
PRP PartNumber 'GRM31CR70J226ME19K'
PRP RoHS 'TRUE'
PRP SizeZ_mm '1.8mm'
PRP TempCo '15%'
PRP Temperature_Characteristic 'X7R'
PRP Tolerance__ '20%'
PRP Value '22¦ÌF'
PRP ValueDisplayed '22uF'
PRP VDC_V '6.3V'
TOP 0 0.1805524 0.4087244 270 N 11 107 1
TOP 1 0.1805524 0.5248663 270 N 25 3 2
#
# CMP 15
CMP 8 0.0471824 0.3159706 270 N L2 BLM18KG121TH1D ;0=1,1=0.0394
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.murata.com/en-global/products/productdata/8796737273886/QNFA9101.pdf'
PRP CompType 'Ferrite Bead'
PRP DCR_ohm '0.04'
PRP Imax_A '1.9A'
PRP LatestRevisionDate ''
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'BLM18KG121TH1D'
PRP Published ''
PRP Publisher ''
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1.0'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-13261-1-ND'
PRP Supplier_Part_Number_2 '81-BLM18KG121TH1D'
PRP Supplier_Part_Number_3 ''
PRP Value '120 ohm'
PRP Value1 '0.04 ohm'
PRP Value2 '1.9A'
PRP ValueDisplayed '120 ohm'
PRP Ztyp@1GHz_Ohm ''
PRP ZTyp@100MHz_Ohm '120'
TOP 0 0.0471824 0.2884115 180 N 54 6 1
TOP 1 0.0471824 0.3435296 180 N 32 6 2
#
# CMP 16
CMP 12 0.8023924 0.7864062 0 N FID6 Fiducial ;0=1,1=0.0000
PRP ClassName 'FiducialMark'
PRP CompType 'Fiducial'
PRP Manufacturer 'N/A'
PRP MountType 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 0.8023924 0.7864062 0 N 0 2 1
#
# CMP 17
CMP 12 0.797686 0.058548 0 N FID4 Fiducial ;0=1,1=0.0000
PRP ClassName 'FiducialMark'
PRP CompType 'Fiducial'
PRP Manufacturer 'N/A'
PRP MountType 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 0.797686 0.058548 0 N 0 0 1
#
# CMP 18
CMP 12 0.0553398 0.056655 0 N FID1 Fiducial ;0=1,1=0.0000
PRP ClassName 'FiducialMark'
PRP CompType 'Fiducial'
PRP Manufacturer 'N/A'
PRP MountType 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 0.0553398 0.056655 0 N 0 1 1
#
# CMP 19
CMP 5 0.7617112 0.3471902 270 N R2 CRCW040240K2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040240K2FKED'
PRP Power_W '63mW'
PRP Res_ohm '40.2k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-40.2KLCT-ND'
PRP Supplier_Part_Number_2 '52K7049'
PRP Supplier_Part_Number_3 '71-CRCW0402-40.2K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '40.2k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '40k2'
PRP ValueDisplayed '40.2k'
PRP VDC_V '50V'
TOP 0 0.7617112 0.3275052 180 N 11 40 1
TOP 1 0.7617112 0.3668753 180 N 3 0 2
#
# CMP 20
CMP 10 0.2568876 0.856577 90 N U1 IWRL6432QGAMF ;0=1,1=0.0000
PRP AEC_Category 'Q200'
PRP AEC_Qualified ''
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/GPN.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/GPN'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/GPN/datasheet'
PRP CompType 'IC'
PRP Datasheet_Path 'datasheets/IC-IWRL6432QGAMF.pdf'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP helpURL 'https://upverter.com/upn/revision/9536c2a4bea7f812/'
PRP Manufacturer 'Texas Instruments'
PRP MountType ''
PRP Operating_Temperature_Range 'to'
PRP PackageDescription ''
PRP PackageReference 'FCCSP102'
PRP Part_Number 'IWRL6432QGAMF'
PRP PartNumber 'IWRL6432QGAMF'
PRP Rating ''
PRP RoHS 'UNKNOWN'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm '0.97mm'
PRP Standoff_Height '0.15mm'
TOP 0 0.3651553 0.9648447 90 N 11 61 A1
TOP 1 0.3651553 0.9451597 90 N 11 62 A2
TOP 2 0.3651553 0.9254746 90 N 50 1 A3
TOP 3 0.3651553 0.9057896 90 N 11 63 A4
TOP 4 0.3651553 0.8861046 90 N 51 1 A5
TOP 5 0.3651553 0.8664195 90 N 11 64 A6
TOP 6 0.3651553 0.8467345 90 N 42 0 A7
TOP 7 0.3651553 0.8270494 90 N 52 1 A8
TOP 8 0.3651553 0.7876794 90 N 19 0 A10
TOP 9 0.3651553 0.7679943 90 N 14 0 A11
TOP 10 0.3651553 0.7483093 90 N 11 65 A12
TOP 11 0.3454703 0.9648447 90 N 55 0 B1
TOP 12 0.3454703 0.9451597 90 N 11 66 B2
TOP 13 0.3454703 0.9254746 90 N 11 67 B3
TOP 14 0.3454703 0.9057896 90 N 11 68 B4
TOP 15 0.3454703 0.8861046 90 N 11 69 B5
TOP 16 0.3454703 0.8664195 90 N 11 70 B6
TOP 17 0.3454703 0.8467345 90 N 11 71 B7
TOP 18 0.3454703 0.8270494 90 N 17 0 B8
TOP 19 0.3454703 0.8073644 90 N 15 0 B9
TOP 20 0.3454703 0.7876794 90 N 16 0 B10
TOP 21 0.3454703 0.7679943 90 N 18 0 B11
TOP 22 0.3454703 0.7483093 90 N 24 0 B12
TOP 23 0.3257852 0.9648447 90 N 11 72 C1
TOP 24 0.3257852 0.9451597 90 N 11 73 C2
TOP 25 0.3257852 0.8664195 90 N 31 5 C6
TOP 26 0.3257852 0.8270494 90 N 31 6 C8
TOP 27 0.3257852 0.8073644 90 N 28 9 C9
TOP 28 0.3257852 0.7679943 90 N 40 0 C11
TOP 29 0.3257852 0.7483093 90 N 36 0 C12
TOP 30 0.3061002 0.9648447 90 N 53 0 D1
TOP 31 0.3061002 0.9451597 90 N 11 74 D2
TOP 32 0.3061002 0.9254746 90 N 30 0 D3
TOP 33 0.3061002 0.7876794 90 N 44 0 D10
TOP 34 0.3061002 0.7679943 90 N 43 0 D11
TOP 35 0.2864152 0.9648447 90 N 11 75 E1
TOP 36 0.2864152 0.9451597 90 N 11 76 E2
TOP 37 0.2864152 0.8861046 90 N 11 77 E5
TOP 38 0.2864152 0.8664195 90 N 11 78 E6
TOP 39 0.2864152 0.8467345 90 N 11 79 E7
TOP 40 0.2864152 0.8270494 90 N 11 80 E8
TOP 41 0.2864152 0.8073644 90 N 11 81 E9
TOP 42 0.2864152 0.7876794 90 N 37 0 E10
TOP 43 0.2864152 0.7679943 90 N 61 1 E11
TOP 44 0.2864152 0.7483093 90 N 33 0 E12
TOP 45 0.2667301 0.9648447 90 N 49 1 F1
TOP 46 0.2667301 0.9451597 90 N 11 82 F2
TOP 47 0.2667301 0.9254746 90 N 31 7 F3
TOP 48 0.2667301 0.8861046 90 N 11 83 F5
TOP 49 0.2667301 0.8664195 90 N 11 84 F6
TOP 50 0.2667301 0.8467345 90 N 11 85 F7
TOP 51 0.2667301 0.8270494 90 N 11 86 F8
TOP 52 0.2667301 0.8073644 90 N 11 87 F9
TOP 53 0.2667301 0.7679943 90 N 38 0 F11
TOP 54 0.2470451 0.9648447 90 N 11 88 G1
TOP 55 0.2470451 0.9451597 90 N 11 89 G2
TOP 56 0.2470451 0.8861046 90 N 29 0 G5
TOP 57 0.2470451 0.8467345 90 N 28 10 G7
TOP 58 0.2470451 0.8270494 90 N 28 11 G8
TOP 59 0.2470451 0.8073644 90 N 28 12 G9
TOP 60 0.2470451 0.7679943 90 N 35 0 G11
TOP 61 0.2470451 0.7483093 90 N 32 12 G12
TOP 62 0.22736 0.9648447 90 N 48 1 H1
TOP 63 0.22736 0.9451597 90 N 11 90 H2
TOP 64 0.22736 0.8861046 90 N 46 0 H5
TOP 65 0.22736 0.8270494 90 N 28 13 H8
TOP 66 0.22736 0.7876794 90 N 23 0 H10
TOP 67 0.22736 0.7679943 90 N 39 0 H11
TOP 68 0.22736 0.7483093 90 N 11 91 H12
TOP 69 0.207675 0.9648447 90 N 11 92 J1
TOP 70 0.207675 0.9451597 90 N 11 93 J2
TOP 71 0.207675 0.8861046 90 N 31 8 J5
TOP 72 0.207675 0.7876794 90 N 45 0 J10
TOP 73 0.207675 0.7679943 90 N 22 0 J11
TOP 74 0.18799 0.9648447 90 N 47 1 K1
TOP 75 0.18799 0.9451597 90 N 11 94 K2
TOP 76 0.18799 0.8467345 90 N 28 14 K7
TOP 77 0.18799 0.8073644 90 N 11 95 K9
TOP 78 0.18799 0.7679943 90 N 2 0 K11
TOP 79 0.18799 0.7483093 90 N 31 9 K12
TOP 80 0.1683049 0.9648447 90 N 11 96 L1
TOP 81 0.1683049 0.9451597 90 N 11 97 L2
TOP 82 0.1683049 0.9254746 90 N 60 4 L3
TOP 83 0.1683049 0.9057896 90 N 27 4 L4
TOP 84 0.1683049 0.8861046 90 N 31 10 L5
TOP 85 0.1683049 0.8664195 90 N 57 0 L6
TOP 86 0.1683049 0.8270494 90 N 31 11 L8
TOP 87 0.1683049 0.8073644 90 N 28 15 L9
TOP 88 0.1683049 0.7876794 90 N 41 2 L10
TOP 89 0.1683049 0.7679943 90 N 1 0 L11
TOP 90 0.1683049 0.7483093 90 N 21 0 L12
TOP 91 0.1486199 0.9648447 90 N 11 98 M1
TOP 92 0.1486199 0.9451597 90 N 11 99 M2
TOP 93 0.1486199 0.9254746 90 N 60 5 M3
TOP 94 0.1486199 0.9057896 90 N 27 5 M4
TOP 95 0.1486199 0.8861046 90 N 31 12 M5
TOP 96 0.1486199 0.8664195 90 N 58 2 M6
TOP 97 0.1486199 0.8467345 90 N 28 16 M7
TOP 98 0.1486199 0.8270494 90 N 31 13 M8
TOP 99 0.1486199 0.7876794 90 N 20 0 M10
TOP 100 0.1486199 0.7679943 90 N 32 13 M11
TOP 101 0.1486199 0.7483093 90 N 11 100 M12
#
# CMP 21
CMP 2 0.3446656 0.6520754 270 N R93 CRCW020133R2FNED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW020133R2FNED'
PRP Power_W '50mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2ABCT-ND'
PRP Supplier_Part_Number_2 '26W8649'
PRP Supplier_Part_Number_3 '71-CRCW020133R2FNED'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.05W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V ''
TOP 0 0.3446656 0.6390833 180 N 34 0 1
TOP 1 0.3446656 0.6650675 180 N 61 0 2
#
# CMP 22
CMP 4 0.3221872 0.1607598 0 N R74 CRCW04022M00FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022M00FKED'
PRP Power_W '63mW'
PRP Res_ohm '2M'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.00MLCT-ND'
PRP Supplier_Part_Number_2 '52K6816'
PRP Supplier_Part_Number_3 '71-CRCW0402-2M-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.00Meg'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2M00'
PRP ValueDisplayed '2.00M'
PRP VDC_V '50V'
TOP 0 0.2985652 0.1607598 270 N 32 18 1
TOP 1 0.3458093 0.1607598 270 N 38 1 2
#
# CMP 23
CMP 4 0.3203908 0.2304212 270 N R73 CRCW04022M00FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022M00FKED'
PRP Power_W '63mW'
PRP Res_ohm '2M'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.00MLCT-ND'
PRP Supplier_Part_Number_2 '52K6816'
PRP Supplier_Part_Number_3 '71-CRCW0402-2M-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.00Meg'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2M00'
PRP ValueDisplayed '2.00M'
PRP VDC_V '50V'
TOP 0 0.3203908 0.2067992 180 N 32 17 1
TOP 1 0.3203908 0.2540433 180 N 37 1 2
#
# CMP 24
CMP 13 0.740313 0.727131 180 N R50 AC0402FR-0747K5L ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.yageo.com/upload/media/product/productsearch/datasheet/rchip/PYu-AC_51_RoHS_L_8.pdf'
PRP DataSheet 'https://www.yageo.com/upload/media/product/productsearch/datasheet/rchip/PYu-AC_51_RoHS_L_8.pdf'
PRP Datasheet_Path 'datasheets/Res-AC0402FR-0747K5L.pdf'
PRP Digikey_Description 'RES SMD 47.5K OHM 1% 1/16W 0402'
PRP Digikey_Part_Number '13-AC0402FR-0747K5LCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/53eb058114c18d9e/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Yageo'
PRP Mouser_Description 'Thick Film Resistors - SMD 1/16W 47.5K ohm 1% AEC-Q200'
PRP Mouser_Part_Number '603-AC0402FR-0747K5L'
PRP Operating_Temperature_Range '-55¡ãC to +155¡ãC'
PRP PackageReference '0402'
PRP Part_Number 'AC0402FR-0747K5L'
PRP PartNumber 'AC0402FR-0747K5L'
PRP Power_W '62.5mW'
PRP Res_ohm '47.5k'
PRP RoHS 'TRUE'
PRP Series 'AC'
PRP SizeZ_mm '0.37mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 '13-AC0402FR-0747K5LCT-ND'
PRP Supplier_Part_Number_2 '603-AC0402FR-0747K5L'
PRP Technology 'Thick Film'
PRP TempCo '100ppm/¡ãC'
PRP Tolerance__ '1%'
PRP Value '47.5k'
PRP VDC_V '50V'
TOP 0 0.759998 0.727131 180 N 32 14 1
TOP 1 0.720628 0.727131 180 N 19 1 2
#
# CMP 25
CMP 4 0.6968156 0.5633478 0 N R49 CRCW04022M00FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022M00FKED'
PRP Power_W '63mW'
PRP Res_ohm '2M'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.00MLCT-ND'
PRP Supplier_Part_Number_2 '52K6816'
PRP Supplier_Part_Number_3 '71-CRCW0402-2M-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.00Meg'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2M00'
PRP ValueDisplayed '2.00M'
PRP VDC_V '50V'
TOP 0 0.6731936 0.5633478 270 N 15 2 1
TOP 1 0.7204377 0.5633478 270 N 32 21 2
#
# CMP 26
CMP 4 0.6109866 0.7576686 180 N R44 CRCW04022M00FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022M00FKED'
PRP Power_W '63mW'
PRP Res_ohm '2M'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.00MLCT-ND'
PRP Supplier_Part_Number_2 '52K6816'
PRP Supplier_Part_Number_3 '71-CRCW0402-2M-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.00Meg'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2M00'
PRP ValueDisplayed '2.00M'
PRP VDC_V '50V'
TOP 0 0.6346086 0.7576686 90 N 16 2 1
TOP 1 0.5873645 0.7576686 90 N 32 19 2
#
# CMP 27
CMP 0 0.201669 0.1519626 0 N C53 GRM033C71A104KE14D ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0201'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033C71A104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-06-05'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'GRM033C71A104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.18'
PRP SizeAreaWB_mm2 '2.08'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-14450-1-ND'
PRP Supplier_Part_Number_2 '81-GRM033C71A104KE4D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'X7S'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '10V'
TOP 0 0.1886769 0.1519626 270 N 11 41 1
TOP 1 0.2146611 0.1519626 270 N 41 0 2
#
# CMP 28
CMP 5 0.7580906 0.6776786 0 N C35 GRM155R70J105KA12D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '1¦ÌF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R70J105KA12-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-06-05'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J105KA12D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '490-10024-1-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J105KA2D'
PRP Supplier_Part_Number_3 '2688505RL'
PRP TaMax_C '125¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '1uF'
PRP VDC_V '6.3V'
TOP 0 0.7384056 0.6776786 270 N 32 7 1
TOP 1 0.7777757 0.6776786 270 N 11 42 2
#
# CMP 29
CMP 0 0.7381414 0.6455122 180 N C34 GRM033C71A104KE14D ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0201'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033C71A104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-06-05'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'GRM033C71A104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.18'
PRP SizeAreaWB_mm2 '2.08'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-14450-1-ND'
PRP Supplier_Part_Number_2 '81-GRM033C71A104KE4D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'X7S'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '10V'
TOP 0 0.7511335 0.6455122 90 N 11 108 1
TOP 1 0.7251493 0.6455122 90 N 32 20 2
#
# CMP 30
CMP 0 0.457182 0.8136974 180 N C31 GRM033C71A104KE14D ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0201'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033C71A104KE14-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-06-05'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'GRM033C71A104KE14D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.18'
PRP SizeAreaWB_mm2 '2.08'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-14450-1-ND'
PRP Supplier_Part_Number_2 '81-GRM033C71A104KE4D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'X7S'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '10V'
TOP 0 0.4701741 0.8136974 90 N 11 43 1
TOP 1 0.4441899 0.8136974 90 N 52 0 2
#
# CMP 31
CMP 5 0.0573418 0.8146222 180 N C26 GRM155R71C224KA12D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '220nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R71C224KA12D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71C224KA12D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-5418-1-ND'
PRP Supplier_Part_Number_2 '81-GRM155R71C224KA2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.22uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '0.22uF'
PRP VDC_V '16V'
TOP 0 0.0770268 0.8146222 90 N 28 7 1
TOP 1 0.0376567 0.8146222 90 N 11 44 2
#
# CMP 32
CMP 5 0.0512298 0.784281 180 N C25 GRM155R71C224KA12D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '220nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R71C224KA12D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71C224KA12D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-5418-1-ND'
PRP Supplier_Part_Number_2 '81-GRM155R71C224KA2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.22uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '0.22uF'
PRP VDC_V '16V'
TOP 0 0.0709148 0.784281 90 N 28 8 1
TOP 1 0.0315447 0.784281 90 N 11 45 2
#
# CMP 33
CMP 8 0.0420048 0.9602486 90 N C23 GRM188Z71A106MA73D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '10¦ÌF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GRM188Z71A106MA73%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GRM188Z71A106MA73D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GRM188Z71A106MA3D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '10uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '10uF'
PRP VDC_V '10V'
TOP 0 0.0420048 0.9878077 0 N 60 1 1
TOP 1 0.0420048 0.9326896 0 N 11 46 2
#
# CMP 34
CMP 5 0.0912066 0.7049405 90 N C21 GRM155R71C224KA12D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '220nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R71C224KA12D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71C224KA12D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-5418-1-ND'
PRP Supplier_Part_Number_2 '81-GRM155R71C224KA2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.22uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '0.22uF'
PRP VDC_V '16V'
TOP 0 0.0912066 0.7246255 0 N 32 8 1
TOP 1 0.0912066 0.6852554 0 N 11 47 2
#
# CMP 35
CMP 5 0.0848942 0.9820504 270 N C19 GRM155R71C224KA12D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '220nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R71C224KA12D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71C224KA12D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-5418-1-ND'
PRP Supplier_Part_Number_2 '81-GRM155R71C224KA2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.22uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '0.22uF'
PRP VDC_V '16V'
TOP 0 0.0848942 0.9623654 180 N 60 2 1
TOP 1 0.0848942 1.0017355 180 N 11 48 2
#
# CMP 36
CMP 5 0.2658685 0.6892282 180 N C16 GRM155R71C224KA12D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '220nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R71C224KA12D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71C224KA12D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-5418-1-ND'
PRP Supplier_Part_Number_2 '81-GRM155R71C224KA2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.22uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '0.22uF'
PRP VDC_V '16V'
TOP 0 0.2855535 0.6892282 90 N 32 9 1
TOP 1 0.2461834 0.6892282 90 N 11 49 2
#
# CMP 37
CMP 8 0.1879092 0.6172186 180 N C13 GRM188Z71A106MA73D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '10¦ÌF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GRM188Z71A106MA73%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GRM188Z71A106MA73D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GRM188Z71A106MA3D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '10uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '10uF'
PRP VDC_V '10V'
TOP 0 0.2154683 0.6172186 90 N 31 4 1
TOP 1 0.1603502 0.6172186 90 N 11 50 2
#
# CMP 38
CMP 19 0.0426886 1.0455902 90 N C9 GRM155R61A225ME01D ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP Cap_F '2.2¦ÌF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.murata.com/en-us/products/productdetail?partno=GRM155R61A225ME01%23'
PRP DataSheet 'https://www.murata.com/en-us/products/productdetail?partno=GRM155R61A225ME01%23'
PRP Datasheet_Path 'datasheets/Cap-GRM155R61A225ME01D.pdf'
PRP helpURL 'https://upverter.com/upn/revision/9c1060debce10243/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Murata'
PRP Operating_Temperature_Range '-55¡ãC to +85¡ãC'
PRP PackageReference '0402'
PRP Part_Number 'GRM155R61A225ME01D'
PRP PartNumber 'GRM155R61A225ME01D'
PRP RoHS 'TRUE'
PRP SizeZ_mm '0.55mm'
PRP TempCo '15%'
PRP Temperature_Characteristic 'X5R'
PRP Tolerance__ '20%'
PRP Value '2.2¦ÌF'
PRP ValueDisplayed '2.2uF'
PRP VDC_V '10V'
TOP 0 0.0426886 1.0613382 90 N 11 51 1
TOP 1 0.0426886 1.0298422 90 N 60 3 2
#
# CMP 39
CMP 5 0.7468588 0.493693 0 N C2 GRM1555C1H100JA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '10pF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM1555C1H100JA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM1555C1H100JA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GRM1555C1H100JA1D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'C0G/NP0'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '10pF'
PRP Value1 'Unknown'
PRP Value2 '50V'
PRP ValueDisplayed '10pF'
PRP VDC_V '50V'
TOP 0 0.7271738 0.493693 270 N 6 2 1
TOP 1 0.7665439 0.493693 270 N 3 1 2
#
# CMP 40
CMP 16 0.198228 0.187088 180 N R165 ERJ-1RHD1002C ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP DataSheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-1RHD1002C.pdf'
PRP Digikey_Description 'RES SMD 10K OHM 0.5% 1/20W 0201'
PRP Digikey_Part_Number 'P15980CT-ND'
PRP helpURL 'https://upverter.com/upn/revision/1ca8f4053101326f/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Current Sense Resistors 0201 10Kohms 0.5% Tolerance'
PRP Mouser_Part_Number '667-ERJ-1RHD1002C'
PRP Operating_Temperature_Range '-55¡ãC to +125¡ãC'
PRP PackageReference '0201'
PRP Part_Number 'ERJ-1RHD1002C'
PRP PartNumber 'ERJ-1RHD1002C'
PRP Power_W '50mW'
PRP Res_ohm '10k'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.26mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P15980CT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-1RHD1002C'
PRP Technology 'Thick Film'
PRP TempCo '50ppm/¡ãC'
PRP Tolerance__ '0.5%'
PRP Value '10k'
PRP VDC_V '15V'
TOP 0 0.210039 0.187088 180 N 41 1 1
TOP 1 0.186417 0.187088 180 N 32 10 2
#
# CMP 41
CMP 8 0.161831 0.251846 0 N C60 GRM188R71C474KA88D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '470nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM188R71C474KA88D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GRM188R71C474KA88D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '490-3295-1-ND'
PRP Supplier_Part_Number_2 '81-GRM188R71C474KA88'
PRP Supplier_Part_Number_3 '1828893'
PRP TaMax_C '125¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.47uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '0.47uF'
PRP VDC_V '16V'
TOP 0 0.1342719 0.251846 270 N 54 7 1
TOP 1 0.18939 0.251846 270 N 11 52 2
#
# CMP 42
CMP 7 0.0892348 0.1837924 180 N C56 GRM188Z71A106MA73D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '10¦ÌF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GRM188Z71A106MA73%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GRM188Z71A106MA73D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GRM188Z71A106MA3D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '10uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '10uF'
PRP VDC_V '10V'
TOP 0 0.1172346 0.1837923 180 N 54 13 1
TOP 1 0.0612347 0.1837924 180 N 11 60 2
#
# CMP 43
CMP 5 0.0711364 0.23777 180 N C69 GRM1555C1H471JA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '470pF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM1555C1H471JA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM1555C1H471JA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '490-1297-1-ND'
PRP Supplier_Part_Number_2 '81-GRM1555C1H471JA01'
PRP Supplier_Part_Number_3 '8819688'
PRP TaMax_C '125¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'C0G/NP0'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '470pF'
PRP Value1 'Unknown'
PRP Value2 '50V'
PRP ValueDisplayed '470pF'
PRP VDC_V '50V'
TOP 0 0.0908214 0.23777 90 N 54 8 1
TOP 1 0.0514512 0.2377701 90 N 11 53 2
#
# CMP 44
CMP 3 0.735873 0.2207304 270 N R175 CRCW0201100KFKED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW0201100KFKED'
PRP Power_W '50mW'
PRP Res_ohm '100k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-100KAABCT-ND'
PRP Supplier_Part_Number_2 '84R1457'
PRP Supplier_Part_Number_3 '71-CRCW0201100KFKED'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '100k'
PRP Value1 '1%'
PRP Value2 '0.05W'
PRP Value_Code '100k'
PRP ValueDisplayed '100k'
PRP VDC_V '30V'
TOP 0 0.735873 0.2097068 180 N 32 11 1
TOP 1 0.735873 0.231754 180 N 5 0 2
#
# CMP 45
CMP 23 0.222499 0.2202642 0 N R176 RC0201JR-070RL ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'http://www.yageo.com/documents/recent/PYu-RC_Group_51_RoHS_L_10.pdf'
PRP Manufacturer 'Yageo'
PRP PackageReference '0201 (0603 Metric)'
PRP PartNumber 'RC0201JR-070RL'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP SizeZ_mm '0.26mm'
PRP Technology 'Thick Film'
PRP TempCo '200ppm/¡ãC'
PRP Tolerance__ '5%'
PRP VDC_V '25V'
TOP 0 0.2124868 0.2202642 0 N 41 3 1
TOP 1 0.2325111 0.2202641 0 N 5 2 2
#
# CMP 46
CMP 14 0.7289736 0.2896604 270 N R180 CRCW040218K0FKEDC ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.vishay.com/docs/28773/crcwce3.pdf'
PRP DataSheet 'https://www.vishay.com/docs/28773/crcwce3.pdf'
PRP Datasheet_Path 'datasheets/Res-CRCW040218K0FKEDC.pdf'
PRP Digikey_Description 'RES 18K OHM 1% 1/16W 0402'
PRP Digikey_Part_Number '541-4757-1-ND'
PRP helpURL 'https://upverter.com/upn/revision/f5433614e467177c/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Vishay'
PRP Mouser_Description 'Res Thick Film 0402 18K Ohm 1% 1/16W ¡À100ppm/¡ãC Molded SMD Paper T/R'
PRP Mouser_Part_Number '71-CRCW040218K0FKEDC'
PRP Operating_Temperature_Range '-55¡ãC to +155¡ãC'
PRP PackageReference '0402'
PRP Part_Number 'CRCW040218K0FKEDC'
PRP PartNumber 'CRCW040218K0FKEDC'
PRP Power_W '63mW'
PRP Res_ohm '18k'
PRP RoHS 'TRUE'
PRP Series 'CRCW-C e3'
PRP SizeZ_mm '0.35mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 '541-4757-1-ND'
PRP Supplier_Part_Number_2 '71-CRCW040218K0FKEDC'
PRP Technology 'Thick Film'
PRP TempCo '100ppm/¡ãC'
PRP Tolerance__ '1%'
PRP Value '18k'
PRP VDC_V '50V'
TOP 0 0.7289736 0.2719439 270 N 9 0 1
TOP 1 0.7289736 0.3073769 270 N 11 101 2
#
# CMP 47
CMP 8 0.5302388 0.4344626 90 N C128 GRM188Z71A106MA73D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '10¦ÌF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GRM188Z71A106MA73%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GRM188Z71A106MA73D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GRM188Z71A106MA3D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '10uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '10uF'
PRP VDC_V '10V'
TOP 0 0.5302388 0.4620217 0 N 6 3 1
TOP 1 0.5302388 0.4069036 0 N 11 54 2
#
# CMP 48
CMP 8 0.4703258 0.4344626 90 N C129 GRM188Z71A106MA73D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '10¦ÌF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GRM188Z71A106MA73%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GRM188Z71A106MA73D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GRM188Z71A106MA3D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '10uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '10uF'
PRP VDC_V '10V'
TOP 0 0.4703258 0.4620217 0 N 6 4 1
TOP 1 0.4703258 0.4069036 0 N 11 55 2
#
# CMP 49
CMP 15 0.6340146 0.4414018 270 N L15 DFE201210U-R47M=P2 ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.murata.com/en-us/products/productdetail?partno=DFE201210U-R47M%23'
PRP DataSheet 'https://www.murata.com/en-us/products/productdetail?partno=DFE201210U-R47M%23'
PRP Datasheet_Path 'datasheets/Ind-DFE201210U-R47M=P2.pdf'
PRP DCR_ohm '42m'
PRP Digikey_Description 'FIXED IND .47UH 3.0A 42MOHM'
PRP Digikey_Part_Number '490-17727-1-ND'
PRP helpURL 'https://upverter.com/upn/revision/7b65c208f048e6ea/'
PRP Ind_H '470nH'
PRP Irms '3A'
PRP Isat '4.4A'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Murata'
PRP Material 'Metal Alloy'
PRP Mouser_Part_Number '81-DFE201210U-R47MP2'
PRP Operating_Temperature_Range '-40¡ãC to +125¡ãC'
PRP PackageReference '0805 (2012)'
PRP Part_Number 'DFE201210U-R47M=P2'
PRP PartNumber 'DFE201210U-R47M=P2'
PRP RoHS 'TRUE'
PRP Shrouded 'true'
PRP SizeZ_mm '1mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 '490-17727-1-ND'
PRP Supplier_Part_Number_2 '81-DFE201210U-R47MP2'
PRP Technology 'Wirewound'
PRP Test_Frequency '1MHz'
PRP Tolerance__ '20%'
PRP Value '0.47uH'
TOP 0 0.6340146 0.4099057 270 N 64 0 1
TOP 1 0.6340145 0.4728978 270 N 6 5 2
#
# CMP 50
CMP 8 0.5245564 0.3101046 270 N C73 GRM188R71C474KA88D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '470nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM188R71C474KA88D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GRM188R71C474KA88D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '490-3295-1-ND'
PRP Supplier_Part_Number_2 '81-GRM188R71C474KA88'
PRP Supplier_Part_Number_3 '1828893'
PRP TaMax_C '125¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.47uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '0.47uF'
PRP VDC_V '16V'
TOP 0 0.5245564 0.2825455 180 N 54 9 1
TOP 1 0.5245564 0.3376636 180 N 11 56 2
#
# CMP 51
CMP 5 0.571904 0.31652 270 N C74 GRM1555C1H471JA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '470pF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM1555C1H471JA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM1555C1H471JA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '490-1297-1-ND'
PRP Supplier_Part_Number_2 '81-GRM1555C1H471JA01'
PRP Supplier_Part_Number_3 '8819688'
PRP TaMax_C '125¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'C0G/NP0'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '470pF'
PRP Value1 'Unknown'
PRP Value2 '50V'
PRP ValueDisplayed '470pF'
PRP VDC_V '50V'
TOP 0 0.571904 0.296835 180 N 54 10 1
TOP 1 0.5719041 0.3362051 180 N 11 57 2
#
# CMP 52
CMP 11 0.6524926 0.3338614 270 N U20 TPS6285020MDRLR ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP Datasheet_Path 'datasheets/IC-TPS6285020MDRLR.pdf'
PRP helpURL 'https://upverter.com/upn/revision/61877cd23c411ac8/'
PRP Manufacturer 'Texas Instruments'
PRP Max_Duty_Cycle '100%'
PRP Max_Supply_Voltage '6V'
PRP Min_Supply_Voltage '2.7V'
PRP Nominal_Supply_Current '17uA'
PRP Number_Of_Outputs '1'
PRP Operating_Temperature_Range '-40¡ãC to +150¡ãC'
PRP Output_Type 'AdjustableProgrammable'
PRP Output_Voltage '0.6-5.5V'
PRP PackageReference 'SOT583'
PRP Part_Number 'TPS6285020MDRLR'
PRP PartNumber 'TPS6285020MDRLR'
PRP RoHS 'UNKNOWN'
PRP SizeZ_mm '0.6mm'
PRP Standoff_Height '0mm'
PRP Switching_Frequency '1.8-4MHz'
PRP Switching_Topology 'Buck'
PRP TJmax_C '+150¡ãC'
TOP 0 0.622965 0.3047275 270 N 54 14 1
TOP 1 0.6426501 0.3047275 270 N 54 15 2
TOP 2 0.6623351 0.3047275 270 N 8 1 3
TOP 3 0.6820202 0.3047275 270 N 9 1 4
TOP 4 0.6820202 0.3629953 270 N 3 3 5
TOP 5 0.6623351 0.3629953 270 N 5 1 6
TOP 6 0.6426501 0.3629953 270 N 64 1 7
TOP 7 0.622965 0.3629953 270 N 11 106 8
#
# CMP 53
CMP 7 0.4703257 0.3002062 270 N C72 GRM188Z71A106MA73D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '10¦ÌF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GRM188Z71A106MA73%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GRM188Z71A106MA73D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GRM188Z71A106MA3D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '10uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '10uF'
PRP VDC_V '10V'
TOP 0 0.4703258 0.2722064 270 N 54 11 1
TOP 1 0.4703257 0.3282063 270 N 11 58 2
#
# CMP 54
CMP 22 0.274263 0.5203754 180 N L1 LQM2MPZR10MJHL ;0=1,1=0.0000
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.murata.com/en-us/products/productdetail?partno=LQM2MPZR10MJH%23'
PRP DataSheet 'https://www.murata.com/en-us/products/productdetail?partno=LQM2MPZR10MJH%23'
PRP Datasheet_Path 'datasheets/Ind-LQM2MPZR10MJHL.pdf'
PRP DCR_ohm '19m'
PRP Digikey_Description 'FIXED IND 0.1UH 4000MA INFOTMT,'
PRP Digikey_Part_Number '490-LQM2MPZR10MJHLCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/c8bba66bb0a41a16/'
PRP Ind_H '100nH'
PRP Irms '4000mA'
PRP Isat '4000mA'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Murata'
PRP Material 'Ferrite'
PRP Mouser_Part_Number '81-LQM2MPZR10MJHL'
PRP Operating_Temperature_Range '-55¡ãC to +125¡ãC'
PRP PackageReference '0806 (2016)'
PRP Part_Number 'LQM2MPZR10MJHL'
PRP PartNumber 'LQM2MPZR10MJHL'
PRP RoHS 'TRUE'
PRP Self_Resonant_Frequency '200MHz'
PRP Shrouded 'true'
PRP SizeZ_mm '1.2mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 '490-LQM2MPZR10MJHLCT-ND'
PRP Supplier_Part_Number_2 '81-LQM2MPZR10MJHL'
PRP Technology 'Multilayer'
PRP Test_Frequency '1MHz'
PRP Tolerance__ '20%'
PRP Value '0.1uH'
TOP 0 0.3057591 0.5203754 180 N 7 2 1
TOP 1 0.2427669 0.5203754 180 N 25 1 2
#
