#
#Component attribute names
#
@0 .comp_mount_type
@1 .comp_height

# CMP 0
CMP 17 0.1967846 0.5773682 270 N R7 ERJ-3GEY0R00V ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP DataSheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-3GEY0R00V.pdf'
PRP Device_Class_L1 'Passive Components'
PRP Device_Class_L2 'Resistors'
PRP Device_Class_L3 'Chip SMD Resistors'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0603'
PRP Digikey_Part_Number 'P0.0GCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/655dc946655e5dbc/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Resistor, Chip Thick Film, 0 Ohm, 0.1w, Resistor, Chip Thick Film, 0 Ohm, 0.1w, 5%'
PRP Mouser_Part_Number '667-ERJ-3GEY0R00V'
PRP Operating_Temperature_Range '-55¡ãC to +155¡ãC'
PRP PackageReference '0603'
PRP Part_Number 'ERJ-3GEY0R00V'
PRP PartNumber 'ERJ-3GEY0R00V'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.55mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0GCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-3GEY0R00V'
PRP Technology 'Thick Film'
PRP TempCo '-100/+600ppm/¡ãC'
PRP Tolerance__ '5%'
PRP VDC_V '75V'
TOP 0 0.1967846 0.5488249 270 N 62 3 1
TOP 1 0.1967846 0.6059115 270 N 28 22 2
#
# CMP 1
CMP 17 0.5029418 0.6892282 0 N R6 ERJ-3GEY0R00V ;0=1,1=0.0276
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP DataSheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-3GEY0R00V.pdf'
PRP Device_Class_L1 'Passive Components'
PRP Device_Class_L2 'Resistors'
PRP Device_Class_L3 'Chip SMD Resistors'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0603'
PRP Digikey_Part_Number 'P0.0GCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/655dc946655e5dbc/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Resistor, Chip Thick Film, 0 Ohm, 0.1w, Resistor, Chip Thick Film, 0 Ohm, 0.1w, 5%'
PRP Mouser_Part_Number '667-ERJ-3GEY0R00V'
PRP Operating_Temperature_Range '-55¡ãC to +155¡ãC'
PRP PackageReference '0603'
PRP Part_Number 'ERJ-3GEY0R00V'
PRP PartNumber 'ERJ-3GEY0R00V'
PRP Power_W '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.55mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0GCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-3GEY0R00V'
PRP Technology 'Thick Film'
PRP TempCo '-100/+600ppm/¡ãC'
PRP Tolerance__ '5%'
PRP VDC_V '75V'
TOP 0 0.5314851 0.6892282 180 N 26 2 1
TOP 1 0.4743985 0.6892282 180 N 31 24 2
#
# CMP 2
CMP 24 0.4346242 0.1989212 180 N R3 RC0402JR-070RP ;0=1,1=0.0276
PRP AEC_Qualified 'No'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.yageo.com/upload/media/product/productsearch/datasheet/rchip/PYu-RC_51_RoHS_P_2.pdf'
PRP DataSheet 'https://www.yageo.com/upload/media/product/productsearch/datasheet/rchip/PYu-RC_51_RoHS_P_2.pdf'
PRP Datasheet_Path 'datasheets/Res-RC0402JR-070RP.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/16W 0402'
PRP Digikey_Part_Number 'YAG1279CT-ND'
PRP helpURL 'https://upverter.com/upn/revision/1e1ee5977c47aafb/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Yageo'
PRP Mouser_Description 'RC Series 0402 Jumper Thick Film Chip Resistor'
PRP Mouser_Part_Number '603-RC0402JR-070RP'
PRP Operating_Temperature_Range '-55¡ãC to +155¡ãC'
PRP PackageReference '0402'
PRP Part_Number 'RC0402JR-070RP'
PRP PartNumber 'RC0402JR-070RP'
PRP Power_W '63mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'RC_P'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'YAG1279CT-ND'
PRP Supplier_Part_Number_2 '603-RC0402JR-070RP'
PRP Technology 'Thick Film'
PRP Value '0'
PRP VDC_V '50V'
TOP 0 0.4149392 0.1989212 0 N 8 5 1
TOP 1 0.4543092 0.1989212 0 N 45 2 2
#
# CMP 3
CMP 5 0.1397274 0.6424762 0 N C30 GRM155R71E103KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '10nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R71E103KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E103KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '490-1312-1-ND'
PRP Supplier_Part_Number_2 '81-GRM36X103K25'
PRP Supplier_Part_Number_3 '8819734'
PRP TaMax_C '125¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.01uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.01uF'
PRP VDC_V '25V'
TOP 0 0.1594124 0.6424762 270 N 28 21 1
TOP 1 0.1200423 0.6424762 270 N 11 146 2
#
# CMP 4
CMP 5 0.1388506 0.6052734 0 N C28 GRM155R71C224KA12D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '220nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R71C224KA12D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71C224KA12D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-5418-1-ND'
PRP Supplier_Part_Number_2 '81-GRM155R71C224KA2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.22uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '0.22uF'
PRP VDC_V '16V'
TOP 0 0.1585356 0.6052734 270 N 28 20 1
TOP 1 0.1191655 0.6052734 270 N 11 145 2
#
# CMP 5
CMP 28 0.4274298 0.0865444 90 N J1 GRPB122VWVN-RC ;0=2,1=0.1575
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL 'Y'
PRP Cert_VDE ''
PRP ClassName 'Header'
PRP CNHeader 'TRUE'
PRP Color ''
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.sullinscorp.com/catalogs/82_PAGE90-91_.050_MALE_HDR_ST_RA_SMT.pdf'
PRP CompType 'Header'
PRP ContactFinish 'Gold'
PRP CT 'FALSE'
PRP Current_A '1A'
PRP Gender 'Male'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Sullins Connector Solutions'
PRP MountType 'TH'
PRP Note ''
PRP Orientation 'Vertical'
PRP PackageReference 'Header, 1.27mm, 12x2, TH'
PRP PartNumber 'GRPB122VWVN-RC'
PRP PinCount '12'
PRP Pitch_mm '1.27'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count '2'
PRP RowSpacing_mm '1.27'
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'S9015E-12-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Voltage_V ''
TOP 0 0.1524298 0.1115444 0 N 54 21 1
TOP 1 0.1524298 0.0615444 0 N 54 22 2
TOP 2 0.2024298 0.1115444 0 N 41 4 3
TOP 3 0.2024298 0.0615444 0 N 54 23 4
TOP 4 0.2524298 0.1115444 0 N 39 1 5
TOP 5 0.2524298 0.0615444 0 N 22 1 6
TOP 6 0.3024298 0.1115444 0 N 23 1 7
TOP 7 0.3024298 0.0615444 0 N 21 1 8
TOP 8 0.3524298 0.1115444 0 N 38 2 9
TOP 9 0.3524298 0.0615444 0 N 20 1 10
TOP 10 0.4024298 0.1115444 0 N 37 2 11
TOP 11 0.4024298 0.0615444 0 N 11 152 12
TOP 12 0.4524298 0.1115444 0 N 33 1 13
TOP 13 0.4524298 0.0615444 0 N 36 1 14
TOP 14 0.5024298 0.1115444 0 N 34 1 15
TOP 15 0.5024298 0.0615444 0 N 35 1 16
TOP 16 0.5524298 0.1115444 0 N 43 2 17
TOP 17 0.5524298 0.0615444 0 N 11 151 18
TOP 18 0.6024298 0.1115444 0 N 40 1 19
TOP 19 0.6024298 0.0615444 0 N 44 2 20
TOP 20 0.6524298 0.1115444 0 N 24 1 21
TOP 21 0.6524298 0.0615444 0 N 11 150 22
TOP 22 0.7024298 0.1115444 0 N 11 148 23
TOP 23 0.7024298 0.0615444 0 N 11 149 24
#
# CMP 6
CMP 21 0.1349804 0.4990402 180 N C61 GRM31CR70J226ME19K ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP Cap_F '22¦ÌF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.murata.com/en-us/products/productdetail?partno=GRM31CR70J226ME19%23'
PRP DataSheet 'https://www.murata.com/en-us/products/productdetail?partno=GRM31CR70J226ME19%23'
PRP Datasheet_Path 'datasheets/Cap-GRM31CR70J226ME19K.pdf'
PRP helpURL 'https://upverter.com/upn/revision/24953124f7c6a3ae/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Murata'
PRP Operating_Temperature_Range '-55¡ãC to +125¡ãC'
PRP PackageReference '1206'
PRP Part_Number 'GRM31CR70J226ME19K'
PRP PartNumber 'GRM31CR70J226ME19K'
PRP RoHS 'TRUE'
PRP SizeZ_mm '1.8mm'
PRP TempCo '15%'
PRP Temperature_Characteristic 'X7R'
PRP Tolerance__ '20%'
PRP Value '22¦ÌF'
PRP ValueDisplayed '22uF'
PRP VDC_V '6.3V'
TOP 0 0.0769094 0.4990402 0 N 11 142 1
TOP 1 0.1930514 0.4990402 0 N 62 1 2
#
# CMP 7
CMP 20 0.2481134 0.6583874 0 N C27 GRM188C71C475KE21D ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP Cap_F '4.7¦ÌF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.murata.com/en-us/products/productdetail?partno=GRM188C71C475KE21%23'
PRP DataSheet 'https://www.murata.com/en-us/products/productdetail?partno=GRM188C71C475KE21%23'
PRP Datasheet_Path 'datasheets/Cap-GRM188C71C475KE21D.pdf'
PRP helpURL 'https://upverter.com/upn/revision/c0a32e76cec441a2/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Murata'
PRP Operating_Temperature_Range '-55¡ãC to +125¡ãC'
PRP PackageReference '0603'
PRP Part_Number 'GRM188C71C475KE21D'
PRP PartNumber 'GRM188C71C475KE21D'
PRP RoHS 'TRUE'
PRP SizeZ_mm '1mm'
PRP TempCo '22%'
PRP Temperature_Characteristic 'X7S'
PRP Tolerance__ '10%'
PRP Value '4.7¦ÌF'
PRP ValueDisplayed '4.7uF'
PRP VDC_V '16V'
TOP 0 0.2786252 0.6583874 180 N 11 141 1
TOP 1 0.2176016 0.6583874 180 N 28 19 2
#
# CMP 8
CMP 24 0.1849252 0.40636 270 N R119 RC0402JR-070RP ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.yageo.com/upload/media/product/productsearch/datasheet/rchip/PYu-RC_51_RoHS_P_2.pdf'
PRP DataSheet 'https://www.yageo.com/upload/media/product/productsearch/datasheet/rchip/PYu-RC_51_RoHS_P_2.pdf'
PRP Datasheet_Path 'datasheets/Res-RC0402JR-070RP.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/16W 0402'
PRP Digikey_Part_Number 'YAG1279CT-ND'
PRP helpURL 'https://upverter.com/upn/revision/1e1ee5977c47aafb/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Yageo'
PRP Mouser_Description 'RC Series 0402 Jumper Thick Film Chip Resistor'
PRP Mouser_Part_Number '603-RC0402JR-070RP'
PRP Operating_Temperature_Range '-55¡ãC to +155¡ãC'
PRP PackageReference '0402'
PRP Part_Number 'RC0402JR-070RP'
PRP PartNumber 'RC0402JR-070RP'
PRP Power_W '63mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'RC_P'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'YAG1279CT-ND'
PRP Supplier_Part_Number_2 '603-RC0402JR-070RP'
PRP Technology 'Thick Film'
PRP Value '0'
PRP VDC_V '50V'
TOP 0 0.1849252 0.386675 270 N 4 2 1
TOP 1 0.1849252 0.426045 270 N 7 7 2
#
# CMP 9
CMP 15 0.2718294 0.4051375 270 N L14 DFE201210U-R47M=P2 ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.murata.com/en-us/products/productdetail?partno=DFE201210U-R47M%23'
PRP DataSheet 'https://www.murata.com/en-us/products/productdetail?partno=DFE201210U-R47M%23'
PRP Datasheet_Path 'datasheets/Ind-DFE201210U-R47M=P2.pdf'
PRP DCR_ohm '42m'
PRP Digikey_Description 'FIXED IND .47UH 3.0A 42MOHM'
PRP Digikey_Part_Number '490-17727-1-ND'
PRP helpURL 'https://upverter.com/upn/revision/7b65c208f048e6ea/'
PRP Ind_H '470nH'
PRP Irms '3A'
PRP Isat '4.4A'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Murata'
PRP Material 'Metal Alloy'
PRP Mouser_Part_Number '81-DFE201210U-R47MP2'
PRP Operating_Temperature_Range '-40¡ãC to +125¡ãC'
PRP PackageReference '0805 (2012)'
PRP Part_Number 'DFE201210U-R47M=P2'
PRP PartNumber 'DFE201210U-R47M=P2'
PRP RoHS 'TRUE'
PRP Shrouded 'true'
PRP SizeZ_mm '1mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 '490-17727-1-ND'
PRP Supplier_Part_Number_2 '81-DFE201210U-R47MP2'
PRP Technology 'Wirewound'
PRP Test_Frequency '1MHz'
PRP Tolerance__ '20%'
PRP Value '0.47uH'
TOP 0 0.2718294 0.3736414 270 N 63 0 1
TOP 1 0.2718295 0.4366336 270 N 7 6 2
#
# CMP 10
CMP 0 0.0583332 0.6924666 270 N R89 CRCW02011K00FKED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02011K00FKED'
PRP Power_W '50mW'
PRP Res_ohm '1k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '541-1.00KAABCT-ND'
PRP Supplier_Part_Number_2 '71-CRCW02011K00FKED'
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '1.00k'
PRP Value1 '1%'
PRP Value2 '0.05W'
PRP Value_Code '1k00'
PRP ValueDisplayed '1.00k'
PRP VDC_V '30V'
TOP 0 0.0583332 0.6794745 0 N 56 1 1
TOP 1 0.0583332 0.7054587 0 N 57 2 2
#
# CMP 11
CMP 5 0.0346606 0.9667988 90 N C101 GRM155R71C224KA12D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '220nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R71C224KA12D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71C224KA12D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-5418-1-ND'
PRP Supplier_Part_Number_2 '81-GRM155R71C224KA2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.22uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '0.22uF'
PRP VDC_V '16V'
TOP 0 0.0346606 0.9864838 180 N 27 7 1
TOP 1 0.0346606 0.9471137 180 N 11 109 2
#
# CMP 12
CMP 5 0.2219966 0.3072862 270 N R121 RC0402FR-0768K1L ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.yageo.com/documents/recent/PYu-RC_Group_51_RoHS_L_8.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Yageo America'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'RC0402FR-0768K1L'
PRP Power_W '63mW'
PRP Res_ohm '68.1k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'YAG3213CT-ND'
PRP Supplier_Part_Number_2 '66R1635'
PRP Supplier_Part_Number_3 '603-RC0402FR-0768K1L'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '68.1k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '68k1'
PRP ValueDisplayed '68.1k'
PRP VDC_V '50V'
TOP 0 0.2219966 0.2876012 0 N 11 110 1
TOP 1 0.2219966 0.3269713 0 N 4 0 2
#
# CMP 13
CMP 5 0.1307542 0.4063602 90 N C100 GRM1555C1H100JA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '10pF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM1555C1H100JA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM1555C1H100JA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GRM1555C1H100JA1D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'C0G/NP0'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '10pF'
PRP Value1 'Unknown'
PRP Value2 '50V'
PRP ValueDisplayed '10pF'
PRP VDC_V '50V'
TOP 0 0.1307542 0.4260452 180 N 7 3 1
TOP 1 0.1307542 0.3866751 180 N 4 1 2
#
# CMP 14
CMP 18 0.465777 1.0554126 0 N Y1 FW4000044Q ;0=1,1=0.0000
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.diodes.com/assets/Datasheets/FW.pdf'
PRP DataSheet 'https://www.diodes.com/assets/Datasheets/FW.pdf'
PRP Datasheet_Path 'datasheets/Crys-FW4000044Q.pdf'
PRP Digikey_Description 'CRYSTAL CERAMIC SEAM2016R 3K'
PRP Digikey_Part_Number 'FW4000044QDICT-ND'
PRP ESR '50'
PRP Frequency_Stability '50ppm'
PRP Frequency_Tolerance '10ppm'
PRP Frequency_Fixed '40MHz'
PRP helpURL 'https://upverter.com/upn/revision/d451487a111b898c/'
PRP Lead_Free 'Yes'
PRP Load_Capacitance '8pF'
PRP Manufacturer 'Diodes'
PRP Mouser_Part_Number '729-FW4000044Q'
PRP Operating_Temperature_Range '-40¡ãC to +125¡ãC'
PRP PackageReference '4-SMD-2.0x1.6mm'
PRP Part_Number 'FW4000044Q'
PRP PartNumber 'FW4000044Q'
PRP RoHS 'TRUE'
PRP Series 'FW'
PRP SizeZ_mm '0.55mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'FW4000044QDICT-ND'
PRP Supplier_Part_Number_2 '729-FW4000044Q'
PRP Tolerance__ '10ppm'
TOP 0 0.4933361 1.0337591 180 N 55 2 1
TOP 1 0.4382179 1.0337591 180 N 11 139 2
TOP 2 0.4382179 1.0770661 180 N 53 2 3
TOP 3 0.4933361 1.0770661 180 N 11 140 4
#
# CMP 15
CMP 16 0.0779832 0.6558866 0 N R131 ERJ-1RHD1002C ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP DataSheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-1RHD1002C.pdf'
PRP Digikey_Description 'RES SMD 10K OHM 0.5% 1/20W 0201'
PRP Digikey_Part_Number 'P15980CT-ND'
PRP helpURL 'https://upverter.com/upn/revision/1ca8f4053101326f/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Current Sense Resistors 0201 10Kohms 0.5% Tolerance'
PRP Mouser_Part_Number '667-ERJ-1RHD1002C'
PRP Operating_Temperature_Range '-55¡ãC to +125¡ãC'
PRP PackageReference '0201'
PRP Part_Number 'ERJ-1RHD1002C'
PRP PartNumber 'ERJ-1RHD1002C'
PRP Power_W '50mW'
PRP Res_ohm '10k'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.26mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P15980CT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-1RHD1002C'
PRP Technology 'Thick Film'
PRP TempCo '50ppm/¡ãC'
PRP Tolerance__ '0.5%'
PRP Value '10k'
PRP VDC_V '15V'
TOP 0 0.0897942 0.6558866 180 N 11 138 1
TOP 1 0.0661722 0.6558866 180 N 56 2 2
#
# CMP 16
CMP 4 0.8023924 0.4286066 90 N R75 CRCW04022M00FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022M00FKED'
PRP Power_W '63mW'
PRP Res_ohm '2M'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.00MLCT-ND'
PRP Supplier_Part_Number_2 '52K6816'
PRP Supplier_Part_Number_3 '71-CRCW0402-2M-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.00Meg'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2M00'
PRP ValueDisplayed '2.00M'
PRP VDC_V '50V'
TOP 0 0.8023924 0.4522286 180 N 32 23 1
TOP 1 0.8023924 0.4049845 180 N 44 1 2
#
# CMP 17
CMP 16 0.0950876 0.6825686 180 N R67 ERJ-1RHD1002C ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP DataSheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-1RHD1002C.pdf'
PRP Digikey_Description 'RES SMD 10K OHM 0.5% 1/20W 0201'
PRP Digikey_Part_Number 'P15980CT-ND'
PRP helpURL 'https://upverter.com/upn/revision/1ca8f4053101326f/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Current Sense Resistors 0201 10Kohms 0.5% Tolerance'
PRP Mouser_Part_Number '667-ERJ-1RHD1002C'
PRP Operating_Temperature_Range '-55¡ãC to +125¡ãC'
PRP PackageReference '0201'
PRP Part_Number 'ERJ-1RHD1002C'
PRP PartNumber 'ERJ-1RHD1002C'
PRP Power_W '50mW'
PRP Res_ohm '10k'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.26mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P15980CT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-1RHD1002C'
PRP Technology 'Thick Film'
PRP TempCo '50ppm/¡ãC'
PRP Tolerance__ '0.5%'
PRP Value '10k'
PRP VDC_V '15V'
TOP 0 0.0832766 0.6825686 0 N 56 0 1
TOP 1 0.1068986 0.6825686 0 N 31 14 2
#
# CMP 18
CMP 4 0.6512588 0.195926 0 N R4 CRCW04022M00FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022M00FKED'
PRP Power_W '63mW'
PRP Res_ohm '2M'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.00MLCT-ND'
PRP Supplier_Part_Number_2 '52K6816'
PRP Supplier_Part_Number_3 '71-CRCW0402-2M-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.00Meg'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2M00'
PRP ValueDisplayed '2.00M'
PRP VDC_V '50V'
TOP 0 0.6748808 0.195926 270 N 32 22 1
TOP 1 0.6276367 0.195926 270 N 43 1 2
#
# CMP 19
CMP 12 0.797686 0.058548 270 N FID5 Fiducial ;0=1,1=0.0236
PRP ClassName 'FiducialMark'
PRP CompType 'Fiducial'
PRP Manufacturer 'N/A'
PRP MountType 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 0.797686 0.058548 270 N 0 3 1
#
# CMP 20
CMP 12 0.8023924 0.7857282 270 N FID3 Fiducial ;0=1,1=0.0236
PRP ClassName 'FiducialMark'
PRP CompType 'Fiducial'
PRP Manufacturer 'N/A'
PRP MountType 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 0.8023924 0.7857282 270 N 0 4 1
#
# CMP 21
CMP 12 0.0553398 0.056655 270 N FID2 Fiducial ;0=1,1=0.0236
PRP ClassName 'FiducialMark'
PRP CompType 'Fiducial'
PRP Manufacturer 'N/A'
PRP MountType 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 0.0553398 0.056655 270 N 0 5 1
#
# CMP 22
CMP 5 0.5364836 1.0556418 90 N C33 GJM1555C1H4R7BB01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '4.7pF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.murata.com/capacitor/product/GJM1555C1H4R7BB01%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GJM1555C1H4R7BB01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-8102-1-ND'
PRP Supplier_Part_Number_2 '81-GJM1555C1H4R7BB01'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'C0G/NP0'
PRP Tolerance__ '2%'
PRP U/M 'EA'
PRP Value '4.7pF'
PRP Value1 'Unknown'
PRP Value2 '50V'
PRP ValueDisplayed '4.7pF'
PRP VDC_V '50V'
TOP 0 0.5364836 1.0753268 180 N 11 111 1
TOP 1 0.5364836 1.0359567 180 N 55 1 2
#
# CMP 23
CMP 5 0.4758102 1.1232042 0 N C32 GJM1555C1H4R7BB01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '4.7pF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.murata.com/capacitor/product/GJM1555C1H4R7BB01%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GJM1555C1H4R7BB01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-8102-1-ND'
PRP Supplier_Part_Number_2 '81-GJM1555C1H4R7BB01'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'C0G/NP0'
PRP Tolerance__ '2%'
PRP U/M 'EA'
PRP Value '4.7pF'
PRP Value1 'Unknown'
PRP Value2 '50V'
PRP ValueDisplayed '4.7pF'
PRP VDC_V '50V'
TOP 0 0.4954952 1.1232042 270 N 11 112 1
TOP 1 0.4561252 1.1232042 270 N 53 1 2
#
# CMP 24
CMP 5 0.2408607 0.8320286 180 N C29 GRM155R71C224KA12D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '220nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R71C224KA12D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71C224KA12D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-5418-1-ND'
PRP Supplier_Part_Number_2 '81-GRM155R71C224KA2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.22uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '0.22uF'
PRP VDC_V '16V'
TOP 0 0.2211757 0.8320286 90 N 28 17 1
TOP 1 0.2605458 0.8320286 90 N 11 113 2
#
# CMP 25
CMP 6 0.2149306 0.9118854 270 N C22 GRM155R70J105KA12D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '1¦ÌF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R70J105KA12-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-06-05'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J105KA12D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '490-10024-1-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J105KA2D'
PRP Supplier_Part_Number_3 '2688505RL'
PRP TaMax_C '125¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '1uF'
PRP VDC_V '6.3V'
TOP 0 0.2149306 0.8918854 0 N 29 1 1
TOP 1 0.2149306 0.9318854 0 N 11 137 2
#
# CMP 26
CMP 19 0.0853258 0.971735 0 N C20 GRM155R61A225ME01D ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP Cap_F '2.2¦ÌF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.murata.com/en-us/products/productdetail?partno=GRM155R61A225ME01%23'
PRP DataSheet 'https://www.murata.com/en-us/products/productdetail?partno=GRM155R61A225ME01%23'
PRP Datasheet_Path 'datasheets/Cap-GRM155R61A225ME01D.pdf'
PRP helpURL 'https://upverter.com/upn/revision/9c1060debce10243/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Murata'
PRP Operating_Temperature_Range '-55¡ãC to +85¡ãC'
PRP PackageReference '0402'
PRP Part_Number 'GRM155R61A225ME01D'
PRP PartNumber 'GRM155R61A225ME01D'
PRP RoHS 'TRUE'
PRP SizeZ_mm '0.55mm'
PRP TempCo '15%'
PRP Temperature_Characteristic 'X5R'
PRP Tolerance__ '20%'
PRP Value '2.2¦ÌF'
PRP ValueDisplayed '2.2uF'
PRP VDC_V '10V'
TOP 0 0.1010738 0.971735 180 N 11 114 1
TOP 1 0.0695778 0.971735 180 N 27 8 2
#
# CMP 27
CMP 6 0.3067432 0.9018098 90 N C18 GRM155R70J105KA12D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '1¦ÌF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R70J105KA12-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-06-05'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R70J105KA12D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '490-10024-1-ND'
PRP Supplier_Part_Number_2 '81-GRM155R70J105KA2D'
PRP Supplier_Part_Number_3 '2688505RL'
PRP TaMax_C '125¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '1uF'
PRP VDC_V '6.3V'
TOP 0 0.3067432 0.9218098 180 N 30 1 1
TOP 1 0.3067432 0.8818098 180 N 11 115 2
#
# CMP 28
CMP 8 0.5027798 0.7610406 180 N C15 GRM188Z71A106MA73D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '10¦ÌF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GRM188Z71A106MA73%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GRM188Z71A106MA73D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GRM188Z71A106MA3D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '10uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '10uF'
PRP VDC_V '10V'
TOP 0 0.4752207 0.7610406 90 N 31 15 1
TOP 1 0.5303388 0.7610406 90 N 11 116 2
#
# CMP 29
CMP 5 0.3493392 0.8461674 180 N C14 GRM155R71C224KA12D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '220nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R71C224KA12D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71C224KA12D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-5418-1-ND'
PRP Supplier_Part_Number_2 '81-GRM155R71C224KA2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.22uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '0.22uF'
PRP VDC_V '16V'
TOP 0 0.3296542 0.8461674 90 N 31 16 1
TOP 1 0.3690243 0.8461674 90 N 11 117 2
#
# CMP 30
CMP 5 0.0928908 0.7887249 90 N C12 GRM155R71C224KA12D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '220nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R71C224KA12D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71C224KA12D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-5418-1-ND'
PRP Supplier_Part_Number_2 '81-GRM155R71C224KA2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.22uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '0.22uF'
PRP VDC_V '16V'
TOP 0 0.0928908 0.8084099 180 N 31 17 1
TOP 1 0.0928908 0.7690398 180 N 11 118 2
#
# CMP 31
CMP 5 0.124417 0.7916305 90 N C11 GRM155R71C224KA12D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '220nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R71C224KA12D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71C224KA12D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-5418-1-ND'
PRP Supplier_Part_Number_2 '81-GRM155R71C224KA2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.22uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '0.22uF'
PRP VDC_V '16V'
TOP 0 0.124417 0.8113155 180 N 31 18 1
TOP 1 0.124417 0.7719454 180 N 11 119 2
#
# CMP 32
CMP 5 0.5022676 0.798905 180 N C10 GRM155R71C224KA12D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '220nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R71C224KA12D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71C224KA12D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-5418-1-ND'
PRP Supplier_Part_Number_2 '81-GRM155R71C224KA2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.22uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '0.22uF'
PRP VDC_V '16V'
TOP 0 0.4825826 0.798905 90 N 31 19 1
TOP 1 0.5219527 0.798905 90 N 11 120 2
#
# CMP 33
CMP 5 0.1385718 0.8721686 270 N C6 C1005X7R1H473K050BB ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '47nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=C1005X7R1H473K050BB'
PRP CompType 'Capacitor'
PRP ESR_ohm '0.06407'
PRP IRMS_A '6.46122dA'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'C1005X7R1H473K050BB'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '445-7336-1-ND'
PRP Supplier_Part_Number_2 '04X3233'
PRP Supplier_Part_Number_3 '810-C1005X7R1H473K'
PRP TaMax_C '125¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.047uF'
PRP Value1 '0.06407 ohm'
PRP Value2 '50V'
PRP ValueDisplayed '0.047uF'
PRP VDC_V '50V'
TOP 0 0.1385718 0.8524836 0 N 46 1 1
TOP 1 0.1385718 0.8918537 0 N 11 121 2
#
# CMP 34
CMP 5 0.2575896 0.8918576 90 N C5 GRM155R71C224KA12D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '220nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R71C224KA12D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71C224KA12D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-5418-1-ND'
PRP Supplier_Part_Number_2 '81-GRM155R71C224KA2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.22uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '0.22uF'
PRP VDC_V '16V'
TOP 0 0.2575896 0.9115426 180 N 31 20 1
TOP 1 0.2575896 0.8721725 180 N 11 122 2
#
# CMP 35
CMP 27 0.7749703 0.2077469 90 N Q2 BSS123W-7-F ;0=1,1=0.0433
PRP AEC_Category 'Q101'
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer 'None'
PRP Alternate_PartNumber ''
PRP ChType 'N'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.diodes.com/datasheets/ds30368.pdf'
PRP CompType 'MOSFET'
PRP IdsMax_A '170mA'
PRP LatestRevisionDate '2017-03-09'
PRP LatestRevisionNote 'Added parts.'
PRP Manufacturer 'Diodes Inc.'
PRP MountType 'SMT'
PRP PackageReference 'SOT-323'
PRP PartNumber 'BSS123W-7-F'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP QgTyp_nC ''
PRP Rdson45_ohm '10'
PRP RoHS 'Y'
PRP SizeArea_mm2 '4.84'
PRP SizeAreaWB_mm2 '10.24'
PRP SizeX_mm '2.2'
PRP SizeY_mm '2.2'
PRP SizeZ_mm '1.1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'BSS123W-FDICT-ND'
PRP Supplier_Part_Number_2 '621-BSS123W-F'
PRP Supplier_Part_Number_3 ''
PRP U/M 'EA'
PRP Value '100V'
PRP Value1 '1'
PRP Value2 ''
PRP Vault_Folder ''
PRP VdsMax_V '100V'
PRP Vgs_V '20V'
TOP 0 0.7493798 0.2451486 0 N 59 0 1
TOP 1 0.8005609 0.2451486 0 N 11 123 2
TOP 2 0.7749704 0.1703455 0 N 12 1 3
#
# CMP 36
CMP 5 0.7492492 0.3072862 270 N R179 ERJ-2RKF5100X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF5100X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '510'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P510LCT-ND'
PRP Supplier_Part_Number_2 '53W4394'
PRP Supplier_Part_Number_3 '667-ERJ-2RKF5100X'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '510'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '510R'
PRP ValueDisplayed '510'
PRP VDC_V '50V'
TOP 0 0.7492492 0.2876012 0 N 59 1 1
TOP 1 0.7492492 0.3269713 0 N 5 3 2
#
# CMP 37
CMP 1 0.1000084 0.7251551 270 N C78 GRM033R60J105MEA2D ;0=1,1=0.0130
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0201'
PRP Cap_F '1¦ÌF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM033R60J105MEA2-02.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'GRM033R60J105MEA2D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.18'
PRP SizeAreaWB_mm2 '2.08'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.33'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-7229-1-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '85¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'X5R'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '1uF'
PRP VDC_V '6.3V'
TOP 0 0.1000084 0.712163 0 N 57 1 1
TOP 1 0.1000084 0.7381472 0 N 11 124 2
#
# CMP 38
CMP 5 0.1597232 0.9171758 0 N C4 GRM155R71C224KA12D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '220nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R71C224KA12D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71C224KA12D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-5418-1-ND'
PRP Supplier_Part_Number_2 '81-GRM155R71C224KA2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.22uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '0.22uF'
PRP VDC_V '16V'
TOP 0 0.1794082 0.9171758 270 N 31 21 1
TOP 1 0.1400381 0.9171758 270 N 11 125 2
#
# CMP 39
CMP 5 0.3181402 0.6639357 90 N C7 GRM155R71C224KA12D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '220nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R71C224KA12D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71C224KA12D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-5418-1-ND'
PRP Supplier_Part_Number_2 '81-GRM155R71C224KA2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.22uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '0.22uF'
PRP VDC_V '16V'
TOP 0 0.3181402 0.6836207 180 N 31 22 1
TOP 1 0.3181402 0.6442506 180 N 11 126 2
#
# CMP 40
CMP 5 0.1550472 0.7915194 90 N C8 GRM155R71C224KA12D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '220nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R71C224KA12D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71C224KA12D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-5418-1-ND'
PRP Supplier_Part_Number_2 '81-GRM155R71C224KA2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.22uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '0.22uF'
PRP VDC_V '16V'
TOP 0 0.1550472 0.8112044 180 N 31 23 1
TOP 1 0.1550472 0.7718343 180 N 11 127 2
#
# CMP 41
CMP 20 0.0552232 0.833971 270 N C24 GRM188C71C475KE21D ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP Cap_F '4.7¦ÌF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.murata.com/en-us/products/productdetail?partno=GRM188C71C475KE21%23'
PRP DataSheet 'https://www.murata.com/en-us/products/productdetail?partno=GRM188C71C475KE21%23'
PRP Datasheet_Path 'datasheets/Cap-GRM188C71C475KE21D.pdf'
PRP helpURL 'https://upverter.com/upn/revision/c0a32e76cec441a2/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Murata'
PRP Operating_Temperature_Range '-55¡ãC to +125¡ãC'
PRP PackageReference '0603'
PRP Part_Number 'GRM188C71C475KE21D'
PRP PartNumber 'GRM188C71C475KE21D'
PRP RoHS 'TRUE'
PRP SizeZ_mm '1mm'
PRP TempCo '22%'
PRP Temperature_Characteristic 'X7S'
PRP Tolerance__ '10%'
PRP Value '4.7¦ÌF'
PRP ValueDisplayed '4.7uF'
PRP VDC_V '16V'
TOP 0 0.0552232 0.8034592 270 N 11 128 1
TOP 1 0.0552232 0.8644828 270 N 27 9 2
#
# CMP 42
CMP 5 0.243265 0.7630582 180 N C45 GRM155R71E103KA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '10nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R71E103KA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E103KA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '490-1312-1-ND'
PRP Supplier_Part_Number_2 '81-GRM36X103K25'
PRP Supplier_Part_Number_3 '8819734'
PRP TaMax_C '125¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.01uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.01uF'
PRP VDC_V '25V'
TOP 0 0.22358 0.7630582 90 N 28 18 1
TOP 1 0.2629501 0.7630582 90 N 11 129 2
#
# CMP 43
CMP 8 0.044645 1.0511338 270 N C44 GRM188Z71A106MA73D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '10¦ÌF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GRM188Z71A106MA73%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GRM188Z71A106MA73D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GRM188Z71A106MA3D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '10uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '10uF'
PRP VDC_V '10V'
TOP 0 0.044645 1.0235747 0 N 27 10 1
TOP 1 0.044645 1.0786928 0 N 11 130 2
#
# CMP 44
CMP 4 0.3376328 0.1972346 0 N R238 RC0402FR-071ML ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.yageo.com/NewPortal/yageodocoutput?fileName=/pdf/R-Chip/PYu-RC_Group_51_RoHS_L_0.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Yageo America'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'RC0402FR-071ML'
PRP Power_W '63mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '1M'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '311-1.00MLRCT-ND'
PRP Supplier_Part_Number_2 '66R1086'
PRP Supplier_Part_Number_3 '603-RC0402FR-071ML'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '1.00Meg'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '1M00'
PRP ValueDisplayed '1.00M'
PRP VDC_V ''
TOP 0 0.3612548 0.1972346 270 N 11 143 1
TOP 1 0.3140107 0.1972346 270 N 8 3 2
#
# CMP 45
CMP 8 0.3527342 0.4034222 90 N C119 GRM188Z71A106MA73D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '10¦ÌF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GRM188Z71A106MA73%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GRM188Z71A106MA73D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GRM188Z71A106MA3D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '10uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '10uF'
PRP VDC_V '10V'
TOP 0 0.3527342 0.4309813 180 N 7 4 1
TOP 1 0.3527342 0.3758632 180 N 11 131 2
#
# CMP 46
CMP 22 0.2810996 0.514749 0 N L5 LQM2MPZR10MJHL ;0=1,1=0.0000
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.murata.com/en-us/products/productdetail?partno=LQM2MPZR10MJH%23'
PRP DataSheet 'https://www.murata.com/en-us/products/productdetail?partno=LQM2MPZR10MJH%23'
PRP Datasheet_Path 'datasheets/Ind-LQM2MPZR10MJHL.pdf'
PRP DCR_ohm '19m'
PRP Digikey_Description 'FIXED IND 0.1UH 4000MA INFOTMT,'
PRP Digikey_Part_Number '490-LQM2MPZR10MJHLCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/c8bba66bb0a41a16/'
PRP Ind_H '100nH'
PRP Irms '4000mA'
PRP Isat '4000mA'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Murata'
PRP Material 'Ferrite'
PRP Mouser_Part_Number '81-LQM2MPZR10MJHL'
PRP Operating_Temperature_Range '-55¡ãC to +125¡ãC'
PRP PackageReference '0806 (2016)'
PRP Part_Number 'LQM2MPZR10MJHL'
PRP PartNumber 'LQM2MPZR10MJHL'
PRP RoHS 'TRUE'
PRP Self_Resonant_Frequency '200MHz'
PRP Shrouded 'true'
PRP SizeZ_mm '1.2mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 '490-LQM2MPZR10MJHLCT-ND'
PRP Supplier_Part_Number_2 '81-LQM2MPZR10MJHL'
PRP Technology 'Multilayer'
PRP Test_Frequency '1MHz'
PRP Tolerance__ '20%'
PRP Value '0.1uH'
TOP 0 0.3125957 0.514749 180 N 7 8 1
TOP 1 0.2496035 0.514749 180 N 62 2 2
#
# CMP 47
CMP 8 0.4166878 0.4033002 90 N C120 GRM188Z71A106MA73D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '10¦ÌF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GRM188Z71A106MA73%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GRM188Z71A106MA73D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GRM188Z71A106MA3D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '10uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '10uF'
PRP VDC_V '10V'
TOP 0 0.4166878 0.4308593 180 N 7 5 1
TOP 1 0.4166878 0.3757412 180 N 11 132 2
#
# CMP 48
CMP 14 0.2208058 0.2381129 270 N R178 CRCW040218K0FKEDC ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.vishay.com/docs/28773/crcwce3.pdf'
PRP DataSheet 'https://www.vishay.com/docs/28773/crcwce3.pdf'
PRP Datasheet_Path 'datasheets/Res-CRCW040218K0FKEDC.pdf'
PRP Digikey_Description 'RES 18K OHM 1% 1/16W 0402'
PRP Digikey_Part_Number '541-4757-1-ND'
PRP helpURL 'https://upverter.com/upn/revision/f5433614e467177c/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Vishay'
PRP Mouser_Description 'Res Thick Film 0402 18K Ohm 1% 1/16W ¡À100ppm/¡ãC Molded SMD Paper T/R'
PRP Mouser_Part_Number '71-CRCW040218K0FKEDC'
PRP Operating_Temperature_Range '-55¡ãC to +155¡ãC'
PRP PackageReference '0402'
PRP Part_Number 'CRCW040218K0FKEDC'
PRP PartNumber 'CRCW040218K0FKEDC'
PRP Power_W '63mW'
PRP Res_ohm '18k'
PRP RoHS 'TRUE'
PRP Series 'CRCW-C e3'
PRP SizeZ_mm '0.35mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 '541-4757-1-ND'
PRP Supplier_Part_Number_2 '71-CRCW040218K0FKEDC'
PRP Technology 'Thick Film'
PRP TempCo '100ppm/¡ãC'
PRP Tolerance__ '1%'
PRP Value '18k'
PRP VDC_V '50V'
TOP 0 0.2208058 0.2203964 270 N 10 0 1
TOP 1 0.2208058 0.2558294 270 N 11 133 2
#
# CMP 49
CMP 7 0.4695283 0.2810942 270 N C62 GRM188Z71A106MA73D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '10¦ÌF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GRM188Z71A106MA73%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GRM188Z71A106MA73D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GRM188Z71A106MA3D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '10uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '10uF'
PRP VDC_V '10V'
TOP 0 0.4695283 0.2530943 270 N 54 16 1
TOP 1 0.4695283 0.3090943 270 N 11 134 2
#
# CMP 50
CMP 8 0.4174532 0.2858322 270 N C66 GRM188R71C474KA88D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '470nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM188R71C474KA88D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GRM188R71C474KA88D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '490-3295-1-ND'
PRP Supplier_Part_Number_2 '81-GRM188R71C474KA88'
PRP Supplier_Part_Number_3 '1828893'
PRP TaMax_C '125¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.47uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '0.47uF'
PRP VDC_V '16V'
TOP 0 0.4174532 0.2582731 0 N 54 17 1
TOP 1 0.4174532 0.3133912 0 N 11 135 2
#
# CMP 51
CMP 9 0.6773212 0.5675691 0 N C68 GRM31CR60J476ME19L ;0=1,1=0.0709
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '1206'
PRP Cap_F '47¦ÌF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.murata.com/products/catalog/pdf/c02e.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm '3m'
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '1206'
PRP PartNumber 'GRM31CR60J476ME19L'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '5.12'
PRP SizeAreaWB_mm2 '10.92'
PRP SizeX_mm '3.2'
PRP SizeY_mm '1.6'
PRP SizeZ_mm '1.8'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '490-3907-1-ND'
PRP Supplier_Part_Number_2 '81-GRM426X476M6.3L'
PRP Supplier_Part_Number_3 '1735534'
PRP TaMax_C '85¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'X5R'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP Value '47uF'
PRP Value1 '0.003 ohm'
PRP Value2 '6.3V'
PRP ValueDisplayed '47uF'
PRP VDC_V '6.3V'
TOP 0 0.7442503 0.567569 270 N 11 147 1
TOP 1 0.6103924 0.567569 270 N 26 3 2
#
# CMP 52
CMP 22 0.5184136 0.5893286 270 N L6 LQM2MPZR10MJHL ;0=1,1=0.0000
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.murata.com/en-us/products/productdetail?partno=LQM2MPZR10MJH%23'
PRP DataSheet 'https://www.murata.com/en-us/products/productdetail?partno=LQM2MPZR10MJH%23'
PRP Datasheet_Path 'datasheets/Ind-LQM2MPZR10MJHL.pdf'
PRP DCR_ohm '19m'
PRP Digikey_Description 'FIXED IND 0.1UH 4000MA INFOTMT,'
PRP Digikey_Part_Number '490-LQM2MPZR10MJHLCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/c8bba66bb0a41a16/'
PRP Ind_H '100nH'
PRP Irms '4000mA'
PRP Isat '4000mA'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Murata'
PRP Material 'Ferrite'
PRP Mouser_Part_Number '81-LQM2MPZR10MJHL'
PRP Operating_Temperature_Range '-55¡ãC to +125¡ãC'
PRP PackageReference '0806 (2016)'
PRP Part_Number 'LQM2MPZR10MJHL'
PRP PartNumber 'LQM2MPZR10MJHL'
PRP RoHS 'TRUE'
PRP Self_Resonant_Frequency '200MHz'
PRP Shrouded 'true'
PRP SizeZ_mm '1.2mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 '490-LQM2MPZR10MJHLCT-ND'
PRP Supplier_Part_Number_2 '81-LQM2MPZR10MJHL'
PRP Technology 'Multilayer'
PRP Test_Frequency '1MHz'
PRP Tolerance__ '20%'
PRP Value '0.1uH'
TOP 0 0.5184136 0.5578325 270 N 6 7 1
TOP 1 0.5184136 0.6208247 270 N 26 1 2
#
# CMP 53
CMP 5 0.3699146 0.291708 270 N C67 GRM1555C1H471JA01D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '470pF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM1555C1H471JA01D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM1555C1H471JA01D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '490-1297-1-ND'
PRP Supplier_Part_Number_2 '81-GRM1555C1H471JA01'
PRP Supplier_Part_Number_3 '8819688'
PRP TaMax_C '125¡ãC'
PRP TaMin_C '-55¡ãC'
PRP Technology 'Ceramic'
PRP TempCo 'C0G/NP0'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '470pF'
PRP Value1 'Unknown'
PRP Value2 '50V'
PRP ValueDisplayed '470pF'
PRP VDC_V '50V'
TOP 0 0.3699146 0.272023 0 N 54 18 1
TOP 1 0.3699147 0.3113931 0 N 11 136 2
#
# CMP 54
CMP 11 0.2989963 0.2901633 270 N U19 TPS6285020ADRLR ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP Datasheet_Path 'datasheets/IC-TPS6285020ADRLR.pdf'
PRP helpURL 'https://upverter.com/upn/revision/f1b92653d69054c4/'
PRP Manufacturer 'Texas Instruments'
PRP Max_Duty_Cycle '100%'
PRP Max_Supply_Voltage '6V'
PRP Min_Supply_Voltage '2.7V'
PRP Nominal_Supply_Current '17uA'
PRP Number_Of_Outputs '1'
PRP Operating_Temperature_Range '-40¡ãC to +150¡ãC'
PRP Output_Type 'AdjustableProgrammable'
PRP Output_Voltage '0.6-5.5V'
PRP PackageReference 'SOT583'
PRP Part_Number 'TPS6285020ADRLR'
PRP PartNumber 'TPS6285020ADRLR'
PRP RoHS 'UNKNOWN'
PRP SizeZ_mm '0.6mm'
PRP Standoff_Height '0mm'
PRP Switching_Frequency '1.8-4MHz'
PRP Switching_Topology 'Buck'
PRP TJmax_C '+150¡ãC'
TOP 0 0.3285239 0.2610294 270 N 54 19 1
TOP 1 0.3088388 0.2610294 270 N 54 20 2
TOP 2 0.2891538 0.2610294 270 N 8 4 3
TOP 3 0.2694687 0.2610294 270 N 10 1 4
TOP 4 0.2694687 0.3192972 270 N 4 3 5
TOP 5 0.2891538 0.3192972 270 N 5 4 6
TOP 6 0.3088388 0.3192972 270 N 63 1 7
TOP 7 0.3285239 0.3192972 270 N 11 144 8
#
