Field=Fitted~String~Fitted~100|Field=Description~String~Description~100|Field=Designator~String~Designator~100|Field=PartNumber~String~PartNumber~100|Field=Manufacturer~String~Manufacturer~100|Field=Quantity~Integer~Quantity~100|Field=Supplier Part Number 1~String~Supplier Part Number 1~100|Field=Supplier 1~String~Supplier 1~100|ReportField=Currency~<none>|ReportField=ProductionQuantity~1|ReportField=ProjectFileName~MCCB_OPAMP.PrjPCB|ReportField=ProjectFullPath~D:\MCCB_OPAMP\WORK\MCCB_OPAMP_13_01_2014_AFTRBACKANN\MCCB_OPAMP.PrjPCB|ReportField=Title~BOM For Variant [001] of Project [MCCB_OPAMP.PrjPCB] (No PCB Document Selected)|ReportField=TotalQuantity~226|ReportField=ReportTime~7:42:52 PM|ReportField=ReportDate~1/15/2014|ReportField=ReportDateTime~1/15/2014 7:42:52 PM|ReportField=OutputName~BOM|ReportField=OutputType~BOM_PartType|ReportField=GeneratorName~BOM|ReportField=GeneratorDescription~Bill of Materials|ReportField=VariantName~001|ReportField=CopyrightYear~2013|ReportField=PCB_Layout~Who did the Layout?|ReportField=PCB_Rev~E1|ReportField=PRJ_Customer~Public Release|ReportField=PRJ_Engineer~Enter name of project lead|ReportField=PRJ_Number~ISE-MCCB-DAFE-100|ReportField=PRJ_Title~MCCB_OPAMP|ReportField=SCH_Rev~E1|ReportField=TechSupport~http://www.ti.com/support|ReportField=Address1~Not shown in title block|ReportField=Address2~Not shown in title block|ReportField=Address3~Not shown in title block|ReportField=Address4~Not shown in title block|ReportField=ApprovedBy~Not shown in title block|ReportField=Author~Not shown in title block|ReportField=CheckedBy~Not shown in title block|ReportField=CompanyName~Not shown in title block|ReportField=ConfigurationParameters~|ReportField=ConfiguratorName~|ReportField=CurrentDate~1/15/2014|ReportField=CurrentTime~7:41:38 PM|ReportField=Date~Not shown in title block|ReportField=DocumentFullPathAndName~D:\MCCB_OPAMP\WORK\MCCB_OPAMP_13_01_2014_AFTRBACKANN\Pg1 Index Page.SchDoc|ReportField=DocumentName~Pg1 Index Page.SchDoc|ReportField=DocumentNumber~1|ReportField=DrawnBy~|ReportField=Engineer~Not shown in title block|ReportField=ImagePath~Not shown in title block|ReportField=IsUserConfigurable~|ReportField=ModifiedDate~1/13/2014|ReportField=Organization~Not shown in title block|ReportField=PageSetup~Record=PageOptions|CenterHorizontal=True|CenterVertical=True|PrintScale=1.00|XCorrection=1.00|YCorrection=1.00|PrintKind=0|BorderSize=5000000|LeftOffset=0|BottomOffset=0|Orientation=2|PaperLength=1000|PaperWidth=1000|Scale=100|PaperSource=15|PrintQuality=600|MediaType=1|DitherType=10|PaperKind=Letter|PrintScaleMode=1|ReportField=ProjectName~MCCB_OPAMP.PrjPCB|ReportField=Revision~Use project parameter SCH_Rev|ReportField=Rule~|ReportField=SheetNumber~1|ReportField=SheetTotal~6|ReportField=Time~Not shown in title block|ReportField=Title~|ReportField=VersionControl_RevNumber~|ReportField=DataSourceFileName~MCCB_OPAMP.PrjPCB|ReportField=DataSourceFullPath~D:\MCCB_OPAMP\WORK\MCCB_OPAMP_13_01_2014_AFTRBACKANN\MCCB_OPAMP.PrjPCB
Fitted|Printed Circuit Board|!PCB1|ISE-MCCB-DAFE-100|Any|1||
Fitted|CAP, CERM, 0.1uF, 25V, +/-5%, X7R, 0603|C1, C2, C10, C11, C15, C20, C22, C23, C30, C31, C33, C34, C35, C43|06033C104JAT2A|AVX|14|478-3713-1-ND|Digi-Key
Fitted|CAP, CERM, 1000pF, 1000V, +/-10%, X7R, 1206|C3, C12, C21|CC1206KKX7RCBB102|Yageo America|3|311-1144-1-ND|Digi-Key
Fitted|CAP, CERM, 1uF, 16V, +/-10%, X7R, 0603|C4, C7|C1608X7R1C105K|TDK|2|445-1604-1-ND|Digi-Key
Fitted|CAP, CERM, 0.1uF, 50V, +/-10%, X7R, 0603|C5, C8, C29|C0603C104K5RACTU|Kemet|3|399-5089-1-ND|Digi-Key
Fitted|CAP, TA, 4.7uF, 35V, +/-10%, 1.9 ohm, SMD|C6|293D475X9035C2TE3|Vishay-Sprague|1|718-1083-1-ND|Digi-Key
Fitted|CAP, CERM, 22uF, 16V, +/-10%, X5R, 1206|C9|GRM31CR61C226KE15L|MuRata|1|GRM31CR61C226KE15L-ND|Digi-Key
Fitted|CAP, TA, 47uF, 35V, +/-10%, 0.3 ohm, SMD|C13, C28|T495X476K035ATE300|Kemet|2|399-3905-1-ND|Digi-Key
Fitted|CAP, CERM, 1uF, 100V, +/-10%, X7R, 1206|C14|GRM31CR72A105KA01L|MuRata|1|490-3909-1-ND|Digi-Key
Fitted|CAP, CERM, 0.1uF, 100V, +/-10%, X7R, 0805|C16, C25|C0805C104K1RACTU|Kemet|2|399-3486-1-ND|Digi-Key
Fitted|CAP, CERM, 0.01uF, 25V, +/-5%, C0G/NP0, 0603|C17, C26, C47, C48, C49, C50|C1608C0G1E103J|TDK|6|445-2664-1-ND|Digi-Key
Fitted|CAP, CERM, 3300pF, 50V, +/-10%, X7R, 0603|C18|C0603C332K5RACTU|Kemet|1|399-1086-1-ND|Digi-Key
Fitted|CAP, CERM, 1uF, 25V, +/-10%, X5R, 0603|C19|C1608X5R1E105K080AC|TDK|1|445-5146-1-ND|Digi-Key
Fitted|CAP, CERM, 22uF, 16V, +/-20%, X5R, 1206|C24|1206YD226MAT2A|AVX|1|478-5332-1-ND|Digi-Key
Fitted|CAP, AL, 100uF, 100V, +/-20%, 0.12 ohm, TH|C27|100YXJ100M10X20|Rubycon|1|100YXJ100M10X20-ND|Digi-Key
Fitted|CAP, CERM, 100pF, 25V, +/-10%, X7R, 0603|C32, C36, C37, C38, C39, C40, C41, C42, C44, C45, C46|06033C101KAT2A|AVX|11|581-06033C101KAT2A|Mouser
Fitted|Diode, TVS 15V 1500W BIDIR 5% SMC|D1, D3, D5|SMCJ15CA|Littelfuse Inc|3|SMCJ15CALFCT-ND|Digi-Key
Fitted|LED SmartLED Green 570NM|D2|LG L29K-G2J1-24-Z|OSRAM|1|475-2709-2-ND|Digi-Key
Fitted|Diode, Zener, 5.1V, 5W, SMB|D4|SMBJ5338B-TP|Micro Commercial Components|1|SMBJ5338B-TPMSCT-ND|Digi-Key
Fitted|Diode, Schottky, 20V, 1A, SMA|D6|B120-13-F|Diodes Inc.|1|B120-FDICT-ND|Digi-Key
Fitted|Diode, Zener, 39V, 1W, DO41|D7|1N4754A-TP|Micro Commercial Co|1||
Fitted|Diode, Zener, 16V, 1W, DO41|D8|1N4745A-TP|Micro Commercial Co|1||
Fitted|Diode, P-N, 1000V, 1A, TH|D9, D10, D11|1N4007|Fairchild Semiconductor|3|1N4007FSCT-ND|Digi-Key
Fitted|Diode, Switching, 200V, 0.2A, SOT-23|D12|BAS21-7-F|Diodes Inc.|1|BAS21-FDICT-ND|Digi-Key
Fitted|FERRITE CHIP 1000 OHM 300MA 0603|FB1|MMZ1608B102C|TDK Corporation|1|445-8672-2-ND|Digi-Key
Fitted|Machine Screw, Round, #4-40 x 1/4, Nylon, Philips panhead|H1, H2, H4, H5|NY PMS 440 0025 PH|B&F Fastener Supply|4|H542-ND|Digi-Key
Fitted|Mountin hole, NPTH Drill 3.2mm|H3|||1||
Fitted|Standoff, Hex, 0.5"L #4-40 Nylon|H6, H7, H8, H9|1902C|Keystone|4|1902CK-ND|Digi-Key
Fitted|Heatsink, TO-220, Vertical-mount, 5*C/W|HS1|513201|Aavid|1||
Fitted|Header, Male 2x10-pin, 100mil spacing|J1, J4|PEC10DAAN|Sullins|2||
Fitted|TERMINAL BLOCK 5.08MM VERT 2POS, TH|J2, J3, J11, J14, J15, J16, J17|ED120/2DS|On-Shore Technology|7|ED1609-ND|Digi-Key
Fitted|Header, Male 2-pin, 100mil spacing,|J5, J6, J7, J8, J9, J10, J12, J13|PEC02SAAN|Sullins|8||
Fitted|Terminal Block, 3-pin, 15-A, 5.1mm|J18|ED120/3DS|OST|1||
Fitted|Inductor, Common Mode Filter SMD|L1|ACM2012-900-2P-T002|TDK|1||
Fitted|Inductor, 220uH .30A SMD|L2|SRR7032-221M|Bourns|1|SRR7032-221MCT-ND|Digi-Key
Fitted|Inductor, Chip, 3.3uH 770MA 1210 10%|L3|B82422H1332K|EPCOS Inc|1||
Fitted|Thermal Transfer Printable Labels, 0.650" W x 0.200" H - 10,000 per roll|LBL1|THT-14-423-10|Brady|1|2065596|Farnell
Fitted|MOSFET, N-CH, 30V, 22A, SON 2X2 MM|Q1|CSD17571Q2|TEXAS INSTRUMENTS|1||
Fitted|MOSFET, N-CH, 60V, 50A, TO-220AB|Q2|CSD18537NKCS|Texas Instruments|1|296-36456-5-ND|Digi-Key
Fitted|RES, 100 ohm, 1%, 0.1W, 0603|R1, R40, R67, R68, R69, R70|CRCW0603100RFKEA|Vishay-Dale|6|541-100HCT-ND|Digi-Key
Fitted|RES, 470 ohm, 1%, 0.125W, 0805|R2, R9|CRCW0805470RFKEA|Vishay-Dale|2|541-470CCT-ND|Digi-Key
Fitted|RES, 300 ohm, 5%, 0.1W, 0603|R3, R39|CRCW0603300RJNEA|Vishay-Dale|2|541-300GCT-ND|Digi-Key
Fitted|RES, 10k ohm, 5%, 0.1W, 0603|R4, R5, R7|CRCW060310K0JNEA|Vishay-Dale|3|541-10KGCT-ND|Digi-Key
Fitted|RES, 120 ohm, 5%, 0.125W, 0805|R6|CRCW0805120RJNEA|Vishay-Dale|1|541-120ACT-ND|Digi-Key
Fitted|RES, 10.0 ohm, 1%, 0.1W, 0603|R8|CRCW060310R0FKEA|Vishay-Dale|1|541-10.0HCT-ND|Digi-Key
Fitted|RES, 200 ohm, 1%, 0.1W, 0603|R10|CRCW0603200RFKEA|Vishay-Dale|1|541-200HCT-ND|Digi-Key
Fitted|RES, 63.4k ohm, 1%, 0.1W, 0603|R11|CRCW060363K4FKEA|Vishay-Dale|1|541-63.4KHCT-ND|Digi-Key
Fitted|RES, 121k ohm, 0.1%, 0.125W, 0805|R12|RT0805BRD07121KL|Yageo America|1||
Fitted|RES, 10.0k ohm, 1%, 0.1W, 0603|R13, R22|CRCW060310K0FKEA|Vishay-Dale|2|541-10.0KHCT-ND|Digi-Key
Fitted|RES, 1.00k ohm, 1%, 0.1W, 0603|R14|RC0603FR-071KL|Yageo America|1|311-1.00KHRCT-ND|Digi-Key
Fitted|RES, 9.76k ohm, 1%, 0.1W, 0603|R15|CRCW06039K76FKEA|Vishay-Dale|1|541-9.76KHCT-ND|Digi-Key
Fitted|RES, 53.6k ohm, 0.1%, 0.125W, 0805|R16|RG2012P-5362-B-T5|Susumu Co Ltd|1|RG20P53.6KBCT-ND|Digi-Key
Fitted|RES, 100k ohm, 1%, 0.1W, 0603|R17, R25|CRCW0603100KFKEA|Vishay-Dale|2|541-100KHCT-ND|Digi-Key
Fitted|RES, 21.5k ohm, 1%, 0.1W, 0603|R18|CRCW060321K5FKEA|Vishay-Dale|1|541-21.5KHCT-ND|Digi-Key
Fitted|RES, 30k ohm, 5%, 0.1W, 0603|R19, R63|CRCW060330K0JNEA|Vishay-Dale|2|541-30KGCT-ND|Digi-Key
Fitted|RES, 280k ohm, 1%, 0.1W, 0603|R20|CRCW0603280KFKEA|Vishay-Dale|1|541-280KHCT-ND|Digi-Key
Fitted|RES, 10.0k ohm, 1%, 0.25W, 1206|R21, R23, R29|CRCW120610K0FKEA|Vishay-Dale|3|541-10.0KFCT-ND|Digi-Key
Fitted|RES, 43.2k ohm, 1%, 0.1W, 0603|R24|CRCW060343K2FKEA|Vishay-Dale|1|541-43.2KHCT-ND|Digi-Key
Fitted|RES, 68k ohm, 5%, 0.1W, 0603|R26, R27, R28, R59|CRCW060368K0JNEA|Vishay-Dale|4|541-68KGCT-ND|Digi-Key
Fitted|RES, 1.00Meg ohm, 1%, 0.1W, 0603|R30|CRCW06031M00FKEA|Vishay-Dale|1|541-1.00MHCT-ND|Digi-Key
Fitted|RES, 10k ohm, 0.01%, 0.063W, 0603|R31, R32, R33, R34, R35, R36, R37, R38, R55, R56, R57, R58, R62, R64, R65, R66|RNCF0603TKY10K0|Stackpole Electronics Inc|16|RNCF0603TKY10K0CT-ND|Digi-Key
Fitted|RES, 1.00k ohm, 1%, 0.25W, 1206|R41, R42|CRCW12061K00FKEA|Vishay-Dale|2|541-1.00KFCT-ND|Digi-Key
Fitted|RES, 510 ohm, 0.1%, 0.1W, 0603|R43|RG1608P-511-B-T5|Susumu Co Ltd|1|RG16P510BCT-ND|Digi-Key
Fitted|RES, 27k ohm, 5%, 0.1W, 0603|R44, R45, R46|RC0603JR-0727KL|Yageo America|3|311-27KGRCT-ND|Digi-Key
Fitted|RES, 22 ohm, 5%, 0.25W, 1206|R47, R48, R49, R50, R51, R52, R53, R54|CRCW120622R0JNEA|Vishay-Dale|8|541-22ECT-ND|Digi-Key
Fitted|RES, 47k ohm, 5%, 0.125W, 0805|R60|ERJ-6GEYJ473V|Panasonic|1|P47KACT-ND|Digi-Key
Fitted|RES, 470 ohm, 5%, 0.1W, 0603|R61|CRCW0603470RJNEA|Vishay-Dale|1|541-470GCT-ND|Digi-Key
Fitted|Transformer 475uH SMD|T1|760390015|Wurth Electronics Midcom|1|732-4459-1-ND|Digi-Key
Fitted|Test Point, O.040 Hole|TP1, TP2, TP3, TP4, TP5, TP6, TP7, TP8, TP9, TP10, TP11, TP12, TP13, TP14, TP15, TP16, TP17, TP18, TP19, TP20, TP21, TP22, TP23, TP24, TP25, TP26, TP27, TP28, TP29, TP30, TP31, TP32, TP33, TP34, TP35, TP36, TP37, TP38, TP39, TP40, TP41, TP42, TP43, TP44, TP45, TP46, TP47, TP48|STD|STD|48||
Fitted|2.7V, 15.6mV/°C, Temperature Sensor, 3-pin SOT-23|U1|LM62BIM3|National Semiconductor|1|LM62BIM3TR-ND|Digi-Key
Fitted|IC, ISOLATED RS-485 PROFIBUS TRANSCEIVER|U2|ISO1176DW|TI|1||
Fitted|50 mA, 24 V, 3.2-mA Supply Current Low-Dropout Linear Regulator, DCK0005A|U3|TPS71533DCK|Texas Instruments|1||
Fitted|100V, 600mA Constant On-Time Synchronous Buck Regulator, DDA0008B|U4|LM5017MRE/NOPB|Texas Instruments|1||
Fitted|IC, DC-DC Converter|U5|TPS55010RTE|TI|1||
Fitted|IC, Dual Differential Comparators, 2-36 Vin|U6|LM293AD|TI|1||
Fitted|LOW-VOLTAGE RAIL-TO-RAIL OUTPUT OPERATIONAL AMPLIFIERS, PW0014A|U7, U8|LMV324IPW|Texas Instruments|2||
Fitted|IC, Micropower Shunt Voltage Reference 100 ppm/°C, 45µA-12mA,  Adjustable|U9|LM4041BIDBZ|TI|1||
Not Fitted|Fiducial mark.  There is nothing to buy or mount.|FID1, FID2, FID3, FID4, FID5, FID6|N/A|N/A|0||
