Field=#~Integer~#~50|Field=Fitted~String~Fitted~100|Field=Description~String~Description~100|Field=Designator~String~Designator~100|Field=PartNumber~String~PartNumber~100|Field=Quantity~Integer~Quantity~100|Field=Manufacturer~String~Manufacturer~100|Field=PackageReference~String~PackageReference~100|Field=Value~String~Value~100|Field=Alternate Manufacturer~String~Alternate Manufacturer~100|Field=Alternate PartNumber~String~Alternate PartNumber~100|ReportField=Currency~USD|ReportField=ProductionQuantity~100|ReportField=ProjectFileName~PROC106A1.PrjPcb|ReportField=ProjectFullPath~D:\Project\60Ghz_AOP\07_Hardware\Design\LLD_Schematics\77Ghz_xWR1843AOP_NON_EBG_A1\EVM_Compliance\14Dec20\PROC106A1\4 - Sources A1\PROC106A1.PrjPcb|ReportField=Title~BOM (EVM format) For Variant [001] of Project [PROC106A1.PrjPcb] (No PCB Document Selected)|ReportField=ReportTime~14:21:33|ReportField=ReportDate~02-03-2021|ReportField=ReportDateTime~02-03-2021 14:21:33|ReportField=OutputName~BOM (EVM format)|ReportField=OutputType~BOM_PartType|ReportField=GeneratorName~BOM|ReportField=GeneratorDescription~Bill of Materials|ReportField=VariantName~001|ReportField=TotalQuantity~320|ReportField=TotalActualPrice~0|ReportField=TotalTargetPrice~0|ReportField=VersionControl_RevNumber~|ReportField=VersionControl_ProjFolderRevNumber~1414|ReportField=EVM_Orderable~AWR1843AOPEVM|ReportField=CopyrightYear~2019|ReportField=PCB_Layout~Mistral Team|ReportField=PCB_Rev~A1|ReportField=PRJ_Customer~Public Release|ReportField=PRJ_Engineer~Antony/Anand Ram|ReportField=PRJ_Number~PROC106|ReportField=PRJ_Title~xWR1843AOPEVM|ReportField=SCH_Rev~A1|ReportField=TechSupport~http://www.ti.com/support|ReportField=TID~N/A|ReportField=Address1~Not shown in title block|ReportField=Address2~Not shown in title block|ReportField=Address3~Not shown in title block|ReportField=Address4~Not shown in title block|ReportField=Application_BuildNumber~|ReportField=ApprovedBy~Not shown in title block|ReportField=Author~Not shown in title block|ReportField=CheckedBy~Not shown in title block|ReportField=CompanyName~Not shown in title block|ReportField=ConfigurationParameters~|ReportField=ConfiguratorName~|ReportField=CurrentDate~02-03-2021|ReportField=CurrentTime~14:21:29|ReportField=Date~Not shown in title block|ReportField=DocumentFullPathAndName~D:\Project\60Ghz_AOP\07_Hardware\Design\LLD_Schematics\77Ghz_xWR1843AOP_NON_EBG_A1\EVM_Compliance\14Dec20\PROC106A1\4 - Sources A1\PROC106A1_ANALOG_MUX.SchDoc|ReportField=DocumentName~PROC106A1_ANALOG_MUX.SchDoc|ReportField=DocumentNumber~10|ReportField=DrawnBy~Antony/Anand Ram|ReportField=Engineer~Not shown in title block|ReportField=ImagePath~Not shown in title block|ReportField=IsUserConfigurable~|ReportField=ModifiedDate~14-12-2020|ReportField=Organization~Not shown in title block|ReportField=PageSetup~Record=PageOptions:CenterHorizontal=True:CenterVertical=True:PrintScale=1.00:XCorrection=1.00:YCorrection=1.00:PrintKind=0:BorderSize=5000000:LeftOffset=0:BottomOffset=0:Orientation=2:PaperLength=1000:PaperWidth=1000:Scale=100:PaperSource=15:PrintQuality=600:MediaType=1:DitherType=10:PaperKind=Letter:PrintScaleMode=1|ReportField=ProjectName~PROC106A1.PrjPcb|ReportField=Revision~Use project parameter SCH_Rev|ReportField=Rule~|ReportField=SheetNumber~10|ReportField=SheetTotal~12|ReportField=Time~Not shown in title block|ReportField=Title~BREAKAWAY_SECTION4|ReportField=VersionControl_ProjFolderRevNumber~|ReportField=VersionControl_RevNumber~|ReportField=DataSourceFileName~PROC106A1.PrjPcb|ReportField=DataSourceFullPath~D:\Project\60Ghz_AOP\07_Hardware\Design\LLD_Schematics\77Ghz_xWR1843AOP_NON_EBG_A1\EVM_Compliance\14Dec20\PROC106A1\4 - Sources A1\PROC106A1.PrjPcb|ReportField=PCBConfigurationName~Sources|ReportField=Item~|ReportField=ItemRevision~|ReportField=ItemAndRevision~|ReportField=ItemRevisionBase~|ReportField=ItemRevisionLevel1~|ReportField=ItemRevisionLevel2~|ReportField=ItemRevisionLevel1AndBase~|ReportField=ItemRevisionLevel2AndLevel1~
1|Fitted|Printed Circuit Board|!PCB|PROC106|1|Any||||
2|Fitted|RF ANT 2.4GHZ CHIP SOLDER SMD|A1|ANT016008LCS2442MA2|1|TDK Corporation|SMT_ANT|||
3|Fitted|CAP, CERM, 10 uF, 10 V, +/- 10%, X7R, 0805|C1, C4, C50, C51, C52, C53, C55, C59, C62, C65, C70, C76, C78, C82, C112, C113, C121|GCM21BR71A106KE22L|17|MuRata|0805|10uF||
4|Fitted|CAP, CERM, 0.1 uF, 16 V, +/- 10%, X7R, 0402|C2, C3, C91, C92, C101, C126, C130|GCM155R71C104KA55D|7|MuRata|0402|0.1uF||
5|Fitted|Cap Ceramic 0.1uF 35V X5R 10% Pad SMD 0201 85C T/R|C6, C12, C25, C26, C27, C35, C36, C37, C40, C43, C72, C86, C105, C107, C108, C109, C117, C120, C123, C127, C128|GRM033R6YA104KE14D|21|Murata Electronics North America|0201 (0603 Metric)|||
6|Fitted|Cap Ceramic 4.7pF 50V C0G 0.25pF Pad SMD 0201 125°C Automotive T/R|C14, C71|CGA1A2C0G1H4R7C030BA|2|TDK|0201|4.7pF||
7|Fitted|CAP CER 12PF 25V C0G/NP0 0201|C19, C20|250R05L120JV4T|2|Johanson Technology Inc.|0201|||
8|Fitted|CAP, CERM, 12 pF, 50 V, +/- 5%, C0G/NP0, 0402|C21, C93|CL05C120JB5NNNC|2|Samsung Electro-Mechanics|0402|12pF||
9|Fitted|CAP, CERM, 1 pF, 50 V,+/- 25%, C0G/NP0, AEC-Q200 Grade 1, 0402|C22, C23, C41|GCM1555C1H1R0CA16D|3|MuRata|0402|1pF||
10|Fitted|1µF ±20% 16V Ceramic Capacitor X5R 0201|C24, C129|CL03A105MO3NRNH|2|Samsung Electro-Mechanics|0201|||
11|Fitted|CAP CER 22UF 6.3V X5R 0402|C28, C29|CL05A226MQ5N6J8|2|Samsung Electro-Mechanics|0402|||
12|Fitted|CAP, CERM, 0.22 µF, 16 V,+/- 10%, X7R, AEC-Q200 Grade 1, 0402|C30, C56, C57, C58, C60, C61, C63, C64, C66, C67, C68, C80, C81, C84, C85, C87, C88, C94, C95, C96, C97, C98|GCM155R71C224KE02D|22|MuRata|0402|0.22uF||
13|Fitted|CAP, CERM, 390 pF, 50 V,+/- 5%, C0G/NP0, AEC-Q200 Grade 1, 0402|C31, C32, C33, C34|CGA2B2C0G1H391J050BA|4|TDK|0402|390pF||
14|Fitted|CAP, CERM, 10 uF, 10 V, +/- 20%, X5R, 0402|C42, C122|CL05A106MP5NUNC|2|Samsung Electro-Mechanics|0402|10uF||
15|Fitted|CAP, CERM, 22 uF, 10 V, +/- 10%, X7R, AEC-Q200 Grade 1, 1206|C44, C45, C46, C47, C48, C49, C54, C73, C75, C77, C111|GCM31CR71A226KE02L|11|MuRata|1206|22uF||
16|Fitted|CAP, CERM, 0.047 uF, 50 V, +/- 10%, X7R, AEC-Q200 Grade 1, 0402|C69|CGA2B3X7R1H473K050BB|1|TDK|0402|0.047uF||
17|Fitted|CAP, CERM, 2.2 uF, 6.3 V, +/- 10%, X7R, AEC-Q200 Grade 1, 0603|C74, C79, C83, C102, C103|GCM188R70J225KE22D|5|MuRata|0603|2.2uF||
18|Fitted|CAP, CERM, 1 uF, 16 V, +/- 10%, X7R, AEC-Q200 Grade 1, 0603|C89, C90, C100|GCM188R71C105KA64D|3|MuRata|0603|1uF||
19|Fitted|CAP, CERM, 1.8 pF, 50 V,+/- 6%, C0G/NP0, 0402|C99|GJM1555C1H1R8BB01D|1|MuRata|0402|1.8pF||
20|Fitted|CAP, CERM, 4700 pF, 50 V, +/- 10%, X7R, 0402|C106, C110|GRM155R71H472KA01D|2|MuRata|0402|4700pF||
21|Fitted|CAP CER 10000PF 25V X5R 0201|C125|CL03A103KA3NNNC|1|Samsung Electro-Mechanics America, Inc|0201|||
22|Fitted|Diode Schottky 30V 2A Surface Mount SOD-123FL|D1|NRVB230LSFT1G|1|ON Semiconductor|SOD-123F|||
23|Fitted|Inductor, Ferrite Bead, Ferrite, 2.2 A, 0.035 ohm, AEC-Q200 Grade 1, SMD|FL2, FL3, FL12, FL22|BLM15PD300SZ1D|4|MuRata|0402|||
24|Fitted|AWR1843AOPEVM Heatsink|H1|MCH065|1|Any||||160021010002
25|Fitted|Thermal Pad Pink 406.40mm x 203.20mm Rectangular Adhesive - One Side|H2|GPVOUS-0.125-AC-0816|1|Bergquist||||
26|Fitted|AWR1843AOPEVM Mounting stand|H3|MCH066|1|Any||||160021010001
27|Fitted|Connector, Receptacle, Micro-USB Type B, R/A, Bottom Mount SMT|J1|105017-0001|1|Molex|Micro USB receptacle|||
28|Fitted|Receptacle, 0.5 mm, 30x2, Gold, TH|J2, J11|QSH-030-01-L-D-A|2|Samtec|Receptacle, 0.5 mm, 30x2, TH|||
29|Fitted|CONN HDR 1.27MM R/A AU 4POS|J3|M50-3930442|1|Harwin Inc.|HDR4|||
30|Fitted|DC Power Jack, R/A, TH|J5|PJ-051AH|1|CUI Inc.|DC Power Jack, R/A, TH|||
31|Fitted|CONN HEADER R/A 10POS 1.27MM|J7|GRPB052MWCN-RC|1|Sullins|HDR10|||
32|Fitted|CONN HEADER R/A 3POS 1.27MM|J8, J10|M50-3930342|2|Harwin|HDR3|||
33|Fitted|Inductor, Multilayer, Air Core, 2.4 nH, 0.3 A, 0.15 ohm, SMD|L1, L6|LQG15HS2N4S02D|2|MuRata|0402 polarized|2.4nH||
34|Fitted|Inductor, Shielded, 470 nH, 4.7 A, 0.021 ohm, SMD|L2, L3, L4, L5|DFE252012PD-R47M|4|MuRata Toko|1008|470nH||
35|Fitted|Inductor, Multilayer, Ferrite, 6.8 uH, 0.11 A, 0.25 ohm, SMD|L7|MLZ2012N6R8LT000|1|TDK|0805|6.8uH||
36|Fitted|Ferrite Bead, 1500 ohm @ 100 MHz, 0.5 A, 0603|L8|BLM18HE152SN1D|1|MuRata|0603|1500 ohm||
37|Fitted|Inductor, Multilayer, Air Core, 2 nH, 0.3 A, 0.1 ohm, SMD|L9, L10|LQG15HS2N0S02D|2|MuRata|0402 polarized|2nH||
38|Fitted|100 Ohms @ 100MHz 1 Power Line Ferrite Bead 0805 (2012 Metric) 4A 20mOhm|L11, L12, L13, L14, L15, L16|MPZ2012S101ATD25|6|TDK|0805|||
39|Fitted|LED, Green, SMD|LD1, LD2, LD3, LD4, LD5, LD6|APHHS1005CGCK|6|Kingbright|0402|Green||
40|Fitted|MOSFET N-CH 100V 170MA SOT23-3|Q1|BSS123-7-F|1|Diodes Incorporated|SOT23|||
41|Fitted|10 kOhms ±0.5% 0.05W, 1/20W Chip Resistor 0201 (0603 Metric)  Thin Film|R1, R94, R95, R104, R110, R118, R122, R124, R125, R134, R177, R178|RR0306P-103-D|12|Susumu|0201|||
42|Fitted|RES, 0, 5%, .05 W, AEC-Q200 Grade 0, 0201|R2, R28, R31, R32, R41, R60, R61, R62, R63|ERJ-1GN0R00C|9|Panasonic|0201|0||
43|Fitted|RES SMD 10K OHM 0.1% 1/20W 0201|R3, R7, R8, R19, R21, R22, R23, R35, R36, R43, R44, R45, R59, R65, R83, R84, R85|ERA-1AEB103C|17|Panasonic|0201|10k||
44|Fitted|100 kOhms ±1% 0.05W, 1/20W Chip Resistor 0201 (0603 Metric) Automotive AEC-Q200 Thick Film|R4, R5, R9, R37|ERJ-1GNF1003C|4|Panasonic Electronic Components|0201|100k||
45|Fitted|Res Thick Film 0201 33.2 Ohm 1% 0.05W(1/20W) ±200ppm/C Pad SMD Automotive T/R|R6, R46, R47, R48, R49|ERJ-1GNF33R2C|5|Panasonic|0201|33.2||
46|Fitted|RES SMD 0 OHM JUMPER 1/20W 0201|R12, R14, R51, R57, R58, R67, R68, R74, R86, R87, R90, R91, R99, R100, R101, R102, R105, R112, R113, R116, R120, R121, R123, R127, R128, R129, R131, R136, R139, R142, R143, R144, R145, R146, R147, R148, R149, R150, R151, R152, R153, R154, R155, R157, R161, R186, R187, R190|RC0201JR-070RL|48|Yageo|0201 (0603 Metric)|||
47|Fitted|RES, 220, 5%, 0.05 W, 0201|R13, R17, R42, R111|RC0201JR-07220RL|4|Yageo America|0201|220||
48|Fitted|220 Ohms ±5% 0.05W, 1/20W Chip Resistor 0201 (0603 Metric) Automotive AEC-Q200 Thick Film|R15|ERJ-1GNJ221C|1|Panasonic Electronic Components|0201|220||
49|Fitted|RES, 7.87 k, 1%, 0.05 W, 0201|R16|RC0201FR-077K87L|1|Yageo America|0201|7.87k||
50|Fitted|RES SMD 200 OHM 1% 1/5W 0402|R24|CRCW0402200RFKEDHP|1|Vishay Dale|0402|||
51|Fitted|4.99 kOhms ±1% 0.05W, 1/20W Chip Resistor 0201 (0603 Metric) Automotive AEC-Q200 Thick Film|R25, R26, R33, R34, R40, R64|ERJ-1GNF4991C|6|Panasonic Electronic Components|0201|4.99k||
52|Fitted|RES, 510, 5%, 0.05 W, 0201|R27, R107, R108|RC0201JR-07510RL|3|Yageo America|0201|510||
53|Fitted|RES, 100 k, 1%, 0.05 W, 0201|R29, R89|CRCW0201100KFKED|2|Vishay-Dale|0201|100k||
54|Fitted|RES, 4.99 k, 1%, 0.05 W, 0201|R38, R69, R141|RC0201FR-074K99L|3|Yageo America|0201|4.99k||
55|Fitted|510 Ohms ±5% 0.05W, 1/20W Chip Resistor 0201 (0603 Metric) Automotive AEC-Q200 Thick Film|R39|ERJ-1GNJ511C|1|Panasonic Electronic Components|0201|510||
56|Fitted|1 kOhms ±5% 0.05W, 1/20W Chip Resistor 0201 (0603 Metric) Automotive AEC-Q200 Thick Film|R50, R75|ERJ-1GNJ102C|2|Panasonic Electronic Components|0201|1k||
57|Fitted|Res Thick Film 0201 1.96K Ohm 1% 1/20W 200ppm/C Molded SMD T/R|R52|ERJ-1GNF1961C|1|Panasonic|0201|1.96k||
58|Fitted|RES, 3.83, 1%, 0.063 W, AEC-Q200 Grade 0, 0402|R53, R54, R55, R56|CRCW04023R83FKED|4|Vishay-Dale|0402|3.83||
59|Fitted|RES, 61.9, 1%, 0.063 W, AEC-Q200 Grade 0, 0402|R114, R117, R119, R126|CRCW040261R9FKED|4|Vishay-Dale|0402|61.9||
60|Fitted|Res Thick Film 0201 82.5K Ohm 1% 1/20W ±200ppm/°C Molded SMD SMD T/R|R158, R170, R172|ERJ-1GNF8252C|3|Panasonic|0201|82.5k||
61|Fitted|Res Thick Film 0201 750 Ohm 5% 0.05W(1/20W) ±200ppm/C Pad SMD Automotive T/R|R159, R171|ERJ-1GNJ751C|2|Panasonic Electronic Components|0201|750||
62|Fitted|Res Thick Film 0201 7.87K Ohm 1% 1/20W ±200ppm/°C Molded SMD SMD T/R|R174, R176|ERJ-1GNF7871C|2|Panasonic|0201|7.87k||
63|Fitted|RES ARRAY 4 RES ZERO OHM 0502|RA1, RA2, RA3, RA4, RA5, RA6, RA7, RA8, RA9|EXB-18VR000X|9|Panasonic Electronic Components|0502|||
64|Fitted|Switch, Slide, SPST 4 poles, SMT|S1, S2|218-4LPST|2|CTS Electrocomponents|SW, SMT Half Pitch 4SPST, 5.8x2.7x6.25 mm|||
65|Fitted|SWITCH SLIDE DIP SPST 100MA 6V|S3|CHS-01TA|1|Nidec Copal Electronics|SMT_SW_5MM4_2MM5|||
66|Fitted|SWITCH TACTILE SPST-NO 0.05A 12V|SW2, SW3|B3U-1000P|2|Omron Electronic Components|3x1.6x2.5mm|||
67|Fitted|PC Test Point, Loop Brass, Tin Plating 0.047" (1.19mm) Hole Diameter Mounting Type|TP20|4953|1|Keystone Electronics|HDR1|||
68|Fitted|4-A + 2.5-A + Two 1.5-A Buck Converters With Integrated Switches, RNF0026C (VQFN-HR-26)|U1|LP87524JRNFRQ1|1|Texas Instruments|RNF0026C||Texas Instruments|LP87524JRNFTQ1
69|Fitted|AWR1843AoPBGALP|U2|AWR1843AoPBGALP|1|Texas Instruments|FCBGA180|||
70|Fitted|I/O Controller Interface IC USB to Dual UART bridge|U3|CP2105-F01-GMR|1|Silicon Labs|QFN24-EP|||
71|Fitted|Automotive Grade, 1.4V-Capable +/-0.5degC Temperature Sensor with Alert Function and I2C/SMBus, DRL0006A (SOT-OTHER-6)|U5|TMP112AQDRLRQ1|1|Texas Instruments|DRL0006A||Texas Instruments|
72|Fitted|8KB I2C SER EEPROM TSOT 23|U6|CAT24C08TDI-GT3|1|ON Semiconductor|TSOT-23-5|||
73|Fitted|SimpleLink(TM) Bluetooth(R) 5 low energy Wireless MCU, RGZ0048A (VQFN-48)|U8|CC2642R1FRGZR|1|Texas Instruments|RGZ0048A||Texas Instruments|CC2642R1FRGZT
74|Fitted|2.3V-3.6V, 16M-BIT [x 1/x 2/x 4] CMOS FLASH Memory, WSON-8|U9|MX25V1635FZNQ|1|Macronix International Co., LTD|WSON-8|||
75|Fitted|Low-Voltage 8-Bit I2C and SMBus I/O Expander, 1.65 to 5.5 V, -40 to 85 degC, 16-pin UQFN (RSV), Green (RoHS & no Sb/Br)|U10|TCA6408ARSVR|1|Texas Instruments|RSV0016A|||
76|Fitted|1-Channel, 2:1 Analog Switch, DSF0006A (X2SON-6)|U11|SN74LVC1G3157DSFR|1|Texas Instruments|DSF0006A|||
77|Fitted|Automotive Fault Protected CAN Transceiver With Flexible Data-Rate, DRB0008F (VSON-8)|U12, U17|TCAN1042HGVDRBRQ1|2|Texas Instruments|DRB0008F||Texas Instruments|TCAN1042HGVDRBTQ1
78|Fitted|10-Ohm Quad SPDT Analog Switch, RSV0016A (UQFN-16)|U13|TS3A5018RSVR|1|Texas Instruments|RSV0016A||Texas Instruments|
79|Fitted|Dual 10-ohm SPDT Analog Switch, RSE0010A (UQFN-10)|U15|TS5A23157RSER|1|Texas Instruments|RSE0010A||Texas Instruments|
80|Fitted|AND Gate IC 1 Channel  6-SON (1x1)|U16|SN74LVC1G11DSFR|1|Texas Instruments|X2SON-6|||
81|Fitted|Automotive Catalog Dual 15-Ohm SPDT Analog Switch, DGS0010A (VSSOP-10)|U18|TS5A23157QDGSRQ1|1|Texas Instruments|DGS0010A||Texas Instruments|
82|Fitted|Dual In / Single Out Autoswitching Power Mux, 2.8 to 5.5 V, -40 to 85 degC, 8-pin SON (DRB), Green (RoHS & no Sb/Br)|U19|TPS2115ADRBR|1|Texas Instruments|DRB0008B|||
83|Fitted|40MHz ±10ppm Crystal 8pF 50 Ohms 4-SMD, No Lead|Y1|FW4000044Q|1|Diodes|4-SMD-2.0x1.6mm|||
84|Fitted|48MHz ±20ppm Crystal 7pF 50 Ohms 4-SMD, No Lead|Y2|CX2016DB48000C0WPLA2|1|Kyocera|SMD4|||
85|Fitted|CRYSTAL 32.768KHZ 4PF SMD|Y3|ABS05W-32.768KHZ-D-2-T|1|Abracon LLC|XTAL_SMT_1MM6_1MM0|||
86|Not Fitted|1µF ±20% 16V Ceramic Capacitor X5R 0201|C5, C11, C15, C16, C115, C116|CL03A105MO3NRNH|0|Samsung Electro-Mechanics|0201|||
87|Not Fitted|CAP, CERM, 10 uF, 10 V, +/- 20%, X5R, 0402|C7|CL05A106MP5NUNC|0|Samsung Electro-Mechanics|0402|10uF||
88|Not Fitted|CAP CER 10000PF 25V X5R 0201|C8|CL03A103KA3NNNC|0|Samsung Electro-Mechanics America, Inc|0201|||
89|Not Fitted|Cap Ceramic 0.1uF 35V X5R 10% Pad SMD 0201 85C T/R|C9, C10, C13, C114, C118, C119|GRM033R6YA104KE14D|0|Murata Electronics North America|0201 (0603 Metric)|||
90|Not Fitted|Cap Ceramic 8pF 50V C0G 0.1pF SMD 0201 125°C Paper T/R|C17, C18|GRM0335C1H8R0BA01D|0|Murata|0201 (0603 metric)|||
91|Not Fitted|CAP CER 12PF 25V C0G/NP0 0201|C38, C39|250R05L120JV4T|0|Johanson Technology Inc.|0201|||
92|Not Fitted|CAP, CERM, 1.8 pF, 50 V,+/- 6%, C0G/NP0, 0402|C104|GJM1555C1H1R8BB01D|0|MuRata|0402|1.8pF||
93|Not Fitted|Fiducial mark.  There is nothing to buy or mount.|FID1, FID2, FID3, FID4, FID5, FID6|N/A|0|N/A|N/A|||
94|Not Fitted|Easy-On™ Type FFC/FPC Connector, Right-Angle, Surface Mount, ZIF, Bottom Contact Style, 1.10mm Mated Height, 10 Circuits|J4, J6|51441-1093|0|Molex|CONN_SMD_FFC|||
95|Not Fitted|RES SMD 20 OHM 1% 1/20W 0201|R10, R11, R88, R130, R132, R133, R135, R137, R138, R140|AC0201FR-0720RL|0|Yageo|0201|||
96|Not Fitted|10 kOhms ±0.5% 0.05W, 1/20W Chip Resistor 0201 (0603 Metric)  Thin Film|R18, R20, R77, R78, R80, R81, R82, R93, R96, R98|RR0306P-103-D|0|Susumu|0201|||
97|Not Fitted|RES SMD 0 OHM JUMPER 1/20W 0201|R30, R66, R70, R71, R72, R73, R76, R97, R106, R115, R160, R166, R168, R182, R183, R184, R185, R188, R189|RC0201JR-070RL|0|Yageo|0201 (0603 Metric)|||
98|Not Fitted|RESISTOR, 0201, 0.05W, 1%, 4K7|R79, R180, R181|ERJ-1GNF4701C|0|Panasonic Electronic Components|0201|||
99|Not Fitted|RES, 100 k, 1%, 0.05 W, 0201|R92|CRCW0201100KFKED|0|Vishay-Dale|0201|100k||
100|Not Fitted|RES, 0, 5%, .05 W, AEC-Q200 Grade 0, 0201|R103|ERJ-1GN0R00C|0|Panasonic|0201|0||
101|Not Fitted|Single Output High PSRR LDO, 200 mA, Fixed 3 V Output, 2.7 to 5.5 V Input, 5-pin SOT-23 (DBV), -40 to 85 degC, Green (RoHS & no Sb/Br)|U4|TPS79330DBVR|0|Texas Instruments|DBV0005A|||
102|Not Fitted|IMU ACCEL/GYRO/MAG I2C 32BIT|U7|BNO085|0|Hillcrest Laboratories, Inc.|LGA28|||
103|Not Fitted|Automotive 4-Bit Bidirectional Voltage-Level Translator with Auto Direction Sensing and +/-15kV ESD, RUT0012A (UQFN-12)|U14|TXB0104QRUTRQ1|0|Texas Instruments|RUT0012A||Texas Instruments|
104|Not Fitted|CRYSTAL 32.768KHZ 4PF SMD|Y4|ABS05W-32.768KHZ-D-2-T|0|Abracon LLC|XTAL_SMT_1MM6_1MM0|||
