Field=Description~String~Description~100|Field=Designator~String~Designator~100|Field=PartNumber~String~PartNumber~100|Field=Manufacturer~String~Manufacturer~100|Field=Quantity~Integer~Quantity~100|ReportField=Currency~<none>|ReportField=ProductionQuantity~1|ReportField=ProjectFileName~SAT0103 E1.1.PrjPcb|ReportField=ProjectFullPath~C:\Users\a0358592\Documents\Systems\BCM Driver Board\CENSORED\Schematics & PCB\SAT0103 E1.1.PrjPcb|ReportField=Title~BOM For Project [SAT0103 E1.1.PrjPcb] (No PCB Document Selected)|ReportField=TotalQuantity~170|ReportField=ReportTime~10:19:16 AM|ReportField=ReportDate~20/08/2014|ReportField=ReportDateTime~20/08/2014 10:19:16 AM|ReportField=OutputName~BOM|ReportField=OutputType~BOM_PartType|ReportField=GeneratorName~BOM|ReportField=GeneratorDescription~Bill of Materials|ReportField=VariantName~None|ReportField=CopyrightYear~2014|ReportField=PCB_Layout~Derrick Kickel|ReportField=PCB_Rev~E1.1|ReportField=PRJ_Customer~Public Release|ReportField=PRJ_Engineer~Derrick Kickel|ReportField=PRJ_Number~SAT0103|ReportField=PRJ_Title~TIDA-00296 - BCM Driver Reference Design|ReportField=SCH_Rev~E1.1|ReportField=TechSupport~http://www.ti.com/support|ReportField=Address1~Not shown in title block|ReportField=Address2~Not shown in title block|ReportField=Address3~Not shown in title block|ReportField=Address4~Not shown in title block|ReportField=ApprovedBy~Not shown in title block|ReportField=Author~Not shown in title block|ReportField=CheckedBy~Not shown in title block|ReportField=CompanyName~Not shown in title block|ReportField=ConfigurationParameters~|ReportField=ConfiguratorName~|ReportField=CurrentDate~20/08/2014|ReportField=CurrentTime~10:18:40 AM|ReportField=Date~Not shown in title block|ReportField=DocumentFullPathAndName~C:\Users\a0358592\Documents\Systems\BCM Driver Board\CENSORED\Schematics & PCB\Hardware.SchDoc|ReportField=DocumentName~Hardware.SchDoc|ReportField=DocumentNumber~11|ReportField=DrawnBy~|ReportField=Engineer~Not shown in title block|ReportField=ImagePath~Not shown in title block|ReportField=IsUserConfigurable~|ReportField=ModifiedDate~19/08/2014|ReportField=Organization~Not shown in title block|ReportField=PageSetup~Record=PageOptions|CenterHorizontal=True|CenterVertical=True|PrintScale=1.00|XCorrection=1.00|YCorrection=1.00|PrintKind=0|BorderSize=5000000|LeftOffset=0|BottomOffset=0|Orientation=2|PaperLength=1000|PaperWidth=1000|Scale=100|PaperSource=15|PrintQuality=600|MediaType=1|DitherType=10|PaperKind=Letter|PrintScaleMode=1|ReportField=ProjectName~SAT0103 E1.1.PrjPcb|ReportField=Revision~Use project parameter SCH_Rev|ReportField=Rule~|ReportField=SheetNumber~11|ReportField=SheetTotal~11|ReportField=Time~Not shown in title block|ReportField=Title~Hardware|ReportField=VersionControl_RevNumber~|ReportField=DataSourceFileName~SAT0103 E1.1.PrjPcb|ReportField=DataSourceFullPath~C:\Users\a0358592\Documents\Systems\BCM Driver Board\CENSORED\Schematics & PCB\SAT0103 E1.1.PrjPcb
Printed Circuit Board|!PCB|SAT0103|Any|1
CAP, CERM, 10uF, 10V, +/-10%, X7R, 0805|C1, C32|GRM21BR71A106KE51L|MuRata|2
CAP, CERM, 0.1uF, 6.3V, +/-10%, X7R, 0402|C2, C10|GRM155R70J104KA01D|MuRata|2
CAP, CERM, 0.1uF, 10V, +/-10%, X7R, 0402|C3|GRM155R71A104KA01D|MuRata|1
CAP, CERM, 2200pF, 6.3V, +/-10%, X7R, 0402|C4|GRM155R70J222KA01D|MuRata|1
CAP, CERM, 0.1uF, 50V, +/-10%, X7R, 0603|C5, C6, C8, C9, C12, C14, C18|06035C104KAT2A|AVX|7
CAP, CERM, 0.01uF, 100V, +/-5%, X7R, 0603|C7|06031C103JAT2A|AVX|1
CAP, AL, 10uF, 50V, +/-20%, 1.52 ohm, SMD|C11|EEE-FK1H100UR|Panasonic|1
CAP, CERM, 0.1uF, 16V, +/-5%, X7R, 0603|C13|0603YC104JAT2A|AVX|1
CAP, CERM, 1uF, 50V, +/-10%, X7R, 0603|C15|UMK107AB7105KA-T|Taiyo Yuden|1
CAP, CERM, 0.1uF, 6.3V, +/-10%, X5R, 0402|C16, C29|C1005X5R0J104K|TDK|2
CAP, AL, 100uF, 50V, +/-20%, 0.23 ohm, SMD|C17|EMVH500ARA101MKE0S|Nippon Chemi-Con|1
CAP, CERM, 0.01uF, 50V, +/-5%, X7R, 0805|C19, C20, C25, C26, C27|08055C103JAT2A|AVX|5
CAP, CERM, 100pF, 25V, +/-10%, X7R, 0603|C21, C22, C23, C24|06033C101KAT2A|AVX|4
CAP, CERM, 2.2uF, 50V, +/-10%, X7R, 1206|C28|GRM31CR71H225KA88L|MuRata|1
CAP, CERM, 1uF, 50V, +/-10%, X7R, 0805|C30|08055C105KAT2A|AVX|1
CAP, CERM, 1uF, 6.3V, +/-10%, X7R, 0603|C31|GRM188R70J105KA01D|MuRata|1
CAP, CERM, 1uF, 10V, +/-10%, X7R, 0603|C33|GRM188R71A105KA61D|MuRata|1
CAP, CERM, 1000pF, 50V, +/-5%, X7R, 0805|C34|C0805C102J5RACTU|Kemet|1
CAP, CERM, 0.1uF, 10V, +/-10%, X7R, 0603|C35|C0603C104K8RACTU|Kemet|1
LED, White, SMD|D1, D2, D3|LW-E6SG|OSRAM|3
Diode, Schottky, 45V, 30A, DDPAK|D4|MBRB2545CTT4G|ON Semiconductor|1
LED, Green, SMD|D5|SML-P12PTT86|Rohm|1
Fiducial mark.  There is nothing to buy or mount.|FID1, FID2, FID3|N/A|N/A|3
Machine Screw, Round, #4-40 x 1/4, Nylon, Philips panhead|H1, H2, H3, H4|NY PMS 440 0025 PH|B&F Fastener Supply|4
Standoff, Hex, 0.5"L #4-40 Nylon|H5, H6, H7, H8|1902C|Keystone|4
Header, 100mil, 2x1, Tin, TH|J1, J12, J17|PEC02SAAN|Sullins Connector Solutions|3
Terminal Block, 6A, 3.5mm Pitch, 2-Pos, TH|J2, J3, J4, J5, J6, J7, J8, J9, J10, J11, J13, J14, J15, J16, J18, J19, J20, J21, J22|ED555/2DS|On-Shore Technology|19
TERMINAL BLOCK 5.08MM VERT 2POS, TH|J23|ED120/2DS|On-Shore Technology|1
Thermal Transfer Printable Labels, 0.650" W x 0.200" H - 10,000 per roll|LBL1|THT-14-423-10|Brady|1
MOSFET, N-CH, 60V, 16A, SO-8|Q1, Q2, Q3, Q4, Q5|SQ4470EY-T1-GE3|Vishay-Siliconix|5
RES, 47k ohm, 5%, 0.063W, 0402|R1, R5|CRCW040247K0JNED|Vishay-Dale|2
RES, 10k ohm, 5%, 0.063W, 0402|R2, R3, R4, R7, R8, R9, R17, R18, R24, R45, R46, R47, R48, R51, R52, R53, R59, R60|CRCW040210K0JNED|Vishay-Dale|18
RES, 4.7k ohm, 5%, 0.063W, 0402|R6, R10|CRCW04024K70JNED|Vishay-Dale|2
RES, 10k ohm, 5%, 0.25W, 1206|R11, R54, R55, R56|CRCW120610K0JNEA|Vishay-Dale|4
RES, 4.99k ohm, 1%, 0.1W, 0603|R12|CRCW06034K99FKEA|Vishay-Dale|1
RES, 10.0k ohm, 1%, 0.1W, 0603|R13, R28, R29, R30, R31, R32, R33, R35, R36, R37, R38, R39, R40|CRCW060310K0FKEA|Vishay-Dale|13
RES, 7.87k ohm, 1%, 0.125W, 0805|R14|CRCW08057K87FKEA|Vishay-Dale|1
RES, 8.25k ohm, 1%, 0.125W, 0805|R15|CRCW08058K25FKEA|Vishay-Dale|1
RES, 0 ohm, 5%, 0.1W, 0603|R16, R20|CRCW06030000Z0EA|Vishay-Dale|2
RES, 0.75 ohm, 1%, 0.5W, 1206|R19, R58|CSR1206FKR750|Stackpole Electronics Inc|2
RES, 1.00k ohm, 1%, 0.125W, 0805|R21|CRCW08051K00FKEA|Vishay-Dale|1
RES, 1.13k ohm, 1%, 0.1W, 0603|R22|CRCW06031K13FKEA|Vishay-Dale|1
RES, 15.4k ohm, 1%, 0.1W, 0603|R23|CRCW060315K4FKEA|Vishay-Dale|1
RES, 100 ohm, 1%, 0.063W, 0402|R25, R26, R27, R34, R41, R42, R43, R44|CRCW0402100RFKED|Vishay-Dale|8
RES, 100k ohm, 1%, 0.125W, 0805|R49|CRCW0805100KFKEA|Vishay-Dale|1
RES, 2.05k ohm, 1%, 0.125W, 0805|R50|CRCW08052K05FKEA|Vishay-Dale|1
RES, 665 ohm, 1%, 0.063W, 0402|R57|CRCW0402665RFKED|Vishay-Dale|1
SWITCH TACTILE SPST-NO 0.05A 12V|S1|B3U-1000P|Omron Electronic Components|1
Test Point, Miniature, White, TH|TP1, TP2, TP7, TP8, TP9, TP10, TP11, TP12|5002|Keystone|8
Test Point, Compact, White, TH|TP3, TP4, TP5, TP6|5007|Keystone|4
MSP-EXP430F5529 LaunchPad|U1|MSP-EXP430F5529 LaunchPad|TI|1
40V 7-Channel Low Side Driver, PW0016A|U2|TPL7407LPW|Texas Instruments|1
Quad High Side Driver, DW0020A|U3|PLMD18400DW|Texas Instruments|1
TRIPLE BUFFER/DRIVER WITH OPEN-DRAIN OUTPUTS, DCU0008A|U4|SN74LVC3G07QDCURQ1|Texas Instruments|1
RAIL-TO-RAIL OUTPUT CMOS OPERATIONAL AMPLIFIERS, DCK0006A|U5|LMV341QDCKRQ1|Texas Instruments|1
|U6, U7||Texas Instruments|2
Power MOSFET Driver with Lossless Protection, 8-pin Narrow SOIC|U8|LM9061M|National Semiconductor|1
4-CHANNEL SERIAL AND PARALLEL HIGH-SIDE PRE-FET DRIVER, DA0032A|U9|TPIC44H01DA|Texas Instruments|1
4-BIT BIDIRECTIONAL VOLTAGE-LEVEL TRANSLATOR WITH AUTOMATIC DIRECTION SENSING AND ±15-kV ESD PROTECTION, PW0014A|U10, U11|TXB0104QPWRQ1|Texas Instruments|2
Three-Channel Linear LED Driver with Analog and PWM Dimming, PWP0016F|U12|TPS92630QPWPRQ1|Texas Instruments|1
Low Voltage 16-Bit I2C and SMBus Low-Power I/O Expander with Interrupt Output, RESET, and Configuration Registers, PW0024A|U13|TCA9539QPWRQ1|Texas Instruments|1
High-Voltage Ultralow-Iq Low-Dropout Regulator, DGN0008D|U14|TPS7A6650QDGNRQ1|Texas Instruments|1
Single Output Automotive LDO, 200 mA, Fixed 3.3 V Output, 2 to 5.5 V Input, with Low IQ, 5-pin SOT (DDC), -40 to 125 degC, Green (RoHS & no Sb/Br)|U15|TLV70033QDDCRQ1|Texas Instruments|1
IC BUFF/DVR SGL 5V OD SOT23-5|U16|SN74LVC1G07QDBVRQ1|Texas Instruments|1
