Field=#~Integer~#~50|Field=Fitted~String~Fitted~146|Field=Description~String~Description~146|Field=Designator~String~Designator~146|Field=PartNumber~String~PartNumber~146|Field=Quantity~Integer~Quantity~146|Field=Manufacturer~String~Manufacturer~146|Field=PackageReference~String~PackageReference~146|Field=Value~String~Value~146|ReportField=Currency~USD|ReportField=ProductionQuantity~100|ReportField=ProjectFileName~TIDA-00204_revE3.PrjPcb|ReportField=ProjectFullPath~C:\MotorDrives\1 - TIDA\TIDA-00204\Design\Altium\TIDA-00204-RevE3.0\TIDA-00204_RevE3\TIDA-00204_revE3.PrjPcb|ReportField=Title~BOM For Variant [002] of Project [TIDA-00204_revE3.PrjPcb] (No PCB Document Selected)|ReportField=TotalQuantity~475|ReportField=ReportTime~10:55:18 AM|ReportField=ReportDate~6/14/2017|ReportField=ReportDateTime~6/14/2017 10:55:18 AM|ReportField=OutputName~BOM|ReportField=OutputType~BOM_PartType|ReportField=GeneratorName~BOM|ReportField=GeneratorDescription~Bill of Materials|ReportField=VariantName~002|ReportField=CopyrightYear~2017|ReportField=EVM_Orderable~N/A|ReportField=PCB_Layout~Klaus Hacker|ReportField=PCB_Rev~E3|ReportField=PRJ_Customer~TI Confidential - NDA|ReportField=PRJ_Engineer~Texas Instruments|ReportField=PRJ_Number~TIDA-00204|ReportField=PRJ_Title~EMI Compliant Dual Port Industrial Gigabit Ethernet PHY|ReportField=SCH_Rev~E3|ReportField=TechSupport~http://www.ti.com/support|ReportField=TID~|ReportField=Address1~Not shown in title block|ReportField=Address2~Not shown in title block|ReportField=Address3~Not shown in title block|ReportField=Address4~Not shown in title block|ReportField=Application_BuildNumber~|ReportField=ApprovedBy~Not shown in title block|ReportField=Author~Not shown in title block|ReportField=CheckedBy~Not shown in title block|ReportField=CompanyName~Not shown in title block|ReportField=ConfigurationParameters~|ReportField=ConfiguratorName~|ReportField=CurrentDate~6/14/2017|ReportField=CurrentTime~10:40:24 AM|ReportField=Date~Not shown in title block|ReportField=DocumentFullPathAndName~C:\MotorDrives\1 - TIDA\TIDA-00204\Design\Altium\TIDA-00204-RevE3.0\TIDA-00204_RevE3\TIDA-00204_Hardware.SchDoc|ReportField=DocumentName~TIDA-00204_Hardware.SchDoc|ReportField=DocumentNumber~10|ReportField=DrawnBy~K. Mogensen|ReportField=Engineer~K. Mogensen|ReportField=ImagePath~Not shown in title block|ReportField=IsUserConfigurable~|ReportField=ModifiedDate~6/14/2017|ReportField=Organization~Not shown in title block|ReportField=PageSetup~Record=PageOptions:CenterHorizontal=True:CenterVertical=True:PrintScale=1.00:XCorrection=1.00:YCorrection=1.00:PrintKind=0:BorderSize=5000000:LeftOffset=0:BottomOffset=0:Orientation=2:PaperLength=1000:PaperWidth=1000:Scale=100:PaperSource=15:PrintQuality=600:MediaType=1:DitherType=10:PaperKind=Letter:PrintScaleMode=1|ReportField=ProjectName~TIDA-00204_revE3.PrjPcb|ReportField=Revision~Use project parameter SCH_Rev|ReportField=Rule~|ReportField=SheetNumber~10|ReportField=SheetTotal~10|ReportField=Time~Not shown in title block|ReportField=Title~TIDA-00204_Hardware.SchDoc|ReportField=VersionControl_RevNumber~|ReportField=DataSourceFileName~TIDA-00204_revE3.PrjPcb|ReportField=DataSourceFullPath~C:\MotorDrives\1 - TIDA\TIDA-00204\Design\Altium\TIDA-00204-RevE3.0\TIDA-00204_RevE3\TIDA-00204_revE3.PrjPcb
1|Fitted|Printed Circuit Board|!PCB1|TIDA-00204|1|Any||
2|Fitted|CAP, CERM, 10 µF, 25 V, +/- 20%, X5R, 0603|C1, C2, C3, C17, C18, C36, C40, C45, C63, C67, C72, C80, C81, C86, C88, C89, C90, C104, C107, C110, C113, C116, C126, C131, C148, C149, C170, C171, C185, C202, C211, C212, C225, C226, C227, C231, C232|C1608X5R1E106M080AC|37|TDK|0603|10uF
3|Fitted|CAP, CERM, 0.47 µF, 100 V, +/- 10%, X7R, 0805|C4|GRM21BR72A474KA73L|1|MuRata|0805|0.47uF
4|Fitted|CAP, CERM, 1 µF, 100 V, +/- 10%, X7S, 0805|C5|C2012X7S2A105K125AB|1|TDK|0805|1uF
5|Fitted|CAP, CERM, 0.1 µF, 100 V, +/- 10%, X7R, 0603|C6, C8|GRM188R72A104KA35D|2|MuRata|0603|0.1uF
6|Fitted|CAP, CERM, 1000 pF, 100 V, +/- 10%, X7R, 0603|C7, C9|GRM188R72A102KA01D|2|MuRata|0603|1000pF
7|Fitted|CAP, CERM, 1 µF, 25 V, +/- 10%, X7R, 0603|C10|GRM188R71E105KA12D|1|MuRata|0603|1uF
8|Fitted|CAP, CERM, 10 µF, 100 V, +/- 20%, X7S, 2220|C11|C5750X7S2A106M|1|TDK|2220|10uF
9|Fitted|CAP, CERM, 4.7 µF, 16 V, +/- 10%, X5R, 0603|C13, C82, C83, C84, C85, C87, C233, C234, C251|GRM188R61C475KAAJ|9|MuRata|0603|4.7uF
10|Fitted|CAP, CERM, 8.2 pF, 25 V, +/- 5%, C0G/NP0, 0402|C14|GRM1555C1E8R2CA01D|1|MuRata|0402|8.2pF
11|Fitted|CAP, CERM, 0.1 µF, 16 V, +/- 10%, X7R, 0402|C15, C22, C27, C28, C29, C30, C55, C56, C57, C58, C206|GRM155R71C104KA88D|11|MuRata|0402|0.1uF
12|Fitted|CAP, CERM, 1 µF, 10 V, +/- 10%, X7R, 0603|C16, C100, C101|GRM188R71A105KA61D|3|MuRata|0603|1uF
13|Fitted|CAP, CERM, 470 pF, 50 V, +/- 10%, X7R, 0402|C21|GRM155R71H471KA01D|1|MuRata|0402|470pF
14|Fitted|CAP, CERM, 2.2 µF, 10 V, +/- 10%, X7R, 0603|C23, C91, C92, C93, C94, C95, C96, C97, C98, C201, C260|GRM188R71A225KE15D|11|MuRata|0603|2.2uF
15|Fitted|CAP, CERM, 0.1 µF, 10 V, +/- 10%, X7R, 0402|C24, C99, C199, C203, C204, C207, C209, C236, C237, C239, C244, C245, C246, C247, C248, C249, C250|GRM155R71A104KA01D|17|MuRata|0402|0.1uF
16|Fitted|CAP, CERM, 1000 pF, 16 V, +/- 10%, X7R, 0201|C25, C26, C38, C39, C42, C43, C44, C47, C48, C49, C50, C53, C54, C65, C66, C69, C70, C71, C74, C75, C76, C77, C197, C210, C253, C257|GRM033R71C102KA01D|26|MuRata|0201|1000pF
17|Fitted|CAP, CERM, 1000 pF, 2000 V, +/- 10%, X7R, 1206_190|C33, C59|202R18W102KV4E|2|Johanson Technology|1206_190|1000pF
18|Fitted|CAP, CERM, 0.01 µF, 10 V, +/- 10%, X7R, 0201|C35, C37, C41, C46, C64, C68, C73, C102, C103, C105, C106, C108, C109, C111, C112, C114, C115, C117, C118, C119, C120, C121, C122, C123, C124, C125, C127, C128, C129, C130, C132, C133, C134, C135, C136, C137, C138, C142, C143, C144, C146, C147, C172, C173, C174, C175, C176, C177, C178, C179, C180, C181, C182, C183, C184, C186, C187, C188, C189, C190, C191, C195, C196, C200, C205, C235, C243, C254, C256|GRM033R71A103KA01D|69|MuRata|0201|0.01uF
19|Fitted|CAP, CERM, 1 µF, 10 V, +/- 20%, X5R, 0201|C139, C140, C141, C145|CL03A105MP3NSNC|4|Samsung|0201|1uF
20|Fitted|CAP, CERM, 0.1 µF, 10 V, +/- 10%, X5R, 0201|C150, C151, C152, C153, C154, C155, C156, C157, C158, C159, C160, C161, C162, C163, C164, C165, C166, C167, C168, C169, C208, C213, C214, C215, C216, C217, C218, C219, C220, C221, C222, C223, C224, C228, C229, C230, C252, C255|CL03A104KP3NNNC|38|Samsung|0201|0.1uF
21|Fitted|CAP, CERM, 18 pF, 50 V, +/- 5%, C0G/NP0, 0402|C194, C198|GRM1555C1H180JA01D|2|MuRata|0402|18pF
22|Fitted|CAP, CERM, 27 pF, 50 V, +/- 5%, C0G/NP0, 0402|C240, C241, C258, C259|GRM1555C1H270JA01D|4|MuRata|0402|27pF
23|Fitted|CAP, CERM, 4.7 pF, 50 V, +/- 5%, C0G/NP0, 0201|C261, C262, C263, C264, C265, C266, C267, C268, C271, C272, C273, C274, C275, C276, C277, C278|GRM0335C1H4R7CA01D|16|MuRata|0201|4.7pF
24|Fitted|Diode, Schottky, 60V, 1A, SMA|D1|MBRA160T3G|1|ON Semiconductor|SMA|60V
25|Fitted|LED, Green, SMD|D2, D3, D6, D11, D14|LG L29K-G2J1-24-Z|5|OSRAM|1.7x0.65x0.8mm|Green
26|Fitted|LED, Yellow, SMD|D4, D9|LY L29K-J1K2-26-Z|2|OSRAM|LED, 1.3x0.65x0.8mm|Yellow
27|Fitted|LED, Red, SMD|D5, D10|LS L29K-G1J2-1-Z|2|OSRAM|SMD, 2-Leads, Body 1.3x0.8mm|Red
28|Fitted|LED, Orange, SMD|D7, D12|LO L29K-J2L1-24-Z|2|OSRAM|SMD, 2-Leads, Body 1.3x0.8mm|Orange
29|Fitted|Diode, TVS, Bi, 5 V, 300 W, SOT-23-6|D8, D13|SRV05-4.TCT|2|Semtech|SOT-23-6|5V
30|Fitted|Machine Screw, Round, #4-40 x 1/4, Nylon, Philips panhead|H1, H2, H3, H4|NY PMS 440 0025 PH|4|B&F Fastener Supply|Screw|
31|Fitted|Standoff, Hex, 0.5"L #4-40 Nylon|H5, H6, H7, H8|1902C|4|Keystone|Standoff|
32|Fitted|Header, 100mil, 2x1, Tin, TH|J1, J3|PEC02SAAN|2|Sullins Connector Solutions|Header, 2 PIN, 100mil, Tin|
33|Fitted|Power Jack, mini, 2.1mm OD, R/A, TH|J2|RAPC722X|1|Switchcraft|Jack, 14.5x11x9mm|
34|Fitted|Modular Jack(Shielded), Gold, R/A, TH|J4, J5|43202-8916|2|Molex|Modular Jack(Shielded), R/A, TH|
35|Fitted|Conncetor, micro SD Card, 1.1 mm, R/A, SMT|J6|502774-0891|1|Molex|SMD, 14-Leads, Body 15x14.3mm, Pitch 1.1mm|
36|Fitted|Receptacle, 0.65 mm, 5x1, Gold, R/A, SMT|J7|10104111-0001LF|1|FCI|SMD, 5-Leads, Body 7.5x5.6mm, Pitch 0.65mm|
37|Fitted|Inductor, Shielded Drum Core, Ferrite, 1 µH, 1.5 A, 0.085 ohm, SMD|L1|LPS3010-102MRB|1|Coilcraft|LPS3010|1uH
38|Fitted|Inductor, Shielded Drum Core, Ferrite, 15 µH, 3.5 A, 0.03 ohm, SMD|L2|MSS1260-153MLB|1|Coilcraft|MSS1260|15uH
39|Fitted|Inductor, Shielded, Ferrite, 2.2 µH, 2.62 A, 0.043 ohm, SMD|L3, L4, L5|VLCF5020T-2R2N2R6-3|3|TDK|5x2x5mm|2.2uH
40|Fitted|Ferrite Bead, 150 ohm @ 100 MHz, 0.8 A, 0805|L6, L7, L9, L10, L11, L12|LI0805H151R-10|6|Laird-Signal Integrity Products|0805|150 ohm
41|Fitted|Common Mode Filter, 90 Ohm, 6 GHz, SMD|L8|ACM2012H-900-2P-T00|1|TDK|SMD, 4-Leads, Body 2x1.2mm|90Ohm
42|Fitted|Ferrite Bead, 120 ohm @ 100 MHz, 0.4 A, 0402|L13, L14|MMZ1005Y121C|2|TDK|0402|120 ohm
43|Fitted|RES, 10 ohm, 5%, 0.25W, 0603|R1|CRCW060310R0JNEAHP|1|Vishay-Dale|0603|10
44|Fitted|RES, 453 k, 1%, 0.063 W, 0402|R2|CRCW0402453KFKED|1|Vishay-Dale|0402|453k
45|Fitted|RES, 750, 5%, 0.063 W, 0402|R3|CRCW0402750RJNED|1|Vishay-Dale|0402|750
46|Fitted|RES, 100 k, 1%, 0.063 W, 0402|R4, R119|CRCW0402100KFKED|2|Vishay-Dale|0402|100k
47|Fitted|RES, 80.6 k, 1%, 0.063 W, 0402|R5|CRCW040280K6FKED|1|Vishay-Dale|0402|80.6k
48|Fitted|RES, 1.00 M, 1%, 0.063 W, 0402|R6|CRCW04021M00FKED|1|Vishay-Dale|0402|1.00Meg
49|Fitted|RES, 249 k, 1%, 0.063 W, 0402|R7|CRCW0402249KFKED|1|Vishay-Dale|0402|249k
50|Fitted|RES, 0, 5%, 0.1 W, 0603|R8, R9, R10, R12, R15, R71, R139, R140, R141, R142, R143, R144, R145, R147|CRCW06030000Z0EA|14|Vishay-Dale|0603|0
51|Fitted|RES, 360, 5%, 0.063 W, 0402|R13|CRCW0402360RJNED|1|Vishay-Dale|0402|360
52|Fitted|RES, 150 k, 1%, 0.063 W, 0402|R14|CRCW0402150KFKED|1|Vishay-Dale|0402|150k
53|Fitted|RES, 110 k, 1%, 0.063 W, 0402|R16|CRCW0402110KFKED|1|Vishay-Dale|0402|110k
54|Fitted|RES, 0, 5%, 0.063 W, 0402|R19, R43, R44, R46, R47, R50, R51, R171, R173, R175|CRCW04020000Z0ED|10|Vishay-Dale|0402|0
55|Fitted|RES, 0, 5%, 0.0625 W, Resistor Array - 8x1|R20|EXB-2HVR000V|1|Panasonic|Resistor Array - 8x1|0
56|Fitted|RES, 10.0 k, 1%, 0.063 W, 0402|R21, R38, R41, R67, R68, R136, R138, R158|CRCW040210K0FKED|8|Vishay-Dale|0402|10.0k
57|Fitted|RES, 75.0, 1%, 0.1 W, 0603|R22, R24, R32, R37, R42, R48, R58, R64|CRCW060375R0FKEA|8|Vishay-Dale|0603|75.0
58|Fitted|RES, 4.7 k, 5%, 0.063 W, 0402|R23, R29, R45, R55, R146, R152, R153, R165, R166|CRCW04024K70JNED|9|Vishay-Dale|0402|4.7k
59|Fitted|RES, 560, 5%, 0.063 W, 0402|R25, R26, R27, R33, R52, R53, R54, R60, R66|CRCW0402560RJNED|9|Vishay-Dale|0402|560
60|Fitted|RES, 11.0 k, 1%, 0.063 W, 0402|R28, R30, R49, R56, R59|CRCW040211K0FKED|5|Vishay-Dale|0402|11.0k
61|Fitted|RES, 2.49 k, 1%, 0.063 W, 0402|R31, R34, R57, R61, R62|CRCW04022K49FKED|5|Vishay-Dale|0402|2.49k
62|Fitted|RES, 22, 5%, 0.0625 W, Resistor Array - 8x1|R69|EXB-2HV220JV|1|Panasonic|Resistor Array - 8x1|22
63|Fitted|RES, 10 k, 5%, 0.063 W, 0402|R70, R84, R94, R95, R96, R120, R121, R122, R123, R124, R125, R131, R135, R137, R148, R149, R150|CRCW040210K0JNED|17|Vishay-Dale|0402|10k
64|Fitted|RES, 22, 5%, 0.063 W, 0402|R72, R73, R74, R75, R77, R78, R79, R80, R81, R82|CRCW040222R0JNED|10|Vishay-Dale|0402|22
65|Fitted|RES, 2.2 k, 5%, 0.063 W, 0402|R76, R117, R118, R154, R156|CRCW04022K20JNED|5|Vishay-Dale|0402|2.2k
66|Fitted|RES, 49.9, 1%, 0.063 W, 0402|R99, R126, R127, R176|CRCW040249R9FKED|4|Vishay-Dale|0402|49.9
67|Fitted|RES, 1.00 k, 1%, 0.063 W, 0402|R100, R129, R169, R177, R178|CRCW04021K00FKED|5|Vishay-Dale|0402|1.00k
68|Fitted|RES, 100 k, 5%, 0.063 W, 0402|R101, R103, R104, R105, R106, R107, R108, R109, R110, R111, R115, R116|CRCW0402100KJNED|12|Vishay-Dale|0402|100k
69|Fitted|RES, 47, 5%, 0.0625 W, Resistor Array - 8x1|R128, R130, R133|EXB-2HV470JV|3|Panasonic|Resistor Array - 8x1|47
70|Fitted|RES, 240, 5%, 0.063 W, 0402|R132|CRCW0402240RJNED|1|Vishay-Dale|0402|240
71|Fitted|RES, 47, 5%, 0.063 W, 0402|R134|CRCW040247R0JNED|1|Vishay-Dale|0402|47
72|Fitted|RES, 4.75 k, 1%, 0.063 W, 0402|R155|CRCW04024K75FKED|1|Vishay-Dale|0402|4.75k
73|Fitted|RES, 12.1 k, 1%, 0.063 W, 0402|R157|CRCW040212K1FKED|1|Vishay-Dale|0402|12.1k
74|Fitted|RES, 36, 5%, 0.063 W, 0402|R167, R182, R183|CRCW040236R0JNED|3|Vishay-Dale|0402|36
75|Fitted|SWITCH TACTILE SPST-NO 0.05A 12V|S1|B3U-1000P|1|Omron Electronic Components|3x1.6x2.5mm|
76|Fitted|Transformer, 325 uH, SMT|T1, T2|HX5008FNL|2|Pulse Engineering|SMD, 17.86x13.16mm|325 uH
77|Fitted|3.5V to 60V 2A Synchronous Step-Down Voltage Regulator, PWP0016A|U1|LM46002PWP|1|Texas Instruments|PWP0016A|
78|Fitted|Single Output LDO, 1 A, Fixed 3.3 V Output, 2.2 to 5.5 V Input, with Reverse Current Protection, 6-pin SOT-223 (DCQ), -40 to 125 degC, Green (RoHS & no Sb/Br)|U2|TPS73733DCQ|1|Texas Instruments|DCQ0006A|
79|Fitted|1A SIMPLE SWITCHER® Nano Module with 5.5V Maximum Input Voltage, SIL0008A|U3|LMZ10501SIL|1|Texas Instruments|SIL0008A|
80|Fitted|350mA, Ultra-Low VIN, RF Low-Dropout Linear Regulator with Bias Pin, DRV0006A|U5|TPS72011DRV|1|Texas Instruments|DRV0006A|
81|Fitted|Robust, Low Power 10/100/1000 Ethernet Physical Layer Transceiver, PAP0064M|U6, U12|DP83867IRPAPR|2|Texas Instruments|PAP0064M|
82|Fitted|1, 4, 6 CHANNEL PROTECTION SOLUTION FOR SUPER-SPEED (UP TO 6 GBPS) INTERFACE, DQA0010A|U7, U9|TPD4E05U06DQA|2|Texas Instruments|DQA0010A|
83|Fitted|Single 2-Input Positive-AND Gate, DCK0005A|U11|SN74AHC1G08DCK|1|Texas Instruments|DCK0005A|
84|Fitted|Integrated Power-Management Unit Top Specification, RSL0048A|U13|TPS65910A3A1RSL|1|Texas Instruments|RSL0048A|
85|Fitted|Single Output High PSRR LDO, 150 mA, Fixed 1.8 V Output, 2.5 to 6.5 V Input, with Low IQ, 6-pin WSON (DSE), -40 to 125 degC, Green (RoHS & no Sb/Br)|U14|TPS71718DSER|1|Texas Instruments|DSE0006A|
86|Fitted|Sitara Processors, ZCZ0324A|U15|AM3359BZCZA80|1|Texas Instruments|ZCZ0324A|
87|Fitted|LOW-POWER DUAL 2-INPUT POSITIVE-AND GATE, DCU0008A|U16|SN74AUP2G08DCU|1|Texas Instruments|DCU0008A|
88|Fitted|2GBIT DDR3 SDRAM, 96-FBGA|U17|MT41J128M16JT-125K TR|1|Micron Technology|BGA, 96-Balls, Body 9x14mm, Pitch 0.8mm|
89|Fitted|Low-Capacitance + / - 15 kV ESD Protection Array for High-Speed Data Interfaces, 6 Channels, -40 to +85 degC, 10-pin UQFN (RSE), Green (RoHS & no Sb/Br)|U18|TPD6E001RSER|1|Texas Instruments|RSE0010A|
90|Fitted|256 kb I2C CMOS Serial EEPROM, SOIC-8|U19|CAT24C256WI-GT3|1|ON Semiconductor|SOIC-8|
91|Fitted|Single Output LDO, 3 A, 2.375 to 3.5 V Input, with DDR Termination, 10-pin SON (DRC), -40 to 85 degC, Green (RoHS & no Sb/Br)|U20|TPS51200DRCR|1|Texas Instruments|DRC0010A|
92|Fitted|USB ESD Solution with Power Clamp, 4 Channels, -40 to +85 degC, 6-pin SON (DRY), Green (RoHS & no Sb/Br)|U21|TPD4S012DRYR|1|Texas Instruments|DRY0006A|
93|Fitted|Dual High Speed USB To Multipurpose UART/FIFO IC, LQFP-64|U22|FT2232HL-REEL|1|FTDI|LQFP_10x10mm|
94|Fitted|2K Microwire Compatible Serial EEPROM, SOT-23-6|U23|93LC56B-I/OT|1|Microchip|SOT-23-6|
95|Fitted|Single Inverter Buffer/Driver With Open-Drain Output, DCK0005A|U24|SN74LVC1G06DCK|1|Texas Instruments|DCK0005A|
96|Fitted|Programmable 1-PLL VCXO Clock Synthesizer With 1.8-V, 2.5-V, and 3.3-V Outputs, PW0014A|U25|CDCE913PW|1|Texas Instruments|PW0014A|
97|Fitted|Crystal, 32.768kHz, 12.5pF, SMD|Y4|MC-306 32.7680K-A0:ROHS|1|Epson|8x2.54x3.8mm|
98|Fitted|Crystal, 12 MHz, 18 pF, SMD|Y5|ABM3-12.000MHZ-D2Y-T|1|Abracon Corportation|ABM3|
99|Fitted|Crystal, 25 MHz, 18 pF, SMD|Y6|ABM3-25.000MHZ-D2Y-T|1|Abracon Corportation|ABM3|
100|Not Fitted|CAP, CERM, 0.022 µF, 50 V, +/- 10%, X7R, 0402|C12|GRM155R71H223KA12D|0|MuRata|0402|0.022uF
101|Not Fitted|CAP, CERM, 27 pF, 50 V, +/- 5%, C0G/NP0, 0402|C31, C32, C60, C61, C192, C193|GRM1555C1H270JA01D|0|MuRata|0402|27pF
102|Not Fitted|CAP, CERM, 1000 pF, 2000 V, +/- 10%, X7R, 1812|C34, C62|1812GC102KA1|0|AVX|1812|1000pF
103|Not Fitted|CAP, CERM, 0.01 µF, 10 V, +/- 10%, X7R, 0201|C238|GRM033R71A103KA01D|0|MuRata|0201|0.01uF
104|Not Fitted|CAP, CERM, 0.1 µF, 10 V, +/- 10%, X7R, 0402|C242|GRM155R71A104KA01D|0|MuRata|0402|0.1uF
105|Not Fitted|CONN SHRD HDR HDR 20 POS 1.27MM SLDR ST SMD|J8|TFM-110-02-S-D-A-K-TR|0|Samtec|15.88x6.35x5.72mm|
106|Not Fitted|RES, 22, 5%, 0.063 W, 0402|R35|CRCW040222R0JNED|0|Vishay-Dale|0402|22
107|Not Fitted|RES, 1.00 M, 1%, 0.063 W, 0402|R36, R65, R168|CRCW04021M00FKED|0|Vishay-Dale|0402|1.00Meg
108|Not Fitted|RES, 0, 5%, 0.063 W, 0402|R63, R170, R172, R174|CRCW04020000Z0ED|0|Vishay-Dale|0402|0
109|Not Fitted|RES, 10 k, 5%, 0.063 W, 0402|R83, R85, R86, R87, R88, R89, R90, R91, R92, R93, R97, R98|CRCW040210K0JNED|0|Vishay-Dale|0402|10k
110|Not Fitted|RES, 100 k, 5%, 0.063 W, 0402|R102, R112, R113, R114|CRCW0402100KJNED|0|Vishay-Dale|0402|100k
111|Not Fitted|RES, 4.7 k, 5%, 0.063 W, 0402|R151|CRCW04024K70JNED|0|Vishay-Dale|0402|4.7k
112|Not Fitted|RES, 0, 5%, 0.1 W, 0603|R159, R160, R161, R162, R163, R164|CRCW06030000Z0EA|0|Vishay-Dale|0603|0
113|Not Fitted|RES, 1.00 k, 1%, 0.063 W, 0402|R179, R180, R181|CRCW04021K00FKED|0|Vishay-Dale|0402|1.00k
114|Not Fitted|1, 4, 6 CHANNEL PROTECTION SOLUTION FOR SUPER-SPEED (UP TO 6 GBPS) INTERFACE, DQA0010A|U8, U10|TPD4E05U06DQA|0|Texas Instruments|DQA0010A|
115|Not Fitted|Crystal, 25 MHz, 18 pF, SMD|Y1, Y2|ABM3-25.000MHZ-D2Y-T|0|Abracon Corportation|ABM3|
116|Not Fitted|Crystal, 24 MHz, 18 pF, SMD|Y3|ABM3-24.000MHZ-D2Y-T|0|Abracon Corportation|ABM3|
