Field=#~Integer~#~50|Field=Fitted~String~Fitted~146|Field=Description~String~Description~146|Field=Designator~String~Designator~146|Field=PartNumber~String~PartNumber~146|Field=Quantity~Integer~Quantity~146|Field=Manufacturer~String~Manufacturer~146|Field=PackageReference~String~PackageReference~146|Field=Value~String~Value~146|ReportField=Currency~USD|ReportField=ProductionQuantity~100|ReportField=ProjectFileName~TIDA-00913.PrjPcb|ReportField=ProjectFullPath~\\dfrs40\industrial_systems\Motor Drives\1_TIDAs\TIDA-00913_Shunt_based_Phase_Current_Sensing_with_48V_3-Phase_Inverters\DESIGN\TIDA-00913_revE1\TIDA-00913.PrjPcb|ReportField=Title~PDF BOM (TI Designs format) For Variant [001] of Project [TIDA-00913.PrjPcb] (No PCB Document Selected)|ReportField=TotalQuantity~162|ReportField=ReportTime~6:29:22 PM|ReportField=ReportDate~10/28/2016|ReportField=ReportDateTime~10/28/2016 6:29:22 PM|ReportField=OutputName~PDF BOM (TI Designs format)|ReportField=OutputType~BOM_PartType|ReportField=GeneratorName~BOM|ReportField=GeneratorDescription~Bill of Materials|ReportField=VariantName~001|ReportField=EVM_Orderable~N/A|ReportField=TID~TIDA-00913|ReportField=TechSupport~http://www.ti.com/support|ReportField=SCH_Rev~E1|ReportField=PRJ_Title~TI Design|ReportField=PRJ_Number~TIDA-00913|ReportField=PRJ_Engineer~Zhou/Staebler|ReportField=PRJ_Customer~Public Release|ReportField=PCB_Rev~E1|ReportField=PCB_Layout~Zhou|ReportField=CopyrightYear~2016|ReportField=Address1~Not shown in title block|ReportField=Address2~Not shown in title block|ReportField=Address3~Not shown in title block|ReportField=Address4~Not shown in title block|ReportField=Application_BuildNumber~|ReportField=ApprovedBy~Not shown in title block|ReportField=Author~Not shown in title block|ReportField=CheckedBy~Not shown in title block|ReportField=CompanyName~Not shown in title block|ReportField=ConfigurationParameters~|ReportField=ConfiguratorName~|ReportField=CurrentDate~10/28/2016|ReportField=CurrentTime~6:26:59 PM|ReportField=Date~Not shown in title block|ReportField=DocumentFullPathAndName~\\dfrs40\industrial_systems\Motor Drives\1_TIDAs\TIDA-00913_Shunt_based_Phase_Current_Sensing_with_48V_3-Phase_Inverters\DESIGN\TIDA-00913_revE1\TIDA-00913_CS.SchDoc|ReportField=DocumentName~TIDA-00913_CS.SchDoc|ReportField=DocumentNumber~1|ReportField=DrawnBy~|ReportField=Engineer~Not shown in title block|ReportField=ImagePath~Not shown in title block|ReportField=IsUserConfigurable~|ReportField=ModifiedDate~10/28/2016|ReportField=Organization~Not shown in title block|ReportField=PageSetup~Record=PageOptions:CenterHorizontal=True:CenterVertical=True:PrintScale=1.00:XCorrection=1.00:YCorrection=1.00:PrintKind=0:BorderSize=5000000:LeftOffset=0:BottomOffset=0:Orientation=2:PaperLength=1000:PaperWidth=1000:Scale=100:PaperSource=15:PrintQuality=600:MediaType=1:DitherType=10:PaperKind=Letter:PrintScaleMode=1|ReportField=ProjectName~TIDA-00913.PrjPcb|ReportField=Revision~Use project parameter SCH_Rev|ReportField=Rule~|ReportField=SheetNumber~1|ReportField=SheetTotal~3|ReportField=Time~Not shown in title block|ReportField=Title~|ReportField=VersionControl_RevNumber~|ReportField=DataSourceFileName~TIDA-00913.PrjPcb|ReportField=DataSourceFullPath~\\dfrs40\industrial_systems\Motor Drives\1_TIDAs\TIDA-00913_Shunt_based_Phase_Current_Sensing_with_48V_3-Phase_Inverters\DESIGN\TIDA-00913_revE1\TIDA-00913.PrjPcb
1|Fitted|CAP, AL, 220 µF, 100 V, +/- 20%, 0.039 ohm, TH|C1|EKYB101ELL221MK25S|1|Chemi-Con|D12.5xL25mm|220uF
2|Fitted|CAP, CERM, 3.3 µF, 100 V, +/- 20%, X7S, 1206_190|C2, C5, C6, C7, C10, C11, C12, C21, C22, C23, C42, C45|C3216X7S2A335M160AB|12|TDK|1206_190|3.3uF
3|Fitted|CAP, CERM, 2.2 µF, 10 V, +/- 10%, X5R, 0402|C3, C8, C19|C1005X5R1A225K050BC|3|TDK|0402|2.2uF
4|Fitted|CAP, CERM, 0.1 µF, 100 V, +/- 5%, C0G/NP0, 1206_190|C4, C9, C20|C3216C0G2A104J160AC|3|TDK|1206_190|0.1uF
5|Fitted|CAP, CERM, 0.1 µF, 16 V, +/- 10%, X7R, 0402|C13, C14, C24, C47, C50, C54, C59|GCM155R71C104KA55D|7|MuRata|0402|0.1uF
6|Fitted|CAP, CERM, 47 pF, 25 V, +/- 5%, C0G/NP0, 0402|C15, C16, C17, C18, C25, C26|GRM1555C1E470JA01D|6|MuRata|0402|47pF
7|Fitted|CAP, CERM, 0.1 µF, 10 V, +/- 10%, X7R, 0402|C27, C32|GRM155R71A104KA01D|2|MuRata|0402|0.1uF
8|Fitted|CAP, CERM, 2200 pF, 16 V, +/- 10%, X7R, 0603|C28, C29, C30, C31, C33, C34, C35, C36|885012206036|8|Wurth Elektronik|0603|2200pF
9|Fitted|CAP, CERM, 0.01 µF, 16 V, +/- 10%, X5R, 0402|C37|GRM155R61C103KA01D|1|MuRata|0402|0.01uF
10|Fitted|CAP, CERM, 3300 pF, 100 V, +/- 10%, X7R, 0603|C38|GRM188R72A332KA01D|1|MuRata|0603|3300pF
11|Fitted|CAP, CERM, 0.01 µF, 50 V, +/- 10%, X7R, 0805|C39|GRM216R71H103KA01D|1|MuRata|0805|0.01uF
12|Fitted|CAP, CERM, 100 µF, 10 V, +/- 20%, X5R, 1206_190|C40|C3216X5R1A107M160AC|1|TDK|1206_190|100uF
13|Fitted|CAP, CERM, 0.1 µF, 25 V, +/- 20%, X7R, 0402|C41|C1005X7R1E104M050BB|1|TDK|0402|0.1uF
14|Fitted|CAP, CERM, 0.1 µF, 100 V, +/- 10%, X7R, 0603|C43, C44|GRM188R72A104KA35D|2|MuRata|0603|0.1uF
15|Fitted|CAP, CERM, 1 µF, 10 V, +/- 10%, X7R, 0603|C46|GRM188R71A105KA61D|1|MuRata|0603|1uF
16|Fitted|CAP, CERM, 1 µF, 10 V, +/- 10%, X7S, AEC-Q200 Grade 1, 0402|C48|GCM155C71A105KE38D|1|MuRata|0402|1uF
17|Fitted|CAP, CERM, 100 µF, 6.3 V, +/- 20%, X5R, 1206|C49|GRM31CR60J107ME39L|1|MuRata|1206|100uF
18|Fitted|CAP, CERM, 0.033 µF, 10 V, +/- 10%, X7R, 0402|C51, C55, C57, C60|GRM155R71A333KA01D|4|MuRata|0402|0.033uF
19|Fitted|CAP, CERM, 0.1 µF, 16 V, +/- 10%, X7R, 0603|C53, C58, C61, C62, C64|GRM188R71C104KA01D|5|MuRata|0603|0.1uF
20|Fitted|Diode, Schottky, 70 V, 0.07 A, SOD-523|D1, D2, D3, D4|1PS79SB70,115|4|NXP Semiconductor|SOD-523|70V
21|Fitted|LED, Green, SMD|D5, D6|150060GS75000|2|Wurth Elektronik|LED_0603|Green
22|Fitted|TERM BLOCK PLUG 2POS 5.08MM|H1|691352510002|1|Wurth Elektronik||
23|Fitted|Connector, Receptacle, 100mil, 10x2, Gold plated, TH|J1, J2|SSW-110-23-F-D|2|Samtec|10x2 Receptacle|
24|Fitted|Terminal Block, 3x1, 5.08 mm, Tin, TH|J3|OSTTC032162|1|On-Shore Technology|Terminal Block, 3x1, 5.08 mm, TH|
25|Fitted|Terminal Block, 2-pole, 200mil, TH|J4|OSTTC022162|1|On-Shore Technology|THD, 2-Leads, Body 10.16x7.6mm, Pitch 5.08mm|
26|Fitted|Header, 100mil, 2x1, Tin, TH|J5, J6|PEC02SAAN|2|Sullins Connector Solutions|Header, 2 PIN, 100mil, Tin|
27|Fitted|Inductor, Shielded Drum Core, Ferrite, 470 µH, 1.4 A, 0.56 ohm, SMD|L1|7447709471|1|Wurth Elektronik|SMD|470uH
28|Fitted|Inductor, Shielded, Ferrite, 33 µH, 0.085 A, 1.4 ohm, SMD|L2|NLFV25T-330K-PF|1|TDK|2.5x1.8x2mm|33uH
29|Fitted|Ferrite Bead, 300 ohm @ 100 MHz, 0.2 A, 0402|L3|74279272|1|Wurth Elektronik|0402|300 ohm
30|Fitted|Thermal Transfer Printable Labels, 0.650" W x 0.200" H - 10,000 per roll|LBL1|THT-14-423-10|1|Brady|PCB Label 0.650"H x 0.200"W|
31|Fitted|RES, 0, 5%, 0.1 W, 0603|R1, R2, R54|MCR03EZPJ000|3|Rohm|0603|0
32|Fitted|RES, 0, 5%, 0.063 W, 0402|R3, R4, R9, R22, R46, R47, R49, R57, R58, R60, R63, R64, R68, R71, R72, R75, R76|CRCW04020000Z0ED|17|Vishay-Dale|0402|0
33|Fitted|RES, 20.0, 1%, 0.063 W, 0402|R5, R6, R7, R8, R10, R11|CRCW040220R0FKED|6|Vishay-Dale|0402|20.0
34|Fitted|RES, 20, 5%, 0.063 W, 0402|R12, R13, R14, R15, R16, R17, R18, R19, R20|CRCW040220R0JNED|9|Vishay-Dale|0402|20
35|Fitted|RES, 10 k, 5%, 0.063 W, 0402|R21, R24, R25, R26, R27, R28, R29, R30, R31, R32, R33, R34, R35, R36, R37, R38|CRCW040210K0JNED|16|Vishay-Dale|0402|10k
36|Fitted|RES, 1.2 k, 5%, 0.063 W, 0402|R39|CRCW04021K20JNED|1|Vishay-Dale|0402|1.2k
37|Fitted|RES, 470 k, 5%, 0.063 W, 0402|R40|CRCW0402470KJNED|1|Vishay-Dale|0402|470k
38|Fitted|RES, 10.0 k, 1%, 0.063 W, 0402|R41, R48|CRCW040210K0FKED|2|Vishay-Dale|0402|10.0k
39|Fitted|RES, 510 k, 1%, 0.1 W, 0603|R42|RC0603FR-07510KL|1|Yageo America|0603|510k
40|Fitted|RES, 100 k, 5%, 0.1 W, 0603|R43|CRCW0603100KJNEA|1|Vishay-Dale|0603|100k
41|Fitted|RES, 3.24 k, 1%, 0.063 W, 0402|R44|CRCW04023K24FKED|1|Vishay-Dale|0402|3.24k
42|Fitted|RES, 20 k, 5%, 0.063 W, 0402|R45|CRCW040220K0JNED|1|Vishay-Dale|0402|20k
43|Fitted|RES, 820, 5%, 0.063 W, 0402|R50|CRCW0402820RJNED|1|Vishay-Dale|0402|820
44|Fitted|RES, 0.005, 1%, 3 W, AEC-Q200 Grade 0, 2512|R55, R61, R69|CRE2512-FZ-R005E-3|3|Bourns|2512|0.005
45|Fitted|RES, 100 k, 1%, 0.063 W, 0402|R56, R62, R66, R70|CRCW0402100KFKED|4|Vishay-Dale|0402|100k
46|Fitted|RES, 4.22 k, 1%, 0.063 W, 0402|R59, R65, R67, R74|CRCW04024K22FKED|4|Vishay-Dale|0402|4.22k
47|Fitted|Test Point, Miniature, Black, TH|TP1, TP2|5001|2|Keystone|Black Miniature Testpoint|
48|Fitted|100V GaN Half Bridge Power Module, MOF0009A|U1, U2, U3|LMG5200MOFT|3|Texas Instruments|MOF0009A|
49|Fitted|8-BIT DUAL-SUPPLY BUS TRANSCEIVER WITH CONFIGURABLE VOLTAGE TRANSLATION AND 3-STATE OUTPUTS, RHL0024A|U4|SN74AVC8T245RHLR|1|Texas Instruments|RHL0024A|
50|Fitted|100V, 300mA Constant On-Time Synchronous Buck Regulator, DDA0008B|U5|LM5018MRX/NOPB|1|Texas Instruments|DDA0008B|
51|Fitted|Automotive Grade, Low-Power, Easy-to-Use, Temperature Switch in MicroPackage, DRL0006A|U6|TMP302BQDRLRQ1|1|Texas Instruments|DRL0006A|
52|Fitted|500mA Low Dropout CMOS Linear Regulators Stable with Ceramic Output Capacitors, 6-pin LLP, Pb-Free|U7|LP38691SD-3.3/NOPB|1|Texas Instruments|SDE06A|
53|Fitted|Wide Common-Mode Range, Voltage Output, High or Low-Side Bi-Directional Zero-Drift Current Shunt Monitor, PW0008A|U8, U9, U11|INA240A1PW|3|Texas Instruments|PW0008A|
54|Fitted|30 ppm / degC Drift, 3.9 uA Voltage Reference, -40 to 125 degC, 3-pin SOT-23 (DBZ), Green (RoHS & no Sb/Br)|U10|REF3333AIDBZR|1|Texas Instruments|DBZ0003A|
55|Not Fitted|CAP, CERM, 1500 pF, 25 V, +/- 5%, C0G/NP0, 0402|C52, C56, C63|C0402H152J3GAC7867|0|Kemet|0402|1500pF
56|Not Fitted|Fiducial mark.  There is nothing to buy or mount.|FID1, FID2, FID3|N/A|0|N/A|Fiducial|
57|Not Fitted|RES, 0, 5%, 0.063 W, 0402|R23, R51, R52, R73|CRCW04020000Z0ED|0|Vishay-Dale|0402|0
58|Not Fitted|RES, 0, 5%, 0.1 W, 0603|R53|MCR03EZPJ000|0|Rohm|0603|0
