OVP SC OTP TO DN IF IP RFU Default: 0 0 0 0 X 0 0 0

Definition: