                                                                   January 19, 2009
 TEXAS INSTRUMENTS
   3535 40th Ave. NW, Suite 103
   ValleyHigh Business Center
   ROCHESTER, MN 55901


   Texas Instruments	
   PART NO. CC1110LNA for Codec
   REV. B


 PCB DESCRIPTION: 4 LAYER PCB, .062" NOMINAL THICKNESS FR4 WITH 1OZ COPPER PER LAYER.

  
 Board layer stack-up: 
 Layer 1 - layer 2 .0122" nominal
 Layer 2 - layer 3 .028" nominal core
 Layer 3 - layer 4 .0122" nominal
 
  
 THIS ARCHIVED (WINZIP) FILE "CC1110LNA for Codec RevB.ZIP" CONTAINS 26 FILES.

   CC1110LNA for Codec.GTO = TOP SILKSCREEN GERBER FILE
   CC1110LNA for Codec.GTS = TOP SOLDER MASK GERBER FILE
   CC1110LNA for Codec.GTL = LAYER 1 TOP SIGNAL GERBER FILE
   CC1110LNA for Codec.GP1 = LAYER 2 INTERNAL GROUND PLANE GERBER FILE
   CC1110LNA for Codec.GP2 = LAYER 3 INTERNAL POWER PLANE GERBER FILE
   CC1110LNA for Codec.GBL = LAYER 4 BOTTOM SIGNAL GERBER FILE
   CC1110LNA for Codec.GBS = BOTTOM SOLDER MASK GERBER FILE
   CC1110LNA for Codec.GTP = TOP SOLDER PASTE STENCIL GERBER FILE
   CC1110LNA for Codec.GBP = BOTTOM SOLDER PASTE STENCIL GERBER FILE
   CC1110LNA for Codec.GG1 = DRILL GUIDE GERBER FILE
   CC1110LNA for Codec.GD1 = DRILL DRAWING GERBER FILE
   CC1110LNA for Codec.GM4 = BOARD OUTLINE GERBER FILE
   CC1110LNA for Codec.GM3 = FAB DIMENSION GERBER FILE (SLOT CALLOUT)
   CC1110LNA for Codec.DRR = DRILL SIZE REPORT
   CC1110LNA for Codec.DRL = NC DRILL BINARY FILE
   CC1110LNA for Codec.TXT = NC DRILL FILE
   CC1110LNA for Codec.GM1 = TOP ASSEMBLY DRAWING GERBER FILE
   CC1110LNA for Codec.GM5 = BOTTOM ASSEMBLY DRAWING GERBER FILE
   CC1110LNA for Codec.APR = APERTURE FILE
   CC1110LNA for Codec ASCII.PCB = BOARD DESIGN IN PROTEL PCB V2.8 ASCII FORMAT
   CC1110LNA for Codec BOM REVB.XLS = BILL OF MATERIALS
   PICK PLACE FOR CC1110LNA for Codec.XLS = PICK AND PLACE SPREADSHEET
   README.TXT = THIS FILE
   CC1110LNA for Codec Schematic RevB.pdf = SCHEMATIC IN PDF FORMAT
   CC1110LNA for Codec Artwork RevB.pdf = ARTWORK IN PDF FORMAT
   CC1110LNA for Codec.DDB = PROTEL DESIGN EXPLORER 99SE DESIGN DATABASE 

READ.ME
