DRC Rules Export File for PCB: C:\1\From2024_4\2025\4-9-4-14\EIS\TIDA-010990-version II\TIDA-010990-Mutiple port DAB.PcbDoc
RuleKind=Clearance|RuleName=Clearance_14|Scope=Board|Minimum=177.17
RuleKind=Clearance|RuleName=Clearance_13|Scope=Board|Minimum=19.69
RuleKind=Clearance|RuleName=Clearance_12|Scope=Board|Minimum=27.56
RuleKind=Clearance|RuleName=Clearance_11|Scope=Board|Minimum=59.06
RuleKind=Clearance|RuleName=Clearance_9|Scope=Board|Minimum=59.06
RuleKind=Clearance|RuleName=Clearance_10|Scope=Board|Minimum=59.06
RuleKind=Clearance|RuleName=Clearance_8|Scope=Board|Minimum=39.37
RuleKind=Clearance|RuleName=Clearance_7|Scope=Board|Minimum=39.37
RuleKind=Clearance|RuleName=Clearance_6|Scope=Board|Minimum=39.37
RuleKind=Clearance|RuleName=Clearance_5|Scope=Board|Minimum=31.50
RuleKind=Clearance|RuleName=Clearance_4|Scope=Board|Minimum=7.87
RuleKind=Clearance|RuleName=Clearance_3|Scope=Board|Minimum=196.85
RuleKind=Clearance|RuleName=Clearance_2|Scope=Board|Minimum=236.22
RuleKind=Clearance|RuleName=Clearance_1|Scope=Board|Minimum=472.44
RuleKind=MinimumAnnularRing|RuleName=MinimumAnnularRing|Scope=Board|Minimum=7.87
RuleKind=MinimumAnnularRing|RuleName=MinimumAnnularRing_ThermalPadVias|Scope=Board|Minimum=5.91
RuleKind=ShortCircuit|RuleName=ShortCircuit|Scope=Board|Allowed=0
RuleKind=SolderMaskExpansion|RuleName=SolderMaskExpansion|Scope=Board|Minimum=1.97
RuleKind=Width|RuleName=Width|Scope=Board|Minimum=6.00
RuleKind=Clearance|RuleName=Clearance|Scope=Board|Minimum=472.44
RuleKind=Clearance|RuleName=Clearance_FiducialMark|Scope=Board|Minimum=10.00
RuleKind=Clearance|RuleName=Clearance_Poly|Scope=Board|Minimum=19.69
RuleKind=Clearance|RuleName=Clearance_Keepouts|Scope=Board|Minimum=0.00
