Field=#~Integer~#~50|Field=Fitted~String~Fitted~125|Field=Description~String~Description~125|Field=Designator~String~Designator~125|Field=LibRef~String~LibRef~125|Field=PartNumber~String~PartNumber~125|Field=Quantity~Integer~Quantity~125|Field=Library Name~String~Library Name~125|Field=Manufacturer~String~Manufacturer~125|Field=RoHS~String~RoHS~125|Field=Supplier 1~String~Supplier 1~125|Field=Supplier Part Number 1~String~Supplier Part Number 1~125|Field=Supplier 2~String~Supplier 2~125|Field=Supplier Part Number 2~String~Supplier Part Number 2~125|ReportField=Currency~<none>|ReportField=ProductionQuantity~1|ReportField=ProjectFileName~TIDA-050030.PrjPcb|ReportField=ProjectFullPath~Z:\pcbs\LPP EVM ARCHIVE\TIDA_Numbers\TIDA-050030\TIDA-050030.PrjPcb|ReportField=Title~Engineering Bill of Materials For Variant [001] of Project [TIDA-050030.PrjPcb] (No PCB Document Selected)|ReportField=ReportTime~3:55:10 PM|ReportField=ReportDate~10/10/2019|ReportField=ReportDateTime~10/10/2019 3:55:10 PM|ReportField=OutputName~Engineering Bill of Materials|ReportField=OutputType~BOM_PartType|ReportField=GeneratorName~BOM|ReportField=GeneratorDescription~Bill of Materials|ReportField=VariantName~001|ReportField=TotalQuantity~301|ReportField=TotalActualPrice~0|ReportField=TotalTargetPrice~0|ReportField=VersionControl_RevNumber~|ReportField=VersionControl_ProjFolderRevNumber~|ReportField=EVM_Orderable~ChangeMe in variant|ReportField=CopyrightYear~2018|ReportField=PCB_Layout~Aaron Hanson|ReportField=PCB_Rev~E2|ReportField=PRJ_Customer~Public Release|ReportField=PRJ_Engineer~Nederbragt, Irwin|ReportField=PRJ_Number~TIDA-050030|ReportField=PRJ_Title~Change in menu Project:Project Options:Parameters|ReportField=SCH_Rev~E2|ReportField=TechSupport~http://www.ti.com/support|ReportField=TID~N/A|ReportField=Address1~Not shown in title block|ReportField=Address2~Not shown in title block|ReportField=Address3~Not shown in title block|ReportField=Address4~Not shown in title block|ReportField=Application_BuildNumber~|ReportField=ApprovedBy~Not shown in title block|ReportField=Author~Not shown in title block|ReportField=CheckedBy~Not shown in title block|ReportField=CompanyName~Not shown in title block|ReportField=ConfigurationParameters~|ReportField=ConfiguratorName~|ReportField=CurrentDate~10/10/2019|ReportField=CurrentTime~3:25:06 PM|ReportField=Date~Not shown in title block|ReportField=DocumentFullPathAndName~Z:\pcbs\LPP EVM ARCHIVE\TIDA_Numbers\TIDA-050030\TIDA-050030_Battery.SchDoc|ReportField=DocumentName~TIDA-050030_Battery.SchDoc|ReportField=DocumentNumber~1|ReportField=DrawnBy~|ReportField=Engineer~Not shown in title block|ReportField=ImagePath~Not shown in title block|ReportField=IsUserConfigurable~|ReportField=ModifiedDate~10/10/2019|ReportField=Organization~Not shown in title block|ReportField=PageSetup~Record=PageOptions:CenterHorizontal=True:CenterVertical=True:PrintScale=1.00:XCorrection=1.00:YCorrection=1.00:PrintKind=0:BorderSize=5000000:LeftOffset=0:BottomOffset=0:Orientation=2:PaperLength=1000:PaperWidth=1000:Scale=100:PaperSource=15:PrintQuality=600:MediaType=1:DitherType=10:PaperKind=Letter:PrintScaleMode=1|ReportField=ProjectName~TIDA-050030.PrjPcb|ReportField=Revision~Use project parameter SCH_Rev|ReportField=Rule~|ReportField=SheetNumber~1|ReportField=SheetTotal~8|ReportField=Time~Not shown in title block|ReportField=Title~|ReportField=VersionControl_ProjFolderRevNumber~|ReportField=VersionControl_RevNumber~|ReportField=DataSourceFileName~TIDA-050030.PrjPcb|ReportField=DataSourceFullPath~Z:\pcbs\LPP EVM ARCHIVE\TIDA_Numbers\TIDA-050030\TIDA-050030.PrjPcb|ReportField=PCBConfigurationName~Sources|ReportField=Item~|ReportField=ItemRevision~|ReportField=ItemAndRevision~|ReportField=ItemRevisionBase~|ReportField=ItemRevisionLevel1~|ReportField=ItemRevisionLevel2~|ReportField=ItemRevisionLevel1AndBase~|ReportField=ItemRevisionLevel2AndLevel1~
1|Fitted|Printed Circuit Board|!PCB1|CMP-0003618-2|TIDA-050030|1|Altium Vault - TI|Any|O||{URL}{URL.TEXT}{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
2|Fitted|CAP, CERM, 0.01 uF, 50 V, +/- 10%, X7R, AEC-Q200 Grade 1, 0603|C1|CMP-0007143-4|GCM188R71H103KA37D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}490-4778-1-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}45Y5166{URL.TIP}Supplier
3|Fitted|CAP, CERM, 0.01 uF, 50 V, +/- 10%, X7R, AEC-Q200 Grade 1, 0603|C2|CMP-0007143-4|GCM188R71H103KA37D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}490-4778-1-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}45Y5166{URL.TIP}Supplier
4|Fitted|CAP, AL, 220 µF, 50 V, +/- 20%, AEC-Q200 Grade 2, SMD|C3|CMP-0086092-1|EMZR500ARA221MHA0G|1|Altium Vault - TI|Chemi-Con|Y||{URL}{URL.TEXT}{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
5|Fitted|CAP, CERM, 0.1 uF, 50 V, +/- 10%, X7R, AEC-Q200 Grade 0, 0805|C4|CMP-0007725-2|C0805C104K5RACAUTO|1|Altium Vault - TI|Kemet|Y|Digi-Key|{URL}{URL.TEXT}399-6928-1-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}86T2620{URL.TIP}Supplier
6|Fitted|CAP, CERM, 4.7 uF, 50 V, +/- 10%, X7R, 1206|C5|CMP-0008702-2|C3216X7R1H475K160AC|1|Altium Vault - TI|TDK|Y|Digi-Key|{URL}{URL.TEXT}445-8032-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}810-C3216X7R1H475K160AC{URL.TIP}Supplier
7|Fitted|CAP, CERM, 0.1 uF, 50 V, +/- 10%, X7R, AEC-Q200 Grade 0, 0805|C6|CMP-0007725-2|C0805C104K5RACAUTO|1|Altium Vault - TI|Kemet|Y|Digi-Key|{URL}{URL.TEXT}399-6928-1-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}86T2620{URL.TIP}Supplier
8|Fitted|CAP, CERM, 10 uF, 50 V, +/- 10%, X7S, AEC-Q200 Grade 1, 1210|C7|CMP-0009164-2|CGA6P3X7S1H106K250AB|1|Altium Vault - TI|TDK|Y|Digi-Key|{URL}{URL.TEXT}445-7004-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}810-CGA6P3X7S1H106K250AB{URL.TIP}Supplier
9|Fitted|CAP, CERM, 10 uF, 50 V, +/- 10%, X7S, AEC-Q200 Grade 1, 1210|C8|CMP-0009164-2|CGA6P3X7S1H106K250AB|1|Altium Vault - TI|TDK|Y|Digi-Key|{URL}{URL.TEXT}445-7004-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}810-CGA6P3X7S1H106K250AB{URL.TIP}Supplier
10|Fitted|CAP, CERM, 10 uF, 50 V, +/- 10%, X7S, AEC-Q200 Grade 1, 1210|C9|CMP-0009164-2|CGA6P3X7S1H106K250AB|1|Altium Vault - TI|TDK|Y|Digi-Key|{URL}{URL.TEXT}445-7004-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}810-CGA6P3X7S1H106K250AB{URL.TIP}Supplier
11|Fitted|CAP, CERM, 10 uF, 50 V, +/- 10%, X7S, AEC-Q200 Grade 1, 1210|C10|CMP-0009164-2|CGA6P3X7S1H106K250AB|1|Altium Vault - TI|TDK|Y|Digi-Key|{URL}{URL.TEXT}445-7004-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}810-CGA6P3X7S1H106K250AB{URL.TIP}Supplier
12|Fitted|CAP, CERM, 0.1 uF, 50 V, +/- 10%, X7R, AEC-Q200 Grade 0, 0805|C11|CMP-0007725-2|C0805C104K5RACAUTO|1|Altium Vault - TI|Kemet|Y|Digi-Key|{URL}{URL.TEXT}399-6928-1-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}86T2620{URL.TIP}Supplier
13|Fitted|CAP, CERM, 10 uF, 50 V, +/- 10%, X7S, AEC-Q200 Grade 1, 1210|C12|CMP-0009164-2|CGA6P3X7S1H106K250AB|1|Altium Vault - TI|TDK|Y|Digi-Key|{URL}{URL.TEXT}445-7004-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}810-CGA6P3X7S1H106K250AB{URL.TIP}Supplier
14|Fitted|CAP, AL, 33 uF, 80 V, +/- 20%, 1.3 ohm, AEC-Q200 Grade 2, SMD|C14|CMP-0011198-2|EEE-FK1K330P|1|Altium Vault - TI|Panasonic|Y|Digi-Key|{URL}{URL.TEXT}PCE3829CT-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}667-EEE-FK1K330P{URL.TIP}Supplier
15|Fitted|CAP, CERM, 4.7 uF, 50 V, +/- 10%, X7R, 1206|C16|CMP-0008702-2|C3216X7R1H475K160AC|1|Altium Vault - TI|TDK|Y|Digi-Key|{URL}{URL.TEXT}445-8032-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}810-C3216X7R1H475K160AC{URL.TIP}Supplier
16|Fitted|CAP, CERM, 4.7 uF, 50 V, +/- 10%, X7R, 1206|C17|CMP-0008702-2|C3216X7R1H475K160AC|1|Altium Vault - TI|TDK|Y|Digi-Key|{URL}{URL.TEXT}445-8032-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}810-C3216X7R1H475K160AC{URL.TIP}Supplier
17|Fitted|CAP, CERM, 0.033 uF, 50 V, +/- 10%, X7R, 0603|C18|CMP-0007451-4|GRM188R71H333KA61D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}490-3286-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}81-GRM188R71H333KA61{URL.TIP}Supplier
18|Fitted|CAP, CERM, 4.7 uF, 100 V, +/- 10%, X7S, AEC-Q200 Grade 1, 1210|C19|CMP-0009150-2|CGA6M3X7S2A475K200AB|1|Altium Vault - TI|TDK|Y|Digi-Key|{URL}{URL.TEXT}445-7005-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}810-CGA6M3X7S2A475K200AB{URL.TIP}Supplier
19|Fitted|CAP, CERM, 4.7 uF, 100 V, +/- 10%, X7S, AEC-Q200 Grade 1, 1210|C20|CMP-0009150-2|CGA6M3X7S2A475K200AB|1|Altium Vault - TI|TDK|Y|Digi-Key|{URL}{URL.TEXT}445-7005-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}810-CGA6M3X7S2A475K200AB{URL.TIP}Supplier
20|Fitted|CAP, CERM, 4.7 uF, 100 V, +/- 10%, X7S, AEC-Q200 Grade 1, 1210|C21|CMP-0009150-2|CGA6M3X7S2A475K200AB|1|Altium Vault - TI|TDK|Y|Digi-Key|{URL}{URL.TEXT}445-7005-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}810-CGA6M3X7S2A475K200AB{URL.TIP}Supplier
21|Fitted|CAP, CERM, 4.7 uF, 100 V, +/- 10%, X7S, AEC-Q200 Grade 1, 1210|C22|CMP-0009150-2|CGA6M3X7S2A475K200AB|1|Altium Vault - TI|TDK|Y|Digi-Key|{URL}{URL.TEXT}445-7005-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}810-CGA6M3X7S2A475K200AB{URL.TIP}Supplier
22|Fitted|CAP, CERM, 10 pF, 50 V, +/- 5%, C0G/NP0, 0603|C23|CMP-0007170-4|GRM1885C1H100JA01D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}490-1403-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}81-GRM39C100D50{URL.TIP}Supplier
23|Fitted|CAP, CERM, 1 uF, 50 V, +/- 10%, X7R, AEC-Q200 Grade 1, 1206|C24|CMP-0008786-2|CGA5L3X7R1H105K160AB|1|Altium Vault - TI|TDK|Y|Digi-Key|{URL}{URL.TEXT}445-5702-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}810-CGA5L3X7R1H105K160AB{URL.TIP}Supplier
24|Fitted|CAP, CERM, 470 pF, 100 V, +/- 5%, C0G/NP0, 0603|C25|CMP-0007272-4|GRM1885C2A471JA01D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}490-1367-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}81-GRM185C2A471JA01D{URL.TIP}Supplier
25|Fitted|CAP, CERM, 1000 pF, 50 V, +/- 10%, X7R, 0603|C26|CMP-0006976-5|C0603X102K5RACTU|1|Altium Vault - TI|Kemet|Y|Digi-Key|{URL}{URL.TEXT}399-5348-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}80-C0603X102K5R{URL.TIP}Supplier
26|Fitted|CAP, CERM, 100 pF, 50 V, +/- 5%, C0G/NP0, AEC-Q200 Grade 0, 0603|C27|CMP-0007075-4|CGA3E2NP01H101J080AA|1|Altium Vault - TI|TDK|Y|Digi-Key|{URL}{URL.TEXT}445-12386-1-ND{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
27|Fitted|CAP, AL, 33 uF, 80 V, +/- 20%, 1.3 ohm, AEC-Q200 Grade 2, SMD|C28|CMP-0011198-2|EEE-FK1K330P|1|Altium Vault - TI|Panasonic|Y|Digi-Key|{URL}{URL.TEXT}PCE3829CT-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}667-EEE-FK1K330P{URL.TIP}Supplier
28|Fitted|CAP, CERM, 4.7 uF, 50 V, +/- 10%, X7R, 1206|C30|CMP-0008702-2|C3216X7R1H475K160AC|1|Altium Vault - TI|TDK|Y|Digi-Key|{URL}{URL.TEXT}445-8032-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}810-C3216X7R1H475K160AC{URL.TIP}Supplier
29|Fitted|CAP, CERM, 4.7 uF, 50 V, +/- 10%, X7R, 1206|C31|CMP-0008702-2|C3216X7R1H475K160AC|1|Altium Vault - TI|TDK|Y|Digi-Key|{URL}{URL.TEXT}445-8032-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}810-C3216X7R1H475K160AC{URL.TIP}Supplier
30|Fitted|CAP, CERM, 4.7 uF, 100 V, +/- 10%, X7S, AEC-Q200 Grade 1, 1210|C32|CMP-0009150-2|CGA6M3X7S2A475K200AB|1|Altium Vault - TI|TDK|Y|Digi-Key|{URL}{URL.TEXT}445-7005-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}810-CGA6M3X7S2A475K200AB{URL.TIP}Supplier
31|Fitted|CAP, CERM, 4.7 uF, 100 V, +/- 10%, X7S, AEC-Q200 Grade 1, 1210|C33|CMP-0009150-2|CGA6M3X7S2A475K200AB|1|Altium Vault - TI|TDK|Y|Digi-Key|{URL}{URL.TEXT}445-7005-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}810-CGA6M3X7S2A475K200AB{URL.TIP}Supplier
32|Fitted|CAP, CERM, 4.7 uF, 100 V, +/- 10%, X7S, AEC-Q200 Grade 1, 1210|C34|CMP-0009150-2|CGA6M3X7S2A475K200AB|1|Altium Vault - TI|TDK|Y|Digi-Key|{URL}{URL.TEXT}445-7005-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}810-CGA6M3X7S2A475K200AB{URL.TIP}Supplier
33|Fitted|CAP, CERM, 4.7 uF, 100 V, +/- 10%, X7S, AEC-Q200 Grade 1, 1210|C35|CMP-0009150-2|CGA6M3X7S2A475K200AB|1|Altium Vault - TI|TDK|Y|Digi-Key|{URL}{URL.TEXT}445-7005-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}810-CGA6M3X7S2A475K200AB{URL.TIP}Supplier
34|Fitted|CAP, CERM, 470 pF, 100 V, +/- 5%, C0G/NP0, 0603|C36|CMP-0007272-4|GRM1885C2A471JA01D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}490-1367-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}81-GRM185C2A471JA01D{URL.TIP}Supplier
35|Fitted|CAP, CERM, 2.2 uF, 16 V, +/- 10%, X7R, 0603|C37|CMP-0007499-4|GRM188Z71C225KE43|1|Altium Vault - TI|MuRata|Y|Mouser|{URL}{URL.TEXT}81-GRM188Z71C225KE3D{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
36|Fitted|CAP, CERM, 1000 pF, 50 V, +/- 10%, X7R, 0603|C38|CMP-0006976-5|C0603X102K5RACTU|1|Altium Vault - TI|Kemet|Y|Digi-Key|{URL}{URL.TEXT}399-5348-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}80-C0603X102K5R{URL.TIP}Supplier
37|Fitted|CAP, CERM, 2.2 uF, 16 V, +/- 10%, X7R, 0603|C39|CMP-0007499-4|GRM188Z71C225KE43|1|Altium Vault - TI|MuRata|Y|Mouser|{URL}{URL.TEXT}81-GRM188Z71C225KE3D{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
38|Fitted|CAP, CERM, 10 pF, 50 V, +/- 5%, C0G/NP0, 0603|C40|CMP-0007170-4|GRM1885C1H100JA01D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}490-1403-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}81-GRM39C100D50{URL.TIP}Supplier
39|Fitted|CAP, CERM, 0.1 uF, 100 V, +/- 10%, X7S, AEC-Q200 Grade 1, 0603|C41|CMP-0007099-4|CGA3E3X7S2A104K080AB|1|Altium Vault - TI|TDK|Y|Digi-Key|{URL}{URL.TEXT}445-6938-1-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}04X3163{URL.TIP}Supplier
40|Fitted|CAP, CERM, 2200 pF, 16 V, +/- 10%, X7R, 0603|C42|CMP-0007387-4|GRM188R71C222KA01D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}GRM188R71C222KA01D-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}81-GRM188R71C222KA1D{URL.TIP}Supplier
41|Fitted|CAP, CERM, 0.1 uF, 25 V, +/- 10%, X7R, AEC-Q200 Grade 1, 0603|C43|CMP-0007077-5|CGA3E2X7R1E104K080AA|1|Altium Vault - TI|TDK|Y|Digi-Key|{URL}{URL.TEXT}445-5667-1-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}79Y4100{URL.TIP}Supplier
42|Fitted|CAP, CERM, 1000 pF, 100 V, +/- 10%, X7R, 0603|C44|CMP-0007467-4|GRM188R72A102KA01D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}490-1472-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}81-GRM18R72A102KA01D{URL.TIP}Supplier
43|Fitted|CAP, CERM, 1.5 uF, 100 V, +/- 10%, X7R, AEC-Q200 Grade 1, 1210|C45|CMP-0009148-2|CGA6M3X7R2A155K200AB|1|Altium Vault - TI|TDK|Y|Digi-Key|{URL}{URL.TEXT}445-13014-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}810-CGA6M3X7R2A155K200AB{URL.TIP}Supplier
44|Fitted|CAP, CERM, 1 uF, 16 V, +/- 10%, X7R, AEC-Q200 Grade 1, 0603|C46|CMP-0007136-5|GCM188R71C105KA64D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}490-5241-6-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}81-GCM188R71C105K64D{URL.TIP}Supplier
45|Fitted|CAP, CERM, 0.1 µF, 16 V,+/- 10%, X7R, 0603|C47|CMP-0085536-1|CL10B104KO8WPNC|1|Altium Vault - TI|Samsung Electro-Mechanics|Y||{URL}{URL.TEXT}{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
46|Fitted|CAP, CERM, 1 uF, 16 V, +/- 10%, X7R, AEC-Q200 Grade 1, 0603|C48|CMP-0007136-5|GCM188R71C105KA64D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}490-5241-6-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}81-GCM188R71C105K64D{URL.TIP}Supplier
47|Fitted|CAP, CERM, 0.1 µF, 16 V,+/- 10%, X7R, 0603|C49|CMP-0085536-1|CL10B104KO8WPNC|1|Altium Vault - TI|Samsung Electro-Mechanics|Y||{URL}{URL.TEXT}{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
48|Fitted|CAP, CERM, 0.1 µF, 16 V,+/- 10%, X7R, 0603|C50|CMP-0085536-1|CL10B104KO8WPNC|1|Altium Vault - TI|Samsung Electro-Mechanics|Y||{URL}{URL.TEXT}{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
49|Fitted|CAP, CERM, 1.5 uF, 100 V, +/- 10%, X7R, AEC-Q200 Grade 1, 1210|C51|CMP-0009148-2|CGA6M3X7R2A155K200AB|1|Altium Vault - TI|TDK|Y|Digi-Key|{URL}{URL.TEXT}445-13014-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}810-CGA6M3X7R2A155K200AB{URL.TIP}Supplier
50|Fitted|CAP, CERM, 0.1 uF, 25 V, +/- 10%, X7R, AEC-Q200 Grade 1, 0603|C52|CMP-0007077-5|CGA3E2X7R1E104K080AA|1|Altium Vault - TI|TDK|Y|Digi-Key|{URL}{URL.TEXT}445-5667-1-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}79Y4100{URL.TIP}Supplier
51|Fitted|CAP, CERM, 1000 pF, 100 V, +/- 10%, X7R, 0603|C53|CMP-0007467-4|GRM188R72A102KA01D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}490-1472-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}81-GRM18R72A102KA01D{URL.TIP}Supplier
52|Fitted|CAP, CERM, 2200 pF, 16 V, +/- 10%, X7R, 0603|C54|CMP-0007387-4|GRM188R71C222KA01D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}GRM188R71C222KA01D-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}81-GRM188R71C222KA1D{URL.TIP}Supplier
53|Fitted|CAP, CERM, 0.1 uF, 100 V, +/- 10%, X7S, AEC-Q200 Grade 1, 0603|C55|CMP-0007099-4|CGA3E3X7S2A104K080AB|1|Altium Vault - TI|TDK|Y|Digi-Key|{URL}{URL.TEXT}445-6938-1-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}04X3163{URL.TIP}Supplier
54|Fitted|CAP, CERM, 0.1 uF, 100 V, +/- 10%, X7S, AEC-Q200 Grade 1, 0603|C56|CMP-0007099-4|CGA3E3X7S2A104K080AB|1|Altium Vault - TI|TDK|Y|Digi-Key|{URL}{URL.TEXT}445-6938-1-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}04X3163{URL.TIP}Supplier
55|Fitted|CAP, CERM, 2200 pF, 16 V, +/- 10%, X7R, 0603|C57|CMP-0007387-4|GRM188R71C222KA01D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}GRM188R71C222KA01D-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}81-GRM188R71C222KA1D{URL.TIP}Supplier
56|Fitted|CAP, CERM, 1000 pF, 100 V, +/- 10%, X7R, 0603|C58|CMP-0007467-4|GRM188R72A102KA01D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}490-1472-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}81-GRM18R72A102KA01D{URL.TIP}Supplier
57|Fitted|CAP, CERM, 0.1 uF, 25 V, +/- 10%, X7R, AEC-Q200 Grade 1, 0603|C59|CMP-0007077-5|CGA3E2X7R1E104K080AA|1|Altium Vault - TI|TDK|Y|Digi-Key|{URL}{URL.TEXT}445-5667-1-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}79Y4100{URL.TIP}Supplier
58|Fitted|CAP, CERM, 1.5 uF, 100 V, +/- 10%, X7R, AEC-Q200 Grade 1, 1210|C60|CMP-0009148-2|CGA6M3X7R2A155K200AB|1|Altium Vault - TI|TDK|Y|Digi-Key|{URL}{URL.TEXT}445-13014-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}810-CGA6M3X7R2A155K200AB{URL.TIP}Supplier
59|Fitted|CAP, CERM, 1 uF, 16 V, +/- 10%, X7R, AEC-Q200 Grade 1, 0603|C61|CMP-0007136-5|GCM188R71C105KA64D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}490-5241-6-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}81-GCM188R71C105K64D{URL.TIP}Supplier
60|Fitted|CAP, CERM, 0.1 µF, 16 V,+/- 10%, X7R, 0603|C62|CMP-0085536-1|CL10B104KO8WPNC|1|Altium Vault - TI|Samsung Electro-Mechanics|Y||{URL}{URL.TEXT}{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
61|Fitted|CAP, CERM, 1 uF, 16 V, +/- 10%, X7R, AEC-Q200 Grade 1, 0603|C63|CMP-0007136-5|GCM188R71C105KA64D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}490-5241-6-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}81-GCM188R71C105K64D{URL.TIP}Supplier
62|Fitted|CAP, CERM, 0.1 µF, 16 V,+/- 10%, X7R, 0603|C64|CMP-0085536-1|CL10B104KO8WPNC|1|Altium Vault - TI|Samsung Electro-Mechanics|Y||{URL}{URL.TEXT}{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
63|Fitted|CAP, CERM, 0.1 µF, 16 V,+/- 10%, X7R, 0603|C65|CMP-0085536-1|CL10B104KO8WPNC|1|Altium Vault - TI|Samsung Electro-Mechanics|Y||{URL}{URL.TEXT}{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
64|Fitted|CAP, CERM, 1.5 uF, 100 V, +/- 10%, X7R, AEC-Q200 Grade 1, 1210|C66|CMP-0009148-2|CGA6M3X7R2A155K200AB|1|Altium Vault - TI|TDK|Y|Digi-Key|{URL}{URL.TEXT}445-13014-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}810-CGA6M3X7R2A155K200AB{URL.TIP}Supplier
65|Fitted|CAP, CERM, 0.1 uF, 25 V, +/- 10%, X7R, AEC-Q200 Grade 1, 0603|C67|CMP-0007077-5|CGA3E2X7R1E104K080AA|1|Altium Vault - TI|TDK|Y|Digi-Key|{URL}{URL.TEXT}445-5667-1-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}79Y4100{URL.TIP}Supplier
66|Fitted|CAP, CERM, 1000 pF, 100 V, +/- 10%, X7R, 0603|C68|CMP-0007467-4|GRM188R72A102KA01D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}490-1472-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}81-GRM18R72A102KA01D{URL.TIP}Supplier
67|Fitted|CAP, CERM, 2200 pF, 16 V, +/- 10%, X7R, 0603|C69|CMP-0007387-4|GRM188R71C222KA01D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}GRM188R71C222KA01D-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}81-GRM188R71C222KA1D{URL.TIP}Supplier
68|Fitted|CAP, CERM, 0.1 uF, 100 V, +/- 10%, X7S, AEC-Q200 Grade 1, 0603|C70|CMP-0007099-4|CGA3E3X7S2A104K080AB|1|Altium Vault - TI|TDK|Y|Digi-Key|{URL}{URL.TEXT}445-6938-1-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}04X3163{URL.TIP}Supplier
69|Fitted|CAP, CERM, 0.1 uF, 16 V, +/- 10%, X7R, 0603|C71|CMP-0007378-5|GRM188R71C104KA01D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}490-1532-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}81-GRM39X104K16{URL.TIP}Supplier
70|Fitted|CAP, CERM, 0.1 uF, 16 V, +/- 10%, X7R, 0603|C72|CMP-0007378-5|GRM188R71C104KA01D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}490-1532-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}81-GRM39X104K16{URL.TIP}Supplier
71|Fitted|CAP, CERM, 4700 pF, 50 V, +/- 10%, X7R, 0603|C73|CMP-0007456-4|GRM188R71H472KA01D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}490-1506-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}81-GRM39X472K50D{URL.TIP}Supplier
72|Fitted|CAP, CERM, 0.22 uF, 50 V, +/- 10%, X7R, 1206|C74|CMP-0008605-2|C1206C224K5RACTU|1|Altium Vault - TI|Kemet|Y|Digi-Key|{URL}{URL.TEXT}399-1251-1-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}70K9309{URL.TIP}Supplier
73|Fitted|CAP, CERM, 0.22 uF, 50 V, +/- 10%, X7R, 1206|C75|CMP-0008605-2|C1206C224K5RACTU|1|Altium Vault - TI|Kemet|Y|Digi-Key|{URL}{URL.TEXT}399-1251-1-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}70K9309{URL.TIP}Supplier
74|Fitted|CAP, CERM, 0.22 uF, 50 V, +/- 10%, X7R, 1206|C76|CMP-0008605-2|C1206C224K5RACTU|1|Altium Vault - TI|Kemet|Y|Digi-Key|{URL}{URL.TEXT}399-1251-1-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}70K9309{URL.TIP}Supplier
75|Fitted|CAP, CERM, 0.22 uF, 50 V, +/- 10%, X7R, 1206|C77|CMP-0008605-2|C1206C224K5RACTU|1|Altium Vault - TI|Kemet|Y|Digi-Key|{URL}{URL.TEXT}399-1251-1-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}70K9309{URL.TIP}Supplier
76|Fitted|CAP, CERM, 0.1 uF, 16 V, +/- 10%, X7R, 0603|C78|CMP-0007378-5|GRM188R71C104KA01D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}490-1532-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}81-GRM39X104K16{URL.TIP}Supplier
77|Fitted|CAP, CERM, 0.1 uF, 16 V, +/- 10%, X7R, 0603|C79|CMP-0007378-5|GRM188R71C104KA01D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}490-1532-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}81-GRM39X104K16{URL.TIP}Supplier
78|Fitted|CAP, CERM, 0.22 uF, 50 V, +/- 10%, X7R, 1206|C80|CMP-0008605-2|C1206C224K5RACTU|1|Altium Vault - TI|Kemet|Y|Digi-Key|{URL}{URL.TEXT}399-1251-1-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}70K9309{URL.TIP}Supplier
79|Fitted|CAP, CERM, 0.22 uF, 50 V, +/- 10%, X7R, 1206|C81|CMP-0008605-2|C1206C224K5RACTU|1|Altium Vault - TI|Kemet|Y|Digi-Key|{URL}{URL.TEXT}399-1251-1-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}70K9309{URL.TIP}Supplier
80|Fitted|CAP, CERM, 0.22 uF, 50 V, +/- 10%, X7R, 1206|C82|CMP-0008605-2|C1206C224K5RACTU|1|Altium Vault - TI|Kemet|Y|Digi-Key|{URL}{URL.TEXT}399-1251-1-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}70K9309{URL.TIP}Supplier
81|Fitted|CAP, CERM, 0.22 uF, 50 V, +/- 10%, X7R, 1206|C83|CMP-0008605-2|C1206C224K5RACTU|1|Altium Vault - TI|Kemet|Y|Digi-Key|{URL}{URL.TEXT}399-1251-1-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}70K9309{URL.TIP}Supplier
82|Fitted|CAP, CERM, 4700 pF, 50 V, +/- 10%, X7R, 0603|C84|CMP-0007456-4|GRM188R71H472KA01D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}490-1506-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}81-GRM39X472K50D{URL.TIP}Supplier
83|Fitted|CAP, CERM, 10 uF, 25 V, +/- 10%, X7R, 1206|C85|CMP-0008965-2|GRM31CR71E106KA12L|1|Altium Vault - TI|MuRata|Y|Mouser|{URL}{URL.TEXT}81-GRM31CR71E106KA12{URL.TIP}Supplier|Farnell|{URL}{URL.TEXT}1828837{URL.TIP}Supplier
84|Fitted|CAP, CERM, 2.2 uF, 50 V, +/- 10%, X7R, 1206|C86|CMP-0008968-2|GRM31CR71H225KA88L|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}490-3367-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}81-GRM31CR71H225KA88{URL.TIP}Supplier
85|Fitted|CAP, CERM, 0.1 uF, 16 V, +/- 10%, X7R, 0402|C87|CMP-0006641-2|GRM155R71C104KA88D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}490-3261-1-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}38K1647{URL.TIP}Supplier
86|Fitted|CAP, CERM, 0.1 uF, 16 V, +/- 10%, X7R, 0402|C88|CMP-0006641-2|GRM155R71C104KA88D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}490-3261-1-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}38K1647{URL.TIP}Supplier
87|Fitted|CAP, CERM, 0.1 uF, 16 V, +/- 10%, X7R, 0402|C89|CMP-0006641-2|GRM155R71C104KA88D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}490-3261-1-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}38K1647{URL.TIP}Supplier
88|Fitted|CAP, CERM, 0.1 uF, 16 V, +/- 10%, X7R, 0402|C90|CMP-0006641-2|GRM155R71C104KA88D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}490-3261-1-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}38K1647{URL.TIP}Supplier
89|Fitted|CAP, CERM, 0.1 uF, 16 V, +/- 10%, X7R, 0402|C91|CMP-0006641-2|GRM155R71C104KA88D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}490-3261-1-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}38K1647{URL.TIP}Supplier
90|Fitted|CAP, CERM, 2.2 uF, 16 V, +/- 10%, X5R, 0603|C92|CMP-0007339-5|GRM188R61C225KE15D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}490-3296-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}81-GRM188R61C225KE15{URL.TIP}Supplier
91|Fitted|CAP, CERM, 1 uF, 10 V, +/- 10%, X5R, 0402|C93|CMP-0006563-2|GRM155R61A105KE15D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}490-3890-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}81-GRM155R61A105KE15{URL.TIP}Supplier
92|Fitted|CAP, CERM, 0.1 uF, 16 V, +/- 10%, X7R, 0402|C94|CMP-0006641-2|GRM155R71C104KA88D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}490-3261-1-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}38K1647{URL.TIP}Supplier
93|Fitted|CAP, CERM, 330 pF, 50 V, +/- 10%, X7R, 0603|C95|CMP-0006921-4|C0603C331K5RACTU|1|Altium Vault - TI|Kemet|Y|Digi-Key|{URL}{URL.TEXT}399-1073-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}80-C0603C331K5R{URL.TIP}Supplier
94|Fitted|CAP, CERM, 330 pF, 50 V, +/- 10%, X7R, 0603|C96|CMP-0006921-4|C0603C331K5RACTU|1|Altium Vault - TI|Kemet|Y|Digi-Key|{URL}{URL.TEXT}399-1073-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}80-C0603C331K5R{URL.TIP}Supplier
95|Fitted|CAP, CERM, 330 pF, 50 V, +/- 10%, X7R, 0603|C97|CMP-0006921-4|C0603C331K5RACTU|1|Altium Vault - TI|Kemet|Y|Digi-Key|{URL}{URL.TEXT}399-1073-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}80-C0603C331K5R{URL.TIP}Supplier
96|Fitted|CAP, CERM, 0.1 uF, 16 V, +/- 10%, X7R, 0402|C98|CMP-0006641-2|GRM155R71C104KA88D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}490-3261-1-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}38K1647{URL.TIP}Supplier
97|Fitted|CAP, CERM, 0.1 uF, 16 V, +/- 10%, X7R, 0402|C99|CMP-0006641-2|GRM155R71C104KA88D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}490-3261-1-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}38K1647{URL.TIP}Supplier
98|Fitted|CAP, CERM, 12 pF, 50 V, +/- 5%, C0G/NP0, 0402|C100|CMP-0006415-2|GRM1555C1H120JA01D|1|Altium Vault - TI|MuRata|Y|Newark|{URL}{URL.TEXT}14T3292{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}81-GRM1555C1H120JA1D{URL.TIP}Supplier
99|Fitted|CAP, CERM, 12 pF, 50 V, +/- 5%, C0G/NP0, 0402|C101|CMP-0006415-2|GRM1555C1H120JA01D|1|Altium Vault - TI|MuRata|Y|Newark|{URL}{URL.TEXT}14T3292{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}81-GRM1555C1H120JA1D{URL.TIP}Supplier
100|Fitted|CAP, CERM, 12 pF, 50 V, +/- 5%, C0G/NP0, 0402|C102|CMP-0006415-2|GRM1555C1H120JA01D|1|Altium Vault - TI|MuRata|Y|Newark|{URL}{URL.TEXT}14T3292{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}81-GRM1555C1H120JA1D{URL.TIP}Supplier
101|Fitted|CAP, CERM, 12 pF, 50 V, +/- 5%, C0G/NP0, 0402|C103|CMP-0006415-2|GRM1555C1H120JA01D|1|Altium Vault - TI|MuRata|Y|Newark|{URL}{URL.TEXT}14T3292{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}81-GRM1555C1H120JA1D{URL.TIP}Supplier
102|Fitted|CAP, CERM, 10 uF, 25 V, +/- 10%, X7R, 1206|C104|CMP-0008965-2|GRM31CR71E106KA12L|1|Altium Vault - TI|MuRata|Y|Mouser|{URL}{URL.TEXT}81-GRM31CR71E106KA12{URL.TIP}Supplier|Farnell|{URL}{URL.TEXT}1828837{URL.TIP}Supplier
103|Fitted|CAP, CERM, 10 uF, 25 V, +/- 10%, X7R, 1206|C105|CMP-0008965-2|GRM31CR71E106KA12L|1|Altium Vault - TI|MuRata|Y|Mouser|{URL}{URL.TEXT}81-GRM31CR71E106KA12{URL.TIP}Supplier|Farnell|{URL}{URL.TEXT}1828837{URL.TIP}Supplier
104|Fitted|CAP, CERM, 0.1 uF, 16 V, +/- 10%, X7R, 0603|C106|CMP-0007378-5|GRM188R71C104KA01D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}490-1532-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}81-GRM39X104K16{URL.TIP}Supplier
105|Fitted|CAP, CERM, 1 uF, 100 V, +/- 10%, X7S, AEC-Q200 Grade 1, 0805|C107|CMP-0007980-2|CGA4J3X7S2A105K125AB|1|Altium Vault - TI|TDK|Y|Digi-Key|{URL}{URL.TEXT}445-6974-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}810-CGA4J3X7S2A105K125AB{URL.TIP}Supplier
106|Fitted|CAP, CERM, 0.1 uF, 100 V, +/- 10%, X7R, AEC-Q200 Grade 1, 0805|C108|CMP-0007969-2|CGA4J2X7R2A104K125AA|1|Altium Vault - TI|TDK|Y|Digi-Key|{URL}{URL.TEXT}445-5827-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}810-CGA4J2X7R2A104K125AA{URL.TIP}Supplier
107|Fitted|CAP, CERM, 10 uF, 25 V, +/- 10%, X7R, 1206|C109|CMP-0008965-2|GRM31CR71E106KA12L|1|Altium Vault - TI|MuRata|Y|Mouser|{URL}{URL.TEXT}81-GRM31CR71E106KA12{URL.TIP}Supplier|Farnell|{URL}{URL.TEXT}1828837{URL.TIP}Supplier
108|Fitted|CAP, CERM, 10 uF, 25 V, +/- 10%, X7R, 1206|C110|CMP-0008965-2|GRM31CR71E106KA12L|1|Altium Vault - TI|MuRata|Y|Mouser|{URL}{URL.TEXT}81-GRM31CR71E106KA12{URL.TIP}Supplier|Farnell|{URL}{URL.TEXT}1828837{URL.TIP}Supplier
109|Fitted|CAP, AL, 100 uF, 16 V, +/- 20%, 0.26 ohm, AEC-Q200 Grade 2, SMD|C111|CMP-0010733-1|EEEFP1C101AP|1|Altium Vault - TI|Panasonic|Y|Digi-Key|{URL}{URL.TEXT}PCE4533CT-ND{URL.TIP}Supplier|Farnell|{URL}{URL.TEXT}1539476{URL.TIP}Supplier
110|Fitted|CAP, CERM, 10 uF, 25 V, +/- 10%, X7R, 1206|C112|CMP-0008965-2|GRM31CR71E106KA12L|1|Altium Vault - TI|MuRata|Y|Mouser|{URL}{URL.TEXT}81-GRM31CR71E106KA12{URL.TIP}Supplier|Farnell|{URL}{URL.TEXT}1828837{URL.TIP}Supplier
111|Fitted|CAP, CERM, 10 uF, 25 V, +/- 10%, X7R, 1206|C113|CMP-0008965-2|GRM31CR71E106KA12L|1|Altium Vault - TI|MuRata|Y|Mouser|{URL}{URL.TEXT}81-GRM31CR71E106KA12{URL.TIP}Supplier|Farnell|{URL}{URL.TEXT}1828837{URL.TIP}Supplier
112|Fitted|CAP, CERM, 1 uF, 25 V, +/- 10%, X7R, 0603|C114|CMP-0007405-4|GRM188R71E105KA12D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}490-5307-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}81-GRM188R71E105KA2D{URL.TIP}Supplier
113|Fitted|CAP, CERM, 5 pF, 100 V, +/- 5%, C0G/NP0, 0402|C117|CMP-0006503-2|GRM1555C2A5R0CA01D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}490-7291-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}81-GRM1555C2A5R0CA1D{URL.TIP}Supplier
114|Fitted|CAP, CERM, 0.022 uF, 100 V, +/- 10%, X7R, AEC-Q200 Grade 1, 0603|C118|CMP-0007086-4|CGA3E2X7R2A223K080AA|1|Altium Vault - TI|TDK|Y|Digi-Key|{URL}{URL.TEXT}445-5814-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}810-CGA3E2X7R2A223K080AA{URL.TIP}Supplier
115|Fitted|CAP, CERM, 3900 pF, 50 V, +/- 10%, X7R, 0603|C119|CMP-0007453-4|GRM188R71H392KA01D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}490-1504-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}81-GRM39X392K50D{URL.TIP}Supplier
116|Fitted|CAP, CERM, 0.01 uF, 100 V, +/- 10%, X7R, 0603|C122|CMP-0007468-5|GRM188R72A103KA01D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}GRM188R72A103KA01D-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}81-GRM188R72A103KA1D{URL.TIP}Supplier
117|Fitted|CAP, CERM, 0.01 uF, 100 V, +/- 10%, X7R, 0603|C123|CMP-0007468-5|GRM188R72A103KA01D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}GRM188R72A103KA01D-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}81-GRM188R72A103KA1D{URL.TIP}Supplier
118|Fitted|CAP, CERM, 0.01 uF, 100 V, +/- 10%, X7R, 0603|C124|CMP-0007468-5|GRM188R72A103KA01D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}GRM188R72A103KA01D-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}81-GRM188R72A103KA1D{URL.TIP}Supplier
119|Fitted|CAP, CERM, 0.01 uF, 100 V, +/- 10%, X7R, 0603|C125|CMP-0007468-5|GRM188R72A103KA01D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}GRM188R72A103KA01D-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}81-GRM188R72A103KA1D{URL.TIP}Supplier
120|Fitted|CAP, CERM, 0.01 uF, 100 V, +/- 10%, X7R, 0603|C126|CMP-0007468-5|GRM188R72A103KA01D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}GRM188R72A103KA01D-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}81-GRM188R72A103KA1D{URL.TIP}Supplier
121|Fitted|CAP, CERM, 0.01 uF, 100 V, +/- 10%, X7R, 0603|C127|CMP-0007468-5|GRM188R72A103KA01D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}GRM188R72A103KA01D-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}81-GRM188R72A103KA1D{URL.TIP}Supplier
122|Fitted|CAP, CERM, 0.01 uF, 100 V, +/- 10%, X7R, 0603|C128|CMP-0007468-5|GRM188R72A103KA01D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}GRM188R72A103KA01D-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}81-GRM188R72A103KA1D{URL.TIP}Supplier
123|Fitted|CAP, CERM, 0.01 uF, 100 V, +/- 10%, X7R, 0603|C129|CMP-0007468-5|GRM188R72A103KA01D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}GRM188R72A103KA01D-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}81-GRM188R72A103KA1D{URL.TIP}Supplier
124|Fitted|CAP, CERM, 0.01 uF, 100 V, +/- 10%, X7R, 0603|C130|CMP-0007468-5|GRM188R72A103KA01D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}GRM188R72A103KA01D-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}81-GRM188R72A103KA1D{URL.TIP}Supplier
125|Fitted|Diode, TVS, Bi, 26 V, 42.1 Vc, AEC-Q101, SMA|D1|CMP-0005455-3|SMAJ26CAHE3/61|1|Altium Vault - TI|Vishay-Semiconductor|Y||{URL}{URL.TEXT}{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
126|Fitted|Diode, Zener, 8.2 V, 500 mW, SOD-123|D2|CMP-0077604-3|MMSZ4694-E3-08|1|Altium Vault - TI|Vishay-Semiconductor|Y||{URL}{URL.TEXT}{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
127|Fitted|Diode, Schottky, 60 V, 1 A, AEC-Q101, SOD-123|D3|CMP-0079239-2|PMEG6010CEGWJ|1|Altium Vault - TI|Nexperia|Y||{URL}{URL.TEXT}{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
128|Fitted|Diode, Schottky, 60 V, 1 A, AEC-Q101, SOD-123|D4|CMP-0079239-2|PMEG6010CEGWJ|1|Altium Vault - TI|Nexperia|Y||{URL}{URL.TEXT}{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
129|Fitted|Diode, Schottky, 60 V, 1 A, AEC-Q101, SOD-123|D5|CMP-0079239-2|PMEG6010CEGWJ|1|Altium Vault - TI|Nexperia|Y||{URL}{URL.TEXT}{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
130|Fitted|Diode, Schottky, 100 V, 5 A, AEC-Q101, PowerDI5|D6|CMP-0080010-2|PDS5100HQ-13|1|Altium Vault - TI|Diodes Inc.|Y||{URL}{URL.TEXT}{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
131|Fitted|Diode, Schottky, 100 V, 5 A, AEC-Q101, PowerDI5|D7|CMP-0080010-2|PDS5100HQ-13|1|Altium Vault - TI|Diodes Inc.|Y||{URL}{URL.TEXT}{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
132|Fitted|Diode, Schottky, 60 V, 1 A, AEC-Q101, PowerDI323|D8|CMP-0028786-2|PD3S160Q-7|1|Altium Vault - TI|Diodes Inc.|Y||{URL}{URL.TEXT}{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
133|Fitted|Diode, Schottky, 60 V, 1 A, AEC-Q101, PowerDI323|D9|CMP-0028786-2|PD3S160Q-7|1|Altium Vault - TI|Diodes Inc.|Y||{URL}{URL.TEXT}{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
134|Fitted|Diode, Schottky, 60 V, 1 A, AEC-Q101, PowerDI323|D10|CMP-0028786-2|PD3S160Q-7|1|Altium Vault - TI|Diodes Inc.|Y||{URL}{URL.TEXT}{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
135|Fitted|Diode, Schottky, 60 V, 1 A, AEC-Q101, PowerDI323|D11|CMP-0028786-2|PD3S160Q-7|1|Altium Vault - TI|Diodes Inc.|Y||{URL}{URL.TEXT}{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
136|Fitted|Diode, Schottky, 60 V, 2 A, AEC-Q101, SMA|D12|CMP-0028837-2|SS26SHE3_A/H|1|Altium Vault - TI|Vishay-Semiconductor|Y||{URL}{URL.TEXT}{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
137|Fitted|Fiducial mark.  There is nothing to buy or mount.|FID1|CMP-0077181-1|N/A|1|Altium Vault - TI|N/A|||{URL}{URL.TEXT}{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
138|Fitted|Fiducial mark.  There is nothing to buy or mount.|FID2|CMP-0077181-1|N/A|1|Altium Vault - TI|N/A|||{URL}{URL.TEXT}{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
139|Fitted|Fiducial mark.  There is nothing to buy or mount.|FID3|CMP-0077181-1|N/A|1|Altium Vault - TI|N/A|||{URL}{URL.TEXT}{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
140|Fitted|347720140|J2|COMPONENT_1||1|347720140.SchLib||||{URL}{URL.TEXT}{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
141|Fitted|Header, 1.27mm, 5x2, Gold, Black, SMT|J3|CMP-0075629-2|FTSH-105-01-F-DV|1|Altium Vault - TI|Samtec|Y|Digi-Key|{URL}{URL.TEXT}SAM8795-ND{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
142|Fitted|Inductor, Shielded, Ferrite, 1 µH, 15 A, 0.0042 ohm, SMD|L1|CMP-0082552-1|SPM10040T-1R0M|1|Altium Vault - TI|TDK|Y||{URL}{URL.TEXT}{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
143|Fitted|Inductor, Shielded, 15 µH, 8.5 A, 0.02299 ohm, AEC-Q200 Grade 0, SMD|L2|CMP-0084137-1|SPM12565VT-150M-D|1|Altium Vault - TI|TDK|Y||{URL}{URL.TEXT}{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
144|Fitted|Inductor, Shielded, 15 µH, 8.5 A, 0.02299 ohm, AEC-Q200 Grade 0, SMD|L3|CMP-0084137-1|SPM12565VT-150M-D|1|Altium Vault - TI|TDK|Y||{URL}{URL.TEXT}{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
145|Fitted|Inductor, Shielded, Metal Composite, 47 µH, 1.5 A, 0.318 ohm, SMD|L4|CMP-0081480-2|SPM6545VT-470M-D|1|Altium Vault - TI|TDK|Y||{URL}{URL.TEXT}{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
146|Fitted|Inductor, Shielded, Metal Composite, 47 µH, 1.5 A, 0.318 ohm, SMD|L5|CMP-0081480-2|SPM6545VT-470M-D|1|Altium Vault - TI|TDK|Y||{URL}{URL.TEXT}{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
147|Fitted|Inductor, Shielded, Metal Composite, 47 µH, 1.5 A, 0.318 ohm, SMD|L6|CMP-0081480-2|SPM6545VT-470M-D|1|Altium Vault - TI|TDK|Y||{URL}{URL.TEXT}{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
148|Fitted|Inductor, Shielded, Metal Composite, 47 µH, 1.5 A, 0.318 ohm, SMD|L7|CMP-0081480-2|SPM6545VT-470M-D|1|Altium Vault - TI|TDK|Y||{URL}{URL.TEXT}{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
149|Fitted|Coupled inductor, 51 uH,  A, 0.14 ohm, SMD|L8|CMP-0013133-2|B82793S513N201|1|Altium Vault - TI|TDK|Y|Digi-Key|{URL}{URL.TEXT}495-1869-1-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}46P6188{URL.TIP}Supplier
150|Fitted|Ferrite Bead, 33 ohm @ 100 MHz, 4 A, 0805|L9|CMP-0003069-1|742792012|1|Altium Vault - TI|Wurth Elektronik|Y|Digi-Key|{URL}{URL.TEXT}732-4636-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}710-742792012{URL.TIP}Supplier
151|Fitted|Ferrite Bead, 33 ohm @ 100 MHz, 4 A, 0805|L10|CMP-0003069-1|742792012|1|Altium Vault - TI|Wurth Elektronik|Y|Digi-Key|{URL}{URL.TEXT}732-4636-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}710-742792012{URL.TIP}Supplier
152|Fitted|Coupled inductor, 51 uH,  A, 0.14 ohm, SMD|L17|CMP-0013133-2|B82793S513N201|1|Altium Vault - TI|TDK|Y|Digi-Key|{URL}{URL.TEXT}495-1869-1-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}46P6188{URL.TIP}Supplier
153|Fitted|Ferrite Bead, 220 ohm @ 100 MHz, 2 A, 0805|L22|CMP-0003363-1|BLM21PG221SN1D|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}490-1054-1-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}73M9167{URL.TIP}Supplier
154|Fitted|Ferrite Bead, 60 ohm @ 100 MHz, 3 A, 0805|L23|CMP-0003306-1|BKP2125HS600-T|1|Altium Vault - TI|Taiyo Yuden|Y|Digi-Key|{URL}{URL.TEXT}587-1932-1-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}30K5394%20LF%20BKP2125HS600-T{URL.TIP}Supplier
155|Fitted|Inductor, Shielded Drum Core, Ferrite, 2.2 uH, 1.1 A, 0.22 ohm, SMD|L24|CMP-0060436-1|LPS3010-222MLB|1|Altium Vault - TI|Coilcraft|Y||{URL}{URL.TEXT}{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
156|Fitted|Inductor, Shielded, Composite, 15 uH, 2.8 A, 0.109 ohm, SMD|L25|CMP-0061649-2|XAL4040-153MEB|1|Altium Vault - TI|Coilcraft|Y|Mouser|{URL}{URL.TEXT}994-XAL4040-153MEB{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
157|Fitted|Ferrite Bead, 33 ohm @ 100 MHz, 4 A, 0805|L27|CMP-0003069-1|742792012|1|Altium Vault - TI|Wurth Elektronik|Y|Digi-Key|{URL}{URL.TEXT}732-4636-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}710-742792012{URL.TIP}Supplier
158|Fitted|Ferrite Bead, 33 ohm @ 100 MHz, 4 A, 0805|L29|CMP-0003069-1|742792012|1|Altium Vault - TI|Wurth Elektronik|Y|Digi-Key|{URL}{URL.TEXT}732-4636-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}710-742792012{URL.TIP}Supplier
159|Fitted|Ferrite Bead, 33 ohm @ 100 MHz, 4 A, 0805|L30|CMP-0003069-1|742792012|1|Altium Vault - TI|Wurth Elektronik|Y|Digi-Key|{URL}{URL.TEXT}732-4636-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}710-742792012{URL.TIP}Supplier
160|Fitted|Ferrite Bead, 33 ohm @ 100 MHz, 4 A, 0805|L31|CMP-0003069-1|742792012|1|Altium Vault - TI|Wurth Elektronik|Y|Digi-Key|{URL}{URL.TEXT}732-4636-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}710-742792012{URL.TIP}Supplier
161|Fitted|Ferrite Bead, 33 ohm @ 100 MHz, 4 A, 0805|L32|CMP-0003069-1|742792012|1|Altium Vault - TI|Wurth Elektronik|Y|Digi-Key|{URL}{URL.TEXT}732-4636-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}710-742792012{URL.TIP}Supplier
162|Fitted|Ferrite Bead, 33 ohm @ 100 MHz, 4 A, 0805|L33|CMP-0003069-1|742792012|1|Altium Vault - TI|Wurth Elektronik|Y|Digi-Key|{URL}{URL.TEXT}732-4636-1-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}710-742792012{URL.TIP}Supplier
163|Fitted|MOSFET, N-CH, 60 V, 53 A, AEC-Q101, SOT669|Q1|CMP-0000807-2|BUK9Y15-60E,115|1|Altium Vault - TI|Nexperia|Y|Digi-Key|{URL}{URL.TEXT}568-10974-1-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}45W7282{URL.TIP}Supplier
164|Fitted|Transistor, NPN, 60 V, 0.5 A, AEC-Q101, SOT-23|Q2|CMP-0000488-2|MMBTA05LT1G|1|Altium Vault - TI|ON Semiconductor|Y|Digi-Key|{URL}{URL.TEXT}MMBTA05LT1GOSCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}45J1527{URL.TIP}Supplier
165|Fitted|MOSFET, N-CH, 80 V, 60 A, AEC-Q101, PowerPAK_SO-8L|Q3|CMP-0086155-1|SQJA90EP-T1_GE3|1|Altium Vault - TI|Vishay-Siliconix|Y||{URL}{URL.TEXT}{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
166|Fitted|MOSFET, N-CH, 80 V, 60 A, AEC-Q101, PowerPAK_SO-8L|Q4|CMP-0086155-1|SQJA90EP-T1_GE3|1|Altium Vault - TI|Vishay-Siliconix|Y||{URL}{URL.TEXT}{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
167|Fitted|MOSFET, P-CH, -20 V, -3.7 A, SOT-23|Q5|CMP-0000092-3|SI2323DS|1|Altium Vault - TI|Vishay-Siliconix|Y||{URL}{URL.TEXT}{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
168|Fitted|Transistor, NPN, 40 V, 0.2 A, SOT-23|Q6|CMP-0000419-2|MMBT3904LT1G|1|Altium Vault - TI|ON Semiconductor|Y|Digi-Key|{URL}{URL.TEXT}MMBT3904LT1GOSCT-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}863-MMBT3904LT1G{URL.TIP}Supplier
169|Fitted|MOSFET, P-CH, -20 V, -3.7 A, SOT-23|Q7|CMP-0000092-3|SI2323DS|1|Altium Vault - TI|Vishay-Siliconix|Y||{URL}{URL.TEXT}{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
170|Fitted|Transistor, NPN, 40 V, 0.2 A, SOT-23|Q8|CMP-0000419-2|MMBT3904LT1G|1|Altium Vault - TI|ON Semiconductor|Y|Digi-Key|{URL}{URL.TEXT}MMBT3904LT1GOSCT-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}863-MMBT3904LT1G{URL.TIP}Supplier
171|Fitted|RES, 100 k, 0.1%, 0.1 W, AEC-Q200 Grade 1, 0603|R1|CMP-0025685-3|TNPW0603100KBEEA|1|Altium Vault - TI|Vishay-Dale|Y|Digi-Key|{URL}{URL.TEXT}TNP100KAACT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}26R4219{URL.TIP}Supplier
172|Fitted|RES, 100 k, 0.1%, 0.1 W, AEC-Q200 Grade 1, 0603|R2|CMP-0025685-3|TNPW0603100KBEEA|1|Altium Vault - TI|Vishay-Dale|Y|Digi-Key|{URL}{URL.TEXT}TNP100KAACT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}26R4219{URL.TIP}Supplier
173|Fitted|RES, 100 k, 0.1%, 0.1 W, AEC-Q200 Grade 1, 0603|R3|CMP-0025685-3|TNPW0603100KBEEA|1|Altium Vault - TI|Vishay-Dale|Y|Digi-Key|{URL}{URL.TEXT}TNP100KAACT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}26R4219{URL.TIP}Supplier
174|Fitted|RES, 100 k, 0.1%, 0.1 W, AEC-Q200 Grade 1, 0603|R4|CMP-0025685-3|TNPW0603100KBEEA|1|Altium Vault - TI|Vishay-Dale|Y|Digi-Key|{URL}{URL.TEXT}TNP100KAACT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}26R4219{URL.TIP}Supplier
175|Fitted|RES, 221 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R5|CMP-0022216-4|CRCW0603221KFKEA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-221KHCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8299{URL.TIP}Supplier
176|Fitted|RES, 7.5, 5%, 0.75 W, AEC-Q200 Grade 0, 2010|R6|CMP-0016180-3|CRCW20107R50JNEF|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-7.5WCT-ND{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
177|Fitted|RES, 10.0 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R7|CMP-0023341-3|RMCF0603FT10K0|1|Altium Vault - TI|Stackpole Electronics Inc|Y|Digi-Key|{URL}{URL.TEXT}RMCF0603FT10K0CT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}78Y4027{URL.TIP}Supplier
178|Fitted|RES, 221 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R8|CMP-0022216-4|CRCW0603221KFKEA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-221KHCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8299{URL.TIP}Supplier
179|Fitted|RES, 100 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R9|CMP-0021990-4|CRCW0603100KFKEA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-100KHCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}42K3668{URL.TIP}Supplier
180|Fitted|RES, 20.0 k, 1%, 0.1 W, 0603|R10|CMP-0022906-5|RC0603FR-0720KL|1|Altium Vault - TI|Yageo|Y|Digi-Key|{URL}{URL.TEXT}311-20.0KHRCT-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}603-RC0603FR-0720KL{URL.TIP}Supplier
181|Fitted|RES, 1.00, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R11|CMP-0022170-4|CRCW06031R00FKEA|1|Altium Vault - TI|Vishay-Dale|E|Newark|{URL}{URL.TEXT}52K8059{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}71-CRCW06031R00FKEA{URL.TIP}Supplier
182|Fitted|RES, 4.99, 1%, 0.1 W, 0603|R12|CMP-0023161-5|RC0603FR-074R99L|1|Altium Vault - TI|Yageo|Y|Digi-Key|{URL}{URL.TEXT}311-4.99HRCT-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}603-RC0603FR-074R99L{URL.TIP}Supplier
183|Fitted|RES, 10.0 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R13|CMP-0023341-3|RMCF0603FT10K0|1|Altium Vault - TI|Stackpole Electronics Inc|Y|Digi-Key|{URL}{URL.TEXT}RMCF0603FT10K0CT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}78Y4027{URL.TIP}Supplier
184|Fitted|RES, 10.0, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R14|CMP-0022003-4|CRCW060310R0FKEA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-10.0HCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8073{URL.TIP}Supplier
185|Fitted|RES, 4.12 k, 1%, 0.1 W, 0603|R15|CMP-0023145-5|RC0603FR-074K12L|1|Altium Vault - TI|Yageo|Y|Digi-Key|{URL}{URL.TEXT}311-4.12KHRCT-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}603-RC0603FR-074K12L{URL.TIP}Supplier
186|Fitted|RES, 10.0 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R16|CMP-0023341-3|RMCF0603FT10K0|1|Altium Vault - TI|Stackpole Electronics Inc|Y|Digi-Key|{URL}{URL.TEXT}RMCF0603FT10K0CT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}78Y4027{URL.TIP}Supplier
187|Fitted|RES, 10.0 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R17|CMP-0023341-3|RMCF0603FT10K0|1|Altium Vault - TI|Stackpole Electronics Inc|Y|Digi-Key|{URL}{URL.TEXT}RMCF0603FT10K0CT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}78Y4027{URL.TIP}Supplier
188|Fitted|RES, 0.01, 1%, 1 W, 2010|R18|CMP-0016536-2|PMR50HZPFU10L0|1|Altium Vault - TI|Rohm|Y|Digi-Key|{URL}{URL.TEXT}RHM.010ASCT-ND{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
189|Fitted|RES, 10.0 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R20|CMP-0023341-3|RMCF0603FT10K0|1|Altium Vault - TI|Stackpole Electronics Inc|Y|Digi-Key|{URL}{URL.TEXT}RMCF0603FT10K0CT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}78Y4027{URL.TIP}Supplier
190|Fitted|RES, 7.5, 5%, 0.75 W, AEC-Q200 Grade 0, 2010|R21|CMP-0016180-3|CRCW20107R50JNEF|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-7.5WCT-ND{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
191|Fitted|RES, 4.99, 1%, 0.1 W, 0603|R22|CMP-0023161-5|RC0603FR-074R99L|1|Altium Vault - TI|Yageo|Y|Digi-Key|{URL}{URL.TEXT}311-4.99HRCT-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}603-RC0603FR-074R99L{URL.TIP}Supplier
192|Fitted|RES, 154 k, 1%, 0.063 W, AEC-Q200 Grade 0, 0402|R23|CMP-0026023-3|CRCW0402154KFKED|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-154KLCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K6723{URL.TIP}Supplier
193|Fitted|RES, 10.0, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R24|CMP-0022003-4|CRCW060310R0FKEA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-10.0HCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8073{URL.TIP}Supplier
194|Fitted|RES, 0.01, 1%, 1 W, 2010|R25|CMP-0016536-2|PMR50HZPFU10L0|1|Altium Vault - TI|Rohm|Y|Digi-Key|{URL}{URL.TEXT}RHM.010ASCT-ND{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
195|Fitted|RES, 15.8 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R27|CMP-0022068-4|CRCW060315K8FKEA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-15.8KHCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8154{URL.TIP}Supplier
196|Fitted|RES, 0.1, 1%, .5 W, AEC-Q200 Grade 0, 0805|R28|CMP-0065345-2|KRL1220E-M-R100-F-T5|1|Altium Vault - TI|Susumu Co Ltd|Y|Digi-Key|{URL}{URL.TEXT}408-1556-1-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}20X7988{URL.TIP}Supplier
197|Fitted|RES, 1.00 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R29|CMP-0022109-5|CRCW06031K00FKEA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-1.00KHCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8015{URL.TIP}Supplier
198|Fitted|RES, 0, 5%, 0.1 W, AEC-Q200 Grade 0, 0603|R30|CMP-0025874-4|ERJ-3GEY0R00V|1|Altium Vault - TI|Panasonic|Y|Digi-Key|{URL}{URL.TEXT}P0.0GCT-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}667-ERJ-3GEY0R00V{URL.TIP}Supplier
199|Fitted|RES, 30.1 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R31|CMP-0022324-4|CRCW060330K1FKEA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-30.1KHCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8401{URL.TIP}Supplier
200|Fitted|RES, 0, 5%, 0.1 W, AEC-Q200 Grade 0, 0603|R32|CMP-0025874-4|ERJ-3GEY0R00V|1|Altium Vault - TI|Panasonic|Y|Digi-Key|{URL}{URL.TEXT}P0.0GCT-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}667-ERJ-3GEY0R00V{URL.TIP}Supplier
201|Fitted|RES, 1.00 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R33|CMP-0022109-5|CRCW06031K00FKEA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-1.00KHCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8015{URL.TIP}Supplier
202|Fitted|RES, 0, 5%, 0.1 W, AEC-Q200 Grade 0, 0603|R34|CMP-0025874-4|ERJ-3GEY0R00V|1|Altium Vault - TI|Panasonic|Y|Digi-Key|{URL}{URL.TEXT}P0.0GCT-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}667-ERJ-3GEY0R00V{URL.TIP}Supplier
203|Fitted|RES, 10.0 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R35|CMP-0023341-3|RMCF0603FT10K0|1|Altium Vault - TI|Stackpole Electronics Inc|Y|Digi-Key|{URL}{URL.TEXT}RMCF0603FT10K0CT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}78Y4027{URL.TIP}Supplier
204|Fitted|RES, 100 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R36|CMP-0021990-4|CRCW0603100KFKEA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-100KHCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}42K3668{URL.TIP}Supplier
205|Fitted|RES, 10.0 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R37|CMP-0023341-3|RMCF0603FT10K0|1|Altium Vault - TI|Stackpole Electronics Inc|Y|Digi-Key|{URL}{URL.TEXT}RMCF0603FT10K0CT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}78Y4027{URL.TIP}Supplier
206|Fitted|RES, 0, 5%, 0.1 W, AEC-Q200 Grade 0, 0603|R38|CMP-0025874-4|ERJ-3GEY0R00V|1|Altium Vault - TI|Panasonic|Y|Digi-Key|{URL}{URL.TEXT}P0.0GCT-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}667-ERJ-3GEY0R00V{URL.TIP}Supplier
207|Fitted|RES, 15.8 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R39|CMP-0022068-4|CRCW060315K8FKEA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-15.8KHCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8154{URL.TIP}Supplier
208|Fitted|RES, 10.0 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R40|CMP-0023341-3|RMCF0603FT10K0|1|Altium Vault - TI|Stackpole Electronics Inc|Y|Digi-Key|{URL}{URL.TEXT}RMCF0603FT10K0CT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}78Y4027{URL.TIP}Supplier
209|Fitted|RES, 1.00 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R41|CMP-0022109-5|CRCW06031K00FKEA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-1.00KHCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8015{URL.TIP}Supplier
210|Fitted|RES, 0.1, 1%, .5 W, AEC-Q200 Grade 0, 0805|R42|CMP-0065345-2|KRL1220E-M-R100-F-T5|1|Altium Vault - TI|Susumu Co Ltd|Y|Digi-Key|{URL}{URL.TEXT}408-1556-1-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}20X7988{URL.TIP}Supplier
211|Fitted|RES, 30.1 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R43|CMP-0022324-4|CRCW060330K1FKEA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-30.1KHCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8401{URL.TIP}Supplier
212|Fitted|RES, 15.8 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R44|CMP-0022068-4|CRCW060315K8FKEA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-15.8KHCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8154{URL.TIP}Supplier
213|Fitted|RES, 0.1, 1%, .5 W, AEC-Q200 Grade 0, 0805|R45|CMP-0065345-2|KRL1220E-M-R100-F-T5|1|Altium Vault - TI|Susumu Co Ltd|Y|Digi-Key|{URL}{URL.TEXT}408-1556-1-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}20X7988{URL.TIP}Supplier
214|Fitted|RES, 1.00 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R46|CMP-0022109-5|CRCW06031K00FKEA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-1.00KHCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8015{URL.TIP}Supplier
215|Fitted|RES, 30.1 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R47|CMP-0022324-4|CRCW060330K1FKEA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-30.1KHCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8401{URL.TIP}Supplier
216|Fitted|RES, 0, 5%, 0.1 W, AEC-Q200 Grade 0, 0603|R48|CMP-0025874-4|ERJ-3GEY0R00V|1|Altium Vault - TI|Panasonic|Y|Digi-Key|{URL}{URL.TEXT}P0.0GCT-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}667-ERJ-3GEY0R00V{URL.TIP}Supplier
217|Fitted|RES, 0, 5%, 0.1 W, AEC-Q200 Grade 0, 0603|R49|CMP-0025874-4|ERJ-3GEY0R00V|1|Altium Vault - TI|Panasonic|Y|Digi-Key|{URL}{URL.TEXT}P0.0GCT-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}667-ERJ-3GEY0R00V{URL.TIP}Supplier
218|Fitted|RES, 1.00 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R50|CMP-0022109-5|CRCW06031K00FKEA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-1.00KHCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8015{URL.TIP}Supplier
219|Fitted|RES, 0, 5%, 0.1 W, AEC-Q200 Grade 0, 0603|R51|CMP-0025874-4|ERJ-3GEY0R00V|1|Altium Vault - TI|Panasonic|Y|Digi-Key|{URL}{URL.TEXT}P0.0GCT-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}667-ERJ-3GEY0R00V{URL.TIP}Supplier
220|Fitted|RES, 10.0 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R52|CMP-0023341-3|RMCF0603FT10K0|1|Altium Vault - TI|Stackpole Electronics Inc|Y|Digi-Key|{URL}{URL.TEXT}RMCF0603FT10K0CT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}78Y4027{URL.TIP}Supplier
221|Fitted|RES, 100 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R53|CMP-0021990-4|CRCW0603100KFKEA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-100KHCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}42K3668{URL.TIP}Supplier
222|Fitted|RES, 10.0 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R54|CMP-0023341-3|RMCF0603FT10K0|1|Altium Vault - TI|Stackpole Electronics Inc|Y|Digi-Key|{URL}{URL.TEXT}RMCF0603FT10K0CT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}78Y4027{URL.TIP}Supplier
223|Fitted|RES, 0, 5%, 0.1 W, AEC-Q200 Grade 0, 0603|R55|CMP-0025874-4|ERJ-3GEY0R00V|1|Altium Vault - TI|Panasonic|Y|Digi-Key|{URL}{URL.TEXT}P0.0GCT-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}667-ERJ-3GEY0R00V{URL.TIP}Supplier
224|Fitted|RES, 10.0 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R56|CMP-0023341-3|RMCF0603FT10K0|1|Altium Vault - TI|Stackpole Electronics Inc|Y|Digi-Key|{URL}{URL.TEXT}RMCF0603FT10K0CT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}78Y4027{URL.TIP}Supplier
225|Fitted|RES, 15.8 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R57|CMP-0022068-4|CRCW060315K8FKEA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-15.8KHCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8154{URL.TIP}Supplier
226|Fitted|RES, 1.00 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R58|CMP-0022109-5|CRCW06031K00FKEA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-1.00KHCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8015{URL.TIP}Supplier
227|Fitted|RES, 0.1, 1%, .5 W, AEC-Q200 Grade 0, 0805|R59|CMP-0065345-2|KRL1220E-M-R100-F-T5|1|Altium Vault - TI|Susumu Co Ltd|Y|Digi-Key|{URL}{URL.TEXT}408-1556-1-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}20X7988{URL.TIP}Supplier
228|Fitted|RES, 30.1 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R60|CMP-0022324-4|CRCW060330K1FKEA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-30.1KHCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8401{URL.TIP}Supplier
229|Fitted|RES, 47.0 k, 1%, 0.1 W, 0603|R61|CMP-0023133-5|RC0603FR-0747KL|1|Altium Vault - TI|Yageo|Y|Digi-Key|{URL}{URL.TEXT}311-47.0KHRCT-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}603-RC0603FR-0747KL{URL.TIP}Supplier
230|Fitted|RES, 0, 5%, 0.1 W, AEC-Q200 Grade 0, 0603|R62|CMP-0025697-4|CRCW06030000Z0EA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-0.0GCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8014{URL.TIP}Supplier
231|Fitted|RES, 0, 5%, 0.1 W, AEC-Q200 Grade 0, 0603|R63|CMP-0025697-4|CRCW06030000Z0EA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-0.0GCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8014{URL.TIP}Supplier
232|Fitted|RES, 61.9, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R64|CMP-0022537-4|CRCW060361R9FKEA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-61.9HCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8648{URL.TIP}Supplier
233|Fitted|RES, 61.9, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R65|CMP-0022537-4|CRCW060361R9FKEA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-61.9HCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8648{URL.TIP}Supplier
234|Fitted|RES, 10.0 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R66|CMP-0021998-4|CRCW060310K0FKEA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-10.0KHCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8062{URL.TIP}Supplier
235|Fitted|RES, 0, 5%, 0.1 W, AEC-Q200 Grade 0, 0603|R71|CMP-0025697-4|CRCW06030000Z0EA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-0.0GCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8014{URL.TIP}Supplier
236|Fitted|RES, 0, 5%, 0.1 W, AEC-Q200 Grade 0, 0603|R72|CMP-0025697-4|CRCW06030000Z0EA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-0.0GCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8014{URL.TIP}Supplier
237|Fitted|RES, 61.9, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R73|CMP-0022537-4|CRCW060361R9FKEA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-61.9HCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8648{URL.TIP}Supplier
238|Fitted|RES, 61.9, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R74|CMP-0022537-4|CRCW060361R9FKEA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-61.9HCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8648{URL.TIP}Supplier
239|Fitted|RES, 10.0 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R75|CMP-0021998-4|CRCW060310K0FKEA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-10.0KHCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8062{URL.TIP}Supplier
240|Fitted|RES, 100, 1%, 0.063 W, AEC-Q200 Grade 0, 0402|R76|CMP-0026763-1|RMCF0402JT100R|1|Altium Vault - TI|Stackpole Electronics Inc|Y|Digi-Key|{URL}{URL.TEXT}RMCF0402JT100RCT-ND{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
241|Fitted|RES, 10.0 k, 1%, 0.063 W, AEC-Q200 Grade 0, 0402|R77|CMP-0026754-1|RMCF0402FT10K0|1|Altium Vault - TI|Stackpole Electronics Inc|Y|Digi-Key|{URL}{URL.TEXT}RMCF0402FT10K0CT-ND{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
242|Fitted|RES, 10.0 k, 1%, 0.063 W, AEC-Q200 Grade 0, 0402|R78|CMP-0026754-1|RMCF0402FT10K0|1|Altium Vault - TI|Stackpole Electronics Inc|Y|Digi-Key|{URL}{URL.TEXT}RMCF0402FT10K0CT-ND{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
243|Fitted|RES, 10.0 k, 1%, 0.063 W, AEC-Q200 Grade 0, 0402|R79|CMP-0026754-1|RMCF0402FT10K0|1|Altium Vault - TI|Stackpole Electronics Inc|Y|Digi-Key|{URL}{URL.TEXT}RMCF0402FT10K0CT-ND{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
244|Fitted|RES, 10.0 k, 1%, 0.063 W, AEC-Q200 Grade 0, 0402|R80|CMP-0026754-1|RMCF0402FT10K0|1|Altium Vault - TI|Stackpole Electronics Inc|Y|Digi-Key|{URL}{URL.TEXT}RMCF0402FT10K0CT-ND{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
245|Fitted|RES, 33.0, 1%, 0.063 W, AEC-Q200 Grade 0, 0402|R81|CMP-0026759-1|RMCF0402FT33R0|1|Altium Vault - TI|Stackpole Electronics Inc|Y|Digi-Key|{URL}{URL.TEXT}RMCF0402FT33R0CT-ND{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
246|Fitted|RES, 33.0, 1%, 0.063 W, AEC-Q200 Grade 0, 0402|R82|CMP-0026759-1|RMCF0402FT33R0|1|Altium Vault - TI|Stackpole Electronics Inc|Y|Digi-Key|{URL}{URL.TEXT}RMCF0402FT33R0CT-ND{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
247|Fitted|RES, 33.0, 1%, 0.063 W, AEC-Q200 Grade 0, 0402|R83|CMP-0026759-1|RMCF0402FT33R0|1|Altium Vault - TI|Stackpole Electronics Inc|Y|Digi-Key|{URL}{URL.TEXT}RMCF0402FT33R0CT-ND{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
248|Fitted|RES, 33.0, 1%, 0.063 W, AEC-Q200 Grade 0, 0402|R84|CMP-0026759-1|RMCF0402FT33R0|1|Altium Vault - TI|Stackpole Electronics Inc|Y|Digi-Key|{URL}{URL.TEXT}RMCF0402FT33R0CT-ND{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
249|Fitted|RES, 0, 5%, 0.1 W, AEC-Q200 Grade 0, 0603|R85|CMP-0025697-4|CRCW06030000Z0EA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-0.0GCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8014{URL.TIP}Supplier
250|Fitted|RES, 1.00 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R86|CMP-0022109-5|CRCW06031K00FKEA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-1.00KHCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8015{URL.TIP}Supplier
251|Fitted|RES, 10.0 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R87|CMP-0023341-3|RMCF0603FT10K0|1|Altium Vault - TI|Stackpole Electronics Inc|Y|Digi-Key|{URL}{URL.TEXT}RMCF0603FT10K0CT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}78Y4027{URL.TIP}Supplier
252|Fitted|RES, 1.00 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R88|CMP-0022109-5|CRCW06031K00FKEA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-1.00KHCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8015{URL.TIP}Supplier
253|Fitted|RES, 1.00 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R89|CMP-0022109-5|CRCW06031K00FKEA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-1.00KHCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8015{URL.TIP}Supplier
254|Fitted|RES, 2.20 k, 1%, 0.1 W, 0603|R90|CMP-0022986-5|RC0603FR-072K2L|1|Altium Vault - TI|Yageo|Y|Digi-Key|{URL}{URL.TEXT}311-2.20KHRCT-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}603-RC0603FR-072K2L{URL.TIP}Supplier
255|Fitted|RES, 0, 5%, 0.1 W, AEC-Q200 Grade 0, 0603|R91|CMP-0025697-4|CRCW06030000Z0EA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-0.0GCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8014{URL.TIP}Supplier
256|Fitted|RES, 51.0, 1%, 0.1 W, 0603|R92|CMP-0023169-5|RC0603FR-0751RL|1|Altium Vault - TI|Yageo|Y|Digi-Key|{URL}{URL.TEXT}311-51.0HRCT-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}603-RC0603FR-0751RL{URL.TIP}Supplier
257|Fitted|RES, 0, 5%, 0.1 W, AEC-Q200 Grade 0, 0603|R93|CMP-0025697-4|CRCW06030000Z0EA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-0.0GCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8014{URL.TIP}Supplier
258|Fitted|RES, 1.00 M, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R94|CMP-0022138-4|CRCW06031M00FKEA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-1.00MHCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8053{URL.TIP}Supplier
259|Fitted|RES, 10.0 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R95|CMP-0023341-3|RMCF0603FT10K0|1|Altium Vault - TI|Stackpole Electronics Inc|Y|Digi-Key|{URL}{URL.TEXT}RMCF0603FT10K0CT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}78Y4027{URL.TIP}Supplier
260|Fitted|RES, 10.0 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R96|CMP-0023341-3|RMCF0603FT10K0|1|Altium Vault - TI|Stackpole Electronics Inc|Y|Digi-Key|{URL}{URL.TEXT}RMCF0603FT10K0CT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}78Y4027{URL.TIP}Supplier
261|Fitted|RES, 10.0 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R97|CMP-0023341-3|RMCF0603FT10K0|1|Altium Vault - TI|Stackpole Electronics Inc|Y|Digi-Key|{URL}{URL.TEXT}RMCF0603FT10K0CT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}78Y4027{URL.TIP}Supplier
262|Fitted|RES, 100, 1%, 0.1 W, 0603|R98|CMP-0022736-4|RC0603FR-07100RL|1|Altium Vault - TI|Yageo|Y|Digi-Key|{URL}{URL.TEXT}311-100HRCT-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}603-RC0603FR-07100RL{URL.TIP}Supplier
263|Fitted|RES, 4.87 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R99|CMP-0022457-4|CRCW06034K87FKEA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-4.87KHCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8498{URL.TIP}Supplier
264|Fitted|RES, 10.0 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R100|CMP-0023341-3|RMCF0603FT10K0|1|Altium Vault - TI|Stackpole Electronics Inc|Y|Digi-Key|{URL}{URL.TEXT}RMCF0603FT10K0CT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}78Y4027{URL.TIP}Supplier
265|Fitted|RES, 1.00 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R101|CMP-0022109-5|CRCW06031K00FKEA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-1.00KHCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8015{URL.TIP}Supplier
266|Fitted|RES, 0, 5%, 0.1 W, AEC-Q200 Grade 0, 0603|R102|CMP-0025697-4|CRCW06030000Z0EA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-0.0GCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8014{URL.TIP}Supplier
267|Fitted|RES, 1.00 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R103|CMP-0022109-5|CRCW06031K00FKEA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-1.00KHCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8015{URL.TIP}Supplier
268|Fitted|RES, 0, 5%, 0.063 W, 0402|R104|CMP-0027004-2|RC0402JR-070RL|1|Altium Vault - TI|Yageo America|Y|Digi-Key|{URL}{URL.TEXT}311-0.0JRCT-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}603-RC0402JR-070RL{URL.TIP}Supplier
269|Fitted|RES, 1.00 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R105|CMP-0022109-5|CRCW06031K00FKEA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-1.00KHCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8015{URL.TIP}Supplier
270|Fitted|RES, 1.00 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R106|CMP-0022109-5|CRCW06031K00FKEA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-1.00KHCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8015{URL.TIP}Supplier
271|Fitted|RES, 2.0 k, 5%, 0.063 W, AEC-Q200 Grade 0, 0402|R107|CMP-0026889-5|CRCW04022K00JNED|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-2.0KJCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}59M6709{URL.TIP}Supplier
272|Fitted|RES, 47.0 k, 1%, 0.1 W, 0603|R108|CMP-0023133-5|RC0603FR-0747KL|1|Altium Vault - TI|Yageo|Y|Digi-Key|{URL}{URL.TEXT}311-47.0KHRCT-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}603-RC0603FR-0747KL{URL.TIP}Supplier
273|Fitted|RES, 523 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R109|CMP-0022484-4|CRCW0603523KFKEA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-523KHCT-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}71-CRCW0603-523K-E3{URL.TIP}Supplier
274|Fitted|RES, 31.6 k, 1%, 0.1 W, 0603|R110|CMP-0023026-5|RC0603FR-0731K6L|1|Altium Vault - TI|Yageo|Y|Digi-Key|{URL}{URL.TEXT}311-31.6KHRCT-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}603-RC0603FR-0731K6L{URL.TIP}Supplier
275|Fitted|RES, 47.0 k, 1%, 0.1 W, 0603|R111|CMP-0023133-5|RC0603FR-0747KL|1|Altium Vault - TI|Yageo|Y|Digi-Key|{URL}{URL.TEXT}311-47.0KHRCT-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}603-RC0603FR-0747KL{URL.TIP}Supplier
276|Fitted|RES, 10.0 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R112|CMP-0021998-4|CRCW060310K0FKEA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-10.0KHCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8062{URL.TIP}Supplier
277|Fitted|RES, 4.7, 5%, 0.1 W, AEC-Q200 Grade 0, 0603|R113|CMP-0025821-4|CRCW06034R70JNEA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-4.7GCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}59M6813{URL.TIP}Supplier
278|Fitted|RES, 133 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R114|CMP-0022038-4|CRCW0603133KFKEA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-133KHCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8129{URL.TIP}Supplier
279|Fitted|RES, 52.3 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R115|CMP-0022486-4|CRCW060352K3FKEA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-52.3KHCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8601{URL.TIP}Supplier
280|Fitted|RES, 95.3 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R117|CMP-0022659-4|CRCW060395K3FKEA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-95.3KHCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8783{URL.TIP}Supplier
281|Fitted|RES, 10.0 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R118|CMP-0021998-4|CRCW060310K0FKEA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-10.0KHCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8062{URL.TIP}Supplier
282|Fitted|RES, 71.5 k, 1%, 0.1 W, AEC-Q200 Grade 0, 0603|R119|CMP-0022581-4|CRCW060371K5FKEA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-71.5KHCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8699{URL.TIP}Supplier
283|Fitted|RES, 47.0 k, 1%, 0.1 W, 0603|R121|CMP-0023133-5|RC0603FR-0747KL|1|Altium Vault - TI|Yageo|Y|Digi-Key|{URL}{URL.TEXT}311-47.0KHRCT-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}603-RC0603FR-0747KL{URL.TIP}Supplier
284|Fitted|RES, 0, 5%, 0.1 W, AEC-Q200 Grade 0, 0603|R122|CMP-0025697-4|CRCW06030000Z0EA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-0.0GCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8014{URL.TIP}Supplier
285|Fitted|RES, 0, 5%, 0.1 W, AEC-Q200 Grade 0, 0603|R123|CMP-0025697-4|CRCW06030000Z0EA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-0.0GCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8014{URL.TIP}Supplier
286|Fitted|RES, 0, 5%, 0.1 W, AEC-Q200 Grade 0, 0603|R125|CMP-0025697-4|CRCW06030000Z0EA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-0.0GCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8014{URL.TIP}Supplier
287|Fitted|RES, 0, 5%, 0.1 W, AEC-Q200 Grade 0, 0603|R126|CMP-0025697-4|CRCW06030000Z0EA|1|Altium Vault - TI|Vishay-Dale|E|Digi-Key|{URL}{URL.TEXT}541-0.0GCT-ND{URL.TIP}Supplier|Newark|{URL}{URL.TEXT}52K8014{URL.TIP}Supplier
288|Fitted|Thermistor NTC, 100k ohm, 5%, 0603|RT1|CMP-0002534-3|NCP18WF104J03RB|1|Altium Vault - TI|MuRata|Y|Digi-Key|{URL}{URL.TEXT}490-2430-1-ND{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
289|Fitted|Switch, SPST, 0.05 A, 12 VDC, SMD|S1|CMP-0002328-1|1188E-1K2-V-TR|1|Altium Vault - TI|Diptronics|Y||{URL}{URL.TEXT}{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
290|Fitted|Terminal, Turret, TH, Double|TP1|CMP-0055120-1|1593-2|1|Altium Vault - TI|Keystone|Y|Digi-Key|{URL}{URL.TEXT}36-1593-2-ND{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
291|Fitted|Terminal, Turret, TH, Double|TP6|CMP-0055113-1|1502-2|1|Altium Vault - TI|Keystone|Y|Digi-Key|{URL}{URL.TEXT}36-1502-2-ND{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
292|Fitted|Dual Channel Constant Voltage and Constant Current Controller with SPI Interface, RHM0032A (VQFNP-32)|U1|CMP-0084188-2|TPS92682QRHMQ1|1|Altium Vault - TI|Texas Instruments|||{URL}{URL.TEXT}{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
293|Fitted|4.5 to 65-V Input Dual 1.6-A Synchronous Buck LED Driver with SPI Control, DAD0032A (HTSSOP-32)|U2|CMP-0082684-2|TPS92520QDADQ1|1|Altium Vault - TI|Texas Instruments|||{URL}{URL.TEXT}{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
294|Fitted|4.5 to 65-V Input Dual 1.6-A Synchronous Buck LED Driver with SPI Control, DAD0032A (HTSSOP-32)|U3|CMP-0082684-2|TPS92520QDADQ1|1|Altium Vault - TI|Texas Instruments|||{URL}{URL.TEXT}{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
295|Fitted|Automotive Fault Protected CAN Transceiver With Flexible Data-Rate, D0008A (SOIC-8)|U4|CMP-0075994-1|TCAN1042VDRQ1|1|Altium Vault - TI|Texas Instruments|Y||{URL}{URL.TEXT}{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
296|Fitted|Automotive Fault Protected CAN Transceiver With Flexible Data-Rate, D0008A (SOIC-8)|U5|CMP-0075994-1|TCAN1042VDRQ1|1|Altium Vault - TI|Texas Instruments|Y||{URL}{URL.TEXT}{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
297|Fitted|Automotive 3.5V to 60V, 1.5A Step Down SWIFT(TM) Converter with Eco-Mode(TM), DGQ0010D (VSSOP-10)|U6|CMP-0074018-2|TPS57160QDGQRQ1|1|Altium Vault - TI|Texas Instruments|Y||{URL}{URL.TEXT}{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
298|Fitted|Dual 2.0A, High Frequency Synchronous Step-Down DC-DC  Regulator, PWP0020A (HTSSOP-20)|U7|CMP-0066062-3|LM26420Q0XMHX/NOPB|1|Altium Vault - TI|Texas Instruments|Y||{URL}{URL.TEXT}{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
299|Fitted|MSP432E401YTPDT, PDT0128A (TQFP-128)|U10|CMP-0077953-1|MSP432E401YTPDT|1|Altium Vault - TI|Texas Instruments|||{URL}{URL.TEXT}{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
300|Fitted|Crystal, 32.768 kHz,  SMD|Y1|CMP-0004653-5|CMR200T-32.768KDZY-UT|1|Altium Vault - TI|Citizen FineDevice|Y|Mouser|{URL}{URL.TEXT}695-CMR200T32.7KY-U{URL.TIP}Supplier|Farnell|{URL}{URL.TEXT}1703589RL{URL.TIP}Supplier
301|Fitted|Crystal, 25 MHz, 8pF, SMD|Y2|CMP-0004652-3|NX3225GA-25.000M-STD-CRG-2|1|Altium Vault - TI|NDK|Y|Digi-Key|{URL}{URL.TEXT}644-1259-1-ND{URL.TIP}Supplier||{URL}{URL.TEXT}{URL.TIP}Supplier
302|Not Fitted|RES, 0.02, 1%, 1 W, 2010|R19|CMP-0016560-2|WSL2010R0200FEA18|0|Altium Vault - TI|Vishay-Dale|Y|Digi-Key|{URL}{URL.TEXT}WSLF-.02CT-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}71-WSL2010R0200FEA18{URL.TIP}Supplier
303|Not Fitted|RES, 0.02, 1%, 1 W, 2010|R26|CMP-0016560-2|WSL2010R0200FEA18|0|Altium Vault - TI|Vishay-Dale|Y|Digi-Key|{URL}{URL.TEXT}WSLF-.02CT-ND{URL.TIP}Supplier|Mouser|{URL}{URL.TEXT}71-WSL2010R0200FEA18{URL.TIP}Supplier
