DRC Rules Export File for PCB: \\dfrs40\industrial_systems\Motor Drives\1_TIDAs\TIDA-00913_Shunt_based_Phase_Current_Sensing_with_48V_3-Phase_Inverters\DESIGN\TIDA-00913_revE1\TIDA-00913.PcbDoc
RuleKind=Clearance|RuleName=Clearance_Keepouts|Scope=Board|Minimum=0.00
RuleKind=Clearance|RuleName=Clearance_Poly|Scope=Board|Minimum=25.00
RuleKind=Clearance|RuleName=Clearance|Scope=Board|Minimum=7.87
RuleKind=Width|RuleName=Width|Scope=Board|Minimum=6.00
RuleKind=SolderMaskExpansion|RuleName=SolderMaskExpansion|Scope=Board|Minimum=1.97
RuleKind=ShortCircuit|RuleName=ShortCircuit|Scope=Board|Allowed=0
RuleKind=MinimumAnnularRing|RuleName=MinimumAnnularRing_ThermalPadVias|Scope=Board|Minimum=5.91
RuleKind=MinimumAnnularRing|RuleName=MinimumAnnularRing|Scope=Board|Minimum=5.50
